From d4cbe80db468dcfaa058f9f00a332784e5dff316 Mon Sep 17 00:00:00 2001
From: Suman Anna <s-anna@ti.com>
Date: Thu, 10 Oct 2013 21:15:35 +0000
Subject: ARM: dts: AM33XX: Add hwspinlock node

Add the hwspinlock device tree node for AM33xx family
of SoCs.

Signed-off-by: Suman Anna <s-anna@ti.com>
Signed-off-by: Tony Lindgren <tony@atomide.com>
---
--- a/arch/arm/boot/dts/am33xx.dtsi
+++ b/arch/arm/boot/dts/am33xx.dtsi
@@ -278,6 +278,12 @@
 			status = "disabled";
 		};
 
+		hwspinlock: spinlock@480ca000 {
+			compatible = "ti,omap4-hwspinlock";
+			reg = <0x480ca000 0x1000>;
+			ti,hwmods = "spinlock";
+		};
+
 		wdt2: wdt@44e35000 {
 			compatible = "ti,omap3-wdt";
 			ti,hwmods = "wd_timer2";
