From de1defdad7554d6ba885a6d3dc55105e01e9a07e Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Thu, 2 May 2013 14:59:01 +0200
Subject: [PATCH 27/33] mmc: MIPS: ralink: add sdhci for mt7620a SoC

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/mmc/host/Kconfig        |   11 +
 drivers/mmc/host/Makefile       |    1 +
 drivers/mmc/host/mt6575_sd.h    | 1068 ++++++++++++++++++
 drivers/mmc/host/sdhci-mt7620.c | 2314 +++++++++++++++++++++++++++++++++++++++
 4 files changed, 3394 insertions(+)
 create mode 100644 drivers/mmc/host/mt6575_sd.h
 create mode 100644 drivers/mmc/host/sdhci-mt7620.c

--- a/drivers/mmc/host/Kconfig
+++ b/drivers/mmc/host/Kconfig
@@ -260,6 +260,17 @@ config MMC_SDHCI_BCM2835
 
 	  If unsure, say N.
 
+config MMC_SDHCI_MT7620
+	tristate "SDHCI platform support for the MT7620 SD/MMC Controller"
+	depends on SOC_MT7620
+	depends on MMC_SDHCI_PLTFM
+	select MMC_SDHCI_IO_ACCESSORS
+	help
+	  This selects the BCM2835 SD/MMC controller. If you have a BCM2835
+	  platform with SD or MMC devices, say Y or M here.
+
+	  If unsure, say N.
+
 config MMC_OMAP
 	tristate "TI OMAP Multimedia Card Interface support"
 	depends on ARCH_OMAP
--- a/drivers/mmc/host/Makefile
+++ b/drivers/mmc/host/Makefile
@@ -62,6 +62,7 @@ obj-$(CONFIG_MMC_SDHCI_TEGRA)		+= sdhci-
 obj-$(CONFIG_MMC_SDHCI_OF_ESDHC)	+= sdhci-of-esdhc.o
 obj-$(CONFIG_MMC_SDHCI_OF_HLWD)		+= sdhci-of-hlwd.o
 obj-$(CONFIG_MMC_SDHCI_BCM2835)		+= sdhci-bcm2835.o
+obj-$(CONFIG_MMC_SDHCI_MT7620)		+= sdhci-mt7620.o
 
 ifeq ($(CONFIG_CB710_DEBUG),y)
 	CFLAGS-cb710-mmc	+= -DDEBUG
--- /dev/null
+++ b/drivers/mmc/host/mt6575_sd.h
@@ -0,0 +1,1068 @@
+/* Copyright Statement:
+ *
+ * This software/firmware and related documentation ("MediaTek Software") are
+ * protected under relevant copyright laws. The information contained herein
+ * is confidential and proprietary to MediaTek Inc. and/or its licensors.
+ * Without the prior written permission of MediaTek inc. and/or its licensors,
+ * any reproduction, modification, use or disclosure of MediaTek Software,
+ * and information contained herein, in whole or in part, shall be strictly prohibited.
+ */
+/* MediaTek Inc. (C) 2010. All rights reserved.
+ *
+ * BY OPENING THIS FILE, RECEIVER HEREBY UNEQUIVOCALLY ACKNOWLEDGES AND AGREES
+ * THAT THE SOFTWARE/FIRMWARE AND ITS DOCUMENTATIONS ("MEDIATEK SOFTWARE")
+ * RECEIVED FROM MEDIATEK AND/OR ITS REPRESENTATIVES ARE PROVIDED TO RECEIVER ON
+ * AN "AS-IS" BASIS ONLY. MEDIATEK EXPRESSLY DISCLAIMS ANY AND ALL WARRANTIES,
+ * EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE OR NONINFRINGEMENT.
+ * NEITHER DOES MEDIATEK PROVIDE ANY WARRANTY WHATSOEVER WITH RESPECT TO THE
+ * SOFTWARE OF ANY THIRD PARTY WHICH MAY BE USED BY, INCORPORATED IN, OR
+ * SUPPLIED WITH THE MEDIATEK SOFTWARE, AND RECEIVER AGREES TO LOOK ONLY TO SUCH
+ * THIRD PARTY FOR ANY WARRANTY CLAIM RELATING THERETO. RECEIVER EXPRESSLY ACKNOWLEDGES
+ * THAT IT IS RECEIVER'S SOLE RESPONSIBILITY TO OBTAIN FROM ANY THIRD PARTY ALL PROPER LICENSES
+ * CONTAINED IN MEDIATEK SOFTWARE. MEDIATEK SHALL ALSO NOT BE RESPONSIBLE FOR ANY MEDIATEK
+ * SOFTWARE RELEASES MADE TO RECEIVER'S SPECIFICATION OR TO CONFORM TO A PARTICULAR
+ * STANDARD OR OPEN FORUM. RECEIVER'S SOLE AND EXCLUSIVE REMEDY AND MEDIATEK'S ENTIRE AND
+ * CUMULATIVE LIABILITY WITH RESPECT TO THE MEDIATEK SOFTWARE RELEASED HEREUNDER WILL BE,
+ * AT MEDIATEK'S OPTION, TO REVISE OR REPLACE THE MEDIATEK SOFTWARE AT ISSUE,
+ * OR REFUND ANY SOFTWARE LICENSE FEES OR SERVICE CHARGE PAID BY RECEIVER TO
+ * MEDIATEK FOR SUCH MEDIATEK SOFTWARE AT ISSUE.
+ *
+ * The following software/firmware and/or related documentation ("MediaTek Software")
+ * have been modified by MediaTek Inc. All revisions are subject to any receiver's
+ * applicable license agreements with MediaTek Inc.
+ */
+
+#ifndef MT6575_SD_H
+#define MT6575_SD_H
+
+#include <linux/bitops.h>
+#include <linux/mmc/host.h>
+
+// #include <mach/mt6575_reg_base.h> /* --- by chhung */
+
+typedef void (*sdio_irq_handler_t)(void*);  /* external irq handler */
+typedef void (*pm_callback_t)(pm_message_t state, void *data);
+
+#define MSDC_CD_PIN_EN      (1 << 0)  /* card detection pin is wired   */
+#define MSDC_WP_PIN_EN      (1 << 1)  /* write protection pin is wired */
+#define MSDC_RST_PIN_EN     (1 << 2)  /* emmc reset pin is wired       */
+#define MSDC_SDIO_IRQ       (1 << 3)  /* use internal sdio irq (bus)   */
+#define MSDC_EXT_SDIO_IRQ   (1 << 4)  /* use external sdio irq         */
+#define MSDC_REMOVABLE      (1 << 5)  /* removable slot                */
+#define MSDC_SYS_SUSPEND    (1 << 6)  /* suspended by system           */
+#define MSDC_HIGHSPEED      (1 << 7)  /* high-speed mode support       */
+#define MSDC_UHS1           (1 << 8)  /* uhs-1 mode support            */
+#define MSDC_DDR            (1 << 9)  /* ddr mode support              */
+#define MSDC_SPE            (1 << 10)  /* special support              */
+#define MSDC_INTERNAL_CLK   (1 << 11)  /* Force Internal clock */
+#define MSDC_TABDRV	(1 << 12)  /* TABLET */
+
+
+#define MSDC_SMPL_RISING    (0)
+#define MSDC_SMPL_FALLING   (1)
+
+#define MSDC_CMD_PIN        (0)
+#define MSDC_DAT_PIN        (1)
+#define MSDC_CD_PIN         (2)
+#define MSDC_WP_PIN         (3)
+#define MSDC_RST_PIN        (4)
+
+enum {
+    MSDC_CLKSRC_26MHZ = 0,
+    MSDC_CLKSRC_197MHZ = 1,
+    MSDC_CLKSRC_208MHZ = 2
+};
+
+struct msdc_hw {
+	unsigned char  clk_src;          /* host clock source */
+	unsigned char  cmd_edge;         /* command latch edge */
+	unsigned char  data_edge;        /* data latch edge */
+	unsigned char  clk_drv;          /* clock pad driving */
+	unsigned char  cmd_drv;          /* command pad driving */
+	unsigned char  dat_drv;          /* data pad driving */
+	unsigned long  flags;            /* hardware capability flags */
+	unsigned long  data_pins;        /* data pins */
+	unsigned long  data_offset;      /* data address offset */
+
+	/* config gpio pull mode */
+	void (*config_gpio_pin)(int type, int pull);
+
+	/* external power control for card */
+	void (*ext_power_on)(void);
+	void (*ext_power_off)(void);
+
+	/* external sdio irq operations */
+	void (*request_sdio_eirq)(sdio_irq_handler_t sdio_irq_handler, void *data);
+	void (*enable_sdio_eirq)(void);
+	void (*disable_sdio_eirq)(void);
+
+	/* external cd irq operations */
+	void (*request_cd_eirq)(sdio_irq_handler_t cd_irq_handler, void *data);
+	void (*enable_cd_eirq)(void);
+	void (*disable_cd_eirq)(void);
+	int  (*get_cd_status)(void);
+
+	/* power management callback for external module */
+	void (*register_pm)(pm_callback_t pm_cb, void *data);
+};
+
+extern struct msdc_hw msdc0_hw;
+extern struct msdc_hw msdc1_hw;
+extern struct msdc_hw msdc2_hw;
+extern struct msdc_hw msdc3_hw;
+
+    
+/*--------------------------------------------------------------------------*/
+/* Common Macro                                                             */
+/*--------------------------------------------------------------------------*/
+#define REG_ADDR(x)                 ((volatile u32*)(base + OFFSET_##x))
+
+/*--------------------------------------------------------------------------*/
+/* Common Definition                                                        */
+/*--------------------------------------------------------------------------*/
+#define MSDC_FIFO_SZ            (128)
+#define MSDC_FIFO_THD           (64)  // (128)
+#define MSDC_NUM                (4)
+
+#define MSDC_MS                 (0)
+#define MSDC_SDMMC              (1)
+
+#define MSDC_MODE_UNKNOWN       (0)
+#define MSDC_MODE_PIO           (1)
+#define MSDC_MODE_DMA_BASIC     (2)
+#define MSDC_MODE_DMA_DESC      (3)
+#define MSDC_MODE_DMA_ENHANCED  (4)
+#define MSDC_MODE_MMC_STREAM    (5)
+
+#define MSDC_BUS_1BITS          (0)
+#define MSDC_BUS_4BITS          (1)
+#define MSDC_BUS_8BITS          (2)
+
+#define MSDC_BRUST_8B           (3)
+#define MSDC_BRUST_16B          (4)
+#define MSDC_BRUST_32B          (5)
+#define MSDC_BRUST_64B          (6)
+
+#define MSDC_PIN_PULL_NONE      (0)
+#define MSDC_PIN_PULL_DOWN      (1)
+#define MSDC_PIN_PULL_UP        (2)
+#define MSDC_PIN_KEEP           (3)
+
+#define MSDC_MAX_SCLK           (48000000) /* +/- by chhung */
+#define MSDC_MIN_SCLK           (260000)
+
+#define MSDC_AUTOCMD12          (0x0001)
+#define MSDC_AUTOCMD23          (0x0002)
+#define MSDC_AUTOCMD19          (0x0003)
+
+#define MSDC_EMMC_BOOTMODE0     (0)     /* Pull low CMD mode */
+#define MSDC_EMMC_BOOTMODE1     (1)     /* Reset CMD mode */
+
+enum {
+    RESP_NONE = 0,
+    RESP_R1,
+    RESP_R2,
+    RESP_R3,
+    RESP_R4,
+    RESP_R5,
+    RESP_R6,
+    RESP_R7,
+    RESP_R1B
+};
+
+/*--------------------------------------------------------------------------*/
+/* Register Offset                                                          */
+/*--------------------------------------------------------------------------*/
+#define OFFSET_MSDC_CFG         (0x0)
+#define OFFSET_MSDC_IOCON       (0x04)
+#define OFFSET_MSDC_PS          (0x08)
+#define OFFSET_MSDC_INT         (0x0c)
+#define OFFSET_MSDC_INTEN       (0x10)
+#define OFFSET_MSDC_FIFOCS      (0x14)
+#define OFFSET_MSDC_TXDATA      (0x18)
+#define OFFSET_MSDC_RXDATA      (0x1c)
+#define OFFSET_SDC_CFG          (0x30)
+#define OFFSET_SDC_CMD          (0x34)
+#define OFFSET_SDC_ARG          (0x38)
+#define OFFSET_SDC_STS          (0x3c)
+#define OFFSET_SDC_RESP0        (0x40)
+#define OFFSET_SDC_RESP1        (0x44)
+#define OFFSET_SDC_RESP2        (0x48)
+#define OFFSET_SDC_RESP3        (0x4c)
+#define OFFSET_SDC_BLK_NUM      (0x50)
+#define OFFSET_SDC_CSTS         (0x58)
+#define OFFSET_SDC_CSTS_EN      (0x5c)
+#define OFFSET_SDC_DCRC_STS     (0x60)
+#define OFFSET_EMMC_CFG0        (0x70)
+#define OFFSET_EMMC_CFG1        (0x74)
+#define OFFSET_EMMC_STS         (0x78)
+#define OFFSET_EMMC_IOCON       (0x7c)
+#define OFFSET_SDC_ACMD_RESP    (0x80)
+#define OFFSET_SDC_ACMD19_TRG   (0x84)
+#define OFFSET_SDC_ACMD19_STS   (0x88)
+#define OFFSET_MSDC_DMA_SA      (0x90)
+#define OFFSET_MSDC_DMA_CA      (0x94)
+#define OFFSET_MSDC_DMA_CTRL    (0x98)
+#define OFFSET_MSDC_DMA_CFG     (0x9c)
+#define OFFSET_MSDC_DBG_SEL     (0xa0)
+#define OFFSET_MSDC_DBG_OUT     (0xa4)
+#define OFFSET_MSDC_PATCH_BIT   (0xb0)
+#define OFFSET_MSDC_PATCH_BIT1  (0xb4)
+#define OFFSET_MSDC_PAD_CTL0    (0xe0)
+#define OFFSET_MSDC_PAD_CTL1    (0xe4)
+#define OFFSET_MSDC_PAD_CTL2    (0xe8)
+#define OFFSET_MSDC_PAD_TUNE    (0xec)
+#define OFFSET_MSDC_DAT_RDDLY0  (0xf0)
+#define OFFSET_MSDC_DAT_RDDLY1  (0xf4)
+#define OFFSET_MSDC_HW_DBG      (0xf8)
+#define OFFSET_MSDC_VERSION     (0x100)
+#define OFFSET_MSDC_ECO_VER     (0x104)
+
+/*--------------------------------------------------------------------------*/
+/* Register Address                                                         */
+/*--------------------------------------------------------------------------*/
+
+/* common register */
+#define MSDC_CFG                REG_ADDR(MSDC_CFG)
+#define MSDC_IOCON              REG_ADDR(MSDC_IOCON)
+#define MSDC_PS                 REG_ADDR(MSDC_PS)
+#define MSDC_INT                REG_ADDR(MSDC_INT)
+#define MSDC_INTEN              REG_ADDR(MSDC_INTEN)
+#define MSDC_FIFOCS             REG_ADDR(MSDC_FIFOCS)
+#define MSDC_TXDATA             REG_ADDR(MSDC_TXDATA)
+#define MSDC_RXDATA             REG_ADDR(MSDC_RXDATA)
+#define MSDC_PATCH_BIT0         REG_ADDR(MSDC_PATCH_BIT)
+
+/* sdmmc register */
+#define SDC_CFG                 REG_ADDR(SDC_CFG)
+#define SDC_CMD                 REG_ADDR(SDC_CMD)
+#define SDC_ARG                 REG_ADDR(SDC_ARG)
+#define SDC_STS                 REG_ADDR(SDC_STS)
+#define SDC_RESP0               REG_ADDR(SDC_RESP0)
+#define SDC_RESP1               REG_ADDR(SDC_RESP1)
+#define SDC_RESP2               REG_ADDR(SDC_RESP2)
+#define SDC_RESP3               REG_ADDR(SDC_RESP3)
+#define SDC_BLK_NUM             REG_ADDR(SDC_BLK_NUM)
+#define SDC_CSTS                REG_ADDR(SDC_CSTS)
+#define SDC_CSTS_EN             REG_ADDR(SDC_CSTS_EN)
+#define SDC_DCRC_STS            REG_ADDR(SDC_DCRC_STS)
+
+/* emmc register*/
+#define EMMC_CFG0               REG_ADDR(EMMC_CFG0)
+#define EMMC_CFG1               REG_ADDR(EMMC_CFG1)
+#define EMMC_STS                REG_ADDR(EMMC_STS)
+#define EMMC_IOCON              REG_ADDR(EMMC_IOCON)
+
+/* auto command register */
+#define SDC_ACMD_RESP           REG_ADDR(SDC_ACMD_RESP)
+#define SDC_ACMD19_TRG          REG_ADDR(SDC_ACMD19_TRG)
+#define SDC_ACMD19_STS          REG_ADDR(SDC_ACMD19_STS)
+
+/* dma register */
+#define MSDC_DMA_SA             REG_ADDR(MSDC_DMA_SA)
+#define MSDC_DMA_CA             REG_ADDR(MSDC_DMA_CA)
+#define MSDC_DMA_CTRL           REG_ADDR(MSDC_DMA_CTRL)
+#define MSDC_DMA_CFG            REG_ADDR(MSDC_DMA_CFG)
+
+/* pad ctrl register */
+#define MSDC_PAD_CTL0           REG_ADDR(MSDC_PAD_CTL0)
+#define MSDC_PAD_CTL1           REG_ADDR(MSDC_PAD_CTL1)
+#define MSDC_PAD_CTL2           REG_ADDR(MSDC_PAD_CTL2)
+
+/* data read delay */
+#define MSDC_DAT_RDDLY0         REG_ADDR(MSDC_DAT_RDDLY0)
+#define MSDC_DAT_RDDLY1         REG_ADDR(MSDC_DAT_RDDLY1)
+
+/* debug register */
+#define MSDC_DBG_SEL            REG_ADDR(MSDC_DBG_SEL)
+#define MSDC_DBG_OUT            REG_ADDR(MSDC_DBG_OUT)
+
+/* misc register */
+#define MSDC_PATCH_BIT          REG_ADDR(MSDC_PATCH_BIT)
+#define MSDC_PATCH_BIT1         REG_ADDR(MSDC_PATCH_BIT1)
+#define MSDC_PAD_TUNE           REG_ADDR(MSDC_PAD_TUNE)
+#define MSDC_HW_DBG             REG_ADDR(MSDC_HW_DBG)
+#define MSDC_VERSION            REG_ADDR(MSDC_VERSION)
+#define MSDC_ECO_VER            REG_ADDR(MSDC_ECO_VER) /* ECO Version */
+
+/*--------------------------------------------------------------------------*/
+/* Register Mask                                                            */
+/*--------------------------------------------------------------------------*/
+
+/* MSDC_CFG mask */
+#define MSDC_CFG_MODE           (0x1  << 0)     /* RW */
+#define MSDC_CFG_CKPDN          (0x1  << 1)     /* RW */
+#define MSDC_CFG_RST            (0x1  << 2)     /* RW */
+#define MSDC_CFG_PIO            (0x1  << 3)     /* RW */
+#define MSDC_CFG_CKDRVEN        (0x1  << 4)     /* RW */
+#define MSDC_CFG_BV18SDT        (0x1  << 5)     /* RW */
+#define MSDC_CFG_BV18PSS        (0x1  << 6)     /* R  */
+#define MSDC_CFG_CKSTB          (0x1  << 7)     /* R  */
+#define MSDC_CFG_CKDIV          (0xff << 8)     /* RW */
+#define MSDC_CFG_CKMOD          (0x3  << 16)    /* RW */
+
+/* MSDC_IOCON mask */
+#define MSDC_IOCON_SDR104CKS    (0x1  << 0)     /* RW */
+#define MSDC_IOCON_RSPL         (0x1  << 1)     /* RW */
+#define MSDC_IOCON_DSPL         (0x1  << 2)     /* RW */
+#define MSDC_IOCON_DDLSEL       (0x1  << 3)     /* RW */
+#define MSDC_IOCON_DDR50CKD     (0x1  << 4)     /* RW */
+#define MSDC_IOCON_DSPLSEL      (0x1  << 5)     /* RW */
+#define MSDC_IOCON_D0SPL        (0x1  << 16)    /* RW */
+#define MSDC_IOCON_D1SPL        (0x1  << 17)    /* RW */
+#define MSDC_IOCON_D2SPL        (0x1  << 18)    /* RW */
+#define MSDC_IOCON_D3SPL        (0x1  << 19)    /* RW */
+#define MSDC_IOCON_D4SPL        (0x1  << 20)    /* RW */
+#define MSDC_IOCON_D5SPL        (0x1  << 21)    /* RW */
+#define MSDC_IOCON_D6SPL        (0x1  << 22)    /* RW */
+#define MSDC_IOCON_D7SPL        (0x1  << 23)    /* RW */
+#define MSDC_IOCON_RISCSZ       (0x3  << 24)    /* RW */
+
+/* MSDC_PS mask */
+#define MSDC_PS_CDEN            (0x1  << 0)     /* RW */
+#define MSDC_PS_CDSTS           (0x1  << 1)     /* R  */
+#define MSDC_PS_CDDEBOUNCE      (0xf  << 12)    /* RW */
+#define MSDC_PS_DAT             (0xff << 16)    /* R  */
+#define MSDC_PS_CMD             (0x1  << 24)    /* R  */
+#define MSDC_PS_WP              (0x1UL<< 31)    /* R  */
+
+/* MSDC_INT mask */
+#define MSDC_INT_MMCIRQ         (0x1  << 0)     /* W1C */
+#define MSDC_INT_CDSC           (0x1  << 1)     /* W1C */
+#define MSDC_INT_ACMDRDY        (0x1  << 3)     /* W1C */
+#define MSDC_INT_ACMDTMO        (0x1  << 4)     /* W1C */
+#define MSDC_INT_ACMDCRCERR     (0x1  << 5)     /* W1C */
+#define MSDC_INT_DMAQ_EMPTY     (0x1  << 6)     /* W1C */
+#define MSDC_INT_SDIOIRQ        (0x1  << 7)     /* W1C */
+#define MSDC_INT_CMDRDY         (0x1  << 8)     /* W1C */
+#define MSDC_INT_CMDTMO         (0x1  << 9)     /* W1C */
+#define MSDC_INT_RSPCRCERR      (0x1  << 10)    /* W1C */
+#define MSDC_INT_CSTA           (0x1  << 11)    /* R */
+#define MSDC_INT_XFER_COMPL     (0x1  << 12)    /* W1C */
+#define MSDC_INT_DXFER_DONE     (0x1  << 13)    /* W1C */
+#define MSDC_INT_DATTMO         (0x1  << 14)    /* W1C */
+#define MSDC_INT_DATCRCERR      (0x1  << 15)    /* W1C */
+#define MSDC_INT_ACMD19_DONE    (0x1  << 16)    /* W1C */
+
+/* MSDC_INTEN mask */
+#define MSDC_INTEN_MMCIRQ       (0x1  << 0)     /* RW */
+#define MSDC_INTEN_CDSC         (0x1  << 1)     /* RW */
+#define MSDC_INTEN_ACMDRDY      (0x1  << 3)     /* RW */
+#define MSDC_INTEN_ACMDTMO      (0x1  << 4)     /* RW */
+#define MSDC_INTEN_ACMDCRCERR   (0x1  << 5)     /* RW */
+#define MSDC_INTEN_DMAQ_EMPTY   (0x1  << 6)     /* RW */
+#define MSDC_INTEN_SDIOIRQ      (0x1  << 7)     /* RW */
+#define MSDC_INTEN_CMDRDY       (0x1  << 8)     /* RW */
+#define MSDC_INTEN_CMDTMO       (0x1  << 9)     /* RW */
+#define MSDC_INTEN_RSPCRCERR    (0x1  << 10)    /* RW */
+#define MSDC_INTEN_CSTA         (0x1  << 11)    /* RW */
+#define MSDC_INTEN_XFER_COMPL   (0x1  << 12)    /* RW */
+#define MSDC_INTEN_DXFER_DONE   (0x1  << 13)    /* RW */
+#define MSDC_INTEN_DATTMO       (0x1  << 14)    /* RW */
+#define MSDC_INTEN_DATCRCERR    (0x1  << 15)    /* RW */
+#define MSDC_INTEN_ACMD19_DONE  (0x1  << 16)    /* RW */
+
+/* MSDC_FIFOCS mask */
+#define MSDC_FIFOCS_RXCNT       (0xff << 0)     /* R */
+#define MSDC_FIFOCS_TXCNT       (0xff << 16)    /* R */
+#define MSDC_FIFOCS_CLR         (0x1UL<< 31)    /* RW */
+
+/* SDC_CFG mask */
+#define SDC_CFG_SDIOINTWKUP     (0x1  << 0)     /* RW */
+#define SDC_CFG_INSWKUP         (0x1  << 1)     /* RW */
+#define SDC_CFG_BUSWIDTH        (0x3  << 16)    /* RW */
+#define SDC_CFG_SDIO            (0x1  << 19)    /* RW */
+#define SDC_CFG_SDIOIDE         (0x1  << 20)    /* RW */      
+#define SDC_CFG_INTATGAP        (0x1  << 21)    /* RW */
+#define SDC_CFG_DTOC            (0xffUL << 24)  /* RW */
+
+/* SDC_CMD mask */
+#define SDC_CMD_OPC             (0x3f << 0)     /* RW */
+#define SDC_CMD_BRK             (0x1  << 6)     /* RW */
+#define SDC_CMD_RSPTYP          (0x7  << 7)     /* RW */
+#define SDC_CMD_DTYP            (0x3  << 11)    /* RW */
+#define SDC_CMD_DTYP            (0x3  << 11)    /* RW */
+#define SDC_CMD_RW              (0x1  << 13)    /* RW */
+#define SDC_CMD_STOP            (0x1  << 14)    /* RW */
+#define SDC_CMD_GOIRQ           (0x1  << 15)    /* RW */
+#define SDC_CMD_BLKLEN          (0xfff<< 16)    /* RW */
+#define SDC_CMD_AUTOCMD         (0x3  << 28)    /* RW */
+#define SDC_CMD_VOLSWTH         (0x1  << 30)    /* RW */
+
+/* SDC_STS mask */
+#define SDC_STS_SDCBUSY         (0x1  << 0)     /* RW */
+#define SDC_STS_CMDBUSY         (0x1  << 1)     /* RW */
+#define SDC_STS_SWR_COMPL       (0x1  << 31)    /* RW */
+
+/* SDC_DCRC_STS mask */
+#define SDC_DCRC_STS_NEG        (0xf  << 8)     /* RO */
+#define SDC_DCRC_STS_POS        (0xff << 0)     /* RO */
+
+/* EMMC_CFG0 mask */
+#define EMMC_CFG0_BOOTSTART     (0x1  << 0)     /* W */
+#define EMMC_CFG0_BOOTSTOP      (0x1  << 1)     /* W */
+#define EMMC_CFG0_BOOTMODE      (0x1  << 2)     /* RW */
+#define EMMC_CFG0_BOOTACKDIS    (0x1  << 3)     /* RW */
+#define EMMC_CFG0_BOOTWDLY      (0x7  << 12)    /* RW */
+#define EMMC_CFG0_BOOTSUPP      (0x1  << 15)    /* RW */
+
+/* EMMC_CFG1 mask */
+#define EMMC_CFG1_BOOTDATTMC    (0xfffff << 0)  /* RW */
+#define EMMC_CFG1_BOOTACKTMC    (0xfffUL << 20) /* RW */
+
+/* EMMC_STS mask */
+#define EMMC_STS_BOOTCRCERR     (0x1  << 0)     /* W1C */
+#define EMMC_STS_BOOTACKERR     (0x1  << 1)     /* W1C */
+#define EMMC_STS_BOOTDATTMO     (0x1  << 2)     /* W1C */
+#define EMMC_STS_BOOTACKTMO     (0x1  << 3)     /* W1C */
+#define EMMC_STS_BOOTUPSTATE    (0x1  << 4)     /* R */
+#define EMMC_STS_BOOTACKRCV     (0x1  << 5)     /* W1C */
+#define EMMC_STS_BOOTDATRCV     (0x1  << 6)     /* R */
+
+/* EMMC_IOCON mask */
+#define EMMC_IOCON_BOOTRST      (0x1  << 0)     /* RW */
+
+/* SDC_ACMD19_TRG mask */
+#define SDC_ACMD19_TRG_TUNESEL  (0xf  << 0)     /* RW */
+
+/* MSDC_DMA_CTRL mask */
+#define MSDC_DMA_CTRL_START     (0x1  << 0)     /* W */
+#define MSDC_DMA_CTRL_STOP      (0x1  << 1)     /* W */
+#define MSDC_DMA_CTRL_RESUME    (0x1  << 2)     /* W */
+#define MSDC_DMA_CTRL_MODE      (0x1  << 8)     /* RW */
+#define MSDC_DMA_CTRL_LASTBUF   (0x1  << 10)    /* RW */
+#define MSDC_DMA_CTRL_BRUSTSZ   (0x7  << 12)    /* RW */
+#define MSDC_DMA_CTRL_XFERSZ    (0xffffUL << 16)/* RW */
+
+/* MSDC_DMA_CFG mask */
+#define MSDC_DMA_CFG_STS        (0x1  << 0)     /* R */
+#define MSDC_DMA_CFG_DECSEN     (0x1  << 1)     /* RW */
+#define MSDC_DMA_CFG_BDCSERR    (0x1  << 4)     /* R */
+#define MSDC_DMA_CFG_GPDCSERR   (0x1  << 5)     /* R */
+
+/* MSDC_PATCH_BIT mask */
+#define MSDC_PATCH_BIT_WFLSMODE (0x1  << 0)     /* RW */
+#define MSDC_PATCH_BIT_ODDSUPP  (0x1  << 1)     /* RW */
+#define MSDC_PATCH_BIT_CKGEN_CK (0x1  << 6)     /* E2: Fixed to 1 */
+#define MSDC_PATCH_BIT_IODSSEL  (0x1  << 16)    /* RW */
+#define MSDC_PATCH_BIT_IOINTSEL (0x1  << 17)    /* RW */
+#define MSDC_PATCH_BIT_BUSYDLY  (0xf  << 18)    /* RW */
+#define MSDC_PATCH_BIT_WDOD     (0xf  << 22)    /* RW */
+#define MSDC_PATCH_BIT_IDRTSEL  (0x1  << 26)    /* RW */
+#define MSDC_PATCH_BIT_CMDFSEL  (0x1  << 27)    /* RW */
+#define MSDC_PATCH_BIT_INTDLSEL (0x1  << 28)    /* RW */
+#define MSDC_PATCH_BIT_SPCPUSH  (0x1  << 29)    /* RW */
+#define MSDC_PATCH_BIT_DECRCTMO (0x1  << 30)    /* RW */
+
+/* MSDC_PATCH_BIT1 mask */
+#define MSDC_PATCH_BIT1_WRDAT_CRCS  (0x7 << 3)
+#define MSDC_PATCH_BIT1_CMD_RSP     (0x7 << 0)
+
+/* MSDC_PAD_CTL0 mask */
+#define MSDC_PAD_CTL0_CLKDRVN   (0x7  << 0)     /* RW */
+#define MSDC_PAD_CTL0_CLKDRVP   (0x7  << 4)     /* RW */
+#define MSDC_PAD_CTL0_CLKSR     (0x1  << 8)     /* RW */
+#define MSDC_PAD_CTL0_CLKPD     (0x1  << 16)    /* RW */
+#define MSDC_PAD_CTL0_CLKPU     (0x1  << 17)    /* RW */
+#define MSDC_PAD_CTL0_CLKSMT    (0x1  << 18)    /* RW */
+#define MSDC_PAD_CTL0_CLKIES    (0x1  << 19)    /* RW */
+#define MSDC_PAD_CTL0_CLKTDSEL  (0xf  << 20)    /* RW */
+#define MSDC_PAD_CTL0_CLKRDSEL  (0xffUL<< 24)   /* RW */
+
+/* MSDC_PAD_CTL1 mask */
+#define MSDC_PAD_CTL1_CMDDRVN   (0x7  << 0)     /* RW */
+#define MSDC_PAD_CTL1_CMDDRVP   (0x7  << 4)     /* RW */
+#define MSDC_PAD_CTL1_CMDSR     (0x1  << 8)     /* RW */
+#define MSDC_PAD_CTL1_CMDPD     (0x1  << 16)    /* RW */
+#define MSDC_PAD_CTL1_CMDPU     (0x1  << 17)    /* RW */
+#define MSDC_PAD_CTL1_CMDSMT    (0x1  << 18)    /* RW */
+#define MSDC_PAD_CTL1_CMDIES    (0x1  << 19)    /* RW */
+#define MSDC_PAD_CTL1_CMDTDSEL  (0xf  << 20)    /* RW */
+#define MSDC_PAD_CTL1_CMDRDSEL  (0xffUL<< 24)   /* RW */
+
+/* MSDC_PAD_CTL2 mask */
+#define MSDC_PAD_CTL2_DATDRVN   (0x7  << 0)     /* RW */
+#define MSDC_PAD_CTL2_DATDRVP   (0x7  << 4)     /* RW */
+#define MSDC_PAD_CTL2_DATSR     (0x1  << 8)     /* RW */
+#define MSDC_PAD_CTL2_DATPD     (0x1  << 16)    /* RW */
+#define MSDC_PAD_CTL2_DATPU     (0x1  << 17)    /* RW */
+#define MSDC_PAD_CTL2_DATIES    (0x1  << 19)    /* RW */
+#define MSDC_PAD_CTL2_DATSMT    (0x1  << 18)    /* RW */
+#define MSDC_PAD_CTL2_DATTDSEL  (0xf  << 20)    /* RW */
+#define MSDC_PAD_CTL2_DATRDSEL  (0xffUL<< 24)   /* RW */
+
+/* MSDC_PAD_TUNE mask */
+#define MSDC_PAD_TUNE_DATWRDLY  (0x1F << 0)     /* RW */
+#define MSDC_PAD_TUNE_DATRRDLY  (0x1F << 8)     /* RW */
+#define MSDC_PAD_TUNE_CMDRDLY   (0x1F << 16)    /* RW */
+#define MSDC_PAD_TUNE_CMDRRDLY  (0x1FUL << 22)  /* RW */
+#define MSDC_PAD_TUNE_CLKTXDLY  (0x1FUL << 27)  /* RW */
+
+/* MSDC_DAT_RDDLY0/1 mask */
+#define MSDC_DAT_RDDLY0_D0      (0x1F << 0)     /* RW */
+#define MSDC_DAT_RDDLY0_D1      (0x1F << 8)     /* RW */
+#define MSDC_DAT_RDDLY0_D2      (0x1F << 16)    /* RW */
+#define MSDC_DAT_RDDLY0_D3      (0x1F << 24)    /* RW */
+
+#define MSDC_DAT_RDDLY1_D4      (0x1F << 0)     /* RW */
+#define MSDC_DAT_RDDLY1_D5      (0x1F << 8)     /* RW */
+#define MSDC_DAT_RDDLY1_D6      (0x1F << 16)    /* RW */
+#define MSDC_DAT_RDDLY1_D7      (0x1F << 24)    /* RW */
+
+#define MSDC_CKGEN_MSDC_DLY_SEL   (0x1F<<10)
+#define MSDC_INT_DAT_LATCH_CK_SEL  (0x7<<7)
+#define MSDC_CKGEN_MSDC_CK_SEL     (0x1<<6)
+#define CARD_READY_FOR_DATA             (1<<8)
+#define CARD_CURRENT_STATE(x)           ((x&0x00001E00)>>9)
+
+/*--------------------------------------------------------------------------*/
+/* Descriptor Structure                                                     */
+/*--------------------------------------------------------------------------*/
+typedef struct {
+    u32  hwo:1; /* could be changed by hw */
+    u32  bdp:1;
+    u32  rsv0:6;
+    u32  chksum:8;
+    u32  intr:1;
+    u32  rsv1:15;
+    void *next;
+    void *ptr;
+    u32  buflen:16;
+    u32  extlen:8;
+    u32  rsv2:8;
+    u32  arg;
+    u32  blknum;
+    u32  cmd;
+} gpd_t;
+
+typedef struct {
+    u32  eol:1;
+    u32  rsv0:7;
+    u32  chksum:8;
+    u32  rsv1:1;
+    u32  blkpad:1;
+    u32  dwpad:1;
+    u32  rsv2:13;
+    void *next;
+    void *ptr;
+    u32  buflen:16;
+    u32  rsv3:16;
+} bd_t;
+
+/*--------------------------------------------------------------------------*/
+/* Register Debugging Structure                                             */
+/*--------------------------------------------------------------------------*/
+
+typedef struct {
+    u32 msdc:1;
+    u32 ckpwn:1;
+    u32 rst:1;
+    u32 pio:1;
+    u32 ckdrven:1;
+    u32 start18v:1;
+    u32 pass18v:1;
+    u32 ckstb:1;
+    u32 ckdiv:8;
+    u32 ckmod:2;
+    u32 pad:14;		
+} msdc_cfg_reg;
+typedef struct {
+    u32 sdr104cksel:1;
+    u32 rsmpl:1;
+    u32 dsmpl:1;
+    u32 ddlysel:1;
+    u32 ddr50ckd:1;
+    u32 dsplsel:1;
+    u32 pad1:10;
+    u32 d0spl:1;
+    u32 d1spl:1;
+    u32 d2spl:1;
+    u32 d3spl:1;
+    u32 d4spl:1;
+    u32 d5spl:1;
+    u32 d6spl:1;
+    u32 d7spl:1;
+    u32 riscsz:1;
+    u32 pad2:7;
+} msdc_iocon_reg;
+typedef struct {
+    u32 cden:1;
+    u32 cdsts:1;
+    u32 pad1:10;
+    u32 cddebounce:4;
+    u32 dat:8;
+    u32 cmd:1;
+    u32 pad2:6;
+    u32 wp:1;
+} msdc_ps_reg;
+typedef struct {
+    u32 mmcirq:1;
+    u32 cdsc:1;
+    u32 pad1:1;
+    u32 atocmdrdy:1;
+    u32 atocmdtmo:1;
+    u32 atocmdcrc:1;
+    u32 dmaqempty:1;
+    u32 sdioirq:1;
+    u32 cmdrdy:1;
+    u32 cmdtmo:1;
+    u32 rspcrc:1;
+    u32 csta:1;
+    u32 xfercomp:1;
+    u32 dxferdone:1;
+    u32 dattmo:1;
+    u32 datcrc:1;
+    u32 atocmd19done:1;
+    u32 pad2:15;
+} msdc_int_reg;
+typedef struct {
+    u32 mmcirq:1;
+    u32 cdsc:1;
+    u32 pad1:1;
+    u32 atocmdrdy:1;
+    u32 atocmdtmo:1;
+    u32 atocmdcrc:1;
+    u32 dmaqempty:1;
+    u32 sdioirq:1;
+    u32 cmdrdy:1;
+    u32 cmdtmo:1;
+    u32 rspcrc:1;
+    u32 csta:1;
+    u32 xfercomp:1;
+    u32 dxferdone:1;
+    u32 dattmo:1;
+    u32 datcrc:1;
+    u32 atocmd19done:1;
+    u32 pad2:15;
+} msdc_inten_reg;
+typedef struct {
+    u32 rxcnt:8;
+    u32 pad1:8;
+    u32 txcnt:8;
+    u32 pad2:7;
+    u32 clr:1;
+} msdc_fifocs_reg;
+typedef struct {
+    u32 val;
+} msdc_txdat_reg;
+typedef struct {
+    u32 val;
+} msdc_rxdat_reg;
+typedef struct {
+    u32 sdiowkup:1;
+    u32 inswkup:1;
+    u32 pad1:14;
+    u32 buswidth:2;
+    u32 pad2:1;
+    u32 sdio:1;
+    u32 sdioide:1;
+    u32 intblkgap:1;
+    u32 pad4:2;
+    u32 dtoc:8;
+} sdc_cfg_reg;
+typedef struct {
+    u32 cmd:6;
+    u32 brk:1;
+    u32 rsptyp:3;
+    u32 pad1:1;
+    u32 dtype:2;
+    u32 rw:1;
+    u32 stop:1;
+    u32 goirq:1;    
+    u32 blklen:12;
+    u32 atocmd:2;
+    u32 volswth:1;
+    u32 pad2:1;
+} sdc_cmd_reg;
+typedef struct {
+    u32 arg;
+} sdc_arg_reg;
+typedef struct {
+    u32 sdcbusy:1;
+    u32 cmdbusy:1;
+    u32 pad:29;
+    u32 swrcmpl:1;
+} sdc_sts_reg;
+typedef struct {
+    u32 val;
+} sdc_resp0_reg;
+typedef struct {
+    u32 val;	
+} sdc_resp1_reg;
+typedef struct {
+    u32 val;	
+} sdc_resp2_reg;
+typedef struct {
+    u32 val;	
+} sdc_resp3_reg;
+typedef struct {
+    u32 num;	
+} sdc_blknum_reg;
+typedef struct {
+    u32 sts;
+} sdc_csts_reg;
+typedef struct {
+    u32 sts;
+} sdc_cstsen_reg;
+typedef struct {
+    u32 datcrcsts:8;
+    u32 ddrcrcsts:4;
+    u32 pad:20;
+} sdc_datcrcsts_reg;
+typedef struct {
+    u32 bootstart:1;
+    u32 bootstop:1;
+    u32 bootmode:1;
+    u32 pad1:9;
+    u32 bootwaidly:3;
+    u32 bootsupp:1;
+    u32 pad2:16;
+} emmc_cfg0_reg;
+typedef struct {
+    u32 bootcrctmc:16;
+    u32 pad:4;
+    u32 bootacktmc:12;
+} emmc_cfg1_reg;
+typedef struct {
+    u32 bootcrcerr:1;
+    u32 bootackerr:1;
+    u32 bootdattmo:1;
+    u32 bootacktmo:1;
+    u32 bootupstate:1;
+    u32 bootackrcv:1;
+    u32 bootdatrcv:1;
+    u32 pad:25;
+} emmc_sts_reg;
+typedef struct {
+    u32 bootrst:1;
+    u32 pad:31;
+} emmc_iocon_reg;
+typedef struct {
+    u32 val;
+} msdc_acmd_resp_reg;
+typedef struct {
+    u32 tunesel:4;
+    u32 pad:28;
+} msdc_acmd19_trg_reg;
+typedef struct {
+    u32 val;
+} msdc_acmd19_sts_reg;
+typedef struct {
+    u32 addr;
+} msdc_dma_sa_reg;
+typedef struct {
+    u32 addr;
+} msdc_dma_ca_reg;
+typedef struct {
+    u32 start:1;
+    u32 stop:1;
+    u32 resume:1;
+    u32 pad1:5;
+    u32 mode:1;
+    u32 pad2:1;
+    u32 lastbuf:1;
+    u32 pad3:1;
+    u32 brustsz:3;
+    u32 pad4:1;
+    u32 xfersz:16;
+} msdc_dma_ctrl_reg;
+typedef struct {
+    u32 status:1;
+    u32 decsen:1;
+    u32 pad1:2;
+    u32 bdcsen:1;
+    u32 gpdcsen:1;
+    u32 pad2:26;
+} msdc_dma_cfg_reg;
+typedef struct {
+    u32 sel:16;
+    u32 pad2:16;
+} msdc_dbg_sel_reg;
+typedef struct {
+    u32 val;
+} msdc_dbg_out_reg;
+typedef struct {
+    u32 clkdrvn:3;
+    u32 rsv0:1;
+    u32 clkdrvp:3;
+    u32 rsv1:1;
+    u32 clksr:1;
+    u32 rsv2:7;
+    u32 clkpd:1;    
+    u32 clkpu:1;
+    u32 clksmt:1;
+    u32 clkies:1;
+    u32 clktdsel:4;
+    u32 clkrdsel:8;
+} msdc_pad_ctl0_reg;
+typedef struct {
+    u32 cmddrvn:3;
+    u32 rsv0:1;    
+    u32 cmddrvp:3;
+    u32 rsv1:1;
+    u32 cmdsr:1;
+    u32 rsv2:7;
+    u32 cmdpd:1;    
+    u32 cmdpu:1;
+    u32 cmdsmt:1;
+    u32 cmdies:1;
+    u32 cmdtdsel:4;
+    u32 cmdrdsel:8;
+} msdc_pad_ctl1_reg;
+typedef struct {
+    u32 datdrvn:3;
+    u32 rsv0:1;
+    u32 datdrvp:3;
+    u32 rsv1:1;
+    u32 datsr:1;
+    u32 rsv2:7;
+    u32 datpd:1;    
+    u32 datpu:1;
+    u32 datsmt:1;
+    u32 daties:1;
+    u32 dattdsel:4;
+    u32 datrdsel:8;
+} msdc_pad_ctl2_reg;
+typedef struct {
+    u32 wrrxdly:3;
+    u32 pad1:5;
+    u32 rdrxdly:8;
+    u32 pad2:16;
+} msdc_pad_tune_reg;
+typedef struct {
+    u32 dat0:5;
+    u32 rsv0:3;
+    u32 dat1:5;
+    u32 rsv1:3;
+    u32 dat2:5;
+    u32 rsv2:3;
+    u32 dat3:5;
+    u32 rsv3:3;    
+} msdc_dat_rddly0;
+typedef struct {
+    u32 dat4:5;
+    u32 rsv4:3;
+    u32 dat5:5;
+    u32 rsv5:3;
+    u32 dat6:5;
+    u32 rsv6:3;
+    u32 dat7:5;
+    u32 rsv7:3;
+} msdc_dat_rddly1;
+typedef struct {
+    u32 dbg0sel:8;
+    u32 dbg1sel:6;
+    u32 pad1:2;
+    u32 dbg2sel:6;
+    u32 pad2:2;
+    u32 dbg3sel:6;
+    u32 pad3:2;
+} msdc_hw_dbg_reg;
+typedef struct {
+    u32 val;
+} msdc_version_reg;
+typedef struct {
+    u32 val;
+} msdc_eco_ver_reg;
+
+struct msdc_regs {
+    msdc_cfg_reg        msdc_cfg;      /* base+0x00h */
+    msdc_iocon_reg      msdc_iocon;    /* base+0x04h */
+    msdc_ps_reg         msdc_ps;       /* base+0x08h */
+    msdc_int_reg        msdc_int;      /* base+0x0ch */
+    msdc_inten_reg      msdc_inten;    /* base+0x10h */
+    msdc_fifocs_reg     msdc_fifocs;   /* base+0x14h */
+    msdc_txdat_reg      msdc_txdat;    /* base+0x18h */
+    msdc_rxdat_reg      msdc_rxdat;    /* base+0x1ch */
+    u32                 rsv1[4];
+    sdc_cfg_reg         sdc_cfg;       /* base+0x30h */
+    sdc_cmd_reg         sdc_cmd;       /* base+0x34h */
+    sdc_arg_reg         sdc_arg;       /* base+0x38h */
+    sdc_sts_reg         sdc_sts;       /* base+0x3ch */
+    sdc_resp0_reg       sdc_resp0;     /* base+0x40h */
+    sdc_resp1_reg       sdc_resp1;     /* base+0x44h */
+    sdc_resp2_reg       sdc_resp2;     /* base+0x48h */
+    sdc_resp3_reg       sdc_resp3;     /* base+0x4ch */
+    sdc_blknum_reg      sdc_blknum;    /* base+0x50h */
+    u32                 rsv2[1];
+    sdc_csts_reg        sdc_csts;      /* base+0x58h */
+    sdc_cstsen_reg      sdc_cstsen;    /* base+0x5ch */
+    sdc_datcrcsts_reg   sdc_dcrcsta;   /* base+0x60h */
+    u32                 rsv3[3];
+    emmc_cfg0_reg       emmc_cfg0;     /* base+0x70h */
+    emmc_cfg1_reg       emmc_cfg1;     /* base+0x74h */
+    emmc_sts_reg        emmc_sts;      /* base+0x78h */
+    emmc_iocon_reg      emmc_iocon;    /* base+0x7ch */
+    msdc_acmd_resp_reg  acmd_resp;     /* base+0x80h */
+    msdc_acmd19_trg_reg acmd19_trg;    /* base+0x84h */
+    msdc_acmd19_sts_reg acmd19_sts;    /* base+0x88h */
+    u32                 rsv4[1];
+    msdc_dma_sa_reg     dma_sa;        /* base+0x90h */
+    msdc_dma_ca_reg     dma_ca;        /* base+0x94h */
+    msdc_dma_ctrl_reg   dma_ctrl;      /* base+0x98h */
+    msdc_dma_cfg_reg    dma_cfg;       /* base+0x9ch */
+    msdc_dbg_sel_reg    dbg_sel;       /* base+0xa0h */
+    msdc_dbg_out_reg    dbg_out;       /* base+0xa4h */
+    u32                 rsv5[2];
+    u32                 patch0;        /* base+0xb0h */
+    u32                 patch1;        /* base+0xb4h */
+    u32                 rsv6[10];
+    msdc_pad_ctl0_reg   pad_ctl0;      /* base+0xe0h */
+    msdc_pad_ctl1_reg   pad_ctl1;      /* base+0xe4h */
+    msdc_pad_ctl2_reg   pad_ctl2;      /* base+0xe8h */
+    msdc_pad_tune_reg   pad_tune;      /* base+0xech */
+    msdc_dat_rddly0     dat_rddly0;    /* base+0xf0h */
+    msdc_dat_rddly1     dat_rddly1;    /* base+0xf4h */
+    msdc_hw_dbg_reg     hw_dbg;        /* base+0xf8h */
+    u32                 rsv7[1];       
+    msdc_version_reg    version;       /* base+0x100h */
+    msdc_eco_ver_reg    eco_ver;       /* base+0x104h */
+};
+
+struct scatterlist_ex {
+    u32 cmd;
+    u32 arg;
+    u32 sglen;
+    struct scatterlist *sg;
+};
+
+#define DMA_FLAG_NONE       (0x00000000)
+#define DMA_FLAG_EN_CHKSUM  (0x00000001)
+#define DMA_FLAG_PAD_BLOCK  (0x00000002)
+#define DMA_FLAG_PAD_DWORD  (0x00000004)
+
+struct msdc_dma {
+    u32 flags;                   /* flags */
+    u32 xfersz;                  /* xfer size in bytes */
+    u32 sglen;                   /* size of scatter list */
+    u32 blklen;                  /* block size */
+    struct scatterlist *sg;      /* I/O scatter list */
+    struct scatterlist_ex *esg;  /* extended I/O scatter list */
+    u8  mode;                    /* dma mode        */
+    u8  burstsz;                 /* burst size      */
+    u8  intr;                    /* dma done interrupt */
+    u8  padding;                 /* padding */
+    u32 cmd;                     /* enhanced mode command */
+    u32 arg;                     /* enhanced mode arg */
+    u32 rsp;                     /* enhanced mode command response */
+    u32 autorsp;                 /* auto command response */
+
+    gpd_t *gpd;                  /* pointer to gpd array */
+    bd_t  *bd;                   /* pointer to bd array */
+    dma_addr_t gpd_addr;         /* the physical address of gpd array */
+    dma_addr_t bd_addr;          /* the physical address of bd array */
+    u32 used_gpd;                /* the number of used gpd elements */
+    u32 used_bd;                 /* the number of used bd elements */
+};
+
+struct msdc_host
+{
+    struct msdc_hw              *hw;
+
+    struct mmc_host             *mmc;           /* mmc structure */
+    struct mmc_command          *cmd;
+    struct mmc_data             *data;
+    struct mmc_request          *mrq; 
+    int                         cmd_rsp;
+    int                         cmd_rsp_done;
+    int                         cmd_r1b_done;
+
+    int                         error; 
+    spinlock_t                  lock;           /* mutex */
+    struct semaphore            sem; 
+
+    u32                         blksz;          /* host block size */
+    u32                         base;           /* host base address */    
+    int                         id;             /* host id */
+    int                         pwr_ref;        /* core power reference count */
+
+    u32                         xfer_size;      /* total transferred size */
+
+    struct msdc_dma             dma;            /* dma channel */
+    u32                         dma_addr;       /* dma transfer address */
+    u32                         dma_left_size;  /* dma transfer left size */
+    u32                         dma_xfer_size;  /* dma transfer size in bytes */
+    int                         dma_xfer;       /* dma transfer mode */
+
+    u32                         timeout_ns;     /* data timeout ns */
+    u32                         timeout_clks;   /* data timeout clks */
+
+    atomic_t                    abort;          /* abort transfer */
+
+    int                         irq;            /* host interrupt */
+
+    struct tasklet_struct       card_tasklet;
+
+    struct completion           cmd_done;
+    struct completion           xfer_done;
+    struct pm_message           pm_state;
+
+    u32                         mclk;           /* mmc subsystem clock */
+    u32                         hclk;           /* host clock speed */		
+    u32                         sclk;           /* SD/MS clock speed */
+    u8                          core_clkon;     /* Host core clock on ? */
+    u8                          card_clkon;     /* Card clock on ? */
+    u8                          core_power;     /* core power */    
+    u8                          power_mode;     /* host power mode */
+    u8                          card_inserted;  /* card inserted ? */
+    u8                          suspend;        /* host suspended ? */    
+    u8                          reserved;
+    u8                          app_cmd;        /* for app command */     
+    u32                         app_cmd_arg;    
+    u64                         starttime;
+};
+
+static inline unsigned int uffs(unsigned int x)
+{
+    unsigned int r = 1;
+
+    if (!x)
+        return 0;
+    if (!(x & 0xffff)) {
+        x >>= 16;
+        r += 16;
+    }
+    if (!(x & 0xff)) {
+        x >>= 8;
+        r += 8;
+    }
+    if (!(x & 0xf)) {
+        x >>= 4;
+        r += 4;
+    }
+    if (!(x & 3)) {
+        x >>= 2;
+        r += 2;
+    }
+    if (!(x & 1)) {
+        x >>= 1;
+        r += 1;
+    }
+    return r;
+}
+#define sdr_read8(reg)           __raw_readb(reg)
+#define sdr_read16(reg)          __raw_readw(reg)
+#define sdr_read32(reg)          __raw_readl(reg)
+#define sdr_write8(reg,val)      __raw_writeb(val,reg)
+#define sdr_write16(reg,val)     __raw_writew(val,reg)
+#define sdr_write32(reg,val)     __raw_writel(val,reg)
+
+#define sdr_set_bits(reg,bs)     ((*(volatile u32*)(reg)) |= (u32)(bs))
+#define sdr_clr_bits(reg,bs)     ((*(volatile u32*)(reg)) &= ~((u32)(bs)))
+
+#define sdr_set_field(reg,field,val) \
+    do {	\
+        volatile unsigned int tv = sdr_read32(reg);	\
+        tv &= ~(field); \
+        tv |= ((val) << (uffs((unsigned int)field) - 1)); \
+        sdr_write32(reg,tv); \
+    } while(0)
+#define sdr_get_field(reg,field,val) \
+    do {	\
+        volatile unsigned int tv = sdr_read32(reg);	\
+        val = ((tv & (field)) >> (uffs((unsigned int)field) - 1)); \
+    } while(0)
+
+#endif
+
--- /dev/null
+++ b/drivers/mmc/host/sdhci-mt7620.c
@@ -0,0 +1,2314 @@
+/* Copyright Statement:
+ *
+ * This software/firmware and related documentation ("MediaTek Software") are
+ * protected under relevant copyright laws. The information contained herein
+ * is confidential and proprietary to MediaTek Inc. and/or its licensors.
+ * Without the prior written permission of MediaTek inc. and/or its licensors,
+ * any reproduction, modification, use or disclosure of MediaTek Software,
+ * and information contained herein, in whole or in part, shall be strictly prohibited.
+ *
+ * MediaTek Inc. (C) 2010. All rights reserved.
+ *
+ * BY OPENING THIS FILE, RECEIVER HEREBY UNEQUIVOCALLY ACKNOWLEDGES AND AGREES
+ * THAT THE SOFTWARE/FIRMWARE AND ITS DOCUMENTATIONS ("MEDIATEK SOFTWARE")
+ * RECEIVED FROM MEDIATEK AND/OR ITS REPRESENTATIVES ARE PROVIDED TO RECEIVER ON
+ * AN "AS-IS" BASIS ONLY. MEDIATEK EXPRESSLY DISCLAIMS ANY AND ALL WARRANTIES,
+ * EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE OR NONINFRINGEMENT.
+ * NEITHER DOES MEDIATEK PROVIDE ANY WARRANTY WHATSOEVER WITH RESPECT TO THE
+ * SOFTWARE OF ANY THIRD PARTY WHICH MAY BE USED BY, INCORPORATED IN, OR
+ * SUPPLIED WITH THE MEDIATEK SOFTWARE, AND RECEIVER AGREES TO LOOK ONLY TO SUCH
+ * THIRD PARTY FOR ANY WARRANTY CLAIM RELATING THERETO. RECEIVER EXPRESSLY ACKNOWLEDGES
+ * THAT IT IS RECEIVER'S SOLE RESPONSIBILITY TO OBTAIN FROM ANY THIRD PARTY ALL PROPER LICENSES
+ * CONTAINED IN MEDIATEK SOFTWARE. MEDIATEK SHALL ALSO NOT BE RESPONSIBLE FOR ANY MEDIATEK
+ * SOFTWARE RELEASES MADE TO RECEIVER'S SPECIFICATION OR TO CONFORM TO A PARTICULAR
+ * STANDARD OR OPEN FORUM. RECEIVER'S SOLE AND EXCLUSIVE REMEDY AND MEDIATEK'S ENTIRE AND
+ * CUMULATIVE LIABILITY WITH RESPECT TO THE MEDIATEK SOFTWARE RELEASED HEREUNDER WILL BE,
+ * AT MEDIATEK'S OPTION, TO REVISE OR REPLACE THE MEDIATEK SOFTWARE AT ISSUE,
+ * OR REFUND ANY SOFTWARE LICENSE FEES OR SERVICE CHARGE PAID BY RECEIVER TO
+ * MEDIATEK FOR SUCH MEDIATEK SOFTWARE AT ISSUE.
+ *
+ * The following software/firmware and/or related documentation ("MediaTek Software")
+ * have been modified by MediaTek Inc. All revisions are subject to any receiver's
+ * applicable license agreements with MediaTek Inc.
+ */
+
+#include <linux/module.h>
+#include <linux/moduleparam.h>
+#include <linux/init.h>
+#include <linux/spinlock.h>
+#include <linux/timer.h>
+#include <linux/ioport.h>
+#include <linux/device.h>
+#include <linux/platform_device.h>
+#include <linux/of_platform.h>
+#include <linux/interrupt.h>
+#include <linux/delay.h>
+#include <linux/blkdev.h>
+#include <linux/slab.h>
+#include <linux/mmc/host.h>
+#include <linux/mmc/card.h>
+#include <linux/mmc/core.h>
+#include <linux/mmc/mmc.h>
+#include <linux/mmc/sd.h>
+#include <linux/mmc/sdio.h>
+#include <linux/dma-mapping.h>
+
+#include <linux/types.h>
+#include <linux/kernel.h>
+#include <linux/version.h>
+#include <linux/pm.h>
+
+#define MSDC_SMPL_FALLING   (1)
+#define MSDC_CD_PIN_EN      (1 << 0)  /* card detection pin is wired   */
+#define MSDC_WP_PIN_EN      (1 << 1)  /* write protection pin is wired */
+#define MSDC_REMOVABLE      (1 << 5)  /* removable slot                */
+#define MSDC_SYS_SUSPEND    (1 << 6)  /* suspended by system           */
+#define MSDC_HIGHSPEED      (1 << 7)
+
+#define IRQ_SDC 22
+
+#include <asm/dma.h>
+
+#include "mt6575_sd.h"
+
+#define DRV_NAME            "mtk-sd"
+
+#define HOST_MAX_NUM        (1) /* +/- by chhung */
+
+#define HOST_MAX_MCLK       (48000000) /* +/- by chhung */
+#define HOST_MIN_MCLK       (260000)
+
+#define HOST_MAX_BLKSZ      (2048)
+
+#define MSDC_OCR_AVAIL      (MMC_VDD_28_29 | MMC_VDD_29_30 | MMC_VDD_30_31 | MMC_VDD_31_32 | MMC_VDD_32_33)
+
+#define GPIO_PULL_DOWN      (0)
+#define GPIO_PULL_UP        (1)
+
+#define DEFAULT_DEBOUNCE    (8)       /* 8 cycles */
+#define DEFAULT_DTOC        (40)      /* data timeout counter. 65536x40 sclk. */
+
+#define CMD_TIMEOUT         (HZ/10)     /* 100ms */
+#define DAT_TIMEOUT         (HZ/2 * 5)  /* 500ms x5 */
+
+#define MAX_DMA_CNT         (64 * 1024 - 512)   /* a single transaction for WIFI may be 50K*/
+
+#define MAX_GPD_NUM         (1 + 1)  /* one null gpd */
+#define MAX_BD_NUM          (1024)
+#define MAX_BD_PER_GPD      (MAX_BD_NUM)
+
+#define MAX_HW_SGMTS        (MAX_BD_NUM)
+#define MAX_PHY_SGMTS       (MAX_BD_NUM)
+#define MAX_SGMT_SZ         (MAX_DMA_CNT)
+#define MAX_REQ_SZ          (MAX_SGMT_SZ * 8)  
+
+#ifdef MT6575_SD_DEBUG
+static struct msdc_regs *msdc_reg[HOST_MAX_NUM];
+#endif 
+
+//=================================
+#define PERI_MSDC0_PDN      (15)
+//#define PERI_MSDC1_PDN    (16)
+//#define PERI_MSDC2_PDN    (17)
+//#define PERI_MSDC3_PDN    (18)
+
+struct msdc_host *msdc_6575_host[] = {NULL,NULL,NULL,NULL};
+
+struct msdc_hw msdc0_hw = {
+	.clk_src        = 0,
+	.cmd_edge       = MSDC_SMPL_FALLING,
+	.data_edge      = MSDC_SMPL_FALLING,
+	.clk_drv        = 4,
+	.cmd_drv        = 4,
+	.dat_drv        = 4,
+	.data_pins      = 4,
+	.data_offset    = 0,
+	.flags          = MSDC_SYS_SUSPEND | MSDC_WP_PIN_EN | MSDC_CD_PIN_EN | MSDC_REMOVABLE | MSDC_HIGHSPEED,
+};
+
+static struct resource mtk_sd_resources[] = {
+	[0] = {
+		.start  = 0xb0130000,
+		.end    = 0xb0133fff,
+		.flags  = IORESOURCE_MEM,
+	},
+	[1] = {
+		.start  = IRQ_SDC,	/*FIXME*/
+		.end    = IRQ_SDC,	/*FIXME*/
+		.flags  = IORESOURCE_IRQ,
+	},
+};
+
+static struct platform_device mtk_sd_device = {
+	.name           = "mtk-sd",
+	.id             = 0,
+	.num_resources  = ARRAY_SIZE(mtk_sd_resources),
+	.resource       = mtk_sd_resources,
+};
+/* end of +++ */
+
+static int msdc_rsp[] = {
+    0,  /* RESP_NONE */
+    1,  /* RESP_R1 */
+    2,  /* RESP_R2 */
+    3,  /* RESP_R3 */
+    4,  /* RESP_R4 */
+    1,  /* RESP_R5 */
+    1,  /* RESP_R6 */
+    1,  /* RESP_R7 */
+    7,  /* RESP_R1b */
+};
+
+/* For Inhanced DMA */
+#define msdc_init_gpd_ex(gpd,extlen,cmd,arg,blknum) \
+    do { \
+        ((gpd_t*)gpd)->extlen = extlen; \
+        ((gpd_t*)gpd)->cmd    = cmd; \
+        ((gpd_t*)gpd)->arg    = arg; \
+        ((gpd_t*)gpd)->blknum = blknum; \
+    }while(0)
+    
+#define msdc_init_bd(bd, blkpad, dwpad, dptr, dlen) \
+    do { \
+        BUG_ON(dlen > 0xFFFFUL); \
+        ((bd_t*)bd)->blkpad = blkpad; \
+        ((bd_t*)bd)->dwpad  = dwpad; \
+        ((bd_t*)bd)->ptr    = (void*)dptr; \
+        ((bd_t*)bd)->buflen = dlen; \
+    }while(0)
+
+#define msdc_txfifocnt()   ((sdr_read32(MSDC_FIFOCS) & MSDC_FIFOCS_TXCNT) >> 16)
+#define msdc_rxfifocnt()   ((sdr_read32(MSDC_FIFOCS) & MSDC_FIFOCS_RXCNT) >> 0)
+#define msdc_fifo_write32(v)   sdr_write32(MSDC_TXDATA, (v))
+#define msdc_fifo_write8(v)    sdr_write8(MSDC_TXDATA, (v))
+#define msdc_fifo_read32()   sdr_read32(MSDC_RXDATA)
+#define msdc_fifo_read8()    sdr_read8(MSDC_RXDATA)	
+
+
+#define msdc_dma_on()        sdr_clr_bits(MSDC_CFG, MSDC_CFG_PIO)
+#define msdc_dma_off()       sdr_set_bits(MSDC_CFG, MSDC_CFG_PIO)
+
+#define msdc_retry(expr,retry,cnt) \
+    do { \
+        int backup = cnt; \
+        while (retry) { \
+            if (!(expr)) break; \
+            if (cnt-- == 0) { \
+                retry--; mdelay(1); cnt = backup; \
+            } \
+        } \
+        WARN_ON(retry == 0); \
+    } while(0)
+
+#if 0 /* +/- chhung */
+#define msdc_reset() \
+    do { \
+        int retry = 3, cnt = 1000; \
+        sdr_set_bits(MSDC_CFG, MSDC_CFG_RST); \
+        dsb(); \
+        msdc_retry(sdr_read32(MSDC_CFG) & MSDC_CFG_RST, retry, cnt); \
+    } while(0)
+#else
+#define msdc_reset() \
+    do { \
+        int retry = 3, cnt = 1000; \
+        sdr_set_bits(MSDC_CFG, MSDC_CFG_RST); \
+        msdc_retry(sdr_read32(MSDC_CFG) & MSDC_CFG_RST, retry, cnt); \
+    } while(0)
+#endif /* end of +/- */
+
+#define msdc_clr_int() \
+    do { \
+        volatile u32 val = sdr_read32(MSDC_INT); \
+        sdr_write32(MSDC_INT, val); \
+    } while(0)
+
+#define msdc_clr_fifo() \
+    do { \
+        int retry = 3, cnt = 1000; \
+        sdr_set_bits(MSDC_FIFOCS, MSDC_FIFOCS_CLR); \
+        msdc_retry(sdr_read32(MSDC_FIFOCS) & MSDC_FIFOCS_CLR, retry, cnt); \
+    } while(0)
+
+#define msdc_irq_save(val) \
+    do { \
+        val = sdr_read32(MSDC_INTEN); \
+        sdr_clr_bits(MSDC_INTEN, val); \
+    } while(0)
+	
+#define msdc_irq_restore(val) \
+    do { \
+        sdr_set_bits(MSDC_INTEN, val); \
+    } while(0)
+
+/* clock source for host: global */
+static u32 hclks[] = {48000000}; /* +/- by chhung */
+
+//============================================
+// the power for msdc host controller: global
+//    always keep the VMC on. 
+//============================================
+#define msdc_vcore_on(host) \
+    do { \
+        printk("[+]VMC ref. count<%d>\n", ++host->pwr_ref); \
+        (void)hwPowerOn(MT65XX_POWER_LDO_VMC, VOL_3300, "SD"); \
+    } while (0)
+#define msdc_vcore_off(host) \
+    do { \
+        printk("[-]VMC ref. count<%d>\n", --host->pwr_ref); \
+        (void)hwPowerDown(MT65XX_POWER_LDO_VMC, "SD"); \
+    } while (0)
+
+//====================================
+// the vdd output for card: global 
+//   always keep the VMCH on. 
+//==================================== 
+#define msdc_vdd_on(host) \
+    do { \
+        (void)hwPowerOn(MT65XX_POWER_LDO_VMCH, VOL_3300, "SD"); \
+    } while (0)   
+#define msdc_vdd_off(host) \
+    do { \
+        (void)hwPowerDown(MT65XX_POWER_LDO_VMCH, "SD"); \
+    } while (0)      
+
+#define sdc_is_busy()          (sdr_read32(SDC_STS) & SDC_STS_SDCBUSY)
+#define sdc_is_cmd_busy()      (sdr_read32(SDC_STS) & SDC_STS_CMDBUSY)
+
+#define sdc_send_cmd(cmd,arg) \
+    do { \
+        sdr_write32(SDC_ARG, (arg)); \
+        sdr_write32(SDC_CMD, (cmd)); \
+    } while(0)
+
+// can modify to read h/w register.
+//#define is_card_present(h)   ((sdr_read32(MSDC_PS) & MSDC_PS_CDSTS) ? 0 : 1);
+#define is_card_present(h)     (((struct msdc_host*)(h))->card_inserted)
+
+/* +++ chhung */
+#ifndef __ASSEMBLY__
+#define PHYSADDR(a)             (((unsigned long)(a)) & 0x1fffffff)
+#else
+#define PHYSADDR(a)             ((a) & 0x1fffffff)
+#endif
+/* end of +++ */
+static unsigned int msdc_do_command(struct msdc_host   *host, 
+                                      struct mmc_command *cmd,
+                                      int                 tune,
+                                      unsigned long       timeout);  
+                                     
+static int msdc_tune_cmdrsp(struct msdc_host*host,struct mmc_command *cmd);
+
+#ifdef MT6575_SD_DEBUG
+static void msdc_dump_card_status(struct msdc_host *host, u32 status)
+{
+    static char *state[] = {
+        "Idle",			/* 0 */
+        "Ready",		/* 1 */
+        "Ident",		/* 2 */
+        "Stby",			/* 3 */
+        "Tran",			/* 4 */
+        "Data",			/* 5 */
+        "Rcv",			/* 6 */
+        "Prg",			/* 7 */
+        "Dis",			/* 8 */
+        "Reserved",		/* 9 */
+        "Reserved",		/* 10 */
+        "Reserved",		/* 11 */
+        "Reserved",		/* 12 */
+        "Reserved",		/* 13 */
+        "Reserved",		/* 14 */
+        "I/O mode",		/* 15 */
+    };
+    if (status & R1_OUT_OF_RANGE)
+        printk("[CARD_STATUS] Out of Range\n");
+    if (status & R1_ADDRESS_ERROR)
+        printk("[CARD_STATUS] Address Error\n");
+    if (status & R1_BLOCK_LEN_ERROR)
+        printk("[CARD_STATUS] Block Len Error\n");
+    if (status & R1_ERASE_SEQ_ERROR)
+        printk("[CARD_STATUS] Erase Seq Error\n");
+    if (status & R1_ERASE_PARAM)
+        printk("[CARD_STATUS] Erase Param\n");
+    if (status & R1_WP_VIOLATION)
+        printk("[CARD_STATUS] WP Violation\n");
+    if (status & R1_CARD_IS_LOCKED)
+        printk("[CARD_STATUS] Card is Locked\n");
+    if (status & R1_LOCK_UNLOCK_FAILED)
+        printk("[CARD_STATUS] Lock/Unlock Failed\n");
+    if (status & R1_COM_CRC_ERROR)
+        printk("[CARD_STATUS] Command CRC Error\n");
+    if (status & R1_ILLEGAL_COMMAND)
+        printk("[CARD_STATUS] Illegal Command\n");
+    if (status & R1_CARD_ECC_FAILED)
+        printk("[CARD_STATUS] Card ECC Failed\n");
+    if (status & R1_CC_ERROR)
+        printk("[CARD_STATUS] CC Error\n");
+    if (status & R1_ERROR)
+        printk("[CARD_STATUS] Error\n");
+    if (status & R1_UNDERRUN)
+        printk("[CARD_STATUS] Underrun\n");
+    if (status & R1_OVERRUN)
+        printk("[CARD_STATUS] Overrun\n");
+    if (status & R1_CID_CSD_OVERWRITE)
+        printk("[CARD_STATUS] CID/CSD Overwrite\n");
+    if (status & R1_WP_ERASE_SKIP)
+        printk("[CARD_STATUS] WP Eraser Skip\n");
+    if (status & R1_CARD_ECC_DISABLED)
+        printk("[CARD_STATUS] Card ECC Disabled\n");
+    if (status & R1_ERASE_RESET)
+        printk("[CARD_STATUS] Erase Reset\n");
+    if (status & R1_READY_FOR_DATA)
+        printk("[CARD_STATUS] Ready for Data\n");
+    if (status & R1_SWITCH_ERROR)
+        printk("[CARD_STATUS] Switch error\n");
+    if (status & R1_APP_CMD)
+        printk("[CARD_STATUS] App Command\n");
+    
+    printk("[CARD_STATUS] '%s' State\n", state[R1_CURRENT_STATE(status)]);
+}
+
+static void msdc_dump_ocr_reg(struct msdc_host *host, u32 resp)
+{
+    if (resp & (1 << 7))
+        printk("[OCR] Low Voltage Range\n");
+    if (resp & (1 << 15))
+        printk("[OCR] 2.7-2.8 volt\n");
+    if (resp & (1 << 16))
+        printk("[OCR] 2.8-2.9 volt\n");
+    if (resp & (1 << 17))
+        printk("[OCR] 2.9-3.0 volt\n");
+    if (resp & (1 << 18))
+        printk("[OCR] 3.0-3.1 volt\n");
+    if (resp & (1 << 19))
+        printk("[OCR] 3.1-3.2 volt\n");
+    if (resp & (1 << 20))
+        printk("[OCR] 3.2-3.3 volt\n");
+    if (resp & (1 << 21))
+        printk("[OCR] 3.3-3.4 volt\n");
+    if (resp & (1 << 22))
+        printk("[OCR] 3.4-3.5 volt\n");
+    if (resp & (1 << 23))
+        printk("[OCR] 3.5-3.6 volt\n");
+    if (resp & (1 << 24))
+        printk("[OCR] Switching to 1.8V Accepted (S18A)\n");
+    if (resp & (1 << 30))
+        printk("[OCR] Card Capacity Status (CCS)\n");
+    if (resp & (1 << 31))
+        printk("[OCR] Card Power Up Status (Idle)\n");
+    else
+        printk("[OCR] Card Power Up Status (Busy)\n");
+}
+
+static void msdc_dump_rca_resp(struct msdc_host *host, u32 resp)
+{
+    u32 status = (((resp >> 15) & 0x1) << 23) |
+                 (((resp >> 14) & 0x1) << 22) |
+                 (((resp >> 13) & 0x1) << 19) |
+                   (resp & 0x1fff);
+
+    printk("[RCA] 0x%.4x\n", resp >> 16);
+    
+    msdc_dump_card_status(host, status);
+}
+
+static void msdc_dump_io_resp(struct msdc_host *host, u32 resp)
+{
+    u32 flags = (resp >> 8) & 0xFF;
+    char *state[] = {"DIS", "CMD", "TRN", "RFU"};
+
+    if (flags & (1 << 7))
+        printk("[IO] COM_CRC_ERR\n");
+    if (flags & (1 << 6))
+        printk("[IO] Illgal command\n");
+    if (flags & (1 << 3))
+        printk("[IO] Error\n");
+    if (flags & (1 << 2))
+        printk("[IO] RFU\n");
+    if (flags & (1 << 1))
+        printk("[IO] Function number error\n");
+    if (flags & (1 << 0))
+        printk("[IO] Out of range\n");
+
+    printk("[IO] State: %s, Data:0x%x\n", state[(resp >> 12) & 0x3], resp & 0xFF);
+}
+#endif
+
+static void msdc_set_timeout(struct msdc_host *host, u32 ns, u32 clks)
+{
+	u32 base = host->base;
+	u32 timeout, clk_ns;
+
+	host->timeout_ns = ns;
+	host->timeout_clks = clks;
+
+	clk_ns = 1000000000UL / host->sclk;
+	timeout = ns / clk_ns + clks;
+	timeout = timeout >> 16; /* in 65536 sclk cycle unit */
+	timeout = timeout > 1 ? timeout - 1 : 0;
+	timeout = timeout > 255 ? 255 : timeout;
+
+	sdr_set_field(SDC_CFG, SDC_CFG_DTOC, timeout);
+
+/*	printk("Set read data timeout: %dns %dclks -> %d x 65536 cycles\n",
+		ns, clks, timeout + 1);*/
+}
+
+static void msdc_eirq_sdio(void *data)
+{
+	struct msdc_host *host = (struct msdc_host *)data;
+
+//	printk("SDIO EINT\n");
+
+	mmc_signal_sdio_irq(host->mmc);
+}
+
+static void msdc_eirq_cd(void *data)
+{
+	struct msdc_host *host = (struct msdc_host *)data;
+
+//	printk("CD EINT\n");
+
+	tasklet_hi_schedule(&host->card_tasklet);
+}
+
+static void msdc_tasklet_card(unsigned long arg)
+{
+	struct msdc_host *host = (struct msdc_host *)arg;
+	struct msdc_hw *hw = host->hw;
+	u32 base = host->base;
+	u32 inserted;
+	u32 status = 0;
+
+	spin_lock(&host->lock);
+
+	if (hw->get_cd_status) {
+		inserted = hw->get_cd_status();
+	} else {
+		status = sdr_read32(MSDC_PS);
+		inserted = (status & MSDC_PS_CDSTS) ? 0 : 1;
+	}
+
+	host->card_inserted = inserted;
+
+	if (!host->suspend) {
+		host->mmc->f_max = HOST_MAX_MCLK;
+		mmc_detect_change(host->mmc, msecs_to_jiffies(20));
+	}
+
+//	printk("card found<%s>\n", inserted ? "inserted" : "removed");
+
+	spin_unlock(&host->lock);
+}
+
+static void msdc_set_mclk(struct msdc_host *host, int ddr, unsigned int hz)
+{
+	u32 base = host->base;
+	u32 hclk = host->hclk;
+	u32 mode, flags, div, sclk;
+
+	if (!hz) {
+//		printk("set mclk to 0!!!\n");
+		msdc_reset();
+		return;
+	}
+
+	msdc_irq_save(flags);
+
+	if (ddr) {
+		mode = 0x2;
+		if (hz >= (hclk >> 2)) {
+			div = 1;
+			sclk = hclk >> 2;
+		} else {
+			div  = (hclk + ((hz << 2) - 1)) / (hz << 2);
+			sclk = (hclk >> 2) / div;
+		}
+	} else if (hz >= hclk) {
+		mode = 0x1;
+		div = 0;
+		sclk = hclk;
+	} else {
+		mode = 0x0;
+		if (hz >= (hclk >> 1)) {
+			div = 0;
+			sclk = hclk >> 1;
+		} else {
+			div = (hclk + ((hz << 2) - 1)) / (hz << 2);
+			sclk = (hclk >> 2) / div;
+		}
+	}
+
+	sdr_set_field(MSDC_CFG, MSDC_CFG_CKMOD, mode);
+	sdr_set_field(MSDC_CFG, MSDC_CFG_CKDIV, div);
+
+	while (!(sdr_read32(MSDC_CFG) & MSDC_CFG_CKSTB));
+
+	host->sclk = sclk;
+	host->mclk = hz;
+	msdc_set_timeout(host, host->timeout_ns, host->timeout_clks);
+
+/*	printk("!!! Set<%dKHz> Source<%dKHz> -> sclk<%dKHz>\n",
+		hz / 1000, hclk / 1000, sclk / 1000);
+*/
+	msdc_irq_restore(flags);
+}
+
+static void msdc_abort_data(struct msdc_host *host)
+{
+	u32 base = host->base;
+	struct mmc_command *stop = host->mrq->stop;
+
+//	printk("Need to Abort. dma<%d>\n", host->dma_xfer);
+
+	msdc_reset();
+	msdc_clr_fifo();
+	msdc_clr_int();
+
+	if (stop) {
+//		printk("stop when abort CMD<%d>\n", stop->opcode);
+		msdc_do_command(host, stop, 0, CMD_TIMEOUT);
+	}
+}
+
+static unsigned int msdc_command_start(struct msdc_host *host,
+		struct mmc_command *cmd, int tune, unsigned long timeout)
+{
+	u32 wints = MSDC_INT_CMDRDY | MSDC_INT_RSPCRCERR | MSDC_INT_CMDTMO |
+		MSDC_INT_ACMDRDY | MSDC_INT_ACMDCRCERR | MSDC_INT_ACMDTMO |
+		MSDC_INT_ACMD19_DONE;
+	u32 base = host->base;
+	u32 opcode = cmd->opcode;
+	u32 rawcmd;
+	u32 resp;
+	unsigned long tmo;
+
+	if (opcode == MMC_SEND_OP_COND || opcode == SD_APP_OP_COND)
+		resp = RESP_R3;
+	else if (opcode == MMC_SET_RELATIVE_ADDR || opcode == SD_SEND_RELATIVE_ADDR)
+		resp = (mmc_cmd_type(cmd) == MMC_CMD_BCR) ? RESP_R6 : RESP_R1;
+	else if (opcode == MMC_FAST_IO)
+		resp = RESP_R4;
+	else if (opcode == MMC_GO_IRQ_STATE)
+		resp = RESP_R5;
+	else if (opcode == MMC_SELECT_CARD)
+		resp = (cmd->arg != 0) ? RESP_R1B : RESP_NONE;
+	else if (opcode == SD_IO_RW_DIRECT || opcode == SD_IO_RW_EXTENDED)
+		resp = RESP_R1;
+	else if (opcode == SD_SEND_IF_COND && (mmc_cmd_type(cmd) == MMC_CMD_BCR))
+		resp = RESP_R1;
+	else {
+		switch (mmc_resp_type(cmd)) {
+		case MMC_RSP_R1:
+			resp = RESP_R1;
+			break;
+		case MMC_RSP_R1B:
+			resp = RESP_R1B;
+			break;
+		case MMC_RSP_R2:
+			resp = RESP_R2;
+			break;
+		case MMC_RSP_R3:
+			resp = RESP_R3;
+			break;
+		case MMC_RSP_NONE:
+		default:
+			resp = RESP_NONE;
+			break;
+		}
+	}
+
+	cmd->error = 0;
+	rawcmd = opcode | msdc_rsp[resp] << 7 | host->blksz << 16;
+
+	if (opcode == MMC_READ_MULTIPLE_BLOCK) {
+		rawcmd |= (2 << 11);
+	} else if (opcode == MMC_READ_SINGLE_BLOCK) {
+		rawcmd |= (1 << 11);
+	} else if (opcode == MMC_WRITE_MULTIPLE_BLOCK) {
+		rawcmd |= ((2 << 11) | (1 << 13));
+	} else if (opcode == MMC_WRITE_BLOCK) {
+		rawcmd |= ((1 << 11) | (1 << 13));
+	} else if (opcode == SD_IO_RW_EXTENDED) {
+		if (cmd->data->flags & MMC_DATA_WRITE)
+			rawcmd |= (1 << 13);
+		if (cmd->data->blocks > 1)
+			rawcmd |= (2 << 11);
+		else
+			rawcmd |= (1 << 11);
+	} else if (opcode == SD_IO_RW_DIRECT && cmd->flags == (unsigned int)-1) {
+		rawcmd |= (1 << 14);
+	} else if ((opcode == SD_APP_SEND_SCR) ||
+			(opcode == SD_APP_SEND_NUM_WR_BLKS) ||
+			(opcode == SD_SWITCH && (mmc_cmd_type(cmd) == MMC_CMD_ADTC)) ||
+			(opcode == SD_APP_SD_STATUS && (mmc_cmd_type(cmd) == MMC_CMD_ADTC)) ||
+			(opcode == MMC_SEND_EXT_CSD && (mmc_cmd_type(cmd) == MMC_CMD_ADTC))) {
+		rawcmd |= (1 << 11);
+	} else if (opcode == MMC_STOP_TRANSMISSION) {
+		rawcmd |= (1 << 14);
+		rawcmd &= ~(0x0FFF << 16);
+	}
+
+//	printk("CMD<%d><0x%.8x> Arg<0x%.8x>\n", opcode , rawcmd, cmd->arg);
+
+	tmo = jiffies + timeout;
+
+	if (opcode == MMC_SEND_STATUS) {
+		for (;;) {
+			if (!sdc_is_cmd_busy())
+				break;
+
+			if (time_after(jiffies, tmo)) {
+				//printk("XXX cmd_busy timeout: before CMD<%d>\n", opcode);
+				cmd->error = (unsigned int)-ETIMEDOUT;
+				msdc_reset();
+				goto end;
+			}
+		}
+	} else {
+		for (;;) {
+			if (!sdc_is_busy())
+				break;
+			if (time_after(jiffies, tmo)) {
+				//printk("XXX sdc_busy timeout: before CMD<%d>\n", opcode);
+				cmd->error = (unsigned int)-ETIMEDOUT;
+				msdc_reset();
+				goto end;
+			}
+		}
+	}
+
+	//BUG_ON(in_interrupt());
+	host->cmd = cmd;
+	host->cmd_rsp = resp;
+	init_completion(&host->cmd_done);
+	sdr_set_bits(MSDC_INTEN, wints);
+	sdc_send_cmd(rawcmd, cmd->arg);
+
+end:
+	return cmd->error;
+}
+
+static unsigned int msdc_command_resp(struct msdc_host *host, struct mmc_command *cmd,
+				int tune, unsigned long timeout)
+{
+	u32 base = host->base;
+	//u32 opcode = cmd->opcode;
+	u32 resp;
+	u32 wints = MSDC_INT_CMDRDY | MSDC_INT_RSPCRCERR | MSDC_INT_CMDTMO |
+		MSDC_INT_ACMDRDY | MSDC_INT_ACMDCRCERR | MSDC_INT_ACMDTMO |
+		MSDC_INT_ACMD19_DONE;
+
+	resp = host->cmd_rsp;
+
+	BUG_ON(in_interrupt());
+	spin_unlock(&host->lock);
+	if (!wait_for_completion_timeout(&host->cmd_done, 10*timeout)) {
+		//printk("XXX CMD<%d> wait_for_completion timeout ARG<0x%.8x>\n", opcode, cmd->arg);
+		cmd->error = (unsigned int)-ETIMEDOUT;
+		msdc_reset();
+	}
+	spin_lock(&host->lock);
+
+	sdr_clr_bits(MSDC_INTEN, wints);
+	host->cmd = NULL;
+
+	if (!tune)
+		return cmd->error;
+
+	/* memory card CRC */
+	if (host->hw->flags & MSDC_REMOVABLE && cmd->error == (unsigned int)(-EIO) ) {
+		if (sdr_read32(SDC_CMD) & 0x1800) {
+			msdc_abort_data(host);
+		} else {
+			msdc_reset();
+			msdc_clr_fifo();
+			msdc_clr_int();
+		}
+		cmd->error = msdc_tune_cmdrsp(host,cmd);
+	}
+
+	return cmd->error;
+}
+
+static unsigned int msdc_do_command(struct msdc_host *host, struct mmc_command *cmd,
+			int tune, unsigned long timeout)
+{
+	if (!msdc_command_start(host, cmd, tune, timeout))
+		msdc_command_resp(host, cmd, tune, timeout);
+
+	//printk("        return<%d> resp<0x%.8x>\n", cmd->error, cmd->resp[0]);
+	return cmd->error;
+}
+
+static int msdc_pio_abort(struct msdc_host *host, struct mmc_data *data, unsigned long tmo)
+{
+	u32  base = host->base;
+	int  ret = 0;
+
+	if (atomic_read(&host->abort))
+		ret = 1;
+
+	if (time_after(jiffies, tmo)) {
+		data->error = (unsigned int)-ETIMEDOUT;
+		//printk("XXX PIO Data Timeout: CMD<%d>\n", host->mrq->cmd->opcode);
+		ret = 1;
+	}
+
+	if (ret) {
+		msdc_reset();
+		msdc_clr_fifo();
+		msdc_clr_int();
+		//printk("msdc pio find abort\n");
+	}
+
+	return ret;
+}
+
+static int msdc_pio_read(struct msdc_host *host, struct mmc_data *data)
+{
+	struct scatterlist *sg = data->sg;
+	u32  base = host->base;
+	u32  num = data->sg_len;
+	u32 *ptr;
+	u8  *u8ptr;
+	u32  left;
+	u32  count, size = 0;
+	u32  wints = MSDC_INTEN_DATTMO | MSDC_INTEN_DATCRCERR;
+	unsigned long tmo = jiffies + DAT_TIMEOUT;
+
+	sdr_set_bits(MSDC_INTEN, wints);
+	while (num) {
+		left = sg_dma_len(sg);
+		ptr = sg_virt(sg);
+		while (left) {
+			if ((left >=  MSDC_FIFO_THD) && (msdc_rxfifocnt() >= MSDC_FIFO_THD)) {
+				count = MSDC_FIFO_THD >> 2;
+				do {
+					*ptr++ = msdc_fifo_read32();
+				} while (--count);
+				left -= MSDC_FIFO_THD;
+			} else if ((left < MSDC_FIFO_THD) && msdc_rxfifocnt() >= left) {
+				while (left > 3) {
+					*ptr++ = msdc_fifo_read32();
+					left -= 4;
+				}
+
+				u8ptr = (u8 *)ptr;
+				while(left) {
+					* u8ptr++ = msdc_fifo_read8();
+					left--;
+				}
+			}
+
+			if (msdc_pio_abort(host, data, tmo))
+				goto end;
+		}
+		size += sg_dma_len(sg);
+		sg = sg_next(sg); num--;
+	}
+end:
+	data->bytes_xfered += size;
+	//printk("        PIO Read<%d>bytes\n", size);
+
+	sdr_clr_bits(MSDC_INTEN, wints);
+	if(data->error)
+		printk("read pio data->error<%d> left<%d> size<%d>\n", data->error, left, size);
+
+	return data->error;
+}
+
+static int msdc_pio_write(struct msdc_host* host, struct mmc_data *data)
+{
+	u32  base = host->base;
+	struct scatterlist *sg = data->sg;
+	u32  num = data->sg_len;
+	u32 *ptr;
+	u8  *u8ptr;
+	u32  left;
+	u32  count, size = 0;
+	u32  wints = MSDC_INTEN_DATTMO | MSDC_INTEN_DATCRCERR;
+	unsigned long tmo = jiffies + DAT_TIMEOUT;
+
+	sdr_set_bits(MSDC_INTEN, wints);
+	while (num) {
+		left = sg_dma_len(sg);
+		ptr = sg_virt(sg);
+
+		while (left) {
+			if (left >= MSDC_FIFO_SZ && msdc_txfifocnt() == 0) {
+				count = MSDC_FIFO_SZ >> 2;
+				do {
+					msdc_fifo_write32(*ptr); ptr++;
+				} while (--count);
+				left -= MSDC_FIFO_SZ;
+			} else if (left < MSDC_FIFO_SZ && msdc_txfifocnt() == 0) {
+				while (left > 3) {
+					msdc_fifo_write32(*ptr); ptr++;
+					left -= 4;
+				}
+
+				u8ptr = (u8*)ptr;
+				while( left) {
+					msdc_fifo_write8(*u8ptr);
+					u8ptr++;
+					left--;
+				}
+			}
+
+			if (msdc_pio_abort(host, data, tmo))
+				goto end;
+		}
+		size += sg_dma_len(sg);
+		sg = sg_next(sg); num--;
+	}
+end:
+	data->bytes_xfered += size;
+	//printk("        PIO Write<%d>bytes\n", size);
+	if(data->error)
+		printk("write pio data->error<%d>\n", data->error);
+
+	sdr_clr_bits(MSDC_INTEN, wints);
+
+	return data->error;
+}
+
+static void msdc_dma_start(struct msdc_host *host)
+{
+	u32 base = host->base;
+	u32 wints = MSDC_INTEN_XFER_COMPL | MSDC_INTEN_DATTMO | MSDC_INTEN_DATCRCERR;
+
+	sdr_set_bits(MSDC_INTEN, wints);
+	sdr_set_field(MSDC_DMA_CTRL, MSDC_DMA_CTRL_START, 1);
+
+	//printk("DMA start\n");
+}
+
+static void msdc_dma_stop(struct msdc_host *host)
+{
+	u32 base = host->base;
+	u32 wints = MSDC_INTEN_XFER_COMPL | MSDC_INTEN_DATTMO | MSDC_INTEN_DATCRCERR;
+
+	//printk("DMA status: 0x%.8x\n",sdr_read32(MSDC_DMA_CFG));
+
+	sdr_set_field(MSDC_DMA_CTRL, MSDC_DMA_CTRL_STOP, 1);
+	while (sdr_read32(MSDC_DMA_CFG) & MSDC_DMA_CFG_STS);
+	sdr_clr_bits(MSDC_INTEN, wints); /* Not just xfer_comp */
+
+	//printk("DMA stop\n");
+}
+
+static u8 msdc_dma_calcs(u8 *buf, u32 len)
+{
+	u32 i, sum = 0;
+
+	for (i = 0; i < len; i++)
+		sum += buf[i];
+
+	return 0xFF - (u8)sum;
+}
+
+static int msdc_dma_config(struct msdc_host *host, struct msdc_dma *dma)
+{
+	u32 base = host->base;
+	u32 sglen = dma->sglen;
+	u32 j, num, bdlen;
+	u8  blkpad, dwpad, chksum;
+	struct scatterlist *sg = dma->sg;
+	gpd_t *gpd;
+	bd_t *bd;
+
+	switch (dma->mode) {
+	case MSDC_MODE_DMA_BASIC:
+		BUG_ON(dma->xfersz > 65535);
+		BUG_ON(dma->sglen != 1);
+		sdr_write32(MSDC_DMA_SA, PHYSADDR(sg_dma_address(sg)));
+		sdr_set_field(MSDC_DMA_CTRL, MSDC_DMA_CTRL_LASTBUF, 1);
+		sdr_set_field(MSDC_DMA_CTRL, MSDC_DMA_CTRL_XFERSZ, sg_dma_len(sg));
+		sdr_set_field(MSDC_DMA_CTRL, MSDC_DMA_CTRL_BRUSTSZ, dma->burstsz);
+		sdr_set_field(MSDC_DMA_CTRL, MSDC_DMA_CTRL_MODE, 0);
+		break;
+
+	case MSDC_MODE_DMA_DESC:
+		blkpad = (dma->flags & DMA_FLAG_PAD_BLOCK) ? 1 : 0;
+		dwpad  = (dma->flags & DMA_FLAG_PAD_DWORD) ? 1 : 0;
+		chksum = (dma->flags & DMA_FLAG_EN_CHKSUM) ? 1 : 0;
+
+		num = (sglen + MAX_BD_PER_GPD - 1) / MAX_BD_PER_GPD;
+		BUG_ON(num !=1 );
+
+		gpd = dma->gpd;
+		bd = dma->bd;
+		bdlen = sglen;
+
+		gpd->hwo = 1;  /* hw will clear it */
+		gpd->bdp = 1;
+		gpd->chksum = 0;  /* need to clear first. */
+		gpd->chksum = (chksum ? msdc_dma_calcs((u8 *)gpd, 16) : 0);
+
+		for (j = 0; j < bdlen; j++) {
+			msdc_init_bd(&bd[j], blkpad, dwpad, sg_dma_address(sg), sg_dma_len(sg));
+			if( j == bdlen - 1)
+				bd[j].eol = 1;
+			else
+				bd[j].eol = 0;
+			bd[j].chksum = 0; /* checksume need to clear first */
+			bd[j].chksum = (chksum ? msdc_dma_calcs((u8 *)(&bd[j]), 16) : 0);
+			sg++;
+		}
+
+		dma->used_gpd += 2;
+		dma->used_bd += bdlen;
+
+		sdr_set_field(MSDC_DMA_CFG, MSDC_DMA_CFG_DECSEN, chksum);
+		sdr_set_field(MSDC_DMA_CTRL, MSDC_DMA_CTRL_BRUSTSZ, dma->burstsz);
+		sdr_set_field(MSDC_DMA_CTRL, MSDC_DMA_CTRL_MODE, 1);
+		sdr_write32(MSDC_DMA_SA, PHYSADDR((u32)dma->gpd_addr));
+		break;
+	}
+
+//	printk("DMA_CTRL = 0x%x\n", sdr_read32(MSDC_DMA_CTRL));
+//	printk("DMA_CFG  = 0x%x\n", sdr_read32(MSDC_DMA_CFG));
+//	printk("DMA_SA   = 0x%x\n", sdr_read32(MSDC_DMA_SA));
+
+	return 0;
+}
+
+static void msdc_dma_setup(struct msdc_host *host, struct msdc_dma *dma,
+			struct scatterlist *sg, unsigned int sglen)
+{
+	BUG_ON(sglen > MAX_BD_NUM);
+
+	dma->sg = sg;
+	dma->flags = DMA_FLAG_EN_CHKSUM;
+	dma->sglen = sglen;
+	dma->xfersz = host->xfer_size;
+	dma->burstsz = MSDC_BRUST_64B;
+
+	if (sglen == 1 && sg_dma_len(sg) <= MAX_DMA_CNT)
+		dma->mode = MSDC_MODE_DMA_BASIC;
+	else
+		dma->mode = MSDC_MODE_DMA_DESC;
+
+//	printk("DMA mode<%d> sglen<%d> xfersz<%d>\n", dma->mode, dma->sglen, dma->xfersz);
+
+	msdc_dma_config(host, dma);
+}
+
+static void msdc_set_blknum(struct msdc_host *host, u32 blknum)
+{
+	u32 base = host->base;
+
+	sdr_write32(SDC_BLK_NUM, blknum);
+}
+
+static int msdc_do_request(struct mmc_host*mmc, struct mmc_request*mrq)
+{
+	struct msdc_host *host = mmc_priv(mmc);
+	struct mmc_command *cmd;
+	struct mmc_data *data;
+	u32 base = host->base;
+	unsigned int left=0;
+	int dma = 0, read = 1, dir = DMA_FROM_DEVICE, send_type=0;
+
+#define SND_DAT 0
+#define SND_CMD 1
+
+	BUG_ON(mmc == NULL);
+	BUG_ON(mrq == NULL);
+
+	host->error = 0;
+	atomic_set(&host->abort, 0);
+
+	cmd  = mrq->cmd;
+	data = mrq->cmd->data;
+
+	if (!data) {
+		send_type = SND_CMD;
+		if (msdc_do_command(host, cmd, 1, CMD_TIMEOUT) != 0)
+			goto done;
+	} else {
+		BUG_ON(data->blksz > HOST_MAX_BLKSZ);
+		send_type=SND_DAT;
+
+		data->error = 0;
+		read = data->flags & MMC_DATA_READ ? 1 : 0;
+		host->data = data;
+		host->xfer_size = data->blocks * data->blksz;
+		host->blksz = data->blksz;
+
+		host->dma_xfer = dma = ((host->xfer_size >= 512) ? 1 : 0);
+
+		if (read)
+			if ((host->timeout_ns != data->timeout_ns) ||
+					(host->timeout_clks != data->timeout_clks))
+				msdc_set_timeout(host, data->timeout_ns, data->timeout_clks);
+
+			msdc_set_blknum(host, data->blocks);
+
+			if (dma) {
+				msdc_dma_on();
+				init_completion(&host->xfer_done);
+
+				if (msdc_command_start(host, cmd, 1, CMD_TIMEOUT) != 0)
+					goto done;
+
+				dir = read ? DMA_FROM_DEVICE : DMA_TO_DEVICE;
+				dma_map_sg(mmc_dev(mmc), data->sg, data->sg_len, dir);
+				msdc_dma_setup(host, &host->dma, data->sg, data->sg_len);
+
+				if (msdc_command_resp(host, cmd, 1, CMD_TIMEOUT) != 0)
+					goto done;
+
+				msdc_dma_start(host);
+
+				spin_unlock(&host->lock);
+				if (!wait_for_completion_timeout(&host->xfer_done, DAT_TIMEOUT)) {
+					/*printk("XXX CMD<%d> wait xfer_done<%d> timeout!!\n", cmd->opcode, data->blocks * data->blksz);
+					printk("    DMA_SA   = 0x%x\n", sdr_read32(MSDC_DMA_SA));
+					printk("    DMA_CA   = 0x%x\n", sdr_read32(MSDC_DMA_CA));
+					printk("    DMA_CTRL = 0x%x\n", sdr_read32(MSDC_DMA_CTRL));
+					printk("    DMA_CFG  = 0x%x\n", sdr_read32(MSDC_DMA_CFG));*/
+					data->error = (unsigned int)-ETIMEDOUT;
+
+					msdc_reset();
+					msdc_clr_fifo();
+					msdc_clr_int();
+				}
+				spin_lock(&host->lock);
+				msdc_dma_stop(host);
+			} else {
+				if (msdc_do_command(host, cmd, 1, CMD_TIMEOUT) != 0)
+					goto done;
+
+				if (read) {
+					if (msdc_pio_read(host, data))
+						goto done;
+				} else {
+					if (msdc_pio_write(host, data))
+						goto done;
+				}
+
+			if (!read) {
+				while (1) {
+					left = msdc_txfifocnt();
+					if (left == 0) {
+						break;
+					}
+					if (msdc_pio_abort(host, data, jiffies + DAT_TIMEOUT)) {
+						break;
+					/* Fix me: what about if data error, when stop ? how to? */
+					}
+				}
+			} else {
+				/* Fix me: read case: need to check CRC error */	
+			}
+
+			/* For write case: SDCBUSY and Xfer_Comp will assert when DAT0 not busy. 
+			   For read case : SDCBUSY and Xfer_Comp will assert when last byte read out from FIFO.
+			*/
+
+			/* try not to wait xfer_comp interrupt. 
+			the next command will check SDC_BUSY. 
+			SDC_BUSY means xfer_comp assert 
+			*/ 
+
+		} // PIO mode 
+
+		/* Last: stop transfer */
+		if (data->stop){ 
+			if (msdc_do_command(host, data->stop, 0, CMD_TIMEOUT) != 0) {
+				goto done; 
+			}
+		} 
+	}
+
+done:
+	if (data != NULL) {
+		host->data = NULL;
+		host->dma_xfer = 0;    
+		if (dma != 0) {
+			msdc_dma_off();     
+			host->dma.used_bd  = 0;
+			host->dma.used_gpd = 0;
+			dma_unmap_sg(mmc_dev(mmc), data->sg, data->sg_len, dir);
+		}
+		host->blksz = 0;  
+
+	//	printk("CMD<%d> data<%s %s> blksz<%d> block<%d> error<%d>",cmd->opcode, (dma? "dma":"pio\n"), 
+	//		(read ? "read ":"write") ,data->blksz, data->blocks, data->error);                
+	}
+
+	if (mrq->cmd->error) host->error = 0x001;
+	if (mrq->data && mrq->data->error) host->error |= 0x010;     
+	if (mrq->stop && mrq->stop->error) host->error |= 0x100; 
+
+	//if (host->error) printk("host->error<%d>\n", host->error);     
+
+	return host->error;
+}
+
+static int msdc_app_cmd(struct mmc_host *mmc, struct msdc_host *host)
+{
+    struct mmc_command cmd;    
+    struct mmc_request mrq;
+    u32 err; 
+
+    memset(&cmd, 0, sizeof(struct mmc_command));    
+    cmd.opcode = MMC_APP_CMD;    
+#if 0   /* bug: we meet mmc->card is null when ACMD6 */   
+    cmd.arg = mmc->card->rca << 16;
+#else 
+    cmd.arg = host->app_cmd_arg;     
+#endif    
+    cmd.flags = MMC_RSP_SPI_R1 | MMC_RSP_R1 | MMC_CMD_AC;
+
+    memset(&mrq, 0, sizeof(struct mmc_request));
+    mrq.cmd = &cmd; cmd.mrq = &mrq;
+    cmd.data = NULL;        
+
+    err = msdc_do_command(host, &cmd, 0, CMD_TIMEOUT);     
+    return err;      	
+}
+
+static int msdc_tune_cmdrsp(struct msdc_host*host, struct mmc_command *cmd)
+{
+    int result = -1;
+    u32 base = host->base;
+    u32 rsmpl, cur_rsmpl, orig_rsmpl;
+    u32 rrdly, cur_rrdly = 0, orig_rrdly;
+    u32 skip = 1;
+    
+    /* ==== don't support 3.0 now ====
+           1: R_SMPL[1] 
+           2: PAD_CMD_RESP_RXDLY[26:22] 
+	    ==========================*/
+
+    // save the previous tune result 
+    sdr_get_field(MSDC_IOCON,    MSDC_IOCON_RSPL,        orig_rsmpl);
+    sdr_get_field(MSDC_PAD_TUNE, MSDC_PAD_TUNE_CMDRRDLY, orig_rrdly);
+
+    rrdly = 0; 
+    do {
+        for (rsmpl = 0; rsmpl < 2; rsmpl++) {
+            /* Lv1: R_SMPL[1] */    	
+            cur_rsmpl = (orig_rsmpl + rsmpl) % 2;         
+            if (skip == 1) {
+                skip = 0; 	
+                continue;	
+            }
+            sdr_set_field(MSDC_IOCON, MSDC_IOCON_RSPL, cur_rsmpl); 
+
+            if (host->app_cmd) {
+                result = msdc_app_cmd(host->mmc, host);	
+                if (result) {
+                    //printk("TUNE_CMD app_cmd<%d> failed: RESP_RXDLY<%d>,R_SMPL<%d>\n", 
+                      //   host->mrq->cmd->opcode, cur_rrdly, cur_rsmpl);
+                    continue;
+                } 
+            }          
+            result = msdc_do_command(host, cmd, 0, CMD_TIMEOUT); // not tune.             
+            //printk("TUNE_CMD<%d> %s PAD_CMD_RESP_RXDLY[26:22]<%d> R_SMPL[1]<%d>\n", cmd->opcode,
+//                       (result == 0) ? "PASS" : "FAIL", cur_rrdly, cur_rsmpl);
+                       	
+            if (result == 0) {
+                return 0; 	
+            }                        	
+            if (result != (unsigned int)(-EIO)) { 
+              //  printk("TUNE_CMD<%d> Error<%d> not -EIO\n", cmd->opcode, result);	
+                return result;	 
+            }
+
+            /* should be EIO */
+            if (sdr_read32(SDC_CMD) & 0x1800) { /* check if has data phase */ 
+                msdc_abort_data(host);
+            }
+        }
+		
+        /* Lv2: PAD_CMD_RESP_RXDLY[26:22] */              	
+        cur_rrdly = (orig_rrdly + rrdly + 1) % 32;
+        sdr_set_field(MSDC_PAD_TUNE, MSDC_PAD_TUNE_CMDRRDLY, cur_rrdly);		
+    }while (++rrdly < 32);
+	
+    return result;
+}
+
+/* Support SD2.0 Only */
+static int msdc_tune_bread(struct mmc_host *mmc, struct mmc_request *mrq)
+{
+    struct msdc_host *host = mmc_priv(mmc);
+    u32 base = host->base;
+    u32 ddr=0;
+    u32 dcrc = 0;
+    u32 rxdly, cur_rxdly0, cur_rxdly1;
+    u32 dsmpl, cur_dsmpl,  orig_dsmpl;
+    u32 cur_dat0,  cur_dat1,  cur_dat2,  cur_dat3;
+    u32 cur_dat4,  cur_dat5,  cur_dat6,  cur_dat7;
+    u32 orig_dat0, orig_dat1, orig_dat2, orig_dat3;
+    u32 orig_dat4, orig_dat5, orig_dat6, orig_dat7;
+    int result = -1;
+    u32 skip = 1;
+
+    sdr_get_field(MSDC_IOCON, MSDC_IOCON_DSPL, orig_dsmpl);
+	
+    /* Tune Method 2. */
+    sdr_set_field(MSDC_IOCON, MSDC_IOCON_DDLSEL, 1);
+
+    rxdly = 0; 
+    do {
+        for (dsmpl = 0; dsmpl < 2; dsmpl++) {
+            cur_dsmpl = (orig_dsmpl + dsmpl) % 2;
+            if (skip == 1) {
+                skip = 0; 	
+                continue;	
+            }             
+            sdr_set_field(MSDC_IOCON, MSDC_IOCON_DSPL, cur_dsmpl);
+
+            if (host->app_cmd) {
+                result = msdc_app_cmd(host->mmc, host);	
+                if (result) {
+                    //printk("TUNE_BREAD app_cmd<%d> failed\n", host->mrq->cmd->opcode);	
+                    continue;
+                } 
+            } 
+            result = msdc_do_request(mmc,mrq);
+            
+            sdr_get_field(SDC_DCRC_STS, SDC_DCRC_STS_POS|SDC_DCRC_STS_NEG, dcrc); /* RO */
+            if (!ddr) dcrc &= ~SDC_DCRC_STS_NEG;
+            //printk("TUNE_BREAD<%s> dcrc<0x%x> DATRDDLY0/1<0x%x><0x%x> dsmpl<0x%x>\n",
+                       // (result == 0 && dcrc == 0) ? "PASS" : "FAIL", dcrc,
+                       // sdr_read32(MSDC_DAT_RDDLY0), sdr_read32(MSDC_DAT_RDDLY1), cur_dsmpl);
+
+            /* Fix me: result is 0, but dcrc is still exist */
+            if (result == 0 && dcrc == 0) {
+                goto done;
+            } else {
+                /* there is a case: command timeout, and data phase not processed */
+                if (mrq->data->error != 0 && mrq->data->error != (unsigned int)(-EIO)) {
+                    //printk("TUNE_READ: result<0x%x> cmd_error<%d> data_error<%d>\n", 
+                         //      result, mrq->cmd->error, mrq->data->error);	
+                    goto done;     	
+                }
+            }
+        }    
+
+        cur_rxdly0 = sdr_read32(MSDC_DAT_RDDLY0);
+        cur_rxdly1 = sdr_read32(MSDC_DAT_RDDLY1);
+
+        /* E1 ECO. YD: Reverse */
+        if (sdr_read32(MSDC_ECO_VER) >= 4) {
+            orig_dat0 = (cur_rxdly0 >> 24) & 0x1F;
+            orig_dat1 = (cur_rxdly0 >> 16) & 0x1F;
+            orig_dat2 = (cur_rxdly0 >>  8) & 0x1F;
+            orig_dat3 = (cur_rxdly0 >>  0) & 0x1F;
+            orig_dat4 = (cur_rxdly1 >> 24) & 0x1F;
+            orig_dat5 = (cur_rxdly1 >> 16) & 0x1F;
+            orig_dat6 = (cur_rxdly1 >>  8) & 0x1F;
+            orig_dat7 = (cur_rxdly1 >>  0) & 0x1F;
+        } else {   
+            orig_dat0 = (cur_rxdly0 >>  0) & 0x1F;
+            orig_dat1 = (cur_rxdly0 >>  8) & 0x1F;
+            orig_dat2 = (cur_rxdly0 >> 16) & 0x1F;
+            orig_dat3 = (cur_rxdly0 >> 24) & 0x1F;
+            orig_dat4 = (cur_rxdly1 >>  0) & 0x1F;
+            orig_dat5 = (cur_rxdly1 >>  8) & 0x1F;
+            orig_dat6 = (cur_rxdly1 >> 16) & 0x1F;
+            orig_dat7 = (cur_rxdly1 >> 24) & 0x1F;
+        }
+                
+        if (ddr) {
+            cur_dat0 = (dcrc & (1 << 0) || dcrc & (1 << 8))  ? ((orig_dat0 + 1) % 32) : orig_dat0;
+            cur_dat1 = (dcrc & (1 << 1) || dcrc & (1 << 9))  ? ((orig_dat1 + 1) % 32) : orig_dat1;
+            cur_dat2 = (dcrc & (1 << 2) || dcrc & (1 << 10)) ? ((orig_dat2 + 1) % 32) : orig_dat2;
+            cur_dat3 = (dcrc & (1 << 3) || dcrc & (1 << 11)) ? ((orig_dat3 + 1) % 32) : orig_dat3;
+        } else {
+            cur_dat0 = (dcrc & (1 << 0)) ? ((orig_dat0 + 1) % 32) : orig_dat0;
+            cur_dat1 = (dcrc & (1 << 1)) ? ((orig_dat1 + 1) % 32) : orig_dat1;
+            cur_dat2 = (dcrc & (1 << 2)) ? ((orig_dat2 + 1) % 32) : orig_dat2;
+            cur_dat3 = (dcrc & (1 << 3)) ? ((orig_dat3 + 1) % 32) : orig_dat3;
+        }
+        cur_dat4 = (dcrc & (1 << 4)) ? ((orig_dat4 + 1) % 32) : orig_dat4;
+        cur_dat5 = (dcrc & (1 << 5)) ? ((orig_dat5 + 1) % 32) : orig_dat5;
+        cur_dat6 = (dcrc & (1 << 6)) ? ((orig_dat6 + 1) % 32) : orig_dat6;
+        cur_dat7 = (dcrc & (1 << 7)) ? ((orig_dat7 + 1) % 32) : orig_dat7;
+
+        cur_rxdly0 = (cur_dat0 << 24) | (cur_dat1 << 16) | (cur_dat2 << 8) | (cur_dat3 << 0);
+        cur_rxdly1 = (cur_dat4 << 24) | (cur_dat5 << 16) | (cur_dat6 << 8) | (cur_dat7 << 0);
+
+        sdr_write32(MSDC_DAT_RDDLY0, cur_rxdly0);
+        sdr_write32(MSDC_DAT_RDDLY1, cur_rxdly1);
+
+    } while (++rxdly < 32);   
+          
+done:
+    return result;
+}
+
+static int msdc_tune_bwrite(struct mmc_host *mmc,struct mmc_request *mrq)
+{
+	  struct msdc_host *host = mmc_priv(mmc);
+    u32 base = host->base;
+
+    u32 wrrdly, cur_wrrdly = 0, orig_wrrdly;
+    u32 dsmpl,  cur_dsmpl,  orig_dsmpl;
+    u32 rxdly,  cur_rxdly0;
+    u32 orig_dat0, orig_dat1, orig_dat2, orig_dat3;
+    u32 cur_dat0,  cur_dat1,  cur_dat2,  cur_dat3;
+    int result = -1;
+    u32 skip = 1;
+
+    // MSDC_IOCON_DDR50CKD need to check. [Fix me] 
+    
+    sdr_get_field(MSDC_PAD_TUNE, MSDC_PAD_TUNE_DATWRDLY, orig_wrrdly);
+    sdr_get_field(MSDC_IOCON,    MSDC_IOCON_DSPL,        orig_dsmpl );
+
+    /* Tune Method 2. just DAT0 */  
+    sdr_set_field(MSDC_IOCON, MSDC_IOCON_DDLSEL, 1);
+    cur_rxdly0 = sdr_read32(MSDC_DAT_RDDLY0);
+    
+    /* E1 ECO. YD: Reverse */
+    if (sdr_read32(MSDC_ECO_VER) >= 4) {
+        orig_dat0 = (cur_rxdly0 >> 24) & 0x1F;
+        orig_dat1 = (cur_rxdly0 >> 16) & 0x1F;
+        orig_dat2 = (cur_rxdly0 >>  8) & 0x1F;
+        orig_dat3 = (cur_rxdly0 >>  0) & 0x1F;
+    } else {
+        orig_dat0 = (cur_rxdly0 >>  0) & 0x1F;
+        orig_dat1 = (cur_rxdly0 >>  8) & 0x1F;
+        orig_dat2 = (cur_rxdly0 >> 16) & 0x1F;
+        orig_dat3 = (cur_rxdly0 >> 24) & 0x1F;
+    }
+
+    rxdly = 0;
+    do {
+        wrrdly = 0;
+        do {    
+            for (dsmpl = 0; dsmpl < 2; dsmpl++) {
+                cur_dsmpl = (orig_dsmpl + dsmpl) % 2;
+                if (skip == 1) {
+                    skip = 0;
+                    continue; 	
+                }    
+                sdr_set_field(MSDC_IOCON, MSDC_IOCON_DSPL, cur_dsmpl);
+                
+                if (host->app_cmd) {
+                    result = msdc_app_cmd(host->mmc, host);	
+                    if (result) {
+                        //printk("TUNE_BWRITE app_cmd<%d> failed\n", host->mrq->cmd->opcode);	
+                        continue;
+                    } 
+                }             
+                result = msdc_do_request(mmc,mrq);
+            
+                //printk("TUNE_BWRITE<%s> DSPL<%d> DATWRDLY<%d> MSDC_DAT_RDDLY0<0x%x>\n", 
+                  //        result == 0 ? "PASS" : "FAIL", 
+                    //      cur_dsmpl, cur_wrrdly, cur_rxdly0);
+            
+                if (result == 0) {
+                    goto done;
+                }
+                else {
+                    /* there is a case: command timeout, and data phase not processed */
+                    if (mrq->data->error != (unsigned int)(-EIO)) {
+                        //printk("TUNE_READ: result<0x%x> cmd_error<%d> data_error<%d>\n", 
+                        //  &&         result, mrq->cmd->error, mrq->data->error);	
+                        goto done;     	
+                    }
+                }       
+            }
+            cur_wrrdly = (orig_wrrdly + wrrdly + 1) % 32;
+            sdr_set_field(MSDC_PAD_TUNE, MSDC_PAD_TUNE_DATWRDLY, cur_wrrdly);             
+        } while (++wrrdly < 32); 
+        
+        cur_dat0 = (orig_dat0 + rxdly) % 32; /* only adjust bit-1 for crc */
+        cur_dat1 = orig_dat1;
+        cur_dat2 = orig_dat2;
+        cur_dat3 = orig_dat3;                    
+    
+        cur_rxdly0 = (cur_dat0 << 24) | (cur_dat1 << 16) | (cur_dat2 << 8) | (cur_dat3 << 0);       
+        sdr_write32(MSDC_DAT_RDDLY0, cur_rxdly0);    
+    } while (++rxdly < 32); 
+
+done:
+    return result;
+}
+
+static int msdc_get_card_status(struct mmc_host *mmc, struct msdc_host *host, u32 *status)
+{
+	struct mmc_command cmd;
+	struct mmc_request mrq;
+	u32 err;
+
+	memset(&cmd, 0, sizeof(struct mmc_command));
+	cmd.opcode = MMC_SEND_STATUS;
+	if (mmc->card) {
+		cmd.arg = mmc->card->rca << 16;
+	} else {
+		//printk("cmd13 mmc card is null\n");
+		cmd.arg = host->app_cmd_arg;
+	}
+	cmd.flags = MMC_RSP_SPI_R2 | MMC_RSP_R1 | MMC_CMD_AC;
+
+	memset(&mrq, 0, sizeof(struct mmc_request));
+	mrq.cmd = &cmd; cmd.mrq = &mrq;
+	cmd.data = NULL;
+
+	err = msdc_do_command(host, &cmd, 1, CMD_TIMEOUT);
+
+	if (status)
+		*status = cmd.resp[0];
+
+	return err;
+}
+
+static int msdc_check_busy(struct mmc_host *mmc, struct msdc_host *host)
+{
+	u32 err = 0;
+	u32 status = 0;
+
+	do {
+		err = msdc_get_card_status(mmc, host, &status);
+		if (err)
+			return err;
+		/* need cmd12? */
+		//printk("cmd<13> resp<0x%x>\n", status);
+	} while (R1_CURRENT_STATE(status) == 7);
+
+	return err;
+}
+
+static int msdc_tune_request(struct mmc_host *mmc, struct mmc_request *mrq)
+{
+	struct msdc_host *host = mmc_priv(mmc);
+	struct mmc_command *cmd;
+	struct mmc_data *data;
+	int ret=0, read;
+
+	cmd  = mrq->cmd;
+	data = mrq->cmd->data;
+
+	read = data->flags & MMC_DATA_READ ? 1 : 0;
+
+	if (read) {
+		if (data->error == (unsigned int)(-EIO))
+			ret = msdc_tune_bread(mmc,mrq);
+	} else {
+		ret = msdc_check_busy(mmc, host);
+		if (ret){
+			//printk("XXX cmd13 wait program done failed\n");
+			return ret;
+		}
+		/* CRC and TO */
+		/* Fix me: don't care card status? */
+		ret = msdc_tune_bwrite(mmc,mrq);
+	}
+
+	return ret;
+}
+
+static void msdc_ops_request(struct mmc_host *mmc,struct mmc_request *mrq)
+{
+	struct msdc_host *host = mmc_priv(mmc);
+
+	if (host->mrq) {
+		//printk("XXX host->mrq<0x%.8x>\n", (int)host->mrq);
+		BUG();
+	}
+	if (!is_card_present(host) || host->power_mode == MMC_POWER_OFF) {
+		//printk("cmd<%d> card<%d> power<%d>\n", mrq->cmd->opcode, is_card_present(host), host->power_mode);
+		mrq->cmd->error = (unsigned int)-ENOMEDIUM;
+		mrq->done(mrq);
+		return;
+	}
+	spin_lock(&host->lock);
+
+	host->mrq = mrq;
+
+	if (msdc_do_request(mmc,mrq))
+		if(host->hw->flags & MSDC_REMOVABLE && mrq->data && mrq->data->error)
+			msdc_tune_request(mmc,mrq);
+
+	if (mrq->cmd->opcode == MMC_APP_CMD) {
+		host->app_cmd = 1;
+		host->app_cmd_arg = mrq->cmd->arg;  /* save the RCA */
+	} else {
+		host->app_cmd = 0;
+	}
+
+	host->mrq = NULL;
+
+	spin_unlock(&host->lock);
+
+	mmc_request_done(mmc, mrq);
+}
+
+/* called by ops.set_ios */
+static void msdc_set_buswidth(struct msdc_host *host, u32 width)
+{
+    u32 base = host->base;
+    u32 val = sdr_read32(SDC_CFG);
+    
+    val &= ~SDC_CFG_BUSWIDTH;
+    
+    switch (width) {
+    default:
+    case MMC_BUS_WIDTH_1:
+        width = 1;
+        val |= (MSDC_BUS_1BITS << 16);
+        break;
+    case MMC_BUS_WIDTH_4:
+        val |= (MSDC_BUS_4BITS << 16);
+        break;
+    case MMC_BUS_WIDTH_8:
+        val |= (MSDC_BUS_8BITS << 16);
+        break;
+    }
+    
+    sdr_write32(SDC_CFG, val);
+
+    //printk("Bus Width = %d\n", width);
+}
+
+/* ops.set_ios */
+static void msdc_ops_set_ios(struct mmc_host *mmc, struct mmc_ios *ios)
+{
+	struct msdc_host *host = mmc_priv(mmc);
+	struct msdc_hw *hw=host->hw;
+	u32 base = host->base;
+	u32 ddr = 0;
+
+#ifdef MT6575_SD_DEBUG
+	static char *vdd[] = {
+	"1.50v", "1.55v", "1.60v", "1.65v", "1.70v", "1.80v", "1.90v",
+	"2.00v", "2.10v", "2.20v", "2.30v", "2.40v", "2.50v", "2.60v",
+	"2.70v", "2.80v", "2.90v", "3.00v", "3.10v", "3.20v", "3.30v",
+	"3.40v", "3.50v", "3.60v"		
+	};
+	static char *power_mode[] = {
+	"OFF", "UP", "ON"
+	};
+	static char *bus_mode[] = {
+	"UNKNOWN", "OPENDRAIN", "PUSHPULL"
+	};
+	static char *timing[] = {
+	"LEGACY", "MMC_HS", "SD_HS"
+	};
+
+	/*printk("SET_IOS: CLK(%dkHz), BUS(%s), BW(%u), PWR(%s), VDD(%s), TIMING(%s)\n",
+	ios->clock / 1000, bus_mode[ios->bus_mode],
+	(ios->bus_width == MMC_BUS_WIDTH_4) ? 4 : 1,
+	power_mode[ios->power_mode], vdd[ios->vdd], timing[ios->timing]);*/
+#endif
+
+	msdc_set_buswidth(host, ios->bus_width);
+
+	/* Power control ??? */
+	switch (ios->power_mode) {
+	case MMC_POWER_OFF:
+	case MMC_POWER_UP:
+		// msdc_set_power_mode(host, ios->power_mode); /* --- by chhung */
+		break;
+	case MMC_POWER_ON:
+		host->power_mode = MMC_POWER_ON;
+		break;
+	default:
+		break;
+	}
+
+	/* Clock control */
+	if (host->mclk != ios->clock) {
+		if(ios->clock > 25000000) {
+			//printk("SD data latch edge<%d>\n", hw->data_edge);
+			sdr_set_field(MSDC_IOCON, MSDC_IOCON_RSPL, hw->cmd_edge);
+			sdr_set_field(MSDC_IOCON, MSDC_IOCON_DSPL, hw->data_edge);
+		} else {
+			sdr_write32(MSDC_IOCON,      0x00000000);
+			sdr_write32(MSDC_DAT_RDDLY0, 0x10101010);	// for MT7620 E2 and afterward
+			sdr_write32(MSDC_DAT_RDDLY1, 0x00000000);
+			sdr_write32(MSDC_PAD_TUNE,   0x84101010);	// for MT7620 E2 and afterward
+		}
+		msdc_set_mclk(host, ddr, ios->clock);
+	}
+}
+
+/* ops.get_ro */
+static int msdc_ops_get_ro(struct mmc_host *mmc)
+{
+    struct msdc_host *host = mmc_priv(mmc);
+    u32 base = host->base;
+    unsigned long flags;
+    int ro = 0;
+
+    if (host->hw->flags & MSDC_WP_PIN_EN) { /* set for card */
+        spin_lock_irqsave(&host->lock, flags);
+        ro = (sdr_read32(MSDC_PS) >> 31);
+        spin_unlock_irqrestore(&host->lock, flags);
+    }
+    return ro;
+}
+
+/* ops.get_cd */
+static int msdc_ops_get_cd(struct mmc_host *mmc)
+{
+    struct msdc_host *host = mmc_priv(mmc);
+    u32 base = host->base;    
+    unsigned long flags;
+    int present = 1;
+
+    /* for sdio, MSDC_REMOVABLE not set, always return 1 */
+    if (!(host->hw->flags & MSDC_REMOVABLE)) {
+        /* For sdio, read H/W always get<1>, but may timeout some times */       	    	
+#if 1
+        host->card_inserted = 1;       
+        return 1;
+#else
+        host->card_inserted = (host->pm_state.event == PM_EVENT_USER_RESUME) ? 1 : 0; 
+        printk("sdio ops_get_cd<%d>\n", host->card_inserted);
+        return host->card_inserted; 
+#endif
+    }
+
+    /* MSDC_CD_PIN_EN set for card */
+    if (host->hw->flags & MSDC_CD_PIN_EN) {
+        spin_lock_irqsave(&host->lock, flags);
+#if 0        
+        present = host->card_inserted;  /* why not read from H/W: Fix me*/
+#else
+        present = (sdr_read32(MSDC_PS) & MSDC_PS_CDSTS) ? 0 : 1; 
+        host->card_inserted = present;  
+#endif        
+        spin_unlock_irqrestore(&host->lock, flags);
+    } else {
+        present = 0; /* TODO? Check DAT3 pins for card detection */
+    }
+
+    //printk("ops_get_cd return<%d>\n", present);
+    return present;
+}
+
+/* ops.enable_sdio_irq */
+static void msdc_ops_enable_sdio_irq(struct mmc_host *mmc, int enable)
+{
+    struct msdc_host *host = mmc_priv(mmc);
+    struct msdc_hw *hw = host->hw;
+    u32 base = host->base;
+    u32 tmp;
+
+    if (hw->flags & MSDC_EXT_SDIO_IRQ) { /* yes for sdio */
+        if (enable) {
+            hw->enable_sdio_eirq();  /* combo_sdio_enable_eirq */
+        } else {
+            hw->disable_sdio_eirq(); /* combo_sdio_disable_eirq */
+        }
+    } else { 
+    	  //printk("XXX \n");  /* so never enter here */
+        tmp = sdr_read32(SDC_CFG);
+        /* FIXME. Need to interrupt gap detection */
+        if (enable) {
+            tmp |= (SDC_CFG_SDIOIDE | SDC_CFG_SDIOINTWKUP);           
+        } else {
+            tmp &= ~(SDC_CFG_SDIOIDE | SDC_CFG_SDIOINTWKUP);
+        }
+        sdr_write32(SDC_CFG, tmp);      
+    }
+}
+
+static struct mmc_host_ops mt_msdc_ops = {
+    .request         = msdc_ops_request,
+    .set_ios         = msdc_ops_set_ios,
+    .get_ro          = msdc_ops_get_ro,
+    .get_cd          = msdc_ops_get_cd,
+    .enable_sdio_irq = msdc_ops_enable_sdio_irq,
+};
+
+/*--------------------------------------------------------------------------*/
+/* interrupt handler                                                    */
+/*--------------------------------------------------------------------------*/
+static irqreturn_t msdc_irq(int irq, void *dev_id)
+{
+    struct msdc_host  *host = (struct msdc_host *)dev_id;
+    struct mmc_data   *data = host->data;
+    struct mmc_command *cmd = host->cmd;
+    u32 base = host->base;
+        
+    u32 cmdsts = MSDC_INT_RSPCRCERR  | MSDC_INT_CMDTMO  | MSDC_INT_CMDRDY  |
+                 MSDC_INT_ACMDCRCERR | MSDC_INT_ACMDTMO | MSDC_INT_ACMDRDY |
+                 MSDC_INT_ACMD19_DONE;                 
+    u32 datsts = MSDC_INT_DATCRCERR  |MSDC_INT_DATTMO;
+
+    u32 intsts = sdr_read32(MSDC_INT);
+    u32 inten  = sdr_read32(MSDC_INTEN); inten &= intsts; 
+
+    sdr_write32(MSDC_INT, intsts);  /* clear interrupts */
+    /* MSG will cause fatal error */
+        
+    /* card change interrupt */
+    if (intsts & MSDC_INT_CDSC){
+        //printk("MSDC_INT_CDSC irq<0x%.8x>\n", intsts); 
+        tasklet_hi_schedule(&host->card_tasklet);
+        /* tuning when plug card ? */
+    }
+    
+    /* sdio interrupt */
+    if (intsts & MSDC_INT_SDIOIRQ){
+        //printk("XXX MSDC_INT_SDIOIRQ\n");  /* seems not sdio irq */
+        //mmc_signal_sdio_irq(host->mmc);
+    }
+
+    /* transfer complete interrupt */
+    if (data != NULL) {
+        if (inten & MSDC_INT_XFER_COMPL) {       	
+            data->bytes_xfered = host->dma.xfersz;
+            complete(&host->xfer_done);           
+        } 
+        
+        if (intsts & datsts) {         
+            /* do basic reset, or stop command will sdc_busy */
+            msdc_reset();
+            msdc_clr_fifo();        
+            msdc_clr_int();             
+            atomic_set(&host->abort, 1);  /* For PIO mode exit */
+            
+            if (intsts & MSDC_INT_DATTMO){
+               	//printk("XXX CMD<%d> MSDC_INT_DATTMO\n", host->mrq->cmd->opcode);
+               	data->error = (unsigned int)-ETIMEDOUT;
+            }
+            else if (intsts & MSDC_INT_DATCRCERR){
+                //printk("XXX CMD<%d> MSDC_INT_DATCRCERR, SDC_DCRC_STS<0x%x>\n", host->mrq->cmd->opcode, sdr_read32(SDC_DCRC_STS));
+                data->error = (unsigned int)-EIO;
+            }
+                                    
+            //if(sdr_read32(MSDC_INTEN) & MSDC_INT_XFER_COMPL) {  
+            if (host->dma_xfer) {
+                complete(&host->xfer_done); /* Read CRC come fast, XFER_COMPL not enabled */
+            } /* PIO mode can't do complete, because not init */
+        }
+    }
+
+    /* command interrupts */
+    if ((cmd != NULL) && (intsts & cmdsts)) {
+        if ((intsts & MSDC_INT_CMDRDY) || (intsts & MSDC_INT_ACMDRDY) || 
+            (intsts & MSDC_INT_ACMD19_DONE)) {
+            u32 *rsp = &cmd->resp[0];
+            
+            switch (host->cmd_rsp) {
+            case RESP_NONE:
+                break;
+            case RESP_R2:
+                *rsp++ = sdr_read32(SDC_RESP3); *rsp++ = sdr_read32(SDC_RESP2);
+                *rsp++ = sdr_read32(SDC_RESP1); *rsp++ = sdr_read32(SDC_RESP0);
+                break;
+            default: /* Response types 1, 3, 4, 5, 6, 7(1b) */
+                if ((intsts & MSDC_INT_ACMDRDY) || (intsts & MSDC_INT_ACMD19_DONE)) {
+                    *rsp = sdr_read32(SDC_ACMD_RESP);
+                } else {
+                    *rsp = sdr_read32(SDC_RESP0);    
+                }
+                break;
+            }
+        } else if ((intsts & MSDC_INT_RSPCRCERR) || (intsts & MSDC_INT_ACMDCRCERR)) {
+            if(intsts & MSDC_INT_ACMDCRCERR){
+                //printk("XXX CMD<%d> MSDC_INT_ACMDCRCERR\n",cmd->opcode);
+            } 
+            else {
+                //printk("XXX CMD<%d> MSDC_INT_RSPCRCERR\n",cmd->opcode);
+            }
+            cmd->error = (unsigned int)-EIO;
+        } else if ((intsts & MSDC_INT_CMDTMO) || (intsts & MSDC_INT_ACMDTMO)) {
+            if(intsts & MSDC_INT_ACMDTMO){
+                //printk("XXX CMD<%d> MSDC_INT_ACMDTMO\n",cmd->opcode);
+            }
+            else {
+                //printk("XXX CMD<%d> MSDC_INT_CMDTMO\n",cmd->opcode);
+            }
+            cmd->error = (unsigned int)-ETIMEDOUT;
+            msdc_reset();
+            msdc_clr_fifo();        
+            msdc_clr_int();            
+        }
+        complete(&host->cmd_done);
+    }
+
+    /* mmc irq interrupts */
+    if (intsts & MSDC_INT_MMCIRQ) {
+        //printk(KERN_INFO "msdc[%d] MMCIRQ: SDC_CSTS=0x%.8x\r\n", host->id, sdr_read32(SDC_CSTS));    
+    }
+    
+#ifdef MT6575_SD_DEBUG
+    {
+        msdc_int_reg *int_reg = (msdc_int_reg*)&intsts;
+        /*printk("IRQ_EVT(0x%x): MMCIRQ(%d) CDSC(%d), ACRDY(%d), ACTMO(%d), ACCRE(%d) AC19DN(%d)\n", 
+            intsts,
+            int_reg->mmcirq,
+            int_reg->cdsc,
+            int_reg->atocmdrdy,
+            int_reg->atocmdtmo,
+            int_reg->atocmdcrc,
+            int_reg->atocmd19done);
+        printk("IRQ_EVT(0x%x): SDIO(%d) CMDRDY(%d), CMDTMO(%d), RSPCRC(%d), CSTA(%d)\n", 
+            intsts,
+            int_reg->sdioirq,
+            int_reg->cmdrdy,
+            int_reg->cmdtmo,
+            int_reg->rspcrc,
+            int_reg->csta);
+        printk("IRQ_EVT(0x%x): XFCMP(%d) DXDONE(%d), DATTMO(%d), DATCRC(%d), DMAEMP(%d)\n", 
+            intsts,
+            int_reg->xfercomp,
+            int_reg->dxferdone,
+            int_reg->dattmo,
+            int_reg->datcrc,
+            int_reg->dmaqempty);*/
+
+    }
+#endif
+    
+    return IRQ_HANDLED;
+}
+
+/*--------------------------------------------------------------------------*/
+/* platform_driver members                                                      */
+/*--------------------------------------------------------------------------*/
+/* called by msdc_drv_probe/remove */
+static void msdc_enable_cd_irq(struct msdc_host *host, int enable)
+{
+	struct msdc_hw *hw = host->hw;
+	u32 base = host->base;
+
+	/* for sdio, not set */
+	if ((hw->flags & MSDC_CD_PIN_EN) == 0) {
+		/* Pull down card detection pin since it is not avaiable */
+		/*
+		   if (hw->config_gpio_pin) 
+		   hw->config_gpio_pin(MSDC_CD_PIN, GPIO_PULL_DOWN);
+		   */
+		sdr_clr_bits(MSDC_PS, MSDC_PS_CDEN);
+		sdr_clr_bits(MSDC_INTEN, MSDC_INTEN_CDSC);
+		sdr_clr_bits(SDC_CFG, SDC_CFG_INSWKUP);
+		return;
+	}
+
+	//printk("CD IRQ Eanable(%d)\n", enable);
+
+	if (enable) {
+	    if (hw->enable_cd_eirq) { /* not set, never enter */
+		    hw->enable_cd_eirq();
+	    } else {
+		    /* card detection circuit relies on the core power so that the core power 
+		     * shouldn't be turned off. Here adds a reference count to keep 
+		     * the core power alive.
+		     */
+		    //msdc_vcore_on(host); //did in msdc_init_hw()
+
+		    if (hw->config_gpio_pin) /* NULL */
+			    hw->config_gpio_pin(MSDC_CD_PIN, GPIO_PULL_UP);
+
+		    sdr_set_field(MSDC_PS, MSDC_PS_CDDEBOUNCE, DEFAULT_DEBOUNCE);
+		    sdr_set_bits(MSDC_PS, MSDC_PS_CDEN);
+		    sdr_set_bits(MSDC_INTEN, MSDC_INTEN_CDSC);
+		    sdr_set_bits(SDC_CFG, SDC_CFG_INSWKUP);  /* not in document! Fix me */
+	    }
+    } else {
+	    if (hw->disable_cd_eirq) {
+		    hw->disable_cd_eirq();
+	    } else {
+		    if (hw->config_gpio_pin) /* NULL */
+			    hw->config_gpio_pin(MSDC_CD_PIN, GPIO_PULL_DOWN);
+
+		    sdr_clr_bits(SDC_CFG, SDC_CFG_INSWKUP);
+		    sdr_clr_bits(MSDC_PS, MSDC_PS_CDEN);
+		    sdr_clr_bits(MSDC_INTEN, MSDC_INTEN_CDSC);
+
+		    /* Here decreases a reference count to core power since card 
+		     * detection circuit is shutdown.
+		     */
+		    //msdc_vcore_off(host);
+	    }
+    }
+}
+
+/* called by msdc_drv_probe */
+static void msdc_init_hw(struct msdc_host *host)
+{
+    u32 base = host->base;
+    struct msdc_hw *hw = host->hw;
+
+#ifdef MT6575_SD_DEBUG	
+    msdc_reg[host->id] = (struct msdc_regs *)host->base;
+#endif
+
+    /* Power on */
+#if 0 /* --- chhung */
+    msdc_vcore_on(host);
+    msdc_pin_reset(host, MSDC_PIN_PULL_UP);
+    msdc_select_clksrc(host, hw->clk_src);
+    enable_clock(PERI_MSDC0_PDN + host->id, "SD");
+    msdc_vdd_on(host);
+#endif /* end of --- */
+    /* Configure to MMC/SD mode */
+    sdr_set_field(MSDC_CFG, MSDC_CFG_MODE, MSDC_SDMMC); 
+       
+    /* Reset */
+    msdc_reset();
+    msdc_clr_fifo();
+
+    /* Disable card detection */
+    sdr_clr_bits(MSDC_PS, MSDC_PS_CDEN);
+
+    /* Disable and clear all interrupts */
+    sdr_clr_bits(MSDC_INTEN, sdr_read32(MSDC_INTEN));
+    sdr_write32(MSDC_INT, sdr_read32(MSDC_INT));
+    
+#if 1
+	/* reset tuning parameter */
+    sdr_write32(MSDC_PAD_CTL0,   0x00090000);
+    sdr_write32(MSDC_PAD_CTL1,   0x000A0000);
+    sdr_write32(MSDC_PAD_CTL2,   0x000A0000);
+    // sdr_write32(MSDC_PAD_TUNE,   0x00000000);
+    sdr_write32(MSDC_PAD_TUNE,   0x84101010);		// for MT7620 E2 and afterward
+    // sdr_write32(MSDC_DAT_RDDLY0, 0x00000000);
+    sdr_write32(MSDC_DAT_RDDLY0, 0x10101010);		// for MT7620 E2 and afterward
+    sdr_write32(MSDC_DAT_RDDLY1, 0x00000000);
+    sdr_write32(MSDC_IOCON,      0x00000000);
+#if 0 // use MT7620 default value: 0x403c004f
+    sdr_write32(MSDC_PATCH_BIT0, 0x003C000F); /* bit0 modified: Rx Data Clock Source: 1 -> 2.0*/
+#endif
+
+    if (sdr_read32(MSDC_ECO_VER) >= 4) { 
+        if (host->id == 1) {	
+            sdr_set_field(MSDC_PATCH_BIT1, MSDC_PATCH_BIT1_WRDAT_CRCS, 1); 
+            sdr_set_field(MSDC_PATCH_BIT1, MSDC_PATCH_BIT1_CMD_RSP,    1);
+            
+            /* internal clock: latch read data */  
+            sdr_set_bits(MSDC_PATCH_BIT0, MSDC_PATCH_BIT_CKGEN_CK);  
+        }       	
+    }   
+#endif    
+
+    /* for safety, should clear SDC_CFG.SDIO_INT_DET_EN & set SDC_CFG.SDIO in 
+       pre-loader,uboot,kernel drivers. and SDC_CFG.SDIO_INT_DET_EN will be only
+       set when kernel driver wants to use SDIO bus interrupt */
+    /* Configure to enable SDIO mode. it's must otherwise sdio cmd5 failed */
+    sdr_set_bits(SDC_CFG, SDC_CFG_SDIO);
+
+    /* disable detect SDIO device interupt function */
+    sdr_clr_bits(SDC_CFG, SDC_CFG_SDIOIDE);
+
+    /* eneable SMT for glitch filter */
+    sdr_set_bits(MSDC_PAD_CTL0, MSDC_PAD_CTL0_CLKSMT);
+    sdr_set_bits(MSDC_PAD_CTL1, MSDC_PAD_CTL1_CMDSMT);
+    sdr_set_bits(MSDC_PAD_CTL2, MSDC_PAD_CTL2_DATSMT);
+
+#if 1
+    /* set clk, cmd, dat pad driving */
+    sdr_set_field(MSDC_PAD_CTL0, MSDC_PAD_CTL0_CLKDRVN, hw->clk_drv);
+    sdr_set_field(MSDC_PAD_CTL0, MSDC_PAD_CTL0_CLKDRVP, hw->clk_drv);
+    sdr_set_field(MSDC_PAD_CTL1, MSDC_PAD_CTL1_CMDDRVN, hw->cmd_drv);
+    sdr_set_field(MSDC_PAD_CTL1, MSDC_PAD_CTL1_CMDDRVP, hw->cmd_drv);
+    sdr_set_field(MSDC_PAD_CTL2, MSDC_PAD_CTL2_DATDRVN, hw->dat_drv);
+    sdr_set_field(MSDC_PAD_CTL2, MSDC_PAD_CTL2_DATDRVP, hw->dat_drv);
+#else 
+    sdr_set_field(MSDC_PAD_CTL0, MSDC_PAD_CTL0_CLKDRVN, 0);
+    sdr_set_field(MSDC_PAD_CTL0, MSDC_PAD_CTL0_CLKDRVP, 0);
+    sdr_set_field(MSDC_PAD_CTL1, MSDC_PAD_CTL1_CMDDRVN, 0);
+    sdr_set_field(MSDC_PAD_CTL1, MSDC_PAD_CTL1_CMDDRVP, 0);
+    sdr_set_field(MSDC_PAD_CTL2, MSDC_PAD_CTL2_DATDRVN, 0);
+    sdr_set_field(MSDC_PAD_CTL2, MSDC_PAD_CTL2_DATDRVP, 0);
+#endif
+
+    /* set sampling edge */
+
+    /* write crc timeout detection */
+    sdr_set_field(MSDC_PATCH_BIT0, 1 << 30, 1);
+
+    /* Configure to default data timeout */
+    sdr_set_field(SDC_CFG, SDC_CFG_DTOC, DEFAULT_DTOC);
+
+    msdc_set_buswidth(host, MMC_BUS_WIDTH_1);
+
+    //printk("init hardware done!\n");
+}
+
+/* called by msdc_drv_remove */
+static void msdc_deinit_hw(struct msdc_host *host)
+{
+    u32 base = host->base;
+
+    /* Disable and clear all interrupts */
+    sdr_clr_bits(MSDC_INTEN, sdr_read32(MSDC_INTEN));
+    sdr_write32(MSDC_INT, sdr_read32(MSDC_INT));
+
+    /* Disable card detection */
+    msdc_enable_cd_irq(host, 0);
+    // msdc_set_power_mode(host, MMC_POWER_OFF);   /* make sure power down */ /* --- by chhung */
+}
+
+/* init gpd and bd list in msdc_drv_probe */
+static void msdc_init_gpd_bd(struct msdc_host *host, struct msdc_dma *dma)
+{
+    gpd_t *gpd = dma->gpd; 
+    bd_t  *bd  = dma->bd; 	
+    bd_t  *ptr, *prev;
+    
+    /* we just support one gpd */     
+    int bdlen = MAX_BD_PER_GPD;   	
+
+    /* init the 2 gpd */
+    memset(gpd, 0, sizeof(gpd_t) * 2);
+    //gpd->next = (void *)virt_to_phys(gpd + 1); /* pointer to a null gpd, bug! kmalloc <-> virt_to_phys */  
+    //gpd->next = (dma->gpd_addr + 1);    /* bug */
+    gpd->next = (void *)((u32)dma->gpd_addr + sizeof(gpd_t));    
+
+    //gpd->intr = 0;
+    gpd->bdp  = 1;   /* hwo, cs, bd pointer */      
+    //gpd->ptr  = (void*)virt_to_phys(bd); 
+    gpd->ptr = (void *)dma->bd_addr; /* physical address */
+    
+    memset(bd, 0, sizeof(bd_t) * bdlen);
+    ptr = bd + bdlen - 1;
+    //ptr->eol  = 1;  /* 0 or 1 [Fix me]*/
+    //ptr->next = 0;    
+    
+    while (ptr != bd) {
+        prev = ptr - 1;
+        prev->next = (void *)(dma->bd_addr + sizeof(bd_t) *(ptr - bd));
+        ptr = prev;
+    }
+}
+
+static int msdc_drv_probe(struct platform_device *pdev)
+{
+	struct resource *res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	__iomem void *base;
+    struct mmc_host *mmc;
+    struct resource *mem;
+    struct msdc_host *host;
+    struct msdc_hw *hw;
+    int ret, irq;
+     pdev->dev.platform_data = &msdc0_hw;
+ 
+    /* Allocate MMC host for this device */
+    mmc = mmc_alloc_host(sizeof(struct msdc_host), &pdev->dev);
+    if (!mmc) return -ENOMEM;
+
+    hw   = (struct msdc_hw*)pdev->dev.platform_data;
+    mem  = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+    irq  = platform_get_irq(pdev, 0);
+
+    //BUG_ON((!hw) || (!mem) || (irq < 0)); /* --- by chhung */
+    
+	base = devm_request_and_ioremap(&pdev->dev, res);
+	if (IS_ERR(base))
+		return PTR_ERR(base);
+
+/*    mem = request_mem_region(mem->start - 0xa0000000, (mem->end - mem->start + 1) - 0xa0000000, dev_name(&pdev->dev));
+    if (mem == NULL) {
+        mmc_free_host(mmc);
+        return -EBUSY;
+    }
+*/
+    /* Set host parameters to mmc */
+    mmc->ops        = &mt_msdc_ops;
+    mmc->f_min      = HOST_MIN_MCLK;
+    mmc->f_max      = HOST_MAX_MCLK;
+    mmc->ocr_avail  = MSDC_OCR_AVAIL;
+    
+    /* For sd card: MSDC_SYS_SUSPEND | MSDC_WP_PIN_EN | MSDC_CD_PIN_EN | MSDC_REMOVABLE | MSDC_HIGHSPEED, 
+       For sdio   : MSDC_EXT_SDIO_IRQ | MSDC_HIGHSPEED */
+    if (hw->flags & MSDC_HIGHSPEED) {
+        mmc->caps   = MMC_CAP_MMC_HIGHSPEED | MMC_CAP_SD_HIGHSPEED;
+    }
+    if (hw->data_pins == 4) { /* current data_pins are all 4*/
+        mmc->caps  |= MMC_CAP_4_BIT_DATA;
+    } else if (hw->data_pins == 8) {
+        mmc->caps  |= MMC_CAP_8_BIT_DATA;
+    }
+    if ((hw->flags & MSDC_SDIO_IRQ) || (hw->flags & MSDC_EXT_SDIO_IRQ))
+        mmc->caps |= MMC_CAP_SDIO_IRQ;  /* yes for sdio */
+
+    /* MMC core transfer sizes tunable parameters */
+  //  mmc->max_hw_segs   = MAX_HW_SGMTS;
+//    mmc->max_phys_segs = MAX_PHY_SGMTS;
+    mmc->max_seg_size  = MAX_SGMT_SZ;
+    mmc->max_blk_size  = HOST_MAX_BLKSZ;
+    mmc->max_req_size  = MAX_REQ_SZ; 
+    mmc->max_blk_count = mmc->max_req_size;
+
+    host = mmc_priv(mmc);
+    host->hw        = hw;
+    host->mmc       = mmc;
+    host->id        = pdev->id;
+    host->error     = 0;
+    host->irq       = irq;    
+    host->base      = (unsigned long) base;
+    host->mclk      = 0;                   /* mclk: the request clock of mmc sub-system */
+    host->hclk      = hclks[hw->clk_src];  /* hclk: clock of clock source to msdc controller */
+    host->sclk      = 0;                   /* sclk: the really clock after divition */
+    host->pm_state  = PMSG_RESUME;
+    host->suspend   = 0;
+    host->core_clkon = 0;
+    host->card_clkon = 0;    
+    host->core_power = 0;
+    host->power_mode = MMC_POWER_OFF;
+//    host->card_inserted = hw->flags & MSDC_REMOVABLE ? 0 : 1;
+    host->timeout_ns = 0;
+    host->timeout_clks = DEFAULT_DTOC * 65536;
+  
+    host->mrq = NULL; 
+    //init_MUTEX(&host->sem); /* we don't need to support multiple threads access */
+   
+    host->dma.used_gpd = 0;
+    host->dma.used_bd = 0;
+
+    /* using dma_alloc_coherent*/  /* todo: using 1, for all 4 slots */
+    host->dma.gpd = dma_alloc_coherent(NULL, MAX_GPD_NUM * sizeof(gpd_t), &host->dma.gpd_addr, GFP_KERNEL); 
+    host->dma.bd =  dma_alloc_coherent(NULL, MAX_BD_NUM  * sizeof(bd_t),  &host->dma.bd_addr,  GFP_KERNEL); 
+    BUG_ON((!host->dma.gpd) || (!host->dma.bd));    
+    msdc_init_gpd_bd(host, &host->dma);
+    /*for emmc*/
+    msdc_6575_host[pdev->id] = host;
+    
+    tasklet_init(&host->card_tasklet, msdc_tasklet_card, (ulong)host);
+    spin_lock_init(&host->lock);
+    msdc_init_hw(host);
+
+    ret = request_irq((unsigned int)irq, msdc_irq, IRQF_TRIGGER_LOW, dev_name(&pdev->dev), host);
+    if (ret) goto release;
+    // mt65xx_irq_unmask(irq); /* --- by chhung */
+    
+    if (hw->flags & MSDC_CD_PIN_EN) { /* not set for sdio */
+        if (hw->request_cd_eirq) { /* not set for MT6575 */
+            hw->request_cd_eirq(msdc_eirq_cd, (void*)host); /* msdc_eirq_cd will not be used! */
+        }
+    }
+
+    if (hw->request_sdio_eirq) /* set to combo_sdio_request_eirq() for WIFI */
+        hw->request_sdio_eirq(msdc_eirq_sdio, (void*)host); /* msdc_eirq_sdio() will be called when EIRQ */
+
+    if (hw->register_pm) {/* yes for sdio */
+        if(hw->flags & MSDC_SYS_SUSPEND) { /* will not set for WIFI */
+            //printk("MSDC_SYS_SUSPEND and register_pm both set\n");
+        }
+        //mmc->pm_flags |= MMC_PM_IGNORE_PM_NOTIFY; /* pm not controlled by system but by client. */ /* --- by chhung */
+    }
+    
+    platform_set_drvdata(pdev, mmc);
+
+    ret = mmc_add_host(mmc);
+    if (ret) goto free_irq;
+
+    /* Config card detection pin and enable interrupts */
+    if (hw->flags & MSDC_CD_PIN_EN) {  /* set for card */
+        msdc_enable_cd_irq(host, 1);
+    } else {
+        msdc_enable_cd_irq(host, 0);
+    }  
+
+    return 0;
+
+free_irq:
+    free_irq(irq, host);
+release:
+    platform_set_drvdata(pdev, NULL);
+    msdc_deinit_hw(host);
+
+    tasklet_kill(&host->card_tasklet);
+
+/*    if (mem)
+        release_mem_region(mem->start, mem->end - mem->start + 1);
+*/
+    mmc_free_host(mmc);
+
+    return ret;
+}
+
+/* 4 device share one driver, using "drvdata" to show difference */
+static int msdc_drv_remove(struct platform_device *pdev)
+{
+    struct mmc_host *mmc;
+    struct msdc_host *host;
+    struct resource *mem;
+
+
+    mmc  = platform_get_drvdata(pdev);
+    BUG_ON(!mmc);
+    
+    host = mmc_priv(mmc);   
+    BUG_ON(!host);
+
+    //printk("removed !!!\n");
+
+    platform_set_drvdata(pdev, NULL);
+    mmc_remove_host(host->mmc);
+    msdc_deinit_hw(host);
+
+    tasklet_kill(&host->card_tasklet);
+    free_irq(host->irq, host);
+
+    dma_free_coherent(NULL, MAX_GPD_NUM * sizeof(gpd_t), host->dma.gpd, host->dma.gpd_addr);
+    dma_free_coherent(NULL, MAX_BD_NUM  * sizeof(bd_t),  host->dma.bd,  host->dma.bd_addr);
+
+    mem = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+
+    if (mem)
+        release_mem_region(mem->start, mem->end - mem->start + 1);
+
+    mmc_free_host(host->mmc);
+
+    return 0;
+}
+
+static const struct of_device_id mt7620a_sdhci_match[] = {
+	{ .compatible = "ralink,mt7620a-sdhci" },
+	{},
+};
+MODULE_DEVICE_TABLE(of, rt288x_wdt_match);
+
+/* Fix me: Power Flow */
+static struct platform_driver mt_msdc_driver = {
+    .probe   = msdc_drv_probe,
+    .remove  = msdc_drv_remove,
+    .driver  = {
+        .name  = DRV_NAME,
+        .owner = THIS_MODULE,
+        .of_match_table = mt7620a_sdhci_match,
+
+    },
+};
+
+static int __init mt_msdc_init(void)
+{
+    int ret;
+/* +++ chhung */
+    unsigned int reg;
+
+    mtk_sd_device.dev.platform_data = &msdc0_hw;
+    printk("MTK MSDC device init.\n");
+    reg = sdr_read32((__iomem void *) 0xb0000060) & ~(0x3<<18);
+    reg |= 0x1 << 18;
+    sdr_write32((__iomem void *) 0xb0000060, reg);
+/* end of +++ */
+    ret = platform_driver_register(&mt_msdc_driver);
+    if (ret) {
+        printk(KERN_ERR DRV_NAME ": Can't register driver");
+        return ret;
+    }
+    printk(KERN_INFO DRV_NAME ": MediaTek MT6575 MSDC Driver\n");
+
+    //msdc_debug_proc_init();
+    return 0;
+}
+
+static void __exit mt_msdc_exit(void)
+{
+    platform_driver_unregister(&mt_msdc_driver);
+}
+
+module_init(mt_msdc_init);
+module_exit(mt_msdc_exit);
+MODULE_LICENSE("GPL");
+MODULE_DESCRIPTION("MediaTek MT6575 SD/MMC Card Driver");
+MODULE_AUTHOR("Infinity Chen <infinity.chen@mediatek.com>");
+
+EXPORT_SYMBOL(msdc_6575_host);
