--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -147,6 +147,7 @@ dtb-$(CONFIG_MACH_KIRKWOOD) += kirkwood-
 	kirkwood-openrd-base.dtb \
 	kirkwood-openrd-client.dtb \
 	kirkwood-openrd-ultimate.dtb \
+	kirkwood-pogo_e02.dtb \
 	kirkwood-rd88f6192.dtb \
 	kirkwood-rd88f6281-z0.dtb \
 	kirkwood-rd88f6281-a.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/kirkwood-pogo_e02.dts
@@ -0,0 +1,114 @@
+/dts-v1/;
+
+#include "kirkwood.dtsi"
+#include "kirkwood-6281.dtsi"
+
+/ {
+	model = "Cloud Engines Pogoplug E02";
+	compatible = "cloudengines,pogoe02", "marvell,kirkwood-88f6281", "marvell,kirkwood";
+
+	memory {
+		device_type = "memory";
+		reg = <0x00000000 0x10000000>;
+	};
+
+	chosen {
+		bootargs = "console=ttyS0,115200n8 earlyprintk";
+	};
+
+	ocp@f1000000 {
+		pinctrl: pin-controller@10000 {
+			pmx_usb_power_enable: pmx-usb-power-enable {
+				marvell,pins = "mpp29";
+				marvell,function = "gpio";
+			};
+			pmx_led_green: pmx-led_green {
+				marvell,pins = "mpp48";
+				marvell,function = "gpio";
+			};
+			pmx_led_orange: pmx-led_orange {
+				marvell,pins = "mpp49";
+				marvell,function = "gpio";
+			};
+		};
+		serial@12000 {
+			status = "ok";
+		};
+	};
+	gpio-leds {
+		compatible = "gpio-leds";
+		pinctrl-0 = < &pmx_usb_power_enable &pmx_led_orange
+			      &pmx_led_green >;
+		pinctrl-names = "default";
+
+		health {
+			label = "status:green:health";
+			gpios = <&gpio1 16 GPIO_ACTIVE_LOW>;
+			default-state = "keep";
+		};
+		fault {
+			label = "status:orange:fault";
+			gpios = <&gpio1 17 GPIO_ACTIVE_LOW>;
+		};
+	};
+	regulators {
+		compatible = "simple-bus";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		pinctrl-0 = <&pmx_usb_power_enable>;
+		pinctrl-names = "default";
+
+		usb_power: regulator@1 {
+			compatible = "regulator-fixed";
+			reg = <1>;
+			regulator-name = "USB Power";
+			regulator-min-microvolt = <5000000>;
+			regulator-max-microvolt = <5000000>;
+			enable-active-high;
+			regulator-always-on;
+			regulator-boot-on;
+			gpio = <&gpio0 29 GPIO_ACTIVE_HIGH>;
+		};
+	};
+};
+
+&nand {
+	chip-delay = <40>;
+	status = "okay";
+
+	partition@0 {
+		label = "u-boot";
+		reg = <0x0000000 0x100000>;
+		read-only;
+	};
+
+	partition@100000 {
+		label = "uImage";
+		reg = <0x0100000 0x400000>;
+	};
+
+	partition@500000 {
+		label = "pogoplug";
+		reg = <0x0500000 0x2000000>;
+	};
+
+	partition@2500000 {
+		label = "root";
+		reg = <0x02500000 0x5b00000>;
+	};
+};
+
+&mdio {
+	status = "okay";
+
+	ethphy0: ethernet-phy@0 {
+		reg = <0>;
+	};
+};
+
+&eth0 {
+	status = "okay";
+	ethernet0-port@0 {
+		phy-handle = <&ethphy0>;
+	};
+};
