--- a/drivers/gpio/Kconfig
+++ b/drivers/gpio/Kconfig
@@ -748,6 +748,12 @@ config GPIO_MC33880
 	  SPI driver for Freescale MC33880 high-side/low-side switch.
 	  This provides GPIO interface supporting inputs and outputs.
 
+config GPIO_MCS814X
+	tristate "Moschip MCS814x GPIO support"
+	depends on ARCH_MCS814X
+	help
+	   GPIO driver for Moschip MCS814x SoC gpio controllers.
+
 config GPIO_74X164
 	tristate "74x164 serial-in/parallel-out 8-bits shift register"
 	depends on SPI_MASTER && OF
--- a/drivers/gpio/Makefile
+++ b/drivers/gpio/Makefile
@@ -45,6 +45,7 @@ obj-$(CONFIG_GPIO_MAX732X)	+= gpio-max73
 obj-$(CONFIG_GPIO_MC33880)	+= gpio-mc33880.o
 obj-$(CONFIG_GPIO_MC9S08DZ60)	+= gpio-mc9s08dz60.o
 obj-$(CONFIG_GPIO_MCP23S08)	+= gpio-mcp23s08.o
+obj-$(CONFIG_GPIO_MCS814X)	+= gpio-mcs814x.o
 obj-$(CONFIG_GPIO_ML_IOH)	+= gpio-ml-ioh.o
 obj-$(CONFIG_GPIO_MM_LANTIQ)	+= gpio-mm-lantiq.o
 obj-$(CONFIG_GPIO_MOXART)	+= gpio-moxart.o
