From 302a5ef29d497449280422576a1b55c72fc0ba4c Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Thu, 4 Dec 2014 10:22:02 +0100
Subject: [PATCH] ARM: BCM5301X: Add DT for Netgear R6300 V2
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
Signed-off-by: Hauke Mehrtens <hauke@hauke-m.de>
---
 arch/arm/boot/dts/Makefile                     |  4 +-
 arch/arm/boot/dts/bcm4708-netgear-r6300-v2.dts | 84 ++++++++++++++++++++++++++
 2 files changed, 87 insertions(+), 1 deletion(-)
 create mode 100644 arch/arm/boot/dts/bcm4708-netgear-r6300-v2.dts

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -54,7 +54,9 @@ dtb-$(CONFIG_ARCH_AT91)	+= at91-sama5d4e
 dtb-$(CONFIG_ARCH_ATLAS6) += atlas6-evb.dtb
 dtb-$(CONFIG_ARCH_AXXIA) += axm5516-amarillo.dtb
 dtb-$(CONFIG_ARCH_BCM2835) += bcm2835-rpi-b.dtb
-dtb-$(CONFIG_ARCH_BCM_5301X) += bcm4708-netgear-r6250.dtb
+dtb-$(CONFIG_ARCH_BCM_5301X) += \
+	bcm4708-netgear-r6250.dtb \
+	bcm4708-netgear-r6300-v2.dtb
 dtb-$(CONFIG_ARCH_BCM_63XX) += bcm963138dvt.dtb
 dtb-$(CONFIG_ARCH_BCM_MOBILE) += bcm28155-ap.dtb \
 	bcm21664-garnet.dtb
--- /dev/null
+++ b/arch/arm/boot/dts/bcm4708-netgear-r6300-v2.dts
@@ -0,0 +1,84 @@
+/*
+ * Broadcom BCM470X / BCM5301X ARM platform code.
+ * DTS for Netgear R6300 V2
+ *
+ * Copyright (C) 2014 Rafał Miłecki <zajec5@gmail.com>
+ *
+ * Licensed under the GNU/GPL. See COPYING for details.
+ */
+
+/dts-v1/;
+
+#include "bcm4708.dtsi"
+
+/ {
+	compatible = "netgear,r6300v2", "brcm,bcm4708";
+	model = "Netgear R6300 V2 (BCM4708)";
+
+	chosen {
+		bootargs = "console=ttyS0,115200";
+	};
+
+	memory {
+		reg = <0x00000000 0x08000000>;
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		logo {
+			label = "bcm53xx:white:logo";
+			gpios = <&chipcommon 1 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-on";
+		};
+
+		power0 {
+			label = "bcm53xx:green:power";
+			gpios = <&chipcommon 2 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "default-off";
+		};
+
+		power1 {
+			label = "bcm53xx:amber:power";
+			gpios = <&chipcommon 3 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "default-on";
+		};
+
+		usb {
+			label = "bcm53xx:blue:usb";
+			gpios = <&chipcommon 8 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "default-off";
+		};
+
+		wireless {
+			label = "bcm53xx:blue:wireless";
+			gpios = <&chipcommon 11 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "default-off";
+		};
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		poll-interval = <200>;
+
+		wps {
+			label = "WPS";
+			linux,code = <KEY_WPS_BUTTON>;
+			gpios = <&chipcommon 4 GPIO_ACTIVE_LOW>;
+		};
+
+		rfkill {
+			label = "WiFi";
+			linux,code = <KEY_RFKILL>;
+			gpios = <&chipcommon 5 GPIO_ACTIVE_LOW>;
+		};
+
+		restart {
+			label = "Reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&chipcommon 6 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
