--- a/arch/arm/plat-omap/omap_device.c
+++ b/arch/arm/plat-omap/omap_device.c
@@ -619,7 +619,7 @@ static void omap_device_delete(struct om
  * information.  Returns ERR_PTR(-EINVAL) if @oh is NULL; otherwise,
  * passes along the return value of omap_device_build_ss().
  */
-struct platform_device *omap_device_build(const char *pdev_name, int pdev_id,
+struct platform_device *__init omap_device_build(const char *pdev_name, int pdev_id,
 				      struct omap_hwmod *oh, void *pdata,
 				      int pdata_len,
 				      struct omap_device_pm_latency *pm_lats,
@@ -652,7 +652,7 @@ struct platform_device *omap_device_buil
  * platform_device record.  Returns an ERR_PTR() on error, or passes
  * along the return value of omap_device_register().
  */
-struct platform_device *omap_device_build_ss(const char *pdev_name, int pdev_id,
+struct platform_device *__init omap_device_build_ss(const char *pdev_name, int pdev_id,
 					 struct omap_hwmod **ohs, int oh_cnt,
 					 void *pdata, int pdata_len,
 					 struct omap_device_pm_latency *pm_lats,
@@ -717,7 +717,7 @@ odbs_exit:
  * platform_early_add_device() on the underlying platform_device.
  * Returns 0 by default.
  */
-static int omap_early_device_register(struct platform_device *pdev)
+static int __init omap_early_device_register(struct platform_device *pdev)
 {
 	struct platform_device *devices[1];
 
--- a/arch/arm/plat-omap/common.c
+++ b/arch/arm/plat-omap/common.c
@@ -29,7 +29,7 @@
 
 #define NO_LENGTH_CHECK 0xffffffff
 
-struct omap_board_config_kernel *omap_board_config __initdata;
+struct omap_board_config_kernel *omap_board_config;
 int omap_board_config_size;
 
 unsigned char omap_bootloader_tag[1024];
@@ -58,7 +58,7 @@ __tagtable(ATAG_BOARD, parse_tag_omap);
 
 #endif
 
-static const void *__init get_config(u16 tag, size_t len,
+static const void *get_config(u16 tag, size_t len,
 		int skip, size_t *len_out)
 {
 	struct omap_board_config_kernel *kinfo = NULL;
@@ -125,12 +125,12 @@ static const void *__init get_config(u16
 	return kinfo->data;
 }
 
-const void *__init __omap_get_config(u16 tag, size_t len, int nr)
+const void *__omap_get_config(u16 tag, size_t len, int nr)
 {
         return get_config(tag, len, nr, NULL);
 }
 
-const void *__init omap_get_var_config(u16 tag, size_t *len)
+const void *omap_get_var_config(u16 tag, size_t *len)
 {
         return get_config(tag, NO_LENGTH_CHECK, 0, len);
 }
--- a/arch/arm/mach-omap2/devices.c
+++ b/arch/arm/mach-omap2/devices.c
@@ -380,7 +380,7 @@ static inline void omap_init_dmic(void)
 
 #include <plat/mcspi.h>
 
-static int omap_mcspi_init(struct omap_hwmod *oh, void *unused)
+static int __init omap_mcspi_init(struct omap_hwmod *oh, void *unused)
 {
 	struct platform_device *pdev;
 	char *name = "omap2_mcspi";
--- a/arch/arm/mach-omap2/gpio.c
+++ b/arch/arm/mach-omap2/gpio.c
@@ -24,7 +24,7 @@
 #include <plat/omap_hwmod.h>
 #include <plat/omap_device.h>
 
-static int omap2_gpio_dev_init(struct omap_hwmod *oh, void *unused)
+static int __init omap2_gpio_dev_init(struct omap_hwmod *oh, void *unused)
 {
 	struct platform_device *pdev;
 	struct omap_gpio_platform_data *pdata;
--- a/arch/arm/mach-omap2/mcbsp.c
+++ b/arch/arm/mach-omap2/mcbsp.c
@@ -122,7 +122,7 @@ static int omap3_enable_st_clock(unsigne
 	return 0;
 }
 
-static int omap_init_mcbsp(struct omap_hwmod *oh, void *unused)
+static int __init omap_init_mcbsp(struct omap_hwmod *oh, void *unused)
 {
 	int id, count = 1;
 	char *name = "omap-mcbsp";
--- a/arch/arm/plat-omap/include/plat/board.h
+++ b/arch/arm/plat-omap/include/plat/board.h
@@ -159,14 +159,14 @@ struct omap_gpio_switch_config {
 	int key_code:24; /* Linux key code */
 };
 
-extern const void *__init __omap_get_config(u16 tag, size_t len, int nr);
+extern const void * __omap_get_config(u16 tag, size_t len, int nr);
 
 #define omap_get_config(tag, type) \
 	((const type *) __omap_get_config((tag), sizeof(type), 0))
 #define omap_get_nr_config(tag, type, nr) \
 	((const type *) __omap_get_config((tag), sizeof(type), (nr)))
 
-extern const void *__init omap_get_var_config(u16 tag, size_t *len);
+extern const void * omap_get_var_config(u16 tag, size_t *len);
 
 extern struct omap_board_config_kernel *omap_board_config;
 extern int omap_board_config_size;
