From dbe94a8daaa63ef81b7414f2a17bca8e36dd6daa Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Fri, 20 Feb 2015 19:55:32 +0100
Subject: [PATCH 1/6] gpio: add a simple GPIO driver for bcm63xx


Signed-off-by: Jonas Gorski <jogo@openwrt.org>
---
 drivers/gpio/Kconfig        |    8 +++
 drivers/gpio/Makefile       |    1 +
 drivers/gpio/gpio-bcm63xx.c |  117 +++++++++++++++++++++++++++++++++++++++++++
 3 files changed, 126 insertions(+)
 create mode 100644 drivers/gpio/gpio-bcm63xx.c

--- a/drivers/gpio/Kconfig
+++ b/drivers/gpio/Kconfig
@@ -892,6 +892,14 @@ config GPIO_BCM_KONA
 	help
 	  Turn on GPIO support for Broadcom "Kona" chips.
 
+config GPIO_BCM63XX
+	bool "Broadcom BCM63XX GPIO"
+	depends on MIPS || COMPILE_TEST
+	select GPIO_GENERIC
+	help
+	  Turn on GPIO support for Broadcom BCM63XX xDSL chips.
+
+
 comment "USB GPIO expanders:"
 
 config GPIO_VIPERBOARD
--- a/drivers/gpio/Makefile
+++ b/drivers/gpio/Makefile
@@ -19,6 +19,7 @@ obj-$(CONFIG_GPIO_ADP5588)	+= gpio-adp55
 obj-$(CONFIG_GPIO_AMD8111)	+= gpio-amd8111.o
 obj-$(CONFIG_GPIO_ARIZONA)	+= gpio-arizona.o
 obj-$(CONFIG_GPIO_BCM_KONA)	+= gpio-bcm-kona.o
+obj-$(CONFIG_GPIO_BCM63XX)	+= gpio-bcm63xx.o
 obj-$(CONFIG_GPIO_BT8XX)	+= gpio-bt8xx.o
 obj-$(CONFIG_GPIO_CLPS711X)	+= gpio-clps711x.o
 obj-$(CONFIG_GPIO_CS5535)	+= gpio-cs5535.o
--- /dev/null
+++ b/drivers/gpio/gpio-bcm63xx.c
@@ -0,0 +1,117 @@
+/*
+ * Driver for BCM63XX memory-mapped GPIO controllers, based on
+ * Generic driver for memory-mapped GPIO controllers.
+ *
+ * Copyright 2008 MontaVista Software, Inc.
+ * Copyright 2008,2010 Anton Vorontsov <cbouatmailru@gmail.com>
+ * Copyright 2015 Jonas Gorski <jogo@openwrt.org>
+ *
+ * This program is free software; you can redistribute  it and/or modify it
+ * under  the terms of  the GNU General  Public License as published by the
+ * Free Software Foundation;  either version 2 of the  License, or (at your
+ * option) any later version.
+ */
+
+#include <linux/init.h>
+#include <linux/err.h>
+#include <linux/bug.h>
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/spinlock.h>
+#include <linux/compiler.h>
+#include <linux/types.h>
+#include <linux/errno.h>
+#include <linux/log2.h>
+#include <linux/ioport.h>
+#include <linux/io.h>
+#include <linux/gpio.h>
+#include <linux/slab.h>
+#include <linux/platform_device.h>
+#include <linux/mod_devicetable.h>
+#include <linux/basic_mmio_gpio.h>
+#include <linux/of.h>
+#include <linux/of_gpio.h>
+
+static int bcm63xx_gpio_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct resource *dat_r, *dirout_r;
+	void __iomem *dat;
+	void __iomem *dirout;
+	unsigned long sz;
+	int err;
+	struct bgpio_chip *bgc;
+	struct bgpio_pdata *pdata = dev_get_platdata(dev);
+
+	dirout_r = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	dat_r = platform_get_resource(pdev, IORESOURCE_MEM, 1);
+	if (!dat_r || !dirout_r)
+		return -EINVAL;
+
+	if (resource_size(dat_r) != resource_size(dirout_r))
+		return -EINVAL;
+
+	sz = resource_size(dat_r);
+
+	dat = devm_ioremap_resource(dev, dat_r);
+	if (IS_ERR(dat))
+		return PTR_ERR(dat);
+
+	dirout = devm_ioremap_resource(dev, dirout_r);
+	if (IS_ERR(dirout))
+		return PTR_ERR(dirout);
+
+	bgc = devm_kzalloc(&pdev->dev, sizeof(*bgc), GFP_KERNEL);
+	if (!bgc)
+		return -ENOMEM;
+
+	err = bgpio_init(bgc, dev, sz, dat, NULL, NULL, dirout, NULL,
+			 BGPIOF_BIG_ENDIAN_BYTE_ORDER);
+	if (err)
+		return err;
+
+	platform_set_drvdata(pdev, bgc);
+
+	if (dev->of_node) {
+		u32 ngpios;
+
+		if (!of_property_read_u32(dev->of_node, "ngpios", &ngpios))
+			bgc->gc.ngpio = ngpios;
+
+	} else if (pdata) {
+		bgc->gc.base = pdata->base;
+		if (pdata->ngpio > 0)
+			bgc->gc.ngpio = pdata->ngpio;
+	}
+
+	return gpiochip_add(&bgc->gc);
+}
+
+static int bcm63xx_gpio_remove(struct platform_device *pdev)
+{
+	struct bgpio_chip *bgc = platform_get_drvdata(pdev);
+
+	return bgpio_remove(bgc);
+}
+
+#ifdef CONFIG_OF
+static struct of_device_id bcm63xx_gpio_of_match[] = {
+	{ .compatible = "brcm,bcm6345-gpio" },
+	{ },
+};
+#endif
+
+static struct platform_driver bcm63xx_gpio_driver = {
+	.probe = bcm63xx_gpio_probe,
+	.remove = bcm63xx_gpio_remove,
+	.driver = {
+		.name = "bcm63xx-gpio",
+		.of_match_table = of_match_ptr(bcm63xx_gpio_of_match),
+	},
+};
+
+module_platform_driver(bcm63xx_gpio_driver);
+
+MODULE_DESCRIPTION("Driver for BCM63XX memory-mapped GPIO controllers");
+MODULE_AUTHOR("Jonas Gorski <jogo@openwrt.org>");
+MODULE_LICENSE("GPL");
