From e3b20f04e9f9cae1babe091fdc1d08d7703ae344 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Thu, 7 Aug 2014 18:18:00 +0200
Subject: [PATCH 20/36] MTD: lantiq: handle NO_XIP on cfi0001 flash

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/mtd/maps/lantiq-flash.c |    6 +++++-
 1 file changed, 5 insertions(+), 1 deletion(-)

--- a/drivers/mtd/maps/lantiq-flash.c
+++ b/drivers/mtd/maps/lantiq-flash.c
@@ -139,7 +139,11 @@ ltq_mtd_probe(struct platform_device *pd
 	if (!ltq_mtd->map)
 		return -ENOMEM;
 
-	ltq_mtd->map->phys = ltq_mtd->res->start;
+	if (of_find_property(pdev->dev.of_node, "lantiq,noxip", NULL))
+		ltq_mtd->map->phys = NO_XIP;
+	else
+		ltq_mtd->map->phys = ltq_mtd->res->start;
+	ltq_mtd->res->start;
 	ltq_mtd->map->size = resource_size(ltq_mtd->res);
 	ltq_mtd->map->virt = devm_ioremap_resource(&pdev->dev, ltq_mtd->res);
 	if (IS_ERR(ltq_mtd->map->virt))
