From adee2a81f0be488e079498ac457bf01c954a029e Mon Sep 17 00:00:00 2001
From: popcornmix <popcornmix@gmail.com>
Date: Tue, 2 Jul 2013 23:42:01 +0100
Subject: [PATCH 010/114] bcm2708 vchiq driver

Signed-off-by: popcornmix <popcornmix@gmail.com>

vchiq: create_pagelist copes with vmalloc memory

Signed-off-by: Daniel Stone <daniels@collabora.com>

vchiq: fix the shim message release

Signed-off-by: Daniel Stone <daniels@collabora.com>

vchiq: export additional symbols

Signed-off-by: Daniel Stone <daniels@collabora.com>

VCHIQ: Make service closure fully synchronous (drv)

This is one half of a two-part patch, the other half of which is to
the vchiq_lib user library. With these patches, calls to
vchiq_close_service and vchiq_remove_service won't return until any
associated callbacks have been delivered to the callback thread.

VCHIQ: Add per-service tracing

The new service option VCHIQ_SERVICE_OPTION_TRACE is a boolean that
toggles tracing for the specified service.

This commit also introduces vchi_service_set_option and the associated
option VCHI_SERVICE_OPTION_TRACE.

vchiq: Make the synchronous-CLOSE logic more tolerant

vchiq: Move logging control into debugfs

vchiq: Take care of a corner case tickled by VCSM

Closing a connection that isn't fully open requires care, since one
side does not know the other side's port number. Code was present to
handle the case where a CLOSE is sent immediately after an OPEN, i.e.
before the OPENACK has been received, but this was incorrectly being
used when an OPEN from a client using port 0 was rejected.

(In the observed failure, the host was attempting to use the VCSM
service, which isn't present in the 'cutdown' firmware. The failure
was intermittent because sometimes the keepalive service would
grab port 0.)

This case can be distinguished because the client's remoteport will
still be VCHIQ_PORT_FREE, and the srvstate will be OPENING. Either
condition is sufficient to differentiate it from the special case
described above.
---
 drivers/misc/Kconfig                               |    1 +
 drivers/misc/Makefile                              |    1 +
 drivers/misc/vc04_services/Kconfig                 |    9 +
 drivers/misc/vc04_services/Makefile                |   17 +
 .../interface/vchi/connections/connection.h        |  328 ++
 .../interface/vchi/message_drivers/message.h       |  204 ++
 drivers/misc/vc04_services/interface/vchi/vchi.h   |  378 ++
 .../misc/vc04_services/interface/vchi/vchi_cfg.h   |  224 ++
 .../interface/vchi/vchi_cfg_internal.h             |   71 +
 .../vc04_services/interface/vchi/vchi_common.h     |  174 +
 .../misc/vc04_services/interface/vchi/vchi_mh.h    |   42 +
 .../misc/vc04_services/interface/vchiq_arm/vchiq.h |   40 +
 .../vc04_services/interface/vchiq_arm/vchiq_2835.h |   42 +
 .../interface/vchiq_arm/vchiq_2835_arm.c           |  561 +++
 .../vc04_services/interface/vchiq_arm/vchiq_arm.c  | 2883 +++++++++++++++
 .../vc04_services/interface/vchiq_arm/vchiq_arm.h  |  223 ++
 .../interface/vchiq_arm/vchiq_build_info.h         |   37 +
 .../vc04_services/interface/vchiq_arm/vchiq_cfg.h  |   66 +
 .../interface/vchiq_arm/vchiq_connected.c          |  119 +
 .../interface/vchiq_arm/vchiq_connected.h          |   50 +
 .../vc04_services/interface/vchiq_arm/vchiq_core.c | 3861 ++++++++++++++++++++
 .../vc04_services/interface/vchiq_arm/vchiq_core.h |  711 ++++
 .../interface/vchiq_arm/vchiq_debugfs.c            |  383 ++
 .../interface/vchiq_arm/vchiq_debugfs.h            |   52 +
 .../interface/vchiq_arm/vchiq_genversion           |   87 +
 .../vc04_services/interface/vchiq_arm/vchiq_if.h   |  189 +
 .../interface/vchiq_arm/vchiq_ioctl.h              |  131 +
 .../interface/vchiq_arm/vchiq_kern_lib.c           |  456 +++
 .../interface/vchiq_arm/vchiq_memdrv.h             |   71 +
 .../interface/vchiq_arm/vchiq_pagelist.h           |   58 +
 .../vc04_services/interface/vchiq_arm/vchiq_shim.c |  853 +++++
 .../vc04_services/interface/vchiq_arm/vchiq_util.c |  151 +
 .../vc04_services/interface/vchiq_arm/vchiq_util.h |   81 +
 .../interface/vchiq_arm/vchiq_version.c            |   59 +
 34 files changed, 12613 insertions(+)
 create mode 100644 drivers/misc/vc04_services/Kconfig
 create mode 100644 drivers/misc/vc04_services/Makefile
 create mode 100644 drivers/misc/vc04_services/interface/vchi/connections/connection.h
 create mode 100644 drivers/misc/vc04_services/interface/vchi/message_drivers/message.h
 create mode 100644 drivers/misc/vc04_services/interface/vchi/vchi.h
 create mode 100644 drivers/misc/vc04_services/interface/vchi/vchi_cfg.h
 create mode 100644 drivers/misc/vc04_services/interface/vchi/vchi_cfg_internal.h
 create mode 100644 drivers/misc/vc04_services/interface/vchi/vchi_common.h
 create mode 100644 drivers/misc/vc04_services/interface/vchi/vchi_mh.h
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq.h
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_2835.h
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_2835_arm.c
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_arm.c
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_arm.h
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_build_info.h
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_cfg.h
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_connected.c
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_connected.h
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_core.c
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_core.h
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_debugfs.c
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_debugfs.h
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_genversion
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_if.h
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_ioctl.h
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_kern_lib.c
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_memdrv.h
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_pagelist.h
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_shim.c
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_util.c
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_util.h
 create mode 100644 drivers/misc/vc04_services/interface/vchiq_arm/vchiq_version.c

--- a/drivers/misc/Kconfig
+++ b/drivers/misc/Kconfig
@@ -524,6 +524,7 @@ source "drivers/misc/carma/Kconfig"
 source "drivers/misc/altera-stapl/Kconfig"
 source "drivers/misc/mei/Kconfig"
 source "drivers/misc/vmw_vmci/Kconfig"
+source "drivers/misc/vc04_services/Kconfig"
 source "drivers/misc/mic/Kconfig"
 source "drivers/misc/genwqe/Kconfig"
 source "drivers/misc/echo/Kconfig"
--- a/drivers/misc/Makefile
+++ b/drivers/misc/Makefile
@@ -51,6 +51,7 @@ obj-$(CONFIG_INTEL_MEI)		+= mei/
 obj-$(CONFIG_VMWARE_VMCI)	+= vmw_vmci/
 obj-$(CONFIG_LATTICE_ECP3_CONFIG)	+= lattice-ecp3-config.o
 obj-$(CONFIG_SRAM)		+= sram.o
+obj-y				+= vc04_services/
 obj-y				+= mic/
 obj-$(CONFIG_GENWQE)		+= genwqe/
 obj-$(CONFIG_ECHO)		+= echo/
--- /dev/null
+++ b/drivers/misc/vc04_services/Kconfig
@@ -0,0 +1,9 @@
+config BCM2708_VCHIQ
+	tristate "Videocore VCHIQ"
+	depends on MACH_BCM2708
+	default y
+	help
+		Kernel to VideoCore communication interface for the
+		BCM2708 family of products.
+		Defaults to Y when the Broadcom Videocore services
+		are included in the build, N otherwise.
--- /dev/null
+++ b/drivers/misc/vc04_services/Makefile
@@ -0,0 +1,17 @@
+ifeq ($(CONFIG_MACH_BCM2708),y)
+
+obj-$(CONFIG_BCM2708_VCHIQ)	+= vchiq.o
+
+vchiq-objs := \
+   interface/vchiq_arm/vchiq_core.o  \
+   interface/vchiq_arm/vchiq_arm.o \
+   interface/vchiq_arm/vchiq_kern_lib.o \
+   interface/vchiq_arm/vchiq_2835_arm.o \
+   interface/vchiq_arm/vchiq_debugfs.o \
+   interface/vchiq_arm/vchiq_shim.o \
+   interface/vchiq_arm/vchiq_util.o \
+   interface/vchiq_arm/vchiq_connected.o \
+
+ccflags-y += -DVCOS_VERIFY_BKPTS=1 -Idrivers/misc/vc04_services -DUSE_VCHIQ_ARM -D__VCCOREVER__=0x04000000
+
+endif
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchi/connections/connection.h
@@ -0,0 +1,328 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef CONNECTION_H_
+#define CONNECTION_H_
+
+#include <linux/kernel.h>
+#include <linux/types.h>
+#include <linux/semaphore.h>
+
+#include "interface/vchi/vchi_cfg_internal.h"
+#include "interface/vchi/vchi_common.h"
+#include "interface/vchi/message_drivers/message.h"
+
+/******************************************************************************
+ Global defs
+ *****************************************************************************/
+
+// Opaque handle for a connection / service pair
+typedef struct opaque_vchi_connection_connected_service_handle_t *VCHI_CONNECTION_SERVICE_HANDLE_T;
+
+// opaque handle to the connection state information
+typedef struct opaque_vchi_connection_info_t VCHI_CONNECTION_STATE_T;
+
+typedef struct vchi_connection_t VCHI_CONNECTION_T;
+
+
+/******************************************************************************
+ API
+ *****************************************************************************/
+
+// Routine to init a connection with a particular low level driver
+typedef VCHI_CONNECTION_STATE_T * (*VCHI_CONNECTION_INIT_T)( struct vchi_connection_t * connection,
+                                                             const VCHI_MESSAGE_DRIVER_T * driver );
+
+// Routine to control CRC enabling at a connection level
+typedef int32_t (*VCHI_CONNECTION_CRC_CONTROL_T)( VCHI_CONNECTION_STATE_T *state_handle,
+                                                  VCHI_CRC_CONTROL_T control );
+
+// Routine to create a service
+typedef int32_t (*VCHI_CONNECTION_SERVICE_CONNECT_T)( VCHI_CONNECTION_STATE_T *state_handle,
+                                                      int32_t service_id,
+                                                      uint32_t rx_fifo_size,
+                                                      uint32_t tx_fifo_size,
+                                                      int server,
+                                                      VCHI_CALLBACK_T callback,
+                                                      void *callback_param,
+                                                      int32_t want_crc,
+                                                      int32_t want_unaligned_bulk_rx,
+                                                      int32_t want_unaligned_bulk_tx,
+                                                      VCHI_CONNECTION_SERVICE_HANDLE_T *service_handle );
+
+// Routine to close a service
+typedef int32_t (*VCHI_CONNECTION_SERVICE_DISCONNECT_T)( VCHI_CONNECTION_SERVICE_HANDLE_T service_handle );
+
+// Routine to queue a message
+typedef int32_t (*VCHI_CONNECTION_SERVICE_QUEUE_MESSAGE_T)( VCHI_CONNECTION_SERVICE_HANDLE_T service_handle,
+                                                            const void *data,
+                                                            uint32_t data_size,
+                                                            VCHI_FLAGS_T flags,
+                                                            void *msg_handle );
+
+// scatter-gather (vector) message queueing
+typedef int32_t (*VCHI_CONNECTION_SERVICE_QUEUE_MESSAGEV_T)( VCHI_CONNECTION_SERVICE_HANDLE_T service_handle,
+                                                             VCHI_MSG_VECTOR_T *vector,
+                                                             uint32_t count,
+                                                             VCHI_FLAGS_T flags,
+                                                             void *msg_handle );
+
+// Routine to dequeue a message
+typedef int32_t (*VCHI_CONNECTION_SERVICE_DEQUEUE_MESSAGE_T)( VCHI_CONNECTION_SERVICE_HANDLE_T service_handle,
+                                                              void *data,
+                                                              uint32_t max_data_size_to_read,
+                                                              uint32_t *actual_msg_size,
+                                                              VCHI_FLAGS_T flags );
+
+// Routine to peek at a message
+typedef int32_t (*VCHI_CONNECTION_SERVICE_PEEK_MESSAGE_T)( VCHI_CONNECTION_SERVICE_HANDLE_T service_handle,
+                                                           void **data,
+                                                           uint32_t *msg_size,
+                                                           VCHI_FLAGS_T flags );
+
+// Routine to hold a message
+typedef int32_t (*VCHI_CONNECTION_SERVICE_HOLD_MESSAGE_T)( VCHI_CONNECTION_SERVICE_HANDLE_T service_handle,
+                                                           void **data,
+                                                           uint32_t *msg_size,
+                                                           VCHI_FLAGS_T flags,
+                                                           void **message_handle );
+
+// Routine to initialise a received message iterator
+typedef int32_t (*VCHI_CONNECTION_SERVICE_LOOKAHEAD_MESSAGE_T)( VCHI_CONNECTION_SERVICE_HANDLE_T service_handle,
+                                                                VCHI_MSG_ITER_T *iter,
+                                                                VCHI_FLAGS_T flags );
+
+// Routine to release a held message
+typedef int32_t (*VCHI_CONNECTION_HELD_MSG_RELEASE_T)( VCHI_CONNECTION_SERVICE_HANDLE_T service_handle,
+                                                       void *message_handle );
+
+// Routine to get info on a held message
+typedef int32_t (*VCHI_CONNECTION_HELD_MSG_INFO_T)( VCHI_CONNECTION_SERVICE_HANDLE_T service_handle,
+                                                    void *message_handle,
+                                                    void **data,
+                                                    int32_t *msg_size,
+                                                    uint32_t *tx_timestamp,
+                                                    uint32_t *rx_timestamp );
+
+// Routine to check whether the iterator has a next message
+typedef int32_t (*VCHI_CONNECTION_MSG_ITER_HAS_NEXT_T)( VCHI_CONNECTION_SERVICE_HANDLE_T service,
+                                                       const VCHI_MSG_ITER_T *iter );
+
+// Routine to advance the iterator
+typedef int32_t (*VCHI_CONNECTION_MSG_ITER_NEXT_T)( VCHI_CONNECTION_SERVICE_HANDLE_T service,
+                                                    VCHI_MSG_ITER_T *iter,
+                                                    void **data,
+                                                    uint32_t *msg_size );
+
+// Routine to remove the last message returned by the iterator
+typedef int32_t (*VCHI_CONNECTION_MSG_ITER_REMOVE_T)( VCHI_CONNECTION_SERVICE_HANDLE_T service,
+                                                      VCHI_MSG_ITER_T *iter );
+
+// Routine to hold the last message returned by the iterator
+typedef int32_t (*VCHI_CONNECTION_MSG_ITER_HOLD_T)( VCHI_CONNECTION_SERVICE_HANDLE_T service,
+                                                    VCHI_MSG_ITER_T *iter,
+                                                    void **msg_handle );
+
+// Routine to transmit bulk data
+typedef int32_t (*VCHI_CONNECTION_BULK_QUEUE_TRANSMIT_T)( VCHI_CONNECTION_SERVICE_HANDLE_T service_handle,
+                                                          const void *data_src,
+                                                          uint32_t data_size,
+                                                          VCHI_FLAGS_T flags,
+                                                          void *bulk_handle );
+
+// Routine to receive data
+typedef int32_t (*VCHI_CONNECTION_BULK_QUEUE_RECEIVE_T)( VCHI_CONNECTION_SERVICE_HANDLE_T service_handle,
+                                                         void *data_dst,
+                                                         uint32_t data_size,
+                                                         VCHI_FLAGS_T flags,
+                                                         void *bulk_handle );
+
+// Routine to report if a server is available
+typedef int32_t (*VCHI_CONNECTION_SERVER_PRESENT)( VCHI_CONNECTION_STATE_T *state, int32_t service_id, int32_t peer_flags );
+
+// Routine to report the number of RX slots available
+typedef int (*VCHI_CONNECTION_RX_SLOTS_AVAILABLE)( const VCHI_CONNECTION_STATE_T *state );
+
+// Routine to report the RX slot size
+typedef uint32_t (*VCHI_CONNECTION_RX_SLOT_SIZE)( const VCHI_CONNECTION_STATE_T *state );
+
+// Callback to indicate that the other side has added a buffer to the rx bulk DMA FIFO
+typedef void (*VCHI_CONNECTION_RX_BULK_BUFFER_ADDED)(VCHI_CONNECTION_STATE_T *state,
+                                                     int32_t service,
+                                                     uint32_t length,
+                                                     MESSAGE_TX_CHANNEL_T channel,
+                                                     uint32_t channel_params,
+                                                     uint32_t data_length,
+                                                     uint32_t data_offset);
+
+// Callback to inform a service that a Xon or Xoff message has been received
+typedef void (*VCHI_CONNECTION_FLOW_CONTROL)(VCHI_CONNECTION_STATE_T *state, int32_t service_id, int32_t xoff);
+
+// Callback to inform a service that a server available reply message has been received
+typedef void (*VCHI_CONNECTION_SERVER_AVAILABLE_REPLY)(VCHI_CONNECTION_STATE_T *state, int32_t service_id, uint32_t flags);
+
+// Callback to indicate that bulk auxiliary messages have arrived
+typedef void (*VCHI_CONNECTION_BULK_AUX_RECEIVED)(VCHI_CONNECTION_STATE_T *state);
+
+// Callback to indicate that bulk auxiliary messages have arrived
+typedef void (*VCHI_CONNECTION_BULK_AUX_TRANSMITTED)(VCHI_CONNECTION_STATE_T *state, void *handle);
+
+// Callback with all the connection info you require
+typedef void (*VCHI_CONNECTION_INFO)(VCHI_CONNECTION_STATE_T *state, uint32_t protocol_version, uint32_t slot_size, uint32_t num_slots, uint32_t min_bulk_size);
+
+// Callback to inform of a disconnect
+typedef void (*VCHI_CONNECTION_DISCONNECT)(VCHI_CONNECTION_STATE_T *state, uint32_t flags);
+
+// Callback to inform of a power control request
+typedef void (*VCHI_CONNECTION_POWER_CONTROL)(VCHI_CONNECTION_STATE_T *state, MESSAGE_TX_CHANNEL_T channel, int32_t enable);
+
+// allocate memory suitably aligned for this connection
+typedef void * (*VCHI_BUFFER_ALLOCATE)(VCHI_CONNECTION_SERVICE_HANDLE_T service_handle, uint32_t * length);
+
+// free memory allocated by buffer_allocate
+typedef void   (*VCHI_BUFFER_FREE)(VCHI_CONNECTION_SERVICE_HANDLE_T service_handle, void * address);
+
+
+/******************************************************************************
+ System driver struct
+ *****************************************************************************/
+
+struct opaque_vchi_connection_api_t
+{
+   // Routine to init the connection
+   VCHI_CONNECTION_INIT_T                      init;
+
+   // Connection-level CRC control
+   VCHI_CONNECTION_CRC_CONTROL_T               crc_control;
+
+   // Routine to connect to or create service
+   VCHI_CONNECTION_SERVICE_CONNECT_T           service_connect;
+
+   // Routine to disconnect from a service
+   VCHI_CONNECTION_SERVICE_DISCONNECT_T        service_disconnect;
+
+   // Routine to queue a message
+   VCHI_CONNECTION_SERVICE_QUEUE_MESSAGE_T     service_queue_msg;
+
+   // scatter-gather (vector) message queue
+   VCHI_CONNECTION_SERVICE_QUEUE_MESSAGEV_T    service_queue_msgv;
+
+   // Routine to dequeue a message
+   VCHI_CONNECTION_SERVICE_DEQUEUE_MESSAGE_T   service_dequeue_msg;
+
+   // Routine to peek at a message
+   VCHI_CONNECTION_SERVICE_PEEK_MESSAGE_T      service_peek_msg;
+
+   // Routine to hold a message
+   VCHI_CONNECTION_SERVICE_HOLD_MESSAGE_T      service_hold_msg;
+
+   // Routine to initialise a received message iterator
+   VCHI_CONNECTION_SERVICE_LOOKAHEAD_MESSAGE_T service_look_ahead_msg;
+
+   // Routine to release a message
+   VCHI_CONNECTION_HELD_MSG_RELEASE_T          held_msg_release;
+
+   // Routine to get information on a held message
+   VCHI_CONNECTION_HELD_MSG_INFO_T             held_msg_info;
+
+   // Routine to check for next message on iterator
+   VCHI_CONNECTION_MSG_ITER_HAS_NEXT_T         msg_iter_has_next;
+
+   // Routine to get next message on iterator
+   VCHI_CONNECTION_MSG_ITER_NEXT_T             msg_iter_next;
+
+   // Routine to remove the last message returned by iterator
+   VCHI_CONNECTION_MSG_ITER_REMOVE_T           msg_iter_remove;
+
+   // Routine to hold the last message returned by iterator
+   VCHI_CONNECTION_MSG_ITER_HOLD_T             msg_iter_hold;
+
+   // Routine to transmit bulk data
+   VCHI_CONNECTION_BULK_QUEUE_TRANSMIT_T       bulk_queue_transmit;
+
+   // Routine to receive data
+   VCHI_CONNECTION_BULK_QUEUE_RECEIVE_T        bulk_queue_receive;
+
+   // Routine to report the available servers
+   VCHI_CONNECTION_SERVER_PRESENT              server_present;
+
+   // Routine to report the number of RX slots available
+   VCHI_CONNECTION_RX_SLOTS_AVAILABLE          connection_rx_slots_available;
+
+   // Routine to report the RX slot size
+   VCHI_CONNECTION_RX_SLOT_SIZE                connection_rx_slot_size;
+
+   // Callback to indicate that the other side has added a buffer to the rx bulk DMA FIFO
+   VCHI_CONNECTION_RX_BULK_BUFFER_ADDED        rx_bulk_buffer_added;
+
+   // Callback to inform a service that a Xon or Xoff message has been received
+   VCHI_CONNECTION_FLOW_CONTROL                flow_control;
+
+   // Callback to inform a service that a server available reply message has been received
+   VCHI_CONNECTION_SERVER_AVAILABLE_REPLY      server_available_reply;
+
+   // Callback to indicate that bulk auxiliary messages have arrived
+   VCHI_CONNECTION_BULK_AUX_RECEIVED           bulk_aux_received;
+
+   // Callback to indicate that a bulk auxiliary message has been transmitted
+   VCHI_CONNECTION_BULK_AUX_TRANSMITTED        bulk_aux_transmitted;
+
+   // Callback to provide information about the connection
+   VCHI_CONNECTION_INFO                        connection_info;
+
+   // Callback to notify that peer has requested disconnect
+   VCHI_CONNECTION_DISCONNECT                  disconnect;
+
+   // Callback to notify that peer has requested power change
+   VCHI_CONNECTION_POWER_CONTROL               power_control;
+
+   // allocate memory suitably aligned for this connection
+   VCHI_BUFFER_ALLOCATE                        buffer_allocate;
+
+   // free memory allocated by buffer_allocate
+   VCHI_BUFFER_FREE                            buffer_free;
+
+};
+
+struct vchi_connection_t {
+   const VCHI_CONNECTION_API_T *api;
+   VCHI_CONNECTION_STATE_T     *state;
+#ifdef VCHI_COARSE_LOCKING
+   struct semaphore             sem;
+#endif
+};
+
+
+#endif /* CONNECTION_H_ */
+
+/****************************** End of file **********************************/
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchi/message_drivers/message.h
@@ -0,0 +1,204 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef _VCHI_MESSAGE_H_
+#define _VCHI_MESSAGE_H_
+
+#include <linux/kernel.h>
+#include <linux/types.h>
+#include <linux/semaphore.h>
+
+#include "interface/vchi/vchi_cfg_internal.h"
+#include "interface/vchi/vchi_common.h"
+
+
+typedef enum message_event_type {
+   MESSAGE_EVENT_NONE,
+   MESSAGE_EVENT_NOP,
+   MESSAGE_EVENT_MESSAGE,
+   MESSAGE_EVENT_SLOT_COMPLETE,
+   MESSAGE_EVENT_RX_BULK_PAUSED,
+   MESSAGE_EVENT_RX_BULK_COMPLETE,
+   MESSAGE_EVENT_TX_COMPLETE,
+   MESSAGE_EVENT_MSG_DISCARDED
+} MESSAGE_EVENT_TYPE_T;
+
+typedef enum vchi_msg_flags
+{
+   VCHI_MSG_FLAGS_NONE                  = 0x0,
+   VCHI_MSG_FLAGS_TERMINATE_DMA         = 0x1
+} VCHI_MSG_FLAGS_T;
+
+typedef enum message_tx_channel
+{
+   MESSAGE_TX_CHANNEL_MESSAGE           = 0,
+   MESSAGE_TX_CHANNEL_BULK              = 1 // drivers may provide multiple bulk channels, from 1 upwards
+} MESSAGE_TX_CHANNEL_T;
+
+// Macros used for cycling through bulk channels
+#define MESSAGE_TX_CHANNEL_BULK_PREV(c) (MESSAGE_TX_CHANNEL_BULK+((c)-MESSAGE_TX_CHANNEL_BULK+VCHI_MAX_BULK_TX_CHANNELS_PER_CONNECTION-1)%VCHI_MAX_BULK_TX_CHANNELS_PER_CONNECTION)
+#define MESSAGE_TX_CHANNEL_BULK_NEXT(c) (MESSAGE_TX_CHANNEL_BULK+((c)-MESSAGE_TX_CHANNEL_BULK+1)%VCHI_MAX_BULK_TX_CHANNELS_PER_CONNECTION)
+
+typedef enum message_rx_channel
+{
+   MESSAGE_RX_CHANNEL_MESSAGE           = 0,
+   MESSAGE_RX_CHANNEL_BULK              = 1 // drivers may provide multiple bulk channels, from 1 upwards
+} MESSAGE_RX_CHANNEL_T;
+
+// Message receive slot information
+typedef struct rx_msg_slot_info {
+
+   struct rx_msg_slot_info *next;
+   //struct slot_info *prev;
+#if !defined VCHI_COARSE_LOCKING
+   struct semaphore   sem;
+#endif
+
+   uint8_t           *addr;               // base address of slot
+   uint32_t           len;                // length of slot in bytes
+
+   uint32_t           write_ptr;          // hardware causes this to advance
+   uint32_t           read_ptr;           // this module does the reading
+   int                active;             // is this slot in the hardware dma fifo?
+   uint32_t           msgs_parsed;        // count how many messages are in this slot
+   uint32_t           msgs_released;      // how many messages have been released
+   void              *state;              // connection state information
+   uint8_t            ref_count[VCHI_MAX_SERVICES_PER_CONNECTION];          // reference count for slots held by services
+} RX_MSG_SLOTINFO_T;
+
+// The message driver no longer needs to know about the fields of RX_BULK_SLOTINFO_T - sort this out.
+// In particular, it mustn't use addr and len - they're the client buffer, but the message
+// driver will be tasked with sending the aligned core section.
+typedef struct rx_bulk_slotinfo_t {
+   struct rx_bulk_slotinfo_t *next;
+
+   struct semaphore *blocking;
+
+   // needed by DMA
+   void        *addr;
+   uint32_t     len;
+
+   // needed for the callback
+   void        *service;
+   void        *handle;
+   VCHI_FLAGS_T flags;
+} RX_BULK_SLOTINFO_T;
+
+
+/* ----------------------------------------------------------------------
+ * each connection driver will have a pool of the following struct.
+ *
+ * the pool will be managed by vchi_qman_*
+ * this means there will be multiple queues (single linked lists)
+ * a given struct message_info will be on exactly one of these queues
+ * at any one time
+ * -------------------------------------------------------------------- */
+typedef struct rx_message_info {
+
+   struct message_info *next;
+   //struct message_info *prev;
+
+   uint8_t    *addr;
+   uint32_t   len;
+   RX_MSG_SLOTINFO_T *slot; // points to whichever slot contains this message
+   uint32_t   tx_timestamp;
+   uint32_t   rx_timestamp;
+
+} RX_MESSAGE_INFO_T;
+
+typedef struct {
+   MESSAGE_EVENT_TYPE_T type;
+
+   struct {
+      // for messages
+      void    *addr;           // address of message
+      uint16_t slot_delta;     // whether this message indicated slot delta
+      uint32_t len;            // length of message
+      RX_MSG_SLOTINFO_T *slot; // slot this message is in
+      int32_t  service;   // service id this message is destined for
+      uint32_t tx_timestamp;   // timestamp from the header
+      uint32_t rx_timestamp;   // timestamp when we parsed it
+   } message;
+
+   // FIXME: cleanup slot reporting...
+   RX_MSG_SLOTINFO_T *rx_msg;
+   RX_BULK_SLOTINFO_T *rx_bulk;
+   void *tx_handle;
+   MESSAGE_TX_CHANNEL_T tx_channel;
+
+} MESSAGE_EVENT_T;
+
+
+// callbacks
+typedef void VCHI_MESSAGE_DRIVER_EVENT_CALLBACK_T( void *state );
+
+typedef struct {
+   VCHI_MESSAGE_DRIVER_EVENT_CALLBACK_T *event_callback;
+} VCHI_MESSAGE_DRIVER_OPEN_T;
+
+
+// handle to this instance of message driver (as returned by ->open)
+typedef struct opaque_mhandle_t *VCHI_MDRIVER_HANDLE_T;
+
+struct opaque_vchi_message_driver_t {
+   VCHI_MDRIVER_HANDLE_T *(*open)( VCHI_MESSAGE_DRIVER_OPEN_T *params, void *state );
+   int32_t (*suspending)( VCHI_MDRIVER_HANDLE_T *handle );
+   int32_t (*resumed)( VCHI_MDRIVER_HANDLE_T *handle );
+   int32_t (*power_control)( VCHI_MDRIVER_HANDLE_T *handle, MESSAGE_TX_CHANNEL_T, int32_t enable );
+   int32_t (*add_msg_rx_slot)( VCHI_MDRIVER_HANDLE_T *handle, RX_MSG_SLOTINFO_T *slot );      // rx message
+   int32_t (*add_bulk_rx)( VCHI_MDRIVER_HANDLE_T *handle, void *data, uint32_t len, RX_BULK_SLOTINFO_T *slot );  // rx data (bulk)
+   int32_t (*send)( VCHI_MDRIVER_HANDLE_T *handle, MESSAGE_TX_CHANNEL_T channel, const void *data, uint32_t len, VCHI_MSG_FLAGS_T flags, void *send_handle );      // tx (message & bulk)
+   void    (*next_event)( VCHI_MDRIVER_HANDLE_T *handle, MESSAGE_EVENT_T *event );     // get the next event from message_driver
+   int32_t (*enable)( VCHI_MDRIVER_HANDLE_T *handle );
+   int32_t (*form_message)( VCHI_MDRIVER_HANDLE_T *handle, int32_t service_id, VCHI_MSG_VECTOR_T *vector, uint32_t count, void
+                            *address, uint32_t length_avail, uint32_t max_total_length, int32_t pad_to_fill, int32_t allow_partial );
+
+   int32_t (*update_message)( VCHI_MDRIVER_HANDLE_T *handle, void *dest, int16_t *slot_count );
+   int32_t (*buffer_aligned)( VCHI_MDRIVER_HANDLE_T *handle, int tx, int uncached, const void *address, const uint32_t length );
+   void *  (*allocate_buffer)( VCHI_MDRIVER_HANDLE_T *handle, uint32_t *length );
+   void    (*free_buffer)( VCHI_MDRIVER_HANDLE_T *handle, void *address );
+   int     (*rx_slot_size)( VCHI_MDRIVER_HANDLE_T *handle, int msg_size );
+   int     (*tx_slot_size)( VCHI_MDRIVER_HANDLE_T *handle, int msg_size );
+
+   int32_t  (*tx_supports_terminate)( const VCHI_MDRIVER_HANDLE_T *handle, MESSAGE_TX_CHANNEL_T channel );
+   uint32_t (*tx_bulk_chunk_size)( const VCHI_MDRIVER_HANDLE_T *handle, MESSAGE_TX_CHANNEL_T channel );
+   int     (*tx_alignment)( const VCHI_MDRIVER_HANDLE_T *handle, MESSAGE_TX_CHANNEL_T channel );
+   int     (*rx_alignment)( const VCHI_MDRIVER_HANDLE_T *handle, MESSAGE_RX_CHANNEL_T channel );
+   void    (*form_bulk_aux)( VCHI_MDRIVER_HANDLE_T *handle, MESSAGE_TX_CHANNEL_T channel, const void *data, uint32_t len, uint32_t chunk_size, const void **aux_data, int32_t *aux_len );
+   void    (*debug)( VCHI_MDRIVER_HANDLE_T *handle );
+};
+
+
+#endif // _VCHI_MESSAGE_H_
+
+/****************************** End of file ***********************************/
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchi/vchi.h
@@ -0,0 +1,378 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHI_H_
+#define VCHI_H_
+
+#include "interface/vchi/vchi_cfg.h"
+#include "interface/vchi/vchi_common.h"
+#include "interface/vchi/connections/connection.h"
+#include "vchi_mh.h"
+
+
+/******************************************************************************
+ Global defs
+ *****************************************************************************/
+
+#define VCHI_BULK_ROUND_UP(x)     ((((unsigned long)(x))+VCHI_BULK_ALIGN-1) & ~(VCHI_BULK_ALIGN-1))
+#define VCHI_BULK_ROUND_DOWN(x)   (((unsigned long)(x)) & ~(VCHI_BULK_ALIGN-1))
+#define VCHI_BULK_ALIGN_NBYTES(x) (VCHI_BULK_ALIGNED(x) ? 0 : (VCHI_BULK_ALIGN - ((unsigned long)(x) & (VCHI_BULK_ALIGN-1))))
+
+#ifdef USE_VCHIQ_ARM
+#define VCHI_BULK_ALIGNED(x)      1
+#else
+#define VCHI_BULK_ALIGNED(x)      (((unsigned long)(x) & (VCHI_BULK_ALIGN-1)) == 0)
+#endif
+
+struct vchi_version {
+	uint32_t version;
+	uint32_t version_min;
+};
+#define VCHI_VERSION(v_) { v_, v_ }
+#define VCHI_VERSION_EX(v_, m_) { v_, m_ }
+
+typedef enum
+{
+   VCHI_VEC_POINTER,
+   VCHI_VEC_HANDLE,
+   VCHI_VEC_LIST
+} VCHI_MSG_VECTOR_TYPE_T;
+
+typedef struct vchi_msg_vector_ex {
+
+   VCHI_MSG_VECTOR_TYPE_T type;
+   union
+   {
+      // a memory handle
+      struct
+      {
+         VCHI_MEM_HANDLE_T handle;
+         uint32_t offset;
+         int32_t vec_len;
+      } handle;
+
+      // an ordinary data pointer
+      struct
+      {
+         const void *vec_base;
+         int32_t vec_len;
+      } ptr;
+
+      // a nested vector list
+      struct
+      {
+         struct vchi_msg_vector_ex *vec;
+         uint32_t vec_len;
+      } list;
+   } u;
+} VCHI_MSG_VECTOR_EX_T;
+
+
+// Construct an entry in a msg vector for a pointer (p) of length (l)
+#define VCHI_VEC_POINTER(p,l)  VCHI_VEC_POINTER, { { (VCHI_MEM_HANDLE_T)(p), (l) } }
+
+// Construct an entry in a msg vector for a message handle (h), starting at offset (o) of length (l)
+#define VCHI_VEC_HANDLE(h,o,l) VCHI_VEC_HANDLE,  { { (h), (o), (l) } }
+
+// Macros to manipulate 'FOURCC' values
+#define MAKE_FOURCC(x) ((int32_t)( (x[0] << 24) | (x[1] << 16) | (x[2] << 8) | x[3] ))
+#define FOURCC_TO_CHAR(x) (x >> 24) & 0xFF,(x >> 16) & 0xFF,(x >> 8) & 0xFF, x & 0xFF
+
+
+// Opaque service information
+struct opaque_vchi_service_t;
+
+// Descriptor for a held message. Allocated by client, initialised by vchi_msg_hold,
+// vchi_msg_iter_hold or vchi_msg_iter_hold_next. Fields are for internal VCHI use only.
+typedef struct
+{
+   struct opaque_vchi_service_t *service;
+   void *message;
+} VCHI_HELD_MSG_T;
+
+
+
+// structure used to provide the information needed to open a server or a client
+typedef struct {
+	struct vchi_version version;
+	int32_t service_id;
+	VCHI_CONNECTION_T *connection;
+	uint32_t rx_fifo_size;
+	uint32_t tx_fifo_size;
+	VCHI_CALLBACK_T callback;
+	void *callback_param;
+	/* client intends to receive bulk transfers of
+		odd lengths or into unaligned buffers */
+	int32_t want_unaligned_bulk_rx;
+	/* client intends to transmit bulk transfers of
+		odd lengths or out of unaligned buffers */
+	int32_t want_unaligned_bulk_tx;
+	/* client wants to check CRCs on (bulk) xfers.
+		Only needs to be set at 1 end - will do both directions. */
+	int32_t want_crc;
+} SERVICE_CREATION_T;
+
+// Opaque handle for a VCHI instance
+typedef struct opaque_vchi_instance_handle_t *VCHI_INSTANCE_T;
+
+// Opaque handle for a server or client
+typedef struct opaque_vchi_service_handle_t *VCHI_SERVICE_HANDLE_T;
+
+// Service registration & startup
+typedef void (*VCHI_SERVICE_INIT)(VCHI_INSTANCE_T initialise_instance, VCHI_CONNECTION_T **connections, uint32_t num_connections);
+
+typedef struct service_info_tag {
+   const char * const vll_filename; /* VLL to load to start this service. This is an empty string if VLL is "static" */
+   VCHI_SERVICE_INIT init;          /* Service initialisation function */
+   void *vll_handle;                /* VLL handle; NULL when unloaded or a "static VLL" in build */
+} SERVICE_INFO_T;
+
+/******************************************************************************
+ Global funcs - implementation is specific to which side you are on (local / remote)
+ *****************************************************************************/
+
+#ifdef __cplusplus
+extern "C" {
+#endif
+
+extern /*@observer@*/ VCHI_CONNECTION_T * vchi_create_connection( const VCHI_CONNECTION_API_T * function_table,
+                                                   const VCHI_MESSAGE_DRIVER_T * low_level);
+
+
+// Routine used to initialise the vchi on both local + remote connections
+extern int32_t vchi_initialise( VCHI_INSTANCE_T *instance_handle );
+
+extern int32_t vchi_exit( void );
+
+extern int32_t vchi_connect( VCHI_CONNECTION_T **connections,
+                             const uint32_t num_connections,
+                             VCHI_INSTANCE_T instance_handle );
+
+//When this is called, ensure that all services have no data pending.
+//Bulk transfers can remain 'queued'
+extern int32_t vchi_disconnect( VCHI_INSTANCE_T instance_handle );
+
+// Global control over bulk CRC checking
+extern int32_t vchi_crc_control( VCHI_CONNECTION_T *connection,
+                                 VCHI_CRC_CONTROL_T control );
+
+// helper functions
+extern void * vchi_allocate_buffer(VCHI_SERVICE_HANDLE_T handle, uint32_t *length);
+extern void vchi_free_buffer(VCHI_SERVICE_HANDLE_T handle, void *address);
+extern uint32_t vchi_current_time(VCHI_INSTANCE_T instance_handle);
+
+
+/******************************************************************************
+ Global service API
+ *****************************************************************************/
+// Routine to create a named service
+extern int32_t vchi_service_create( VCHI_INSTANCE_T instance_handle,
+                                    SERVICE_CREATION_T *setup,
+                                    VCHI_SERVICE_HANDLE_T *handle );
+
+// Routine to destory a service
+extern int32_t vchi_service_destroy( const VCHI_SERVICE_HANDLE_T handle );
+
+// Routine to open a named service
+extern int32_t vchi_service_open( VCHI_INSTANCE_T instance_handle,
+                                  SERVICE_CREATION_T *setup,
+                                  VCHI_SERVICE_HANDLE_T *handle);
+
+extern int32_t vchi_get_peer_version( const VCHI_SERVICE_HANDLE_T handle,
+                                      short *peer_version );
+
+// Routine to close a named service
+extern int32_t vchi_service_close( const VCHI_SERVICE_HANDLE_T handle );
+
+// Routine to increment ref count on a named service
+extern int32_t vchi_service_use( const VCHI_SERVICE_HANDLE_T handle );
+
+// Routine to decrement ref count on a named service
+extern int32_t vchi_service_release( const VCHI_SERVICE_HANDLE_T handle );
+
+// Routine to set a control option for a named service
+extern int32_t vchi_service_set_option( const VCHI_SERVICE_HANDLE_T handle,
+					VCHI_SERVICE_OPTION_T option,
+					int value);
+
+// Routine to send a message across a service
+extern int32_t vchi_msg_queue( VCHI_SERVICE_HANDLE_T handle,
+                               const void *data,
+                               uint32_t data_size,
+                               VCHI_FLAGS_T flags,
+                               void *msg_handle );
+
+// scatter-gather (vector) and send message
+int32_t vchi_msg_queuev_ex( VCHI_SERVICE_HANDLE_T handle,
+                            VCHI_MSG_VECTOR_EX_T *vector,
+                            uint32_t count,
+                            VCHI_FLAGS_T flags,
+                            void *msg_handle );
+
+// legacy scatter-gather (vector) and send message, only handles pointers
+int32_t vchi_msg_queuev( VCHI_SERVICE_HANDLE_T handle,
+                         VCHI_MSG_VECTOR_T *vector,
+                         uint32_t count,
+                         VCHI_FLAGS_T flags,
+                         void *msg_handle );
+
+// Routine to receive a msg from a service
+// Dequeue is equivalent to hold, copy into client buffer, release
+extern int32_t vchi_msg_dequeue( VCHI_SERVICE_HANDLE_T handle,
+                                 void *data,
+                                 uint32_t max_data_size_to_read,
+                                 uint32_t *actual_msg_size,
+                                 VCHI_FLAGS_T flags );
+
+// Routine to look at a message in place.
+// The message is not dequeued, so a subsequent call to peek or dequeue
+// will return the same message.
+extern int32_t vchi_msg_peek( VCHI_SERVICE_HANDLE_T handle,
+                              void **data,
+                              uint32_t *msg_size,
+                              VCHI_FLAGS_T flags );
+
+// Routine to remove a message after it has been read in place with peek
+// The first message on the queue is dequeued.
+extern int32_t vchi_msg_remove( VCHI_SERVICE_HANDLE_T handle );
+
+// Routine to look at a message in place.
+// The message is dequeued, so the caller is left holding it; the descriptor is
+// filled in and must be released when the user has finished with the message.
+extern int32_t vchi_msg_hold( VCHI_SERVICE_HANDLE_T handle,
+                              void **data,        // } may be NULL, as info can be
+                              uint32_t *msg_size, // } obtained from HELD_MSG_T
+                              VCHI_FLAGS_T flags,
+                              VCHI_HELD_MSG_T *message_descriptor );
+
+// Initialise an iterator to look through messages in place
+extern int32_t vchi_msg_look_ahead( VCHI_SERVICE_HANDLE_T handle,
+                                    VCHI_MSG_ITER_T *iter,
+                                    VCHI_FLAGS_T flags );
+
+/******************************************************************************
+ Global service support API - operations on held messages and message iterators
+ *****************************************************************************/
+
+// Routine to get the address of a held message
+extern void *vchi_held_msg_ptr( const VCHI_HELD_MSG_T *message );
+
+// Routine to get the size of a held message
+extern int32_t vchi_held_msg_size( const VCHI_HELD_MSG_T *message );
+
+// Routine to get the transmit timestamp as written into the header by the peer
+extern uint32_t vchi_held_msg_tx_timestamp( const VCHI_HELD_MSG_T *message );
+
+// Routine to get the reception timestamp, written as we parsed the header
+extern uint32_t vchi_held_msg_rx_timestamp( const VCHI_HELD_MSG_T *message );
+
+// Routine to release a held message after it has been processed
+extern int32_t vchi_held_msg_release( VCHI_HELD_MSG_T *message );
+
+// Indicates whether the iterator has a next message.
+extern int32_t vchi_msg_iter_has_next( const VCHI_MSG_ITER_T *iter );
+
+// Return the pointer and length for the next message and advance the iterator.
+extern int32_t vchi_msg_iter_next( VCHI_MSG_ITER_T *iter,
+                                   void **data,
+                                   uint32_t *msg_size );
+
+// Remove the last message returned by vchi_msg_iter_next.
+// Can only be called once after each call to vchi_msg_iter_next.
+extern int32_t vchi_msg_iter_remove( VCHI_MSG_ITER_T *iter );
+
+// Hold the last message returned by vchi_msg_iter_next.
+// Can only be called once after each call to vchi_msg_iter_next.
+extern int32_t vchi_msg_iter_hold( VCHI_MSG_ITER_T *iter,
+                                   VCHI_HELD_MSG_T *message );
+
+// Return information for the next message, and hold it, advancing the iterator.
+extern int32_t vchi_msg_iter_hold_next( VCHI_MSG_ITER_T *iter,
+                                        void **data,        // } may be NULL
+                                        uint32_t *msg_size, // }
+                                        VCHI_HELD_MSG_T *message );
+
+
+/******************************************************************************
+ Global bulk API
+ *****************************************************************************/
+
+// Routine to prepare interface for a transfer from the other side
+extern int32_t vchi_bulk_queue_receive( VCHI_SERVICE_HANDLE_T handle,
+                                        void *data_dst,
+                                        uint32_t data_size,
+                                        VCHI_FLAGS_T flags,
+                                        void *transfer_handle );
+
+
+// Prepare interface for a transfer from the other side into relocatable memory.
+int32_t vchi_bulk_queue_receive_reloc( const VCHI_SERVICE_HANDLE_T handle,
+                                       VCHI_MEM_HANDLE_T h_dst,
+                                       uint32_t offset,
+                                       uint32_t data_size,
+                                       const VCHI_FLAGS_T flags,
+                                       void * const bulk_handle );
+
+// Routine to queue up data ready for transfer to the other (once they have signalled they are ready)
+extern int32_t vchi_bulk_queue_transmit( VCHI_SERVICE_HANDLE_T handle,
+                                         const void *data_src,
+                                         uint32_t data_size,
+                                         VCHI_FLAGS_T flags,
+                                         void *transfer_handle );
+
+
+/******************************************************************************
+ Configuration plumbing
+ *****************************************************************************/
+
+// function prototypes for the different mid layers (the state info gives the different physical connections)
+extern const VCHI_CONNECTION_API_T *single_get_func_table( void );
+//extern const VCHI_CONNECTION_API_T *local_server_get_func_table( void );
+//extern const VCHI_CONNECTION_API_T *local_client_get_func_table( void );
+
+// declare all message drivers here
+const VCHI_MESSAGE_DRIVER_T *vchi_mphi_message_driver_func_table( void );
+
+#ifdef __cplusplus
+}
+#endif
+
+extern int32_t vchi_bulk_queue_transmit_reloc( VCHI_SERVICE_HANDLE_T handle,
+                                               VCHI_MEM_HANDLE_T h_src,
+                                               uint32_t offset,
+                                               uint32_t data_size,
+                                               VCHI_FLAGS_T flags,
+                                               void *transfer_handle );
+#endif /* VCHI_H_ */
+
+/****************************** End of file **********************************/
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchi/vchi_cfg.h
@@ -0,0 +1,224 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHI_CFG_H_
+#define VCHI_CFG_H_
+
+/****************************************************************************************
+ * Defines in this first section are part of the VCHI API and may be examined by VCHI
+ * services.
+ ***************************************************************************************/
+
+/* Required alignment of base addresses for bulk transfer, if unaligned transfers are not enabled */
+/* Really determined by the message driver, and should be available from a run-time call. */
+#ifndef VCHI_BULK_ALIGN
+#   if __VCCOREVER__ >= 0x04000000
+#       define VCHI_BULK_ALIGN 32 // Allows for the need to do cache cleans
+#   else
+#       define VCHI_BULK_ALIGN 16
+#   endif
+#endif
+
+/* Required length multiple for bulk transfers, if unaligned transfers are not enabled */
+/* May be less than or greater than VCHI_BULK_ALIGN */
+/* Really determined by the message driver, and should be available from a run-time call. */
+#ifndef VCHI_BULK_GRANULARITY
+#   if __VCCOREVER__ >= 0x04000000
+#       define VCHI_BULK_GRANULARITY 32 // Allows for the need to do cache cleans
+#   else
+#       define VCHI_BULK_GRANULARITY 16
+#   endif
+#endif
+
+/* The largest possible message to be queued with vchi_msg_queue. */
+#ifndef VCHI_MAX_MSG_SIZE
+#   if defined VCHI_LOCAL_HOST_PORT
+#       define VCHI_MAX_MSG_SIZE     16384         // makes file transfers fast, but should they be using bulk?
+#   else
+#       define VCHI_MAX_MSG_SIZE      4096 // NOTE: THIS MUST BE LARGER THAN OR EQUAL TO THE SIZE OF THE KHRONOS MERGE BUFFER!!
+#   endif
+#endif
+
+/******************************************************************************************
+ * Defines below are system configuration options, and should not be used by VCHI services.
+ *****************************************************************************************/
+
+/* How many connections can we support? A localhost implementation uses 2 connections,
+ * 1 for host-app, 1 for VMCS, and these are hooked together by a loopback MPHI VCFW
+ * driver. */
+#ifndef VCHI_MAX_NUM_CONNECTIONS
+#   define VCHI_MAX_NUM_CONNECTIONS 3
+#endif
+
+/* How many services can we open per connection? Extending this doesn't cost processing time, just a small
+ * amount of static memory. */
+#ifndef VCHI_MAX_SERVICES_PER_CONNECTION
+#  define VCHI_MAX_SERVICES_PER_CONNECTION 36
+#endif
+
+/* Adjust if using a message driver that supports more logical TX channels */
+#ifndef VCHI_MAX_BULK_TX_CHANNELS_PER_CONNECTION
+#   define VCHI_MAX_BULK_TX_CHANNELS_PER_CONNECTION 9 // 1 MPHI + 8 CCP2 logical channels
+#endif
+
+/* Adjust if using a message driver that supports more logical RX channels */
+#ifndef VCHI_MAX_BULK_RX_CHANNELS_PER_CONNECTION
+#   define VCHI_MAX_BULK_RX_CHANNELS_PER_CONNECTION 1 // 1 MPHI
+#endif
+
+/* How many receive slots do we use. This times VCHI_MAX_MSG_SIZE gives the effective
+ * receive queue space, less message headers. */
+#ifndef VCHI_NUM_READ_SLOTS
+#  if defined(VCHI_LOCAL_HOST_PORT)
+#     define VCHI_NUM_READ_SLOTS 4
+#  else
+#     define VCHI_NUM_READ_SLOTS 48
+#  endif
+#endif
+
+/* Do we utilise overrun facility for receive message slots? Can aid peer transmit
+ * performance. Only define on VideoCore end, talking to host.
+ */
+//#define VCHI_MSG_RX_OVERRUN
+
+/* How many transmit slots do we use. Generally don't need many, as the hardware driver
+ * underneath VCHI will usually have its own buffering. */
+#ifndef VCHI_NUM_WRITE_SLOTS
+#  define VCHI_NUM_WRITE_SLOTS 4
+#endif
+
+/* If a service has held or queued received messages in VCHI_XOFF_THRESHOLD or more slots,
+ * then it's taking up too much buffer space, and the peer service will be told to stop
+ * transmitting with an XOFF message. For this to be effective, the VCHI_NUM_READ_SLOTS
+ * needs to be considerably bigger than VCHI_NUM_WRITE_SLOTS, or the transmit latency
+ * is too high. */
+#ifndef VCHI_XOFF_THRESHOLD
+#  define VCHI_XOFF_THRESHOLD (VCHI_NUM_READ_SLOTS / 2)
+#endif
+
+/* After we've sent an XOFF, the peer will be told to resume transmission once the local
+ * service has dequeued/released enough messages that it's now occupying
+ * VCHI_XON_THRESHOLD slots or fewer. */
+#ifndef VCHI_XON_THRESHOLD
+#  define VCHI_XON_THRESHOLD (VCHI_NUM_READ_SLOTS / 4)
+#endif
+
+/* A size below which a bulk transfer omits the handshake completely and always goes
+ * via the message channel, if bulk auxiliary is being sent on that service. (The user
+ * can guarantee this by enabling unaligned transmits).
+ * Not API. */
+#ifndef VCHI_MIN_BULK_SIZE
+#  define VCHI_MIN_BULK_SIZE    ( VCHI_MAX_MSG_SIZE / 2 < 4096 ? VCHI_MAX_MSG_SIZE / 2 : 4096 )
+#endif
+
+/* Maximum size of bulk transmission chunks, for each interface type. A trade-off between
+ * speed and latency; the smaller the chunk size the better change of messages and other
+ * bulk transmissions getting in when big bulk transfers are happening. Set to 0 to not
+ * break transmissions into chunks.
+ */
+#ifndef VCHI_MAX_BULK_CHUNK_SIZE_MPHI
+#  define VCHI_MAX_BULK_CHUNK_SIZE_MPHI (16 * 1024)
+#endif
+
+/* NB Chunked CCP2 transmissions violate the letter of the CCP2 spec by using "JPEG8" mode
+ * with multiple-line frames. Only use if the receiver can cope. */
+#ifndef VCHI_MAX_BULK_CHUNK_SIZE_CCP2
+#  define VCHI_MAX_BULK_CHUNK_SIZE_CCP2 0
+#endif
+
+/* How many TX messages can we have pending in our transmit slots. Once exhausted,
+ * vchi_msg_queue will be blocked. */
+#ifndef VCHI_TX_MSG_QUEUE_SIZE
+#  define VCHI_TX_MSG_QUEUE_SIZE           256
+#endif
+
+/* How many RX messages can we have parsed in the receive slots. Once exhausted, parsing
+ * will be suspended until older messages are dequeued/released. */
+#ifndef VCHI_RX_MSG_QUEUE_SIZE
+#  define VCHI_RX_MSG_QUEUE_SIZE           256
+#endif
+
+/* Really should be able to cope if we run out of received message descriptors, by
+ * suspending parsing as the comment above says, but we don't. This sweeps the issue
+ * under the carpet. */
+#if VCHI_RX_MSG_QUEUE_SIZE < (VCHI_MAX_MSG_SIZE/16 + 1) * VCHI_NUM_READ_SLOTS
+#  undef VCHI_RX_MSG_QUEUE_SIZE
+#  define VCHI_RX_MSG_QUEUE_SIZE (VCHI_MAX_MSG_SIZE/16 + 1) * VCHI_NUM_READ_SLOTS
+#endif
+
+/* How many bulk transmits can we have pending. Once exhausted, vchi_bulk_queue_transmit
+ * will be blocked. */
+#ifndef VCHI_TX_BULK_QUEUE_SIZE
+#  define VCHI_TX_BULK_QUEUE_SIZE           64
+#endif
+
+/* How many bulk receives can we have pending. Once exhausted, vchi_bulk_queue_receive
+ * will be blocked. */
+#ifndef VCHI_RX_BULK_QUEUE_SIZE
+#  define VCHI_RX_BULK_QUEUE_SIZE           64
+#endif
+
+/* A limit on how many outstanding bulk requests we expect the peer to give us. If
+ * the peer asks for more than this, VCHI will fail and assert. The number is determined
+ * by the peer's hardware - it's the number of outstanding requests that can be queued
+ * on all bulk channels. VC3's MPHI peripheral allows 16. */
+#ifndef VCHI_MAX_PEER_BULK_REQUESTS
+#  define VCHI_MAX_PEER_BULK_REQUESTS       32
+#endif
+
+/* Define VCHI_CCP2TX_MANUAL_POWER if the host tells us when to turn the CCP2
+ * transmitter on and off.
+ */
+/*#define VCHI_CCP2TX_MANUAL_POWER*/
+
+#ifndef VCHI_CCP2TX_MANUAL_POWER
+
+/* Timeout (in milliseconds) for putting the CCP2TX interface into IDLE state. Set
+ * negative for no IDLE.
+ */
+#  ifndef VCHI_CCP2TX_IDLE_TIMEOUT
+#    define VCHI_CCP2TX_IDLE_TIMEOUT        5
+#  endif
+
+/* Timeout (in milliseconds) for putting the CCP2TX interface into OFF state. Set
+ * negative for no OFF.
+ */
+#  ifndef VCHI_CCP2TX_OFF_TIMEOUT
+#    define VCHI_CCP2TX_OFF_TIMEOUT         1000
+#  endif
+
+#endif /* VCHI_CCP2TX_MANUAL_POWER */
+
+#endif /* VCHI_CFG_H_ */
+
+/****************************** End of file **********************************/
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchi/vchi_cfg_internal.h
@@ -0,0 +1,71 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHI_CFG_INTERNAL_H_
+#define VCHI_CFG_INTERNAL_H_
+
+/****************************************************************************************
+ * Control optimisation attempts.
+ ***************************************************************************************/
+
+// Don't use lots of short-term locks - use great long ones, reducing the overall locks-per-second
+#define VCHI_COARSE_LOCKING
+
+// Avoid lock then unlock on exit from blocking queue operations (msg tx, bulk rx/tx)
+// (only relevant if VCHI_COARSE_LOCKING)
+#define VCHI_ELIDE_BLOCK_EXIT_LOCK
+
+// Avoid lock on non-blocking peek
+// (only relevant if VCHI_COARSE_LOCKING)
+#define VCHI_AVOID_PEEK_LOCK
+
+// Use one slot-handler thread per connection, rather than 1 thread dealing with all connections in rotation.
+#define VCHI_MULTIPLE_HANDLER_THREADS
+
+// Put free descriptors onto the head of the free queue, rather than the tail, so that we don't thrash
+// our way through the pool of descriptors.
+#define VCHI_PUSH_FREE_DESCRIPTORS_ONTO_HEAD
+
+// Don't issue a MSG_AVAILABLE callback for every single message. Possibly only safe if VCHI_COARSE_LOCKING.
+#define VCHI_FEWER_MSG_AVAILABLE_CALLBACKS
+
+// Don't use message descriptors for TX messages that don't need them
+#define VCHI_MINIMISE_TX_MSG_DESCRIPTORS
+
+// Nano-locks for multiqueue
+//#define VCHI_MQUEUE_NANOLOCKS
+
+// Lock-free(er) dequeuing
+//#define VCHI_RX_NANOLOCKS
+
+#endif /*VCHI_CFG_INTERNAL_H_*/
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchi/vchi_common.h
@@ -0,0 +1,174 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHI_COMMON_H_
+#define VCHI_COMMON_H_
+
+
+//flags used when sending messages (must be bitmapped)
+typedef enum
+{
+   VCHI_FLAGS_NONE                      = 0x0,
+   VCHI_FLAGS_BLOCK_UNTIL_OP_COMPLETE   = 0x1,   // waits for message to be received, or sent (NB. not the same as being seen on other side)
+   VCHI_FLAGS_CALLBACK_WHEN_OP_COMPLETE = 0x2,   // run a callback when message sent
+   VCHI_FLAGS_BLOCK_UNTIL_QUEUED        = 0x4,   // return once the transfer is in a queue ready to go
+   VCHI_FLAGS_ALLOW_PARTIAL             = 0x8,
+   VCHI_FLAGS_BLOCK_UNTIL_DATA_READ     = 0x10,
+   VCHI_FLAGS_CALLBACK_WHEN_DATA_READ   = 0x20,
+
+   VCHI_FLAGS_ALIGN_SLOT            = 0x000080,  // internal use only
+   VCHI_FLAGS_BULK_AUX_QUEUED       = 0x010000,  // internal use only
+   VCHI_FLAGS_BULK_AUX_COMPLETE     = 0x020000,  // internal use only
+   VCHI_FLAGS_BULK_DATA_QUEUED      = 0x040000,  // internal use only
+   VCHI_FLAGS_BULK_DATA_COMPLETE    = 0x080000,  // internal use only
+   VCHI_FLAGS_INTERNAL              = 0xFF0000
+} VCHI_FLAGS_T;
+
+// constants for vchi_crc_control()
+typedef enum {
+   VCHI_CRC_NOTHING = -1,
+   VCHI_CRC_PER_SERVICE = 0,
+   VCHI_CRC_EVERYTHING = 1,
+} VCHI_CRC_CONTROL_T;
+
+//callback reasons when an event occurs on a service
+typedef enum
+{
+   VCHI_CALLBACK_REASON_MIN,
+
+   //This indicates that there is data available
+   //handle is the msg id that was transmitted with the data
+   //    When a message is received and there was no FULL message available previously, send callback
+   //    Tasks get kicked by the callback, reset their event and try and read from the fifo until it fails
+   VCHI_CALLBACK_MSG_AVAILABLE,
+   VCHI_CALLBACK_MSG_SENT,
+   VCHI_CALLBACK_MSG_SPACE_AVAILABLE, // XXX not yet implemented
+
+   // This indicates that a transfer from the other side has completed
+   VCHI_CALLBACK_BULK_RECEIVED,
+   //This indicates that data queued up to be sent has now gone
+   //handle is the msg id that was used when sending the data
+   VCHI_CALLBACK_BULK_SENT,
+   VCHI_CALLBACK_BULK_RX_SPACE_AVAILABLE, // XXX not yet implemented
+   VCHI_CALLBACK_BULK_TX_SPACE_AVAILABLE, // XXX not yet implemented
+
+   VCHI_CALLBACK_SERVICE_CLOSED,
+
+   // this side has sent XOFF to peer due to lack of data consumption by service
+   // (suggests the service may need to take some recovery action if it has
+   // been deliberately holding off consuming data)
+   VCHI_CALLBACK_SENT_XOFF,
+   VCHI_CALLBACK_SENT_XON,
+
+   // indicates that a bulk transfer has finished reading the source buffer
+   VCHI_CALLBACK_BULK_DATA_READ,
+
+   // power notification events (currently host side only)
+   VCHI_CALLBACK_PEER_OFF,
+   VCHI_CALLBACK_PEER_SUSPENDED,
+   VCHI_CALLBACK_PEER_ON,
+   VCHI_CALLBACK_PEER_RESUMED,
+   VCHI_CALLBACK_FORCED_POWER_OFF,
+
+#ifdef USE_VCHIQ_ARM
+   // some extra notifications provided by vchiq_arm
+   VCHI_CALLBACK_SERVICE_OPENED,
+   VCHI_CALLBACK_BULK_RECEIVE_ABORTED,
+   VCHI_CALLBACK_BULK_TRANSMIT_ABORTED,
+#endif
+
+   VCHI_CALLBACK_REASON_MAX
+} VCHI_CALLBACK_REASON_T;
+
+// service control options
+typedef enum
+{
+   VCHI_SERVICE_OPTION_MIN,
+
+   VCHI_SERVICE_OPTION_TRACE,
+
+   VCHI_SERVICE_OPTION_MAX
+} VCHI_SERVICE_OPTION_T;
+
+
+//Callback used by all services / bulk transfers
+typedef void (*VCHI_CALLBACK_T)( void *callback_param, //my service local param
+                                 VCHI_CALLBACK_REASON_T reason,
+                                 void *handle ); //for transmitting msg's only
+
+
+
+/*
+ * Define vector struct for scatter-gather (vector) operations
+ * Vectors can be nested - if a vector element has negative length, then
+ * the data pointer is treated as pointing to another vector array, with
+ * '-vec_len' elements. Thus to append a header onto an existing vector,
+ * you can do this:
+ *
+ * void foo(const VCHI_MSG_VECTOR_T *v, int n)
+ * {
+ *    VCHI_MSG_VECTOR_T nv[2];
+ *    nv[0].vec_base = my_header;
+ *    nv[0].vec_len = sizeof my_header;
+ *    nv[1].vec_base = v;
+ *    nv[1].vec_len = -n;
+ *    ...
+ *
+ */
+typedef struct vchi_msg_vector {
+   const void *vec_base;
+   int32_t vec_len;
+} VCHI_MSG_VECTOR_T;
+
+// Opaque type for a connection API
+typedef struct opaque_vchi_connection_api_t VCHI_CONNECTION_API_T;
+
+// Opaque type for a message driver
+typedef struct opaque_vchi_message_driver_t VCHI_MESSAGE_DRIVER_T;
+
+
+// Iterator structure for reading ahead through received message queue. Allocated by client,
+// initialised by vchi_msg_look_ahead. Fields are for internal VCHI use only.
+// Iterates over messages in queue at the instant of the call to vchi_msg_lookahead -
+// will not proceed to messages received since. Behaviour is undefined if an iterator
+// is used again after messages for that service are removed/dequeued by any
+// means other than vchi_msg_iter_... calls on the iterator itself.
+typedef struct {
+   struct opaque_vchi_service_t *service;
+   void *last;
+   void *next;
+   void *remove;
+} VCHI_MSG_ITER_T;
+
+
+#endif // VCHI_COMMON_H_
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchi/vchi_mh.h
@@ -0,0 +1,42 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHI_MH_H_
+#define VCHI_MH_H_
+
+#include <linux/types.h>
+
+typedef int32_t VCHI_MEM_HANDLE_T;
+#define VCHI_MEM_HANDLE_INVALID 0
+
+#endif
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq.h
@@ -0,0 +1,40 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHIQ_VCHIQ_H
+#define VCHIQ_VCHIQ_H
+
+#include "vchiq_if.h"
+#include "vchiq_util.h"
+
+#endif
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_2835.h
@@ -0,0 +1,42 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHIQ_2835_H
+#define VCHIQ_2835_H
+
+#include "vchiq_pagelist.h"
+
+#define VCHIQ_PLATFORM_FRAGMENTS_OFFSET_IDX 0
+#define VCHIQ_PLATFORM_FRAGMENTS_COUNT_IDX  1
+
+#endif /* VCHIQ_2835_H */
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_2835_arm.c
@@ -0,0 +1,561 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#include <linux/kernel.h>
+#include <linux/types.h>
+#include <linux/errno.h>
+#include <linux/interrupt.h>
+#include <linux/irq.h>
+#include <linux/pagemap.h>
+#include <linux/dma-mapping.h>
+#include <linux/version.h>
+#include <linux/io.h>
+#include <linux/uaccess.h>
+#include <asm/pgtable.h>
+
+#include <mach/irqs.h>
+
+#include <mach/platform.h>
+#include <mach/vcio.h>
+
+#define TOTAL_SLOTS (VCHIQ_SLOT_ZERO_SLOTS + 2 * 32)
+
+#define VCHIQ_DOORBELL_IRQ IRQ_ARM_DOORBELL_0
+#define VCHIQ_ARM_ADDRESS(x) ((void *)__virt_to_bus((unsigned)x))
+
+#include "vchiq_arm.h"
+#include "vchiq_2835.h"
+#include "vchiq_connected.h"
+
+#define MAX_FRAGMENTS (VCHIQ_NUM_CURRENT_BULKS * 2)
+
+typedef struct vchiq_2835_state_struct {
+   int inited;
+   VCHIQ_ARM_STATE_T arm_state;
+} VCHIQ_2835_ARM_STATE_T;
+
+static char *g_slot_mem;
+static int g_slot_mem_size;
+dma_addr_t g_slot_phys;
+static FRAGMENTS_T *g_fragments_base;
+static FRAGMENTS_T *g_free_fragments;
+struct semaphore g_free_fragments_sema;
+
+extern int vchiq_arm_log_level;
+
+static DEFINE_SEMAPHORE(g_free_fragments_mutex);
+
+static irqreturn_t
+vchiq_doorbell_irq(int irq, void *dev_id);
+
+static int
+create_pagelist(char __user *buf, size_t count, unsigned short type,
+                struct task_struct *task, PAGELIST_T ** ppagelist);
+
+static void
+free_pagelist(PAGELIST_T *pagelist, int actual);
+
+int __init
+vchiq_platform_init(VCHIQ_STATE_T *state)
+{
+	VCHIQ_SLOT_ZERO_T *vchiq_slot_zero;
+	int frag_mem_size;
+	int err;
+	int i;
+
+	/* Allocate space for the channels in coherent memory */
+	g_slot_mem_size = PAGE_ALIGN(TOTAL_SLOTS * VCHIQ_SLOT_SIZE);
+	frag_mem_size = PAGE_ALIGN(sizeof(FRAGMENTS_T) * MAX_FRAGMENTS);
+
+	g_slot_mem = dma_alloc_coherent(NULL, g_slot_mem_size + frag_mem_size,
+		&g_slot_phys, GFP_ATOMIC);
+
+	if (!g_slot_mem) {
+		vchiq_log_error(vchiq_arm_log_level,
+			"Unable to allocate channel memory");
+		err = -ENOMEM;
+		goto failed_alloc;
+	}
+
+	WARN_ON(((int)g_slot_mem & (PAGE_SIZE - 1)) != 0);
+
+	vchiq_slot_zero = vchiq_init_slots(g_slot_mem, g_slot_mem_size);
+	if (!vchiq_slot_zero) {
+		err = -EINVAL;
+		goto failed_init_slots;
+	}
+
+	vchiq_slot_zero->platform_data[VCHIQ_PLATFORM_FRAGMENTS_OFFSET_IDX] =
+		(int)g_slot_phys + g_slot_mem_size;
+	vchiq_slot_zero->platform_data[VCHIQ_PLATFORM_FRAGMENTS_COUNT_IDX] =
+		MAX_FRAGMENTS;
+
+	g_fragments_base = (FRAGMENTS_T *)(g_slot_mem + g_slot_mem_size);
+	g_slot_mem_size += frag_mem_size;
+
+	g_free_fragments = g_fragments_base;
+	for (i = 0; i < (MAX_FRAGMENTS - 1); i++) {
+		*(FRAGMENTS_T **)&g_fragments_base[i] =
+			&g_fragments_base[i + 1];
+	}
+	*(FRAGMENTS_T **)&g_fragments_base[i] = NULL;
+	sema_init(&g_free_fragments_sema, MAX_FRAGMENTS);
+
+	if (vchiq_init_state(state, vchiq_slot_zero, 0/*slave*/) !=
+		VCHIQ_SUCCESS) {
+		err = -EINVAL;
+		goto failed_vchiq_init;
+	}
+
+	err = request_irq(VCHIQ_DOORBELL_IRQ, vchiq_doorbell_irq,
+		IRQF_IRQPOLL, "VCHIQ doorbell",
+		state);
+	if (err < 0) {
+		vchiq_log_error(vchiq_arm_log_level, "%s: failed to register "
+			"irq=%d err=%d", __func__,
+			VCHIQ_DOORBELL_IRQ, err);
+		goto failed_request_irq;
+	}
+
+	/* Send the base address of the slots to VideoCore */
+
+	dsb(); /* Ensure all writes have completed */
+
+	bcm_mailbox_write(MBOX_CHAN_VCHIQ, (unsigned int)g_slot_phys);
+
+	vchiq_log_info(vchiq_arm_log_level,
+		"vchiq_init - done (slots %x, phys %x)",
+		(unsigned int)vchiq_slot_zero, g_slot_phys);
+
+   vchiq_call_connected_callbacks();
+
+   return 0;
+
+failed_request_irq:
+failed_vchiq_init:
+failed_init_slots:
+   dma_free_coherent(NULL, g_slot_mem_size, g_slot_mem, g_slot_phys);
+
+failed_alloc:
+   return err;
+}
+
+void __exit
+vchiq_platform_exit(VCHIQ_STATE_T *state)
+{
+   free_irq(VCHIQ_DOORBELL_IRQ, state);
+   dma_free_coherent(NULL, g_slot_mem_size,
+                     g_slot_mem, g_slot_phys);
+}
+
+
+VCHIQ_STATUS_T
+vchiq_platform_init_state(VCHIQ_STATE_T *state)
+{
+   VCHIQ_STATUS_T status = VCHIQ_SUCCESS;
+   state->platform_state = kzalloc(sizeof(VCHIQ_2835_ARM_STATE_T), GFP_KERNEL);
+   ((VCHIQ_2835_ARM_STATE_T*)state->platform_state)->inited = 1;
+   status = vchiq_arm_init_state(state, &((VCHIQ_2835_ARM_STATE_T*)state->platform_state)->arm_state);
+   if(status != VCHIQ_SUCCESS)
+   {
+      ((VCHIQ_2835_ARM_STATE_T*)state->platform_state)->inited = 0;
+   }
+   return status;
+}
+
+VCHIQ_ARM_STATE_T*
+vchiq_platform_get_arm_state(VCHIQ_STATE_T *state)
+{
+   if(!((VCHIQ_2835_ARM_STATE_T*)state->platform_state)->inited)
+   {
+      BUG();
+   }
+   return &((VCHIQ_2835_ARM_STATE_T*)state->platform_state)->arm_state;
+}
+
+void
+remote_event_signal(REMOTE_EVENT_T *event)
+{
+	wmb();
+
+	event->fired = 1;
+
+	dsb();         /* data barrier operation */
+
+	if (event->armed) {
+		/* trigger vc interrupt */
+
+		writel(0, __io_address(ARM_0_BELL2));
+	}
+}
+
+int
+vchiq_copy_from_user(void *dst, const void *src, int size)
+{
+	if ((uint32_t)src < TASK_SIZE) {
+		return copy_from_user(dst, src, size);
+	} else {
+		memcpy(dst, src, size);
+		return 0;
+	}
+}
+
+VCHIQ_STATUS_T
+vchiq_prepare_bulk_data(VCHIQ_BULK_T *bulk, VCHI_MEM_HANDLE_T memhandle,
+	void *offset, int size, int dir)
+{
+	PAGELIST_T *pagelist;
+	int ret;
+
+	WARN_ON(memhandle != VCHI_MEM_HANDLE_INVALID);
+
+	ret = create_pagelist((char __user *)offset, size,
+			(dir == VCHIQ_BULK_RECEIVE)
+			? PAGELIST_READ
+			: PAGELIST_WRITE,
+			current,
+			&pagelist);
+	if (ret != 0)
+		return VCHIQ_ERROR;
+
+	bulk->handle = memhandle;
+	bulk->data = VCHIQ_ARM_ADDRESS(pagelist);
+
+	/* Store the pagelist address in remote_data, which isn't used by the
+	   slave. */
+	bulk->remote_data = pagelist;
+
+	return VCHIQ_SUCCESS;
+}
+
+void
+vchiq_complete_bulk(VCHIQ_BULK_T *bulk)
+{
+	if (bulk && bulk->remote_data && bulk->actual)
+		free_pagelist((PAGELIST_T *)bulk->remote_data, bulk->actual);
+}
+
+void
+vchiq_transfer_bulk(VCHIQ_BULK_T *bulk)
+{
+	/*
+	 * This should only be called on the master (VideoCore) side, but
+	 * provide an implementation to avoid the need for ifdefery.
+	 */
+	BUG();
+}
+
+void
+vchiq_dump_platform_state(void *dump_context)
+{
+	char buf[80];
+	int len;
+	len = snprintf(buf, sizeof(buf),
+		"  Platform: 2835 (VC master)");
+	vchiq_dump(dump_context, buf, len + 1);
+}
+
+VCHIQ_STATUS_T
+vchiq_platform_suspend(VCHIQ_STATE_T *state)
+{
+   return VCHIQ_ERROR;
+}
+
+VCHIQ_STATUS_T
+vchiq_platform_resume(VCHIQ_STATE_T *state)
+{
+   return VCHIQ_SUCCESS;
+}
+
+void
+vchiq_platform_paused(VCHIQ_STATE_T *state)
+{
+}
+
+void
+vchiq_platform_resumed(VCHIQ_STATE_T *state)
+{
+}
+
+int
+vchiq_platform_videocore_wanted(VCHIQ_STATE_T* state)
+{
+   return 1; // autosuspend not supported - videocore always wanted
+}
+
+int
+vchiq_platform_use_suspend_timer(void)
+{
+   return 0;
+}
+void
+vchiq_dump_platform_use_state(VCHIQ_STATE_T *state)
+{
+	vchiq_log_info((vchiq_arm_log_level>=VCHIQ_LOG_INFO),"Suspend timer not in use");
+}
+void
+vchiq_platform_handle_timeout(VCHIQ_STATE_T *state)
+{
+	(void)state;
+}
+/*
+ * Local functions
+ */
+
+static irqreturn_t
+vchiq_doorbell_irq(int irq, void *dev_id)
+{
+	VCHIQ_STATE_T *state = dev_id;
+	irqreturn_t ret = IRQ_NONE;
+	unsigned int status;
+
+	/* Read (and clear) the doorbell */
+	status = readl(__io_address(ARM_0_BELL0));
+
+	if (status & 0x4) {  /* Was the doorbell rung? */
+		remote_event_pollall(state);
+		ret = IRQ_HANDLED;
+	}
+
+	return ret;
+}
+
+/* There is a potential problem with partial cache lines (pages?)
+** at the ends of the block when reading. If the CPU accessed anything in
+** the same line (page?) then it may have pulled old data into the cache,
+** obscuring the new data underneath. We can solve this by transferring the
+** partial cache lines separately, and allowing the ARM to copy into the
+** cached area.
+
+** N.B. This implementation plays slightly fast and loose with the Linux
+** driver programming rules, e.g. its use of __virt_to_bus instead of
+** dma_map_single, but it isn't a multi-platform driver and it benefits
+** from increased speed as a result.
+*/
+
+static int
+create_pagelist(char __user *buf, size_t count, unsigned short type,
+	struct task_struct *task, PAGELIST_T ** ppagelist)
+{
+	PAGELIST_T *pagelist;
+	struct page **pages;
+	struct page *page;
+	unsigned long *addrs;
+	unsigned int num_pages, offset, i;
+	char *addr, *base_addr, *next_addr;
+	int run, addridx, actual_pages;
+        unsigned long *need_release;
+
+	offset = (unsigned int)buf & (PAGE_SIZE - 1);
+	num_pages = (count + offset + PAGE_SIZE - 1) / PAGE_SIZE;
+
+	*ppagelist = NULL;
+
+	/* Allocate enough storage to hold the page pointers and the page
+	** list
+	*/
+	pagelist = kmalloc(sizeof(PAGELIST_T) +
+                           (num_pages * sizeof(unsigned long)) +
+                           sizeof(unsigned long) +
+                           (num_pages * sizeof(pages[0])),
+                           GFP_KERNEL);
+
+	vchiq_log_trace(vchiq_arm_log_level,
+		"create_pagelist - %x", (unsigned int)pagelist);
+	if (!pagelist)
+		return -ENOMEM;
+
+	addrs = pagelist->addrs;
+        need_release = (unsigned long *)(addrs + num_pages);
+	pages = (struct page **)(addrs + num_pages + 1);
+
+	if (is_vmalloc_addr(buf)) {
+		for (actual_pages = 0; actual_pages < num_pages; actual_pages++) {
+			pages[actual_pages] = vmalloc_to_page(buf + (actual_pages * PAGE_SIZE));
+		}
+                *need_release = 0; /* do not try and release vmalloc pages */
+	} else {
+		down_read(&task->mm->mmap_sem);
+		actual_pages = get_user_pages(task, task->mm,
+				          (unsigned long)buf & ~(PAGE_SIZE - 1),
+					  num_pages,
+					  (type == PAGELIST_READ) /*Write */ ,
+					  0 /*Force */ ,
+					  pages,
+					  NULL /*vmas */);
+		up_read(&task->mm->mmap_sem);
+
+		if (actual_pages != num_pages) {
+			vchiq_log_info(vchiq_arm_log_level,
+				       "create_pagelist - only %d/%d pages locked",
+				       actual_pages,
+				       num_pages);
+
+			/* This is probably due to the process being killed */
+			while (actual_pages > 0)
+			{
+				actual_pages--;
+				page_cache_release(pages[actual_pages]);
+			}
+			kfree(pagelist);
+			if (actual_pages == 0)
+				actual_pages = -ENOMEM;
+			return actual_pages;
+		}
+                *need_release = 1; /* release user pages */
+	}
+
+	pagelist->length = count;
+	pagelist->type = type;
+	pagelist->offset = offset;
+
+	/* Group the pages into runs of contiguous pages */
+
+	base_addr = VCHIQ_ARM_ADDRESS(page_address(pages[0]));
+	next_addr = base_addr + PAGE_SIZE;
+	addridx = 0;
+	run = 0;
+
+	for (i = 1; i < num_pages; i++) {
+		addr = VCHIQ_ARM_ADDRESS(page_address(pages[i]));
+		if ((addr == next_addr) && (run < (PAGE_SIZE - 1))) {
+			next_addr += PAGE_SIZE;
+			run++;
+		} else {
+			addrs[addridx] = (unsigned long)base_addr + run;
+			addridx++;
+			base_addr = addr;
+			next_addr = addr + PAGE_SIZE;
+			run = 0;
+		}
+	}
+
+	addrs[addridx] = (unsigned long)base_addr + run;
+	addridx++;
+
+	/* Partial cache lines (fragments) require special measures */
+	if ((type == PAGELIST_READ) &&
+		((pagelist->offset & (CACHE_LINE_SIZE - 1)) ||
+		((pagelist->offset + pagelist->length) &
+		(CACHE_LINE_SIZE - 1)))) {
+		FRAGMENTS_T *fragments;
+
+		if (down_interruptible(&g_free_fragments_sema) != 0) {
+			kfree(pagelist);
+			return -EINTR;
+		}
+
+		WARN_ON(g_free_fragments == NULL);
+
+		down(&g_free_fragments_mutex);
+		fragments = (FRAGMENTS_T *) g_free_fragments;
+		WARN_ON(fragments == NULL);
+		g_free_fragments = *(FRAGMENTS_T **) g_free_fragments;
+		up(&g_free_fragments_mutex);
+		pagelist->type =
+			 PAGELIST_READ_WITH_FRAGMENTS + (fragments -
+							 g_fragments_base);
+	}
+
+	for (page = virt_to_page(pagelist);
+		page <= virt_to_page(addrs + num_pages - 1); page++) {
+		flush_dcache_page(page);
+	}
+
+	*ppagelist = pagelist;
+
+	return 0;
+}
+
+static void
+free_pagelist(PAGELIST_T *pagelist, int actual)
+{
+        unsigned long *need_release;
+	struct page **pages;
+	unsigned int num_pages, i;
+
+	vchiq_log_trace(vchiq_arm_log_level,
+		"free_pagelist - %x, %d", (unsigned int)pagelist, actual);
+
+	num_pages =
+		(pagelist->length + pagelist->offset + PAGE_SIZE - 1) /
+		PAGE_SIZE;
+
+        need_release = (unsigned long *)(pagelist->addrs + num_pages);
+	pages = (struct page **)(pagelist->addrs + num_pages + 1);
+
+	/* Deal with any partial cache lines (fragments) */
+	if (pagelist->type >= PAGELIST_READ_WITH_FRAGMENTS) {
+		FRAGMENTS_T *fragments = g_fragments_base +
+			(pagelist->type - PAGELIST_READ_WITH_FRAGMENTS);
+		int head_bytes, tail_bytes;
+		head_bytes = (CACHE_LINE_SIZE - pagelist->offset) &
+			(CACHE_LINE_SIZE - 1);
+		tail_bytes = (pagelist->offset + actual) &
+			(CACHE_LINE_SIZE - 1);
+
+		if ((actual >= 0) && (head_bytes != 0)) {
+			if (head_bytes > actual)
+				head_bytes = actual;
+
+			memcpy((char *)page_address(pages[0]) +
+				pagelist->offset,
+				fragments->headbuf,
+				head_bytes);
+		}
+		if ((actual >= 0) && (head_bytes < actual) &&
+			(tail_bytes != 0)) {
+			memcpy((char *)page_address(pages[num_pages - 1]) +
+				((pagelist->offset + actual) &
+				(PAGE_SIZE - 1) & ~(CACHE_LINE_SIZE - 1)),
+				fragments->tailbuf, tail_bytes);
+		}
+
+		down(&g_free_fragments_mutex);
+		*(FRAGMENTS_T **) fragments = g_free_fragments;
+		g_free_fragments = fragments;
+		up(&g_free_fragments_mutex);
+		up(&g_free_fragments_sema);
+	}
+
+        if (*need_release) {
+		for (i = 0; i < num_pages; i++) {
+			if (pagelist->type != PAGELIST_WRITE)
+				set_page_dirty(pages[i]);
+
+			page_cache_release(pages[i]);
+		}
+        }
+
+	kfree(pagelist);
+}
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_arm.c
@@ -0,0 +1,2883 @@
+/**
+ * Copyright (c) 2014 Raspberry Pi (Trading) Ltd. All rights reserved.
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/types.h>
+#include <linux/errno.h>
+#include <linux/cdev.h>
+#include <linux/fs.h>
+#include <linux/device.h>
+#include <linux/mm.h>
+#include <linux/highmem.h>
+#include <linux/pagemap.h>
+#include <linux/bug.h>
+#include <linux/semaphore.h>
+#include <linux/list.h>
+
+#include "vchiq_core.h"
+#include "vchiq_ioctl.h"
+#include "vchiq_arm.h"
+#include "vchiq_debugfs.h"
+
+#define DEVICE_NAME "vchiq"
+
+/* Override the default prefix, which would be vchiq_arm (from the filename) */
+#undef MODULE_PARAM_PREFIX
+#define MODULE_PARAM_PREFIX DEVICE_NAME "."
+
+#define VCHIQ_MINOR 0
+
+/* Some per-instance constants */
+#define MAX_COMPLETIONS 16
+#define MAX_SERVICES 64
+#define MAX_ELEMENTS 8
+#define MSG_QUEUE_SIZE 64
+
+#define KEEPALIVE_VER 1
+#define KEEPALIVE_VER_MIN KEEPALIVE_VER
+
+/* Run time control of log level, based on KERN_XXX level. */
+int vchiq_arm_log_level = VCHIQ_LOG_DEFAULT;
+int vchiq_susp_log_level = VCHIQ_LOG_ERROR;
+
+#define SUSPEND_TIMER_TIMEOUT_MS 100
+#define SUSPEND_RETRY_TIMER_TIMEOUT_MS 1000
+
+#define VC_SUSPEND_NUM_OFFSET 3 /* number of values before idle which are -ve */
+static const char *const suspend_state_names[] = {
+	"VC_SUSPEND_FORCE_CANCELED",
+	"VC_SUSPEND_REJECTED",
+	"VC_SUSPEND_FAILED",
+	"VC_SUSPEND_IDLE",
+	"VC_SUSPEND_REQUESTED",
+	"VC_SUSPEND_IN_PROGRESS",
+	"VC_SUSPEND_SUSPENDED"
+};
+#define VC_RESUME_NUM_OFFSET 1 /* number of values before idle which are -ve */
+static const char *const resume_state_names[] = {
+	"VC_RESUME_FAILED",
+	"VC_RESUME_IDLE",
+	"VC_RESUME_REQUESTED",
+	"VC_RESUME_IN_PROGRESS",
+	"VC_RESUME_RESUMED"
+};
+/* The number of times we allow force suspend to timeout before actually
+** _forcing_ suspend.  This is to cater for SW which fails to release vchiq
+** correctly - we don't want to prevent ARM suspend indefinitely in this case.
+*/
+#define FORCE_SUSPEND_FAIL_MAX 8
+
+/* The time in ms allowed for videocore to go idle when force suspend has been
+ * requested */
+#define FORCE_SUSPEND_TIMEOUT_MS 200
+
+
+static void suspend_timer_callback(unsigned long context);
+
+
+typedef struct user_service_struct {
+	VCHIQ_SERVICE_T *service;
+	void *userdata;
+	VCHIQ_INSTANCE_T instance;
+	char is_vchi;
+	char dequeue_pending;
+	char close_pending;
+	int message_available_pos;
+	int msg_insert;
+	int msg_remove;
+	struct semaphore insert_event;
+	struct semaphore remove_event;
+	struct semaphore close_event;
+	VCHIQ_HEADER_T * msg_queue[MSG_QUEUE_SIZE];
+} USER_SERVICE_T;
+
+struct bulk_waiter_node {
+	struct bulk_waiter bulk_waiter;
+	int pid;
+	struct list_head list;
+};
+
+struct vchiq_instance_struct {
+	VCHIQ_STATE_T *state;
+	VCHIQ_COMPLETION_DATA_T completions[MAX_COMPLETIONS];
+	int completion_insert;
+	int completion_remove;
+	struct semaphore insert_event;
+	struct semaphore remove_event;
+	struct mutex completion_mutex;
+
+	int connected;
+	int closing;
+	int pid;
+	int mark;
+	int use_close_delivered;
+	int trace;
+
+	struct list_head bulk_waiter_list;
+	struct mutex bulk_waiter_list_mutex;
+
+	VCHIQ_DEBUGFS_NODE_T debugfs_node;
+};
+
+typedef struct dump_context_struct {
+	char __user *buf;
+	size_t actual;
+	size_t space;
+	loff_t offset;
+} DUMP_CONTEXT_T;
+
+static struct cdev    vchiq_cdev;
+static dev_t          vchiq_devid;
+static VCHIQ_STATE_T g_state;
+static struct class  *vchiq_class;
+static struct device *vchiq_dev;
+static DEFINE_SPINLOCK(msg_queue_spinlock);
+
+static const char *const ioctl_names[] = {
+	"CONNECT",
+	"SHUTDOWN",
+	"CREATE_SERVICE",
+	"REMOVE_SERVICE",
+	"QUEUE_MESSAGE",
+	"QUEUE_BULK_TRANSMIT",
+	"QUEUE_BULK_RECEIVE",
+	"AWAIT_COMPLETION",
+	"DEQUEUE_MESSAGE",
+	"GET_CLIENT_ID",
+	"GET_CONFIG",
+	"CLOSE_SERVICE",
+	"USE_SERVICE",
+	"RELEASE_SERVICE",
+	"SET_SERVICE_OPTION",
+	"DUMP_PHYS_MEM",
+	"LIB_VERSION",
+	"CLOSE_DELIVERED"
+};
+
+vchiq_static_assert((sizeof(ioctl_names)/sizeof(ioctl_names[0])) ==
+	(VCHIQ_IOC_MAX + 1));
+
+static void
+dump_phys_mem(void *virt_addr, uint32_t num_bytes);
+
+/****************************************************************************
+*
+*   add_completion
+*
+***************************************************************************/
+
+static VCHIQ_STATUS_T
+add_completion(VCHIQ_INSTANCE_T instance, VCHIQ_REASON_T reason,
+	VCHIQ_HEADER_T *header, USER_SERVICE_T *user_service,
+	void *bulk_userdata)
+{
+	VCHIQ_COMPLETION_DATA_T *completion;
+	DEBUG_INITIALISE(g_state.local)
+
+	while (instance->completion_insert ==
+		(instance->completion_remove + MAX_COMPLETIONS)) {
+		/* Out of space - wait for the client */
+		DEBUG_TRACE(SERVICE_CALLBACK_LINE);
+		vchiq_log_trace(vchiq_arm_log_level,
+			"add_completion - completion queue full");
+		DEBUG_COUNT(COMPLETION_QUEUE_FULL_COUNT);
+		if (down_interruptible(&instance->remove_event) != 0) {
+			vchiq_log_info(vchiq_arm_log_level,
+				"service_callback interrupted");
+			return VCHIQ_RETRY;
+		} else if (instance->closing) {
+			vchiq_log_info(vchiq_arm_log_level,
+				"service_callback closing");
+			return VCHIQ_ERROR;
+		}
+		DEBUG_TRACE(SERVICE_CALLBACK_LINE);
+	}
+
+	completion =
+		 &instance->completions[instance->completion_insert &
+		 (MAX_COMPLETIONS - 1)];
+
+	completion->header = header;
+	completion->reason = reason;
+	/* N.B. service_userdata is updated while processing AWAIT_COMPLETION */
+	completion->service_userdata = user_service->service;
+	completion->bulk_userdata = bulk_userdata;
+
+	if (reason == VCHIQ_SERVICE_CLOSED) {
+		/* Take an extra reference, to be held until
+		   this CLOSED notification is delivered. */
+		lock_service(user_service->service);
+		if (instance->use_close_delivered)
+			user_service->close_pending = 1;
+	}
+
+	/* A write barrier is needed here to ensure that the entire completion
+		record is written out before the insert point. */
+	wmb();
+
+	if (reason == VCHIQ_MESSAGE_AVAILABLE)
+		user_service->message_available_pos =
+			instance->completion_insert;
+	instance->completion_insert++;
+
+	up(&instance->insert_event);
+
+	return VCHIQ_SUCCESS;
+}
+
+/****************************************************************************
+*
+*   service_callback
+*
+***************************************************************************/
+
+static VCHIQ_STATUS_T
+service_callback(VCHIQ_REASON_T reason, VCHIQ_HEADER_T *header,
+	VCHIQ_SERVICE_HANDLE_T handle, void *bulk_userdata)
+{
+	/* How do we ensure the callback goes to the right client?
+	** The service_user data points to a USER_SERVICE_T record containing
+	** the original callback and the user state structure, which contains a
+	** circular buffer for completion records.
+	*/
+	USER_SERVICE_T *user_service;
+	VCHIQ_SERVICE_T *service;
+	VCHIQ_INSTANCE_T instance;
+	DEBUG_INITIALISE(g_state.local)
+
+	DEBUG_TRACE(SERVICE_CALLBACK_LINE);
+
+	service = handle_to_service(handle);
+	BUG_ON(!service);
+	user_service = (USER_SERVICE_T *)service->base.userdata;
+	instance = user_service->instance;
+
+	if (!instance || instance->closing)
+		return VCHIQ_SUCCESS;
+
+	vchiq_log_trace(vchiq_arm_log_level,
+		"service_callback - service %lx(%d,%p), reason %d, header %lx, "
+		"instance %lx, bulk_userdata %lx",
+		(unsigned long)user_service,
+		service->localport, user_service->userdata,
+		reason, (unsigned long)header,
+		(unsigned long)instance, (unsigned long)bulk_userdata);
+
+	if (header && user_service->is_vchi) {
+		spin_lock(&msg_queue_spinlock);
+		while (user_service->msg_insert ==
+			(user_service->msg_remove + MSG_QUEUE_SIZE)) {
+			spin_unlock(&msg_queue_spinlock);
+			DEBUG_TRACE(SERVICE_CALLBACK_LINE);
+			DEBUG_COUNT(MSG_QUEUE_FULL_COUNT);
+			vchiq_log_trace(vchiq_arm_log_level,
+				"service_callback - msg queue full");
+			/* If there is no MESSAGE_AVAILABLE in the completion
+			** queue, add one
+			*/
+			if ((user_service->message_available_pos -
+				instance->completion_remove) < 0) {
+				VCHIQ_STATUS_T status;
+				vchiq_log_info(vchiq_arm_log_level,
+					"Inserting extra MESSAGE_AVAILABLE");
+				DEBUG_TRACE(SERVICE_CALLBACK_LINE);
+				status = add_completion(instance, reason,
+					NULL, user_service, bulk_userdata);
+				if (status != VCHIQ_SUCCESS) {
+					DEBUG_TRACE(SERVICE_CALLBACK_LINE);
+					return status;
+				}
+			}
+
+			DEBUG_TRACE(SERVICE_CALLBACK_LINE);
+			if (down_interruptible(&user_service->remove_event)
+				!= 0) {
+				vchiq_log_info(vchiq_arm_log_level,
+					"service_callback interrupted");
+				DEBUG_TRACE(SERVICE_CALLBACK_LINE);
+				return VCHIQ_RETRY;
+			} else if (instance->closing) {
+				vchiq_log_info(vchiq_arm_log_level,
+					"service_callback closing");
+				DEBUG_TRACE(SERVICE_CALLBACK_LINE);
+				return VCHIQ_ERROR;
+			}
+			DEBUG_TRACE(SERVICE_CALLBACK_LINE);
+			spin_lock(&msg_queue_spinlock);
+		}
+
+		user_service->msg_queue[user_service->msg_insert &
+			(MSG_QUEUE_SIZE - 1)] = header;
+		user_service->msg_insert++;
+		spin_unlock(&msg_queue_spinlock);
+
+		up(&user_service->insert_event);
+
+		/* If there is a thread waiting in DEQUEUE_MESSAGE, or if
+		** there is a MESSAGE_AVAILABLE in the completion queue then
+		** bypass the completion queue.
+		*/
+		if (((user_service->message_available_pos -
+			instance->completion_remove) >= 0) ||
+			user_service->dequeue_pending) {
+			DEBUG_TRACE(SERVICE_CALLBACK_LINE);
+			user_service->dequeue_pending = 0;
+			return VCHIQ_SUCCESS;
+		}
+
+		header = NULL;
+	}
+	DEBUG_TRACE(SERVICE_CALLBACK_LINE);
+
+	return add_completion(instance, reason, header, user_service,
+		bulk_userdata);
+}
+
+/****************************************************************************
+*
+*   user_service_free
+*
+***************************************************************************/
+static void
+user_service_free(void *userdata)
+{
+	kfree(userdata);
+}
+
+/****************************************************************************
+*
+*   close_delivered
+*
+***************************************************************************/
+static void close_delivered(USER_SERVICE_T *user_service)
+{
+	vchiq_log_info(vchiq_arm_log_level,
+		"close_delivered(handle=%x)",
+		user_service->service->handle);
+
+	if (user_service->close_pending) {
+		/* Allow the underlying service to be culled */
+		unlock_service(user_service->service);
+
+		/* Wake the user-thread blocked in close_ or remove_service */
+		up(&user_service->close_event);
+
+		user_service->close_pending = 0;
+	}
+}
+
+/****************************************************************************
+*
+*   vchiq_ioctl
+*
+***************************************************************************/
+static long
+vchiq_ioctl(struct file *file, unsigned int cmd, unsigned long arg)
+{
+	VCHIQ_INSTANCE_T instance = file->private_data;
+	VCHIQ_STATUS_T status = VCHIQ_SUCCESS;
+	VCHIQ_SERVICE_T *service = NULL;
+	long ret = 0;
+	int i, rc;
+	DEBUG_INITIALISE(g_state.local)
+
+	vchiq_log_trace(vchiq_arm_log_level,
+		 "vchiq_ioctl - instance %x, cmd %s, arg %lx",
+		(unsigned int)instance,
+		((_IOC_TYPE(cmd) == VCHIQ_IOC_MAGIC) &&
+		(_IOC_NR(cmd) <= VCHIQ_IOC_MAX)) ?
+		ioctl_names[_IOC_NR(cmd)] : "<invalid>", arg);
+
+	switch (cmd) {
+	case VCHIQ_IOC_SHUTDOWN:
+		if (!instance->connected)
+			break;
+
+		/* Remove all services */
+		i = 0;
+		while ((service = next_service_by_instance(instance->state,
+			instance, &i)) != NULL) {
+			status = vchiq_remove_service(service->handle);
+			unlock_service(service);
+			if (status != VCHIQ_SUCCESS)
+				break;
+		}
+		service = NULL;
+
+		if (status == VCHIQ_SUCCESS) {
+			/* Wake the completion thread and ask it to exit */
+			instance->closing = 1;
+			up(&instance->insert_event);
+		}
+
+		break;
+
+	case VCHIQ_IOC_CONNECT:
+		if (instance->connected) {
+			ret = -EINVAL;
+			break;
+		}
+		rc = mutex_lock_interruptible(&instance->state->mutex);
+		if (rc != 0) {
+			vchiq_log_error(vchiq_arm_log_level,
+				"vchiq: connect: could not lock mutex for "
+				"state %d: %d",
+				instance->state->id, rc);
+			ret = -EINTR;
+			break;
+		}
+		status = vchiq_connect_internal(instance->state, instance);
+		mutex_unlock(&instance->state->mutex);
+
+		if (status == VCHIQ_SUCCESS)
+			instance->connected = 1;
+		else
+			vchiq_log_error(vchiq_arm_log_level,
+				"vchiq: could not connect: %d", status);
+		break;
+
+	case VCHIQ_IOC_CREATE_SERVICE: {
+		VCHIQ_CREATE_SERVICE_T args;
+		USER_SERVICE_T *user_service = NULL;
+		void *userdata;
+		int srvstate;
+
+		if (copy_from_user
+			 (&args, (const void __user *)arg,
+			  sizeof(args)) != 0) {
+			ret = -EFAULT;
+			break;
+		}
+
+		user_service = kmalloc(sizeof(USER_SERVICE_T), GFP_KERNEL);
+		if (!user_service) {
+			ret = -ENOMEM;
+			break;
+		}
+
+		if (args.is_open) {
+			if (!instance->connected) {
+				ret = -ENOTCONN;
+				kfree(user_service);
+				break;
+			}
+			srvstate = VCHIQ_SRVSTATE_OPENING;
+		} else {
+			srvstate =
+				 instance->connected ?
+				 VCHIQ_SRVSTATE_LISTENING :
+				 VCHIQ_SRVSTATE_HIDDEN;
+		}
+
+		userdata = args.params.userdata;
+		args.params.callback = service_callback;
+		args.params.userdata = user_service;
+		service = vchiq_add_service_internal(
+				instance->state,
+				&args.params, srvstate,
+				instance, user_service_free);
+
+		if (service != NULL) {
+			user_service->service = service;
+			user_service->userdata = userdata;
+			user_service->instance = instance;
+			user_service->is_vchi = (args.is_vchi != 0);
+			user_service->dequeue_pending = 0;
+			user_service->close_pending = 0;
+			user_service->message_available_pos =
+				instance->completion_remove - 1;
+			user_service->msg_insert = 0;
+			user_service->msg_remove = 0;
+			sema_init(&user_service->insert_event, 0);
+			sema_init(&user_service->remove_event, 0);
+			sema_init(&user_service->close_event, 0);
+
+			if (args.is_open) {
+				status = vchiq_open_service_internal
+					(service, instance->pid);
+				if (status != VCHIQ_SUCCESS) {
+					vchiq_remove_service(service->handle);
+					service = NULL;
+					ret = (status == VCHIQ_RETRY) ?
+						-EINTR : -EIO;
+					break;
+				}
+			}
+
+			if (copy_to_user((void __user *)
+				&(((VCHIQ_CREATE_SERVICE_T __user *)
+					arg)->handle),
+				(const void *)&service->handle,
+				sizeof(service->handle)) != 0) {
+				ret = -EFAULT;
+				vchiq_remove_service(service->handle);
+			}
+
+			service = NULL;
+		} else {
+			ret = -EEXIST;
+			kfree(user_service);
+		}
+	} break;
+
+	case VCHIQ_IOC_CLOSE_SERVICE: {
+		VCHIQ_SERVICE_HANDLE_T handle = (VCHIQ_SERVICE_HANDLE_T)arg;
+
+		service = find_service_for_instance(instance, handle);
+		if (service != NULL) {
+			USER_SERVICE_T *user_service =
+				(USER_SERVICE_T *)service->base.userdata;
+			/* close_pending is false on first entry, and when the
+                           wait in vchiq_close_service has been interrupted. */
+			if (!user_service->close_pending) {
+				status = vchiq_close_service(service->handle);
+				if (status != VCHIQ_SUCCESS)
+					break;
+			}
+
+			/* close_pending is true once the underlying service
+			   has been closed until the client library calls the
+			   CLOSE_DELIVERED ioctl, signalling close_event. */
+			if (user_service->close_pending &&
+				down_interruptible(&user_service->close_event))
+				status = VCHIQ_RETRY;
+		}
+		else
+			ret = -EINVAL;
+	} break;
+
+	case VCHIQ_IOC_REMOVE_SERVICE: {
+		VCHIQ_SERVICE_HANDLE_T handle = (VCHIQ_SERVICE_HANDLE_T)arg;
+
+		service = find_service_for_instance(instance, handle);
+		if (service != NULL) {
+			USER_SERVICE_T *user_service =
+				(USER_SERVICE_T *)service->base.userdata;
+			/* close_pending is false on first entry, and when the
+                           wait in vchiq_close_service has been interrupted. */
+			if (!user_service->close_pending) {
+				status = vchiq_remove_service(service->handle);
+				if (status != VCHIQ_SUCCESS)
+					break;
+			}
+
+			/* close_pending is true once the underlying service
+			   has been closed until the client library calls the
+			   CLOSE_DELIVERED ioctl, signalling close_event. */
+			if (user_service->close_pending &&
+				down_interruptible(&user_service->close_event))
+				status = VCHIQ_RETRY;
+		}
+		else
+			ret = -EINVAL;
+	} break;
+
+	case VCHIQ_IOC_USE_SERVICE:
+	case VCHIQ_IOC_RELEASE_SERVICE:	{
+		VCHIQ_SERVICE_HANDLE_T handle = (VCHIQ_SERVICE_HANDLE_T)arg;
+
+		service = find_service_for_instance(instance, handle);
+		if (service != NULL) {
+			status = (cmd == VCHIQ_IOC_USE_SERVICE)	?
+				vchiq_use_service_internal(service) :
+				vchiq_release_service_internal(service);
+			if (status != VCHIQ_SUCCESS) {
+				vchiq_log_error(vchiq_susp_log_level,
+					"%s: cmd %s returned error %d for "
+					"service %c%c%c%c:%03d",
+					__func__,
+					(cmd == VCHIQ_IOC_USE_SERVICE) ?
+						"VCHIQ_IOC_USE_SERVICE" :
+						"VCHIQ_IOC_RELEASE_SERVICE",
+					status,
+					VCHIQ_FOURCC_AS_4CHARS(
+						service->base.fourcc),
+					service->client_id);
+				ret = -EINVAL;
+			}
+		} else
+			ret = -EINVAL;
+	} break;
+
+	case VCHIQ_IOC_QUEUE_MESSAGE: {
+		VCHIQ_QUEUE_MESSAGE_T args;
+		if (copy_from_user
+			 (&args, (const void __user *)arg,
+			  sizeof(args)) != 0) {
+			ret = -EFAULT;
+			break;
+		}
+
+		service = find_service_for_instance(instance, args.handle);
+
+		if ((service != NULL) && (args.count <= MAX_ELEMENTS)) {
+			/* Copy elements into kernel space */
+			VCHIQ_ELEMENT_T elements[MAX_ELEMENTS];
+			if (copy_from_user(elements, args.elements,
+				args.count * sizeof(VCHIQ_ELEMENT_T)) == 0)
+				status = vchiq_queue_message
+					(args.handle,
+					elements, args.count);
+			else
+				ret = -EFAULT;
+		} else {
+			ret = -EINVAL;
+		}
+	} break;
+
+	case VCHIQ_IOC_QUEUE_BULK_TRANSMIT:
+	case VCHIQ_IOC_QUEUE_BULK_RECEIVE: {
+		VCHIQ_QUEUE_BULK_TRANSFER_T args;
+		struct bulk_waiter_node *waiter = NULL;
+		VCHIQ_BULK_DIR_T dir =
+			(cmd == VCHIQ_IOC_QUEUE_BULK_TRANSMIT) ?
+			VCHIQ_BULK_TRANSMIT : VCHIQ_BULK_RECEIVE;
+
+		if (copy_from_user
+			(&args, (const void __user *)arg,
+			sizeof(args)) != 0) {
+			ret = -EFAULT;
+			break;
+		}
+
+		service = find_service_for_instance(instance, args.handle);
+		if (!service) {
+			ret = -EINVAL;
+			break;
+		}
+
+		if (args.mode == VCHIQ_BULK_MODE_BLOCKING) {
+			waiter = kzalloc(sizeof(struct bulk_waiter_node),
+				GFP_KERNEL);
+			if (!waiter) {
+				ret = -ENOMEM;
+				break;
+			}
+			args.userdata = &waiter->bulk_waiter;
+		} else if (args.mode == VCHIQ_BULK_MODE_WAITING) {
+			struct list_head *pos;
+			mutex_lock(&instance->bulk_waiter_list_mutex);
+			list_for_each(pos, &instance->bulk_waiter_list) {
+				if (list_entry(pos, struct bulk_waiter_node,
+					list)->pid == current->pid) {
+					waiter = list_entry(pos,
+						struct bulk_waiter_node,
+						list);
+					list_del(pos);
+					break;
+				}
+
+			}
+			mutex_unlock(&instance->bulk_waiter_list_mutex);
+			if (!waiter) {
+				vchiq_log_error(vchiq_arm_log_level,
+					"no bulk_waiter found for pid %d",
+					current->pid);
+				ret = -ESRCH;
+				break;
+			}
+			vchiq_log_info(vchiq_arm_log_level,
+				"found bulk_waiter %x for pid %d",
+				(unsigned int)waiter, current->pid);
+			args.userdata = &waiter->bulk_waiter;
+		}
+		status = vchiq_bulk_transfer
+			(args.handle,
+			 VCHI_MEM_HANDLE_INVALID,
+			 args.data, args.size,
+			 args.userdata, args.mode,
+			 dir);
+		if (!waiter)
+			break;
+		if ((status != VCHIQ_RETRY) || fatal_signal_pending(current) ||
+			!waiter->bulk_waiter.bulk) {
+			if (waiter->bulk_waiter.bulk) {
+				/* Cancel the signal when the transfer
+				** completes. */
+				spin_lock(&bulk_waiter_spinlock);
+				waiter->bulk_waiter.bulk->userdata = NULL;
+				spin_unlock(&bulk_waiter_spinlock);
+			}
+			kfree(waiter);
+		} else {
+			const VCHIQ_BULK_MODE_T mode_waiting =
+				VCHIQ_BULK_MODE_WAITING;
+			waiter->pid = current->pid;
+			mutex_lock(&instance->bulk_waiter_list_mutex);
+			list_add(&waiter->list, &instance->bulk_waiter_list);
+			mutex_unlock(&instance->bulk_waiter_list_mutex);
+			vchiq_log_info(vchiq_arm_log_level,
+				"saved bulk_waiter %x for pid %d",
+				(unsigned int)waiter, current->pid);
+
+			if (copy_to_user((void __user *)
+				&(((VCHIQ_QUEUE_BULK_TRANSFER_T __user *)
+					arg)->mode),
+				(const void *)&mode_waiting,
+				sizeof(mode_waiting)) != 0)
+				ret = -EFAULT;
+		}
+	} break;
+
+	case VCHIQ_IOC_AWAIT_COMPLETION: {
+		VCHIQ_AWAIT_COMPLETION_T args;
+
+		DEBUG_TRACE(AWAIT_COMPLETION_LINE);
+		if (!instance->connected) {
+			ret = -ENOTCONN;
+			break;
+		}
+
+		if (copy_from_user(&args, (const void __user *)arg,
+			sizeof(args)) != 0) {
+			ret = -EFAULT;
+			break;
+		}
+
+		mutex_lock(&instance->completion_mutex);
+
+		DEBUG_TRACE(AWAIT_COMPLETION_LINE);
+		while ((instance->completion_remove ==
+			instance->completion_insert)
+			&& !instance->closing) {
+			int rc;
+			DEBUG_TRACE(AWAIT_COMPLETION_LINE);
+			mutex_unlock(&instance->completion_mutex);
+			rc = down_interruptible(&instance->insert_event);
+			mutex_lock(&instance->completion_mutex);
+			if (rc != 0) {
+				DEBUG_TRACE(AWAIT_COMPLETION_LINE);
+				vchiq_log_info(vchiq_arm_log_level,
+					"AWAIT_COMPLETION interrupted");
+				ret = -EINTR;
+				break;
+			}
+		}
+		DEBUG_TRACE(AWAIT_COMPLETION_LINE);
+
+		/* A read memory barrier is needed to stop prefetch of a stale
+		** completion record
+		*/
+		rmb();
+
+		if (ret == 0) {
+			int msgbufcount = args.msgbufcount;
+			for (ret = 0; ret < args.count; ret++) {
+				VCHIQ_COMPLETION_DATA_T *completion;
+				VCHIQ_SERVICE_T *service;
+				USER_SERVICE_T *user_service;
+				VCHIQ_HEADER_T *header;
+				if (instance->completion_remove ==
+					instance->completion_insert)
+					break;
+				completion = &instance->completions[
+					instance->completion_remove &
+					(MAX_COMPLETIONS - 1)];
+
+				service = completion->service_userdata;
+				user_service = service->base.userdata;
+				completion->service_userdata =
+					user_service->userdata;
+
+				header = completion->header;
+				if (header) {
+					void __user *msgbuf;
+					int msglen;
+
+					msglen = header->size +
+						sizeof(VCHIQ_HEADER_T);
+					/* This must be a VCHIQ-style service */
+					if (args.msgbufsize < msglen) {
+						vchiq_log_error(
+							vchiq_arm_log_level,
+							"header %x: msgbufsize"
+							" %x < msglen %x",
+							(unsigned int)header,
+							args.msgbufsize,
+							msglen);
+						WARN(1, "invalid message "
+							"size\n");
+						if (ret == 0)
+							ret = -EMSGSIZE;
+						break;
+					}
+					if (msgbufcount <= 0)
+						/* Stall here for lack of a
+						** buffer for the message. */
+						break;
+					/* Get the pointer from user space */
+					msgbufcount--;
+					if (copy_from_user(&msgbuf,
+						(const void __user *)
+						&args.msgbufs[msgbufcount],
+						sizeof(msgbuf)) != 0) {
+						if (ret == 0)
+							ret = -EFAULT;
+						break;
+					}
+
+					/* Copy the message to user space */
+					if (copy_to_user(msgbuf, header,
+						msglen) != 0) {
+						if (ret == 0)
+							ret = -EFAULT;
+						break;
+					}
+
+					/* Now it has been copied, the message
+					** can be released. */
+					vchiq_release_message(service->handle,
+						header);
+
+					/* The completion must point to the
+					** msgbuf. */
+					completion->header = msgbuf;
+				}
+
+				if ((completion->reason ==
+					VCHIQ_SERVICE_CLOSED) &&
+					!instance->use_close_delivered)
+					unlock_service(service);
+
+				if (copy_to_user((void __user *)(
+					(size_t)args.buf +
+					ret * sizeof(VCHIQ_COMPLETION_DATA_T)),
+					completion,
+					sizeof(VCHIQ_COMPLETION_DATA_T)) != 0) {
+						if (ret == 0)
+							ret = -EFAULT;
+					break;
+				}
+
+				instance->completion_remove++;
+			}
+
+			if (msgbufcount != args.msgbufcount) {
+				if (copy_to_user((void __user *)
+					&((VCHIQ_AWAIT_COMPLETION_T *)arg)->
+						msgbufcount,
+					&msgbufcount,
+					sizeof(msgbufcount)) != 0) {
+					ret = -EFAULT;
+				}
+			}
+		}
+
+		if (ret != 0)
+			up(&instance->remove_event);
+		mutex_unlock(&instance->completion_mutex);
+		DEBUG_TRACE(AWAIT_COMPLETION_LINE);
+	} break;
+
+	case VCHIQ_IOC_DEQUEUE_MESSAGE: {
+		VCHIQ_DEQUEUE_MESSAGE_T args;
+		USER_SERVICE_T *user_service;
+		VCHIQ_HEADER_T *header;
+
+		DEBUG_TRACE(DEQUEUE_MESSAGE_LINE);
+		if (copy_from_user
+			 (&args, (const void __user *)arg,
+			  sizeof(args)) != 0) {
+			ret = -EFAULT;
+			break;
+		}
+		service = find_service_for_instance(instance, args.handle);
+		if (!service) {
+			ret = -EINVAL;
+			break;
+		}
+		user_service = (USER_SERVICE_T *)service->base.userdata;
+		if (user_service->is_vchi == 0) {
+			ret = -EINVAL;
+			break;
+		}
+
+		spin_lock(&msg_queue_spinlock);
+		if (user_service->msg_remove == user_service->msg_insert) {
+			if (!args.blocking) {
+				spin_unlock(&msg_queue_spinlock);
+				DEBUG_TRACE(DEQUEUE_MESSAGE_LINE);
+				ret = -EWOULDBLOCK;
+				break;
+			}
+			user_service->dequeue_pending = 1;
+			do {
+				spin_unlock(&msg_queue_spinlock);
+				DEBUG_TRACE(DEQUEUE_MESSAGE_LINE);
+				if (down_interruptible(
+					&user_service->insert_event) != 0) {
+					vchiq_log_info(vchiq_arm_log_level,
+						"DEQUEUE_MESSAGE interrupted");
+					ret = -EINTR;
+					break;
+				}
+				spin_lock(&msg_queue_spinlock);
+			} while (user_service->msg_remove ==
+				user_service->msg_insert);
+
+			if (ret)
+				break;
+		}
+
+		BUG_ON((int)(user_service->msg_insert -
+			user_service->msg_remove) < 0);
+
+		header = user_service->msg_queue[user_service->msg_remove &
+			(MSG_QUEUE_SIZE - 1)];
+		user_service->msg_remove++;
+		spin_unlock(&msg_queue_spinlock);
+
+		up(&user_service->remove_event);
+		if (header == NULL)
+			ret = -ENOTCONN;
+		else if (header->size <= args.bufsize) {
+			/* Copy to user space if msgbuf is not NULL */
+			if ((args.buf == NULL) ||
+				(copy_to_user((void __user *)args.buf,
+				header->data,
+				header->size) == 0)) {
+				ret = header->size;
+				vchiq_release_message(
+					service->handle,
+					header);
+			} else
+				ret = -EFAULT;
+		} else {
+			vchiq_log_error(vchiq_arm_log_level,
+				"header %x: bufsize %x < size %x",
+				(unsigned int)header, args.bufsize,
+				header->size);
+			WARN(1, "invalid size\n");
+			ret = -EMSGSIZE;
+		}
+		DEBUG_TRACE(DEQUEUE_MESSAGE_LINE);
+	} break;
+
+	case VCHIQ_IOC_GET_CLIENT_ID: {
+		VCHIQ_SERVICE_HANDLE_T handle = (VCHIQ_SERVICE_HANDLE_T)arg;
+
+		ret = vchiq_get_client_id(handle);
+	} break;
+
+	case VCHIQ_IOC_GET_CONFIG: {
+		VCHIQ_GET_CONFIG_T args;
+		VCHIQ_CONFIG_T config;
+
+		if (copy_from_user(&args, (const void __user *)arg,
+			sizeof(args)) != 0) {
+			ret = -EFAULT;
+			break;
+		}
+		if (args.config_size > sizeof(config)) {
+			ret = -EINVAL;
+			break;
+		}
+		status = vchiq_get_config(instance, args.config_size, &config);
+		if (status == VCHIQ_SUCCESS) {
+			if (copy_to_user((void __user *)args.pconfig,
+				    &config, args.config_size) != 0) {
+				ret = -EFAULT;
+				break;
+			}
+		}
+	} break;
+
+	case VCHIQ_IOC_SET_SERVICE_OPTION: {
+		VCHIQ_SET_SERVICE_OPTION_T args;
+
+		if (copy_from_user(
+			&args, (const void __user *)arg,
+			sizeof(args)) != 0) {
+			ret = -EFAULT;
+			break;
+		}
+
+		service = find_service_for_instance(instance, args.handle);
+		if (!service) {
+			ret = -EINVAL;
+			break;
+		}
+
+		status = vchiq_set_service_option(
+				args.handle, args.option, args.value);
+	} break;
+
+	case VCHIQ_IOC_DUMP_PHYS_MEM: {
+		VCHIQ_DUMP_MEM_T  args;
+
+		if (copy_from_user
+			 (&args, (const void __user *)arg,
+			  sizeof(args)) != 0) {
+			ret = -EFAULT;
+			break;
+		}
+		dump_phys_mem(args.virt_addr, args.num_bytes);
+	} break;
+
+	case VCHIQ_IOC_LIB_VERSION: {
+		unsigned int lib_version = (unsigned int)arg;
+
+		if (lib_version < VCHIQ_VERSION_MIN)
+			ret = -EINVAL;
+		else if (lib_version >= VCHIQ_VERSION_CLOSE_DELIVERED)
+			instance->use_close_delivered = 1;
+	} break;
+
+	case VCHIQ_IOC_CLOSE_DELIVERED: {
+		VCHIQ_SERVICE_HANDLE_T handle = (VCHIQ_SERVICE_HANDLE_T)arg;
+
+		service = find_closed_service_for_instance(instance, handle);
+		if (service != NULL) {
+			USER_SERVICE_T *user_service =
+				(USER_SERVICE_T *)service->base.userdata;
+			close_delivered(user_service);
+		}
+		else
+			ret = -EINVAL;
+	} break;
+
+	default:
+		ret = -ENOTTY;
+		break;
+	}
+
+	if (service)
+		unlock_service(service);
+
+	if (ret == 0) {
+		if (status == VCHIQ_ERROR)
+			ret = -EIO;
+		else if (status == VCHIQ_RETRY)
+			ret = -EINTR;
+	}
+
+	if ((status == VCHIQ_SUCCESS) && (ret < 0) && (ret != -EINTR) &&
+		(ret != -EWOULDBLOCK))
+		vchiq_log_info(vchiq_arm_log_level,
+			"  ioctl instance %lx, cmd %s -> status %d, %ld",
+			(unsigned long)instance,
+			(_IOC_NR(cmd) <= VCHIQ_IOC_MAX) ?
+				ioctl_names[_IOC_NR(cmd)] :
+				"<invalid>",
+			status, ret);
+	else
+		vchiq_log_trace(vchiq_arm_log_level,
+			"  ioctl instance %lx, cmd %s -> status %d, %ld",
+			(unsigned long)instance,
+			(_IOC_NR(cmd) <= VCHIQ_IOC_MAX) ?
+				ioctl_names[_IOC_NR(cmd)] :
+				"<invalid>",
+			status, ret);
+
+	return ret;
+}
+
+/****************************************************************************
+*
+*   vchiq_open
+*
+***************************************************************************/
+
+static int
+vchiq_open(struct inode *inode, struct file *file)
+{
+	int dev = iminor(inode) & 0x0f;
+	vchiq_log_info(vchiq_arm_log_level, "vchiq_open");
+	switch (dev) {
+	case VCHIQ_MINOR: {
+		int ret;
+		VCHIQ_STATE_T *state = vchiq_get_state();
+		VCHIQ_INSTANCE_T instance;
+
+		if (!state) {
+			vchiq_log_error(vchiq_arm_log_level,
+				"vchiq has no connection to VideoCore");
+			return -ENOTCONN;
+		}
+
+		instance = kzalloc(sizeof(*instance), GFP_KERNEL);
+		if (!instance)
+			return -ENOMEM;
+
+		instance->state = state;
+		instance->pid = current->tgid;
+
+		ret = vchiq_debugfs_add_instance(instance);
+		if (ret != 0) {
+			kfree(instance);
+			return ret;
+		}
+
+		sema_init(&instance->insert_event, 0);
+		sema_init(&instance->remove_event, 0);
+		mutex_init(&instance->completion_mutex);
+		mutex_init(&instance->bulk_waiter_list_mutex);
+		INIT_LIST_HEAD(&instance->bulk_waiter_list);
+
+		file->private_data = instance;
+	} break;
+
+	default:
+		vchiq_log_error(vchiq_arm_log_level,
+			"Unknown minor device: %d", dev);
+		return -ENXIO;
+	}
+
+	return 0;
+}
+
+/****************************************************************************
+*
+*   vchiq_release
+*
+***************************************************************************/
+
+static int
+vchiq_release(struct inode *inode, struct file *file)
+{
+	int dev = iminor(inode) & 0x0f;
+	int ret = 0;
+	switch (dev) {
+	case VCHIQ_MINOR: {
+		VCHIQ_INSTANCE_T instance = file->private_data;
+		VCHIQ_STATE_T *state = vchiq_get_state();
+		VCHIQ_SERVICE_T *service;
+		int i;
+
+		vchiq_log_info(vchiq_arm_log_level,
+			"vchiq_release: instance=%lx",
+			(unsigned long)instance);
+
+		if (!state) {
+			ret = -EPERM;
+			goto out;
+		}
+
+		/* Ensure videocore is awake to allow termination. */
+		vchiq_use_internal(instance->state, NULL,
+				USE_TYPE_VCHIQ);
+
+		mutex_lock(&instance->completion_mutex);
+
+		/* Wake the completion thread and ask it to exit */
+		instance->closing = 1;
+		up(&instance->insert_event);
+
+		mutex_unlock(&instance->completion_mutex);
+
+		/* Wake the slot handler if the completion queue is full. */
+		up(&instance->remove_event);
+
+		/* Mark all services for termination... */
+		i = 0;
+		while ((service = next_service_by_instance(state, instance,
+			&i)) !=	NULL) {
+			USER_SERVICE_T *user_service = service->base.userdata;
+
+			/* Wake the slot handler if the msg queue is full. */
+			up(&user_service->remove_event);
+
+			vchiq_terminate_service_internal(service);
+			unlock_service(service);
+		}
+
+		/* ...and wait for them to die */
+		i = 0;
+		while ((service = next_service_by_instance(state, instance, &i))
+			!= NULL) {
+			USER_SERVICE_T *user_service = service->base.userdata;
+
+			down(&service->remove_event);
+
+			BUG_ON(service->srvstate != VCHIQ_SRVSTATE_FREE);
+
+			spin_lock(&msg_queue_spinlock);
+
+			while (user_service->msg_remove !=
+				user_service->msg_insert) {
+				VCHIQ_HEADER_T *header = user_service->
+					msg_queue[user_service->msg_remove &
+						(MSG_QUEUE_SIZE - 1)];
+				user_service->msg_remove++;
+				spin_unlock(&msg_queue_spinlock);
+
+				if (header)
+					vchiq_release_message(
+						service->handle,
+						header);
+				spin_lock(&msg_queue_spinlock);
+			}
+
+			spin_unlock(&msg_queue_spinlock);
+
+			unlock_service(service);
+		}
+
+		/* Release any closed services */
+		while (instance->completion_remove !=
+			instance->completion_insert) {
+			VCHIQ_COMPLETION_DATA_T *completion;
+			VCHIQ_SERVICE_T *service;
+			completion = &instance->completions[
+				instance->completion_remove &
+				(MAX_COMPLETIONS - 1)];
+			service = completion->service_userdata;
+			if (completion->reason == VCHIQ_SERVICE_CLOSED)
+			{
+				USER_SERVICE_T *user_service =
+					service->base.userdata;
+
+				/* Wake any blocked user-thread */
+				if (instance->use_close_delivered)
+					up(&user_service->close_event);
+				unlock_service(service);
+			}
+			instance->completion_remove++;
+		}
+
+		/* Release the PEER service count. */
+		vchiq_release_internal(instance->state, NULL);
+
+		{
+			struct list_head *pos, *next;
+			list_for_each_safe(pos, next,
+				&instance->bulk_waiter_list) {
+				struct bulk_waiter_node *waiter;
+				waiter = list_entry(pos,
+					struct bulk_waiter_node,
+					list);
+				list_del(pos);
+				vchiq_log_info(vchiq_arm_log_level,
+					"bulk_waiter - cleaned up %x "
+					"for pid %d",
+					(unsigned int)waiter, waiter->pid);
+				kfree(waiter);
+			}
+		}
+
+		vchiq_debugfs_remove_instance(instance);
+
+		kfree(instance);
+		file->private_data = NULL;
+	} break;
+
+	default:
+		vchiq_log_error(vchiq_arm_log_level,
+			"Unknown minor device: %d", dev);
+		ret = -ENXIO;
+	}
+
+out:
+	return ret;
+}
+
+/****************************************************************************
+*
+*   vchiq_dump
+*
+***************************************************************************/
+
+void
+vchiq_dump(void *dump_context, const char *str, int len)
+{
+	DUMP_CONTEXT_T *context = (DUMP_CONTEXT_T *)dump_context;
+
+	if (context->actual < context->space) {
+		int copy_bytes;
+		if (context->offset > 0) {
+			int skip_bytes = min(len, (int)context->offset);
+			str += skip_bytes;
+			len -= skip_bytes;
+			context->offset -= skip_bytes;
+			if (context->offset > 0)
+				return;
+		}
+		copy_bytes = min(len, (int)(context->space - context->actual));
+		if (copy_bytes == 0)
+			return;
+		if (copy_to_user(context->buf + context->actual, str,
+			copy_bytes))
+			context->actual = -EFAULT;
+		context->actual += copy_bytes;
+		len -= copy_bytes;
+
+		/* If tne terminating NUL is included in the length, then it
+		** marks the end of a line and should be replaced with a
+		** carriage return. */
+		if ((len == 0) && (str[copy_bytes - 1] == '\0')) {
+			char cr = '\n';
+			if (copy_to_user(context->buf + context->actual - 1,
+				&cr, 1))
+				context->actual = -EFAULT;
+		}
+	}
+}
+
+/****************************************************************************
+*
+*   vchiq_dump_platform_instance_state
+*
+***************************************************************************/
+
+void
+vchiq_dump_platform_instances(void *dump_context)
+{
+	VCHIQ_STATE_T *state = vchiq_get_state();
+	char buf[80];
+	int len;
+	int i;
+
+	/* There is no list of instances, so instead scan all services,
+		marking those that have been dumped. */
+
+	for (i = 0; i < state->unused_service; i++) {
+		VCHIQ_SERVICE_T *service = state->services[i];
+		VCHIQ_INSTANCE_T instance;
+
+		if (service && (service->base.callback == service_callback)) {
+			instance = service->instance;
+			if (instance)
+				instance->mark = 0;
+		}
+	}
+
+	for (i = 0; i < state->unused_service; i++) {
+		VCHIQ_SERVICE_T *service = state->services[i];
+		VCHIQ_INSTANCE_T instance;
+
+		if (service && (service->base.callback == service_callback)) {
+			instance = service->instance;
+			if (instance && !instance->mark) {
+				len = snprintf(buf, sizeof(buf),
+					"Instance %x: pid %d,%s completions "
+						"%d/%d",
+					(unsigned int)instance, instance->pid,
+					instance->connected ? " connected, " :
+						"",
+					instance->completion_insert -
+						instance->completion_remove,
+					MAX_COMPLETIONS);
+
+				vchiq_dump(dump_context, buf, len + 1);
+
+				instance->mark = 1;
+			}
+		}
+	}
+}
+
+/****************************************************************************
+*
+*   vchiq_dump_platform_service_state
+*
+***************************************************************************/
+
+void
+vchiq_dump_platform_service_state(void *dump_context, VCHIQ_SERVICE_T *service)
+{
+	USER_SERVICE_T *user_service = (USER_SERVICE_T *)service->base.userdata;
+	char buf[80];
+	int len;
+
+	len = snprintf(buf, sizeof(buf), "  instance %x",
+		(unsigned int)service->instance);
+
+	if ((service->base.callback == service_callback) &&
+		user_service->is_vchi) {
+		len += snprintf(buf + len, sizeof(buf) - len,
+			", %d/%d messages",
+			user_service->msg_insert - user_service->msg_remove,
+			MSG_QUEUE_SIZE);
+
+		if (user_service->dequeue_pending)
+			len += snprintf(buf + len, sizeof(buf) - len,
+				" (dequeue pending)");
+	}
+
+	vchiq_dump(dump_context, buf, len + 1);
+}
+
+/****************************************************************************
+*
+*   dump_user_mem
+*
+***************************************************************************/
+
+static void
+dump_phys_mem(void *virt_addr, uint32_t num_bytes)
+{
+	int            rc;
+	uint8_t       *end_virt_addr = virt_addr + num_bytes;
+	int            num_pages;
+	int            offset;
+	int            end_offset;
+	int            page_idx;
+	int            prev_idx;
+	struct page   *page;
+	struct page  **pages;
+	uint8_t       *kmapped_virt_ptr;
+
+	/* Align virtAddr and endVirtAddr to 16 byte boundaries. */
+
+	virt_addr = (void *)((unsigned long)virt_addr & ~0x0fuL);
+	end_virt_addr = (void *)(((unsigned long)end_virt_addr + 15uL) &
+		~0x0fuL);
+
+	offset = (int)(long)virt_addr & (PAGE_SIZE - 1);
+	end_offset = (int)(long)end_virt_addr & (PAGE_SIZE - 1);
+
+	num_pages = (offset + num_bytes + PAGE_SIZE - 1) / PAGE_SIZE;
+
+	pages = kmalloc(sizeof(struct page *) * num_pages, GFP_KERNEL);
+	if (pages == NULL) {
+		vchiq_log_error(vchiq_arm_log_level,
+			"Unable to allocation memory for %d pages\n",
+			num_pages);
+		return;
+	}
+
+	down_read(&current->mm->mmap_sem);
+	rc = get_user_pages(current,      /* task */
+		current->mm,              /* mm */
+		(unsigned long)virt_addr, /* start */
+		num_pages,                /* len */
+		0,                        /* write */
+		0,                        /* force */
+		pages,                    /* pages (array of page pointers) */
+		NULL);                    /* vmas */
+	up_read(&current->mm->mmap_sem);
+
+	prev_idx = -1;
+	page = NULL;
+
+	while (offset < end_offset) {
+
+		int page_offset = offset % PAGE_SIZE;
+		page_idx = offset / PAGE_SIZE;
+
+		if (page_idx != prev_idx) {
+
+			if (page != NULL)
+				kunmap(page);
+			page = pages[page_idx];
+			kmapped_virt_ptr = kmap(page);
+
+			prev_idx = page_idx;
+		}
+
+		if (vchiq_arm_log_level >= VCHIQ_LOG_TRACE)
+			vchiq_log_dump_mem("ph",
+				(uint32_t)(unsigned long)&kmapped_virt_ptr[
+					page_offset],
+				&kmapped_virt_ptr[page_offset], 16);
+
+		offset += 16;
+	}
+	if (page != NULL)
+		kunmap(page);
+
+	for (page_idx = 0; page_idx < num_pages; page_idx++)
+		page_cache_release(pages[page_idx]);
+
+	kfree(pages);
+}
+
+/****************************************************************************
+*
+*   vchiq_read
+*
+***************************************************************************/
+
+static ssize_t
+vchiq_read(struct file *file, char __user *buf,
+	size_t count, loff_t *ppos)
+{
+	DUMP_CONTEXT_T context;
+	context.buf = buf;
+	context.actual = 0;
+	context.space = count;
+	context.offset = *ppos;
+
+	vchiq_dump_state(&context, &g_state);
+
+	*ppos += context.actual;
+
+	return context.actual;
+}
+
+VCHIQ_STATE_T *
+vchiq_get_state(void)
+{
+
+	if (g_state.remote == NULL)
+		printk(KERN_ERR "%s: g_state.remote == NULL\n", __func__);
+	else if (g_state.remote->initialised != 1)
+		printk(KERN_NOTICE "%s: g_state.remote->initialised != 1 (%d)\n",
+			__func__, g_state.remote->initialised);
+
+	return ((g_state.remote != NULL) &&
+		(g_state.remote->initialised == 1)) ? &g_state : NULL;
+}
+
+static const struct file_operations
+vchiq_fops = {
+	.owner = THIS_MODULE,
+	.unlocked_ioctl = vchiq_ioctl,
+	.open = vchiq_open,
+	.release = vchiq_release,
+	.read = vchiq_read
+};
+
+/*
+ * Autosuspend related functionality
+ */
+
+int
+vchiq_videocore_wanted(VCHIQ_STATE_T *state)
+{
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+	if (!arm_state)
+		/* autosuspend not supported - always return wanted */
+		return 1;
+	else if (arm_state->blocked_count)
+		return 1;
+	else if (!arm_state->videocore_use_count)
+		/* usage count zero - check for override unless we're forcing */
+		if (arm_state->resume_blocked)
+			return 0;
+		else
+			return vchiq_platform_videocore_wanted(state);
+	else
+		/* non-zero usage count - videocore still required */
+		return 1;
+}
+
+static VCHIQ_STATUS_T
+vchiq_keepalive_vchiq_callback(VCHIQ_REASON_T reason,
+	VCHIQ_HEADER_T *header,
+	VCHIQ_SERVICE_HANDLE_T service_user,
+	void *bulk_user)
+{
+	vchiq_log_error(vchiq_susp_log_level,
+		"%s callback reason %d", __func__, reason);
+	return 0;
+}
+
+static int
+vchiq_keepalive_thread_func(void *v)
+{
+	VCHIQ_STATE_T *state = (VCHIQ_STATE_T *) v;
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+
+	VCHIQ_STATUS_T status;
+	VCHIQ_INSTANCE_T instance;
+	VCHIQ_SERVICE_HANDLE_T ka_handle;
+
+	VCHIQ_SERVICE_PARAMS_T params = {
+		.fourcc      = VCHIQ_MAKE_FOURCC('K', 'E', 'E', 'P'),
+		.callback    = vchiq_keepalive_vchiq_callback,
+		.version     = KEEPALIVE_VER,
+		.version_min = KEEPALIVE_VER_MIN
+	};
+
+	status = vchiq_initialise(&instance);
+	if (status != VCHIQ_SUCCESS) {
+		vchiq_log_error(vchiq_susp_log_level,
+			"%s vchiq_initialise failed %d", __func__, status);
+		goto exit;
+	}
+
+	status = vchiq_connect(instance);
+	if (status != VCHIQ_SUCCESS) {
+		vchiq_log_error(vchiq_susp_log_level,
+			"%s vchiq_connect failed %d", __func__, status);
+		goto shutdown;
+	}
+
+	status = vchiq_add_service(instance, &params, &ka_handle);
+	if (status != VCHIQ_SUCCESS) {
+		vchiq_log_error(vchiq_susp_log_level,
+			"%s vchiq_open_service failed %d", __func__, status);
+		goto shutdown;
+	}
+
+	while (1) {
+		long rc = 0, uc = 0;
+		if (wait_for_completion_interruptible(&arm_state->ka_evt)
+				!= 0) {
+			vchiq_log_error(vchiq_susp_log_level,
+				"%s interrupted", __func__);
+			flush_signals(current);
+			continue;
+		}
+
+		/* read and clear counters.  Do release_count then use_count to
+		 * prevent getting more releases than uses */
+		rc = atomic_xchg(&arm_state->ka_release_count, 0);
+		uc = atomic_xchg(&arm_state->ka_use_count, 0);
+
+		/* Call use/release service the requisite number of times.
+		 * Process use before release so use counts don't go negative */
+		while (uc--) {
+			atomic_inc(&arm_state->ka_use_ack_count);
+			status = vchiq_use_service(ka_handle);
+			if (status != VCHIQ_SUCCESS) {
+				vchiq_log_error(vchiq_susp_log_level,
+					"%s vchiq_use_service error %d",
+					__func__, status);
+			}
+		}
+		while (rc--) {
+			status = vchiq_release_service(ka_handle);
+			if (status != VCHIQ_SUCCESS) {
+				vchiq_log_error(vchiq_susp_log_level,
+					"%s vchiq_release_service error %d",
+					__func__, status);
+			}
+		}
+	}
+
+shutdown:
+	vchiq_shutdown(instance);
+exit:
+	return 0;
+}
+
+
+
+VCHIQ_STATUS_T
+vchiq_arm_init_state(VCHIQ_STATE_T *state, VCHIQ_ARM_STATE_T *arm_state)
+{
+	VCHIQ_STATUS_T status = VCHIQ_SUCCESS;
+
+	if (arm_state) {
+		rwlock_init(&arm_state->susp_res_lock);
+
+		init_completion(&arm_state->ka_evt);
+		atomic_set(&arm_state->ka_use_count, 0);
+		atomic_set(&arm_state->ka_use_ack_count, 0);
+		atomic_set(&arm_state->ka_release_count, 0);
+
+		init_completion(&arm_state->vc_suspend_complete);
+
+		init_completion(&arm_state->vc_resume_complete);
+		/* Initialise to 'done' state.  We only want to block on resume
+		 * completion while videocore is suspended. */
+		set_resume_state(arm_state, VC_RESUME_RESUMED);
+
+		init_completion(&arm_state->resume_blocker);
+		/* Initialise to 'done' state.  We only want to block on this
+		 * completion while resume is blocked */
+		complete_all(&arm_state->resume_blocker);
+
+		init_completion(&arm_state->blocked_blocker);
+		/* Initialise to 'done' state.  We only want to block on this
+		 * completion while things are waiting on the resume blocker */
+		complete_all(&arm_state->blocked_blocker);
+
+		arm_state->suspend_timer_timeout = SUSPEND_TIMER_TIMEOUT_MS;
+		arm_state->suspend_timer_running = 0;
+		init_timer(&arm_state->suspend_timer);
+		arm_state->suspend_timer.data = (unsigned long)(state);
+		arm_state->suspend_timer.function = suspend_timer_callback;
+
+		arm_state->first_connect = 0;
+
+	}
+	return status;
+}
+
+/*
+** Functions to modify the state variables;
+**	set_suspend_state
+**	set_resume_state
+**
+** There are more state variables than we might like, so ensure they remain in
+** step.  Suspend and resume state are maintained separately, since most of
+** these state machines can operate independently.  However, there are a few
+** states where state transitions in one state machine cause a reset to the
+** other state machine.  In addition, there are some completion events which
+** need to occur on state machine reset and end-state(s), so these are also
+** dealt with in these functions.
+**
+** In all states we set the state variable according to the input, but in some
+** cases we perform additional steps outlined below;
+**
+** VC_SUSPEND_IDLE - Initialise the suspend completion at the same time.
+**			The suspend completion is completed after any suspend
+**			attempt.  When we reset the state machine we also reset
+**			the completion.  This reset occurs when videocore is
+**			resumed, and also if we initiate suspend after a suspend
+**			failure.
+**
+** VC_SUSPEND_IN_PROGRESS - This state is considered the point of no return for
+**			suspend - ie from this point on we must try to suspend
+**			before resuming can occur.  We therefore also reset the
+**			resume state machine to VC_RESUME_IDLE in this state.
+**
+** VC_SUSPEND_SUSPENDED - Suspend has completed successfully. Also call
+**			complete_all on the suspend completion to notify
+**			anything waiting for suspend to happen.
+**
+** VC_SUSPEND_REJECTED - Videocore rejected suspend. Videocore will also
+**			initiate resume, so no need to alter resume state.
+**			We call complete_all on the suspend completion to notify
+**			of suspend rejection.
+**
+** VC_SUSPEND_FAILED - We failed to initiate videocore suspend.  We notify the
+**			suspend completion and reset the resume state machine.
+**
+** VC_RESUME_IDLE - Initialise the resume completion at the same time.  The
+**			resume completion is in it's 'done' state whenever
+**			videcore is running.  Therfore, the VC_RESUME_IDLE state
+**			implies that videocore is suspended.
+**			Hence, any thread which needs to wait until videocore is
+**			running can wait on this completion - it will only block
+**			if videocore is suspended.
+**
+** VC_RESUME_RESUMED - Resume has completed successfully.  Videocore is running.
+**			Call complete_all on the resume completion to unblock
+**			any threads waiting for resume.	 Also reset the suspend
+**			state machine to it's idle state.
+**
+** VC_RESUME_FAILED - Currently unused - no mechanism to fail resume exists.
+*/
+
+inline void
+set_suspend_state(VCHIQ_ARM_STATE_T *arm_state,
+	enum vc_suspend_status new_state)
+{
+	/* set the state in all cases */
+	arm_state->vc_suspend_state = new_state;
+
+	/* state specific additional actions */
+	switch (new_state) {
+	case VC_SUSPEND_FORCE_CANCELED:
+		complete_all(&arm_state->vc_suspend_complete);
+		break;
+	case VC_SUSPEND_REJECTED:
+		complete_all(&arm_state->vc_suspend_complete);
+		break;
+	case VC_SUSPEND_FAILED:
+		complete_all(&arm_state->vc_suspend_complete);
+		arm_state->vc_resume_state = VC_RESUME_RESUMED;
+		complete_all(&arm_state->vc_resume_complete);
+		break;
+	case VC_SUSPEND_IDLE:
+		reinit_completion(&arm_state->vc_suspend_complete);
+		break;
+	case VC_SUSPEND_REQUESTED:
+		break;
+	case VC_SUSPEND_IN_PROGRESS:
+		set_resume_state(arm_state, VC_RESUME_IDLE);
+		break;
+	case VC_SUSPEND_SUSPENDED:
+		complete_all(&arm_state->vc_suspend_complete);
+		break;
+	default:
+		BUG();
+		break;
+	}
+}
+
+inline void
+set_resume_state(VCHIQ_ARM_STATE_T *arm_state,
+	enum vc_resume_status new_state)
+{
+	/* set the state in all cases */
+	arm_state->vc_resume_state = new_state;
+
+	/* state specific additional actions */
+	switch (new_state) {
+	case VC_RESUME_FAILED:
+		break;
+	case VC_RESUME_IDLE:
+		reinit_completion(&arm_state->vc_resume_complete);
+		break;
+	case VC_RESUME_REQUESTED:
+		break;
+	case VC_RESUME_IN_PROGRESS:
+		break;
+	case VC_RESUME_RESUMED:
+		complete_all(&arm_state->vc_resume_complete);
+		set_suspend_state(arm_state, VC_SUSPEND_IDLE);
+		break;
+	default:
+		BUG();
+		break;
+	}
+}
+
+
+/* should be called with the write lock held */
+inline void
+start_suspend_timer(VCHIQ_ARM_STATE_T *arm_state)
+{
+	del_timer(&arm_state->suspend_timer);
+	arm_state->suspend_timer.expires = jiffies +
+		msecs_to_jiffies(arm_state->
+			suspend_timer_timeout);
+	add_timer(&arm_state->suspend_timer);
+	arm_state->suspend_timer_running = 1;
+}
+
+/* should be called with the write lock held */
+static inline void
+stop_suspend_timer(VCHIQ_ARM_STATE_T *arm_state)
+{
+	if (arm_state->suspend_timer_running) {
+		del_timer(&arm_state->suspend_timer);
+		arm_state->suspend_timer_running = 0;
+	}
+}
+
+static inline int
+need_resume(VCHIQ_STATE_T *state)
+{
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+	return (arm_state->vc_suspend_state > VC_SUSPEND_IDLE) &&
+			(arm_state->vc_resume_state < VC_RESUME_REQUESTED) &&
+			vchiq_videocore_wanted(state);
+}
+
+static int
+block_resume(VCHIQ_ARM_STATE_T *arm_state)
+{
+	int status = VCHIQ_SUCCESS;
+	const unsigned long timeout_val =
+				msecs_to_jiffies(FORCE_SUSPEND_TIMEOUT_MS);
+	int resume_count = 0;
+
+	/* Allow any threads which were blocked by the last force suspend to
+	 * complete if they haven't already.  Only give this one shot; if
+	 * blocked_count is incremented after blocked_blocker is completed
+	 * (which only happens when blocked_count hits 0) then those threads
+	 * will have to wait until next time around */
+	if (arm_state->blocked_count) {
+		reinit_completion(&arm_state->blocked_blocker);
+		write_unlock_bh(&arm_state->susp_res_lock);
+		vchiq_log_info(vchiq_susp_log_level, "%s wait for previously "
+			"blocked clients", __func__);
+		if (wait_for_completion_interruptible_timeout(
+				&arm_state->blocked_blocker, timeout_val)
+					<= 0) {
+			vchiq_log_error(vchiq_susp_log_level, "%s wait for "
+				"previously blocked clients failed" , __func__);
+			status = VCHIQ_ERROR;
+			write_lock_bh(&arm_state->susp_res_lock);
+			goto out;
+		}
+		vchiq_log_info(vchiq_susp_log_level, "%s previously blocked "
+			"clients resumed", __func__);
+		write_lock_bh(&arm_state->susp_res_lock);
+	}
+
+	/* We need to wait for resume to complete if it's in process */
+	while (arm_state->vc_resume_state != VC_RESUME_RESUMED &&
+			arm_state->vc_resume_state > VC_RESUME_IDLE) {
+		if (resume_count > 1) {
+			status = VCHIQ_ERROR;
+			vchiq_log_error(vchiq_susp_log_level, "%s waited too "
+				"many times for resume" , __func__);
+			goto out;
+		}
+		write_unlock_bh(&arm_state->susp_res_lock);
+		vchiq_log_info(vchiq_susp_log_level, "%s wait for resume",
+			__func__);
+		if (wait_for_completion_interruptible_timeout(
+				&arm_state->vc_resume_complete, timeout_val)
+					<= 0) {
+			vchiq_log_error(vchiq_susp_log_level, "%s wait for "
+				"resume failed (%s)", __func__,
+				resume_state_names[arm_state->vc_resume_state +
+							VC_RESUME_NUM_OFFSET]);
+			status = VCHIQ_ERROR;
+			write_lock_bh(&arm_state->susp_res_lock);
+			goto out;
+		}
+		vchiq_log_info(vchiq_susp_log_level, "%s resumed", __func__);
+		write_lock_bh(&arm_state->susp_res_lock);
+		resume_count++;
+	}
+	reinit_completion(&arm_state->resume_blocker);
+	arm_state->resume_blocked = 1;
+
+out:
+	return status;
+}
+
+static inline void
+unblock_resume(VCHIQ_ARM_STATE_T *arm_state)
+{
+	complete_all(&arm_state->resume_blocker);
+	arm_state->resume_blocked = 0;
+}
+
+/* Initiate suspend via slot handler. Should be called with the write lock
+ * held */
+VCHIQ_STATUS_T
+vchiq_arm_vcsuspend(VCHIQ_STATE_T *state)
+{
+	VCHIQ_STATUS_T status = VCHIQ_ERROR;
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+
+	if (!arm_state)
+		goto out;
+
+	vchiq_log_trace(vchiq_susp_log_level, "%s", __func__);
+	status = VCHIQ_SUCCESS;
+
+
+	switch (arm_state->vc_suspend_state) {
+	case VC_SUSPEND_REQUESTED:
+		vchiq_log_info(vchiq_susp_log_level, "%s: suspend already "
+			"requested", __func__);
+		break;
+	case VC_SUSPEND_IN_PROGRESS:
+		vchiq_log_info(vchiq_susp_log_level, "%s: suspend already in "
+			"progress", __func__);
+		break;
+
+	default:
+		/* We don't expect to be in other states, so log but continue
+		 * anyway */
+		vchiq_log_error(vchiq_susp_log_level,
+			"%s unexpected suspend state %s", __func__,
+			suspend_state_names[arm_state->vc_suspend_state +
+						VC_SUSPEND_NUM_OFFSET]);
+		/* fall through */
+	case VC_SUSPEND_REJECTED:
+	case VC_SUSPEND_FAILED:
+		/* Ensure any idle state actions have been run */
+		set_suspend_state(arm_state, VC_SUSPEND_IDLE);
+		/* fall through */
+	case VC_SUSPEND_IDLE:
+		vchiq_log_info(vchiq_susp_log_level,
+			"%s: suspending", __func__);
+		set_suspend_state(arm_state, VC_SUSPEND_REQUESTED);
+		/* kick the slot handler thread to initiate suspend */
+		request_poll(state, NULL, 0);
+		break;
+	}
+
+out:
+	vchiq_log_trace(vchiq_susp_log_level, "%s exit %d", __func__, status);
+	return status;
+}
+
+void
+vchiq_platform_check_suspend(VCHIQ_STATE_T *state)
+{
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+	int susp = 0;
+
+	if (!arm_state)
+		goto out;
+
+	vchiq_log_trace(vchiq_susp_log_level, "%s", __func__);
+
+	write_lock_bh(&arm_state->susp_res_lock);
+	if (arm_state->vc_suspend_state == VC_SUSPEND_REQUESTED &&
+			arm_state->vc_resume_state == VC_RESUME_RESUMED) {
+		set_suspend_state(arm_state, VC_SUSPEND_IN_PROGRESS);
+		susp = 1;
+	}
+	write_unlock_bh(&arm_state->susp_res_lock);
+
+	if (susp)
+		vchiq_platform_suspend(state);
+
+out:
+	vchiq_log_trace(vchiq_susp_log_level, "%s exit", __func__);
+	return;
+}
+
+
+static void
+output_timeout_error(VCHIQ_STATE_T *state)
+{
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+	char service_err[50] = "";
+	int vc_use_count = arm_state->videocore_use_count;
+	int active_services = state->unused_service;
+	int i;
+
+	if (!arm_state->videocore_use_count) {
+		snprintf(service_err, 50, " Videocore usecount is 0");
+		goto output_msg;
+	}
+	for (i = 0; i < active_services; i++) {
+		VCHIQ_SERVICE_T *service_ptr = state->services[i];
+		if (service_ptr && service_ptr->service_use_count &&
+			(service_ptr->srvstate != VCHIQ_SRVSTATE_FREE)) {
+			snprintf(service_err, 50, " %c%c%c%c(%d) service has "
+				"use count %d%s", VCHIQ_FOURCC_AS_4CHARS(
+					service_ptr->base.fourcc),
+				 service_ptr->client_id,
+				 service_ptr->service_use_count,
+				 service_ptr->service_use_count ==
+					 vc_use_count ? "" : " (+ more)");
+			break;
+		}
+	}
+
+output_msg:
+	vchiq_log_error(vchiq_susp_log_level,
+		"timed out waiting for vc suspend (%d).%s",
+		 arm_state->autosuspend_override, service_err);
+
+}
+
+/* Try to get videocore into suspended state, regardless of autosuspend state.
+** We don't actually force suspend, since videocore may get into a bad state
+** if we force suspend at a bad time.  Instead, we wait for autosuspend to
+** determine a good point to suspend.  If this doesn't happen within 100ms we
+** report failure.
+**
+** Returns VCHIQ_SUCCESS if videocore suspended successfully, VCHIQ_RETRY if
+** videocore failed to suspend in time or VCHIQ_ERROR if interrupted.
+*/
+VCHIQ_STATUS_T
+vchiq_arm_force_suspend(VCHIQ_STATE_T *state)
+{
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+	VCHIQ_STATUS_T status = VCHIQ_ERROR;
+	long rc = 0;
+	int repeat = -1;
+
+	if (!arm_state)
+		goto out;
+
+	vchiq_log_trace(vchiq_susp_log_level, "%s", __func__);
+
+	write_lock_bh(&arm_state->susp_res_lock);
+
+	status = block_resume(arm_state);
+	if (status != VCHIQ_SUCCESS)
+		goto unlock;
+	if (arm_state->vc_suspend_state == VC_SUSPEND_SUSPENDED) {
+		/* Already suspended - just block resume and exit */
+		vchiq_log_info(vchiq_susp_log_level, "%s already suspended",
+			__func__);
+		status = VCHIQ_SUCCESS;
+		goto unlock;
+	} else if (arm_state->vc_suspend_state <= VC_SUSPEND_IDLE) {
+		/* initiate suspend immediately in the case that we're waiting
+		 * for the timeout */
+		stop_suspend_timer(arm_state);
+		if (!vchiq_videocore_wanted(state)) {
+			vchiq_log_info(vchiq_susp_log_level, "%s videocore "
+				"idle, initiating suspend", __func__);
+			status = vchiq_arm_vcsuspend(state);
+		} else if (arm_state->autosuspend_override <
+						FORCE_SUSPEND_FAIL_MAX) {
+			vchiq_log_info(vchiq_susp_log_level, "%s letting "
+				"videocore go idle", __func__);
+			status = VCHIQ_SUCCESS;
+		} else {
+			vchiq_log_warning(vchiq_susp_log_level, "%s failed too "
+				"many times - attempting suspend", __func__);
+			status = vchiq_arm_vcsuspend(state);
+		}
+	} else {
+		vchiq_log_info(vchiq_susp_log_level, "%s videocore suspend "
+			"in progress - wait for completion", __func__);
+		status = VCHIQ_SUCCESS;
+	}
+
+	/* Wait for suspend to happen due to system idle (not forced..) */
+	if (status != VCHIQ_SUCCESS)
+		goto unblock_resume;
+
+	do {
+		write_unlock_bh(&arm_state->susp_res_lock);
+
+		rc = wait_for_completion_interruptible_timeout(
+				&arm_state->vc_suspend_complete,
+				msecs_to_jiffies(FORCE_SUSPEND_TIMEOUT_MS));
+
+		write_lock_bh(&arm_state->susp_res_lock);
+		if (rc < 0) {
+			vchiq_log_warning(vchiq_susp_log_level, "%s "
+				"interrupted waiting for suspend", __func__);
+			status = VCHIQ_ERROR;
+			goto unblock_resume;
+		} else if (rc == 0) {
+			if (arm_state->vc_suspend_state > VC_SUSPEND_IDLE) {
+				/* Repeat timeout once if in progress */
+				if (repeat < 0) {
+					repeat = 1;
+					continue;
+				}
+			}
+			arm_state->autosuspend_override++;
+			output_timeout_error(state);
+
+			status = VCHIQ_RETRY;
+			goto unblock_resume;
+		}
+	} while (0 < (repeat--));
+
+	/* Check and report state in case we need to abort ARM suspend */
+	if (arm_state->vc_suspend_state != VC_SUSPEND_SUSPENDED) {
+		status = VCHIQ_RETRY;
+		vchiq_log_error(vchiq_susp_log_level,
+			"%s videocore suspend failed (state %s)", __func__,
+			suspend_state_names[arm_state->vc_suspend_state +
+						VC_SUSPEND_NUM_OFFSET]);
+		/* Reset the state only if it's still in an error state.
+		 * Something could have already initiated another suspend. */
+		if (arm_state->vc_suspend_state < VC_SUSPEND_IDLE)
+			set_suspend_state(arm_state, VC_SUSPEND_IDLE);
+
+		goto unblock_resume;
+	}
+
+	/* successfully suspended - unlock and exit */
+	goto unlock;
+
+unblock_resume:
+	/* all error states need to unblock resume before exit */
+	unblock_resume(arm_state);
+
+unlock:
+	write_unlock_bh(&arm_state->susp_res_lock);
+
+out:
+	vchiq_log_trace(vchiq_susp_log_level, "%s exit %d", __func__, status);
+	return status;
+}
+
+void
+vchiq_check_suspend(VCHIQ_STATE_T *state)
+{
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+
+	if (!arm_state)
+		goto out;
+
+	vchiq_log_trace(vchiq_susp_log_level, "%s", __func__);
+
+	write_lock_bh(&arm_state->susp_res_lock);
+	if (arm_state->vc_suspend_state != VC_SUSPEND_SUSPENDED &&
+			arm_state->first_connect &&
+			!vchiq_videocore_wanted(state)) {
+		vchiq_arm_vcsuspend(state);
+	}
+	write_unlock_bh(&arm_state->susp_res_lock);
+
+out:
+	vchiq_log_trace(vchiq_susp_log_level, "%s exit", __func__);
+	return;
+}
+
+
+int
+vchiq_arm_allow_resume(VCHIQ_STATE_T *state)
+{
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+	int resume = 0;
+	int ret = -1;
+
+	if (!arm_state)
+		goto out;
+
+	vchiq_log_trace(vchiq_susp_log_level, "%s", __func__);
+
+	write_lock_bh(&arm_state->susp_res_lock);
+	unblock_resume(arm_state);
+	resume = vchiq_check_resume(state);
+	write_unlock_bh(&arm_state->susp_res_lock);
+
+	if (resume) {
+		if (wait_for_completion_interruptible(
+			&arm_state->vc_resume_complete) < 0) {
+			vchiq_log_error(vchiq_susp_log_level,
+				"%s interrupted", __func__);
+			/* failed, cannot accurately derive suspend
+			 * state, so exit early. */
+			goto out;
+		}
+	}
+
+	read_lock_bh(&arm_state->susp_res_lock);
+	if (arm_state->vc_suspend_state == VC_SUSPEND_SUSPENDED) {
+		vchiq_log_info(vchiq_susp_log_level,
+				"%s: Videocore remains suspended", __func__);
+	} else {
+		vchiq_log_info(vchiq_susp_log_level,
+				"%s: Videocore resumed", __func__);
+		ret = 0;
+	}
+	read_unlock_bh(&arm_state->susp_res_lock);
+out:
+	vchiq_log_trace(vchiq_susp_log_level, "%s exit %d", __func__, ret);
+	return ret;
+}
+
+/* This function should be called with the write lock held */
+int
+vchiq_check_resume(VCHIQ_STATE_T *state)
+{
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+	int resume = 0;
+
+	if (!arm_state)
+		goto out;
+
+	vchiq_log_trace(vchiq_susp_log_level, "%s", __func__);
+
+	if (need_resume(state)) {
+		set_resume_state(arm_state, VC_RESUME_REQUESTED);
+		request_poll(state, NULL, 0);
+		resume = 1;
+	}
+
+out:
+	vchiq_log_trace(vchiq_susp_log_level, "%s exit", __func__);
+	return resume;
+}
+
+void
+vchiq_platform_check_resume(VCHIQ_STATE_T *state)
+{
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+	int res = 0;
+
+	if (!arm_state)
+		goto out;
+
+	vchiq_log_trace(vchiq_susp_log_level, "%s", __func__);
+
+	write_lock_bh(&arm_state->susp_res_lock);
+	if (arm_state->wake_address == 0) {
+		vchiq_log_info(vchiq_susp_log_level,
+					"%s: already awake", __func__);
+		goto unlock;
+	}
+	if (arm_state->vc_resume_state == VC_RESUME_IN_PROGRESS) {
+		vchiq_log_info(vchiq_susp_log_level,
+					"%s: already resuming", __func__);
+		goto unlock;
+	}
+
+	if (arm_state->vc_resume_state == VC_RESUME_REQUESTED) {
+		set_resume_state(arm_state, VC_RESUME_IN_PROGRESS);
+		res = 1;
+	} else
+		vchiq_log_trace(vchiq_susp_log_level,
+				"%s: not resuming (resume state %s)", __func__,
+				resume_state_names[arm_state->vc_resume_state +
+							VC_RESUME_NUM_OFFSET]);
+
+unlock:
+	write_unlock_bh(&arm_state->susp_res_lock);
+
+	if (res)
+		vchiq_platform_resume(state);
+
+out:
+	vchiq_log_trace(vchiq_susp_log_level, "%s exit", __func__);
+	return;
+
+}
+
+
+
+VCHIQ_STATUS_T
+vchiq_use_internal(VCHIQ_STATE_T *state, VCHIQ_SERVICE_T *service,
+		enum USE_TYPE_E use_type)
+{
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+	VCHIQ_STATUS_T ret = VCHIQ_SUCCESS;
+	char entity[16];
+	int *entity_uc;
+	int local_uc, local_entity_uc;
+
+	if (!arm_state)
+		goto out;
+
+	vchiq_log_trace(vchiq_susp_log_level, "%s", __func__);
+
+	if (use_type == USE_TYPE_VCHIQ) {
+		sprintf(entity, "VCHIQ:   ");
+		entity_uc = &arm_state->peer_use_count;
+	} else if (service) {
+		sprintf(entity, "%c%c%c%c:%03d",
+			VCHIQ_FOURCC_AS_4CHARS(service->base.fourcc),
+			service->client_id);
+		entity_uc = &service->service_use_count;
+	} else {
+		vchiq_log_error(vchiq_susp_log_level, "%s null service "
+				"ptr", __func__);
+		ret = VCHIQ_ERROR;
+		goto out;
+	}
+
+	write_lock_bh(&arm_state->susp_res_lock);
+	while (arm_state->resume_blocked) {
+		/* If we call 'use' while force suspend is waiting for suspend,
+		 * then we're about to block the thread which the force is
+		 * waiting to complete, so we're bound to just time out. In this
+		 * case, set the suspend state such that the wait will be
+		 * canceled, so we can complete as quickly as possible. */
+		if (arm_state->resume_blocked && arm_state->vc_suspend_state ==
+				VC_SUSPEND_IDLE) {
+			set_suspend_state(arm_state, VC_SUSPEND_FORCE_CANCELED);
+			break;
+		}
+		/* If suspend is already in progress then we need to block */
+		if (!try_wait_for_completion(&arm_state->resume_blocker)) {
+			/* Indicate that there are threads waiting on the resume
+			 * blocker.  These need to be allowed to complete before
+			 * a _second_ call to force suspend can complete,
+			 * otherwise low priority threads might never actually
+			 * continue */
+			arm_state->blocked_count++;
+			write_unlock_bh(&arm_state->susp_res_lock);
+			vchiq_log_info(vchiq_susp_log_level, "%s %s resume "
+				"blocked - waiting...", __func__, entity);
+			if (wait_for_completion_killable(
+					&arm_state->resume_blocker) != 0) {
+				vchiq_log_error(vchiq_susp_log_level, "%s %s "
+					"wait for resume blocker interrupted",
+					__func__, entity);
+				ret = VCHIQ_ERROR;
+				write_lock_bh(&arm_state->susp_res_lock);
+				arm_state->blocked_count--;
+				write_unlock_bh(&arm_state->susp_res_lock);
+				goto out;
+			}
+			vchiq_log_info(vchiq_susp_log_level, "%s %s resume "
+				"unblocked", __func__, entity);
+			write_lock_bh(&arm_state->susp_res_lock);
+			if (--arm_state->blocked_count == 0)
+				complete_all(&arm_state->blocked_blocker);
+		}
+	}
+
+	stop_suspend_timer(arm_state);
+
+	local_uc = ++arm_state->videocore_use_count;
+	local_entity_uc = ++(*entity_uc);
+
+	/* If there's a pending request which hasn't yet been serviced then
+	 * just clear it.  If we're past VC_SUSPEND_REQUESTED state then
+	 * vc_resume_complete will block until we either resume or fail to
+	 * suspend */
+	if (arm_state->vc_suspend_state <= VC_SUSPEND_REQUESTED)
+		set_suspend_state(arm_state, VC_SUSPEND_IDLE);
+
+	if ((use_type != USE_TYPE_SERVICE_NO_RESUME) && need_resume(state)) {
+		set_resume_state(arm_state, VC_RESUME_REQUESTED);
+		vchiq_log_info(vchiq_susp_log_level,
+			"%s %s count %d, state count %d",
+			__func__, entity, local_entity_uc, local_uc);
+		request_poll(state, NULL, 0);
+	} else
+		vchiq_log_trace(vchiq_susp_log_level,
+			"%s %s count %d, state count %d",
+			__func__, entity, *entity_uc, local_uc);
+
+
+	write_unlock_bh(&arm_state->susp_res_lock);
+
+	/* Completion is in a done state when we're not suspended, so this won't
+	 * block for the non-suspended case. */
+	if (!try_wait_for_completion(&arm_state->vc_resume_complete)) {
+		vchiq_log_info(vchiq_susp_log_level, "%s %s wait for resume",
+			__func__, entity);
+		if (wait_for_completion_killable(
+				&arm_state->vc_resume_complete) != 0) {
+			vchiq_log_error(vchiq_susp_log_level, "%s %s wait for "
+				"resume interrupted", __func__, entity);
+			ret = VCHIQ_ERROR;
+			goto out;
+		}
+		vchiq_log_info(vchiq_susp_log_level, "%s %s resumed", __func__,
+			entity);
+	}
+
+	if (ret == VCHIQ_SUCCESS) {
+		VCHIQ_STATUS_T status = VCHIQ_SUCCESS;
+		long ack_cnt = atomic_xchg(&arm_state->ka_use_ack_count, 0);
+		while (ack_cnt && (status == VCHIQ_SUCCESS)) {
+			/* Send the use notify to videocore */
+			status = vchiq_send_remote_use_active(state);
+			if (status == VCHIQ_SUCCESS)
+				ack_cnt--;
+			else
+				atomic_add(ack_cnt,
+					&arm_state->ka_use_ack_count);
+		}
+	}
+
+out:
+	vchiq_log_trace(vchiq_susp_log_level, "%s exit %d", __func__, ret);
+	return ret;
+}
+
+VCHIQ_STATUS_T
+vchiq_release_internal(VCHIQ_STATE_T *state, VCHIQ_SERVICE_T *service)
+{
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+	VCHIQ_STATUS_T ret = VCHIQ_SUCCESS;
+	char entity[16];
+	int *entity_uc;
+	int local_uc, local_entity_uc;
+
+	if (!arm_state)
+		goto out;
+
+	vchiq_log_trace(vchiq_susp_log_level, "%s", __func__);
+
+	if (service) {
+		sprintf(entity, "%c%c%c%c:%03d",
+			VCHIQ_FOURCC_AS_4CHARS(service->base.fourcc),
+			service->client_id);
+		entity_uc = &service->service_use_count;
+	} else {
+		sprintf(entity, "PEER:   ");
+		entity_uc = &arm_state->peer_use_count;
+	}
+
+	write_lock_bh(&arm_state->susp_res_lock);
+	if (!arm_state->videocore_use_count || !(*entity_uc)) {
+		/* Don't use BUG_ON - don't allow user thread to crash kernel */
+		WARN_ON(!arm_state->videocore_use_count);
+		WARN_ON(!(*entity_uc));
+		ret = VCHIQ_ERROR;
+		goto unlock;
+	}
+	local_uc = --arm_state->videocore_use_count;
+	local_entity_uc = --(*entity_uc);
+
+	if (!vchiq_videocore_wanted(state)) {
+		if (vchiq_platform_use_suspend_timer() &&
+				!arm_state->resume_blocked) {
+			/* Only use the timer if we're not trying to force
+			 * suspend (=> resume_blocked) */
+			start_suspend_timer(arm_state);
+		} else {
+			vchiq_log_info(vchiq_susp_log_level,
+				"%s %s count %d, state count %d - suspending",
+				__func__, entity, *entity_uc,
+				arm_state->videocore_use_count);
+			vchiq_arm_vcsuspend(state);
+		}
+	} else
+		vchiq_log_trace(vchiq_susp_log_level,
+			"%s %s count %d, state count %d",
+			__func__, entity, *entity_uc,
+			arm_state->videocore_use_count);
+
+unlock:
+	write_unlock_bh(&arm_state->susp_res_lock);
+
+out:
+	vchiq_log_trace(vchiq_susp_log_level, "%s exit %d", __func__, ret);
+	return ret;
+}
+
+void
+vchiq_on_remote_use(VCHIQ_STATE_T *state)
+{
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+	vchiq_log_trace(vchiq_susp_log_level, "%s", __func__);
+	atomic_inc(&arm_state->ka_use_count);
+	complete(&arm_state->ka_evt);
+}
+
+void
+vchiq_on_remote_release(VCHIQ_STATE_T *state)
+{
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+	vchiq_log_trace(vchiq_susp_log_level, "%s", __func__);
+	atomic_inc(&arm_state->ka_release_count);
+	complete(&arm_state->ka_evt);
+}
+
+VCHIQ_STATUS_T
+vchiq_use_service_internal(VCHIQ_SERVICE_T *service)
+{
+	return vchiq_use_internal(service->state, service, USE_TYPE_SERVICE);
+}
+
+VCHIQ_STATUS_T
+vchiq_release_service_internal(VCHIQ_SERVICE_T *service)
+{
+	return vchiq_release_internal(service->state, service);
+}
+
+VCHIQ_DEBUGFS_NODE_T *
+vchiq_instance_get_debugfs_node(VCHIQ_INSTANCE_T instance)
+{
+	return &instance->debugfs_node;
+}
+
+int
+vchiq_instance_get_use_count(VCHIQ_INSTANCE_T instance)
+{
+	VCHIQ_SERVICE_T *service;
+	int use_count = 0, i;
+	i = 0;
+	while ((service = next_service_by_instance(instance->state,
+		instance, &i)) != NULL) {
+		use_count += service->service_use_count;
+		unlock_service(service);
+	}
+	return use_count;
+}
+
+int
+vchiq_instance_get_pid(VCHIQ_INSTANCE_T instance)
+{
+	return instance->pid;
+}
+
+int
+vchiq_instance_get_trace(VCHIQ_INSTANCE_T instance)
+{
+	return instance->trace;
+}
+
+void
+vchiq_instance_set_trace(VCHIQ_INSTANCE_T instance, int trace)
+{
+	VCHIQ_SERVICE_T *service;
+	int i;
+	i = 0;
+	while ((service = next_service_by_instance(instance->state,
+		instance, &i)) != NULL) {
+		service->trace = trace;
+		unlock_service(service);
+	}
+	instance->trace = (trace != 0);
+}
+
+static void suspend_timer_callback(unsigned long context)
+{
+	VCHIQ_STATE_T *state = (VCHIQ_STATE_T *)context;
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+	if (!arm_state)
+		goto out;
+	vchiq_log_info(vchiq_susp_log_level,
+		"%s - suspend timer expired - check suspend", __func__);
+	vchiq_check_suspend(state);
+out:
+	return;
+}
+
+VCHIQ_STATUS_T
+vchiq_use_service_no_resume(VCHIQ_SERVICE_HANDLE_T handle)
+{
+	VCHIQ_STATUS_T ret = VCHIQ_ERROR;
+	VCHIQ_SERVICE_T *service = find_service_by_handle(handle);
+	if (service) {
+		ret = vchiq_use_internal(service->state, service,
+				USE_TYPE_SERVICE_NO_RESUME);
+		unlock_service(service);
+	}
+	return ret;
+}
+
+VCHIQ_STATUS_T
+vchiq_use_service(VCHIQ_SERVICE_HANDLE_T handle)
+{
+	VCHIQ_STATUS_T ret = VCHIQ_ERROR;
+	VCHIQ_SERVICE_T *service = find_service_by_handle(handle);
+	if (service) {
+		ret = vchiq_use_internal(service->state, service,
+				USE_TYPE_SERVICE);
+		unlock_service(service);
+	}
+	return ret;
+}
+
+VCHIQ_STATUS_T
+vchiq_release_service(VCHIQ_SERVICE_HANDLE_T handle)
+{
+	VCHIQ_STATUS_T ret = VCHIQ_ERROR;
+	VCHIQ_SERVICE_T *service = find_service_by_handle(handle);
+	if (service) {
+		ret = vchiq_release_internal(service->state, service);
+		unlock_service(service);
+	}
+	return ret;
+}
+
+void
+vchiq_dump_service_use_state(VCHIQ_STATE_T *state)
+{
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+	int i, j = 0;
+	/* Only dump 64 services */
+	static const int local_max_services = 64;
+	/* If there's more than 64 services, only dump ones with
+	 * non-zero counts */
+	int only_nonzero = 0;
+	static const char *nz = "<-- preventing suspend";
+
+	enum vc_suspend_status vc_suspend_state;
+	enum vc_resume_status  vc_resume_state;
+	int peer_count;
+	int vc_use_count;
+	int active_services;
+	struct service_data_struct {
+		int fourcc;
+		int clientid;
+		int use_count;
+	} service_data[local_max_services];
+
+	if (!arm_state)
+		return;
+
+	read_lock_bh(&arm_state->susp_res_lock);
+	vc_suspend_state = arm_state->vc_suspend_state;
+	vc_resume_state  = arm_state->vc_resume_state;
+	peer_count = arm_state->peer_use_count;
+	vc_use_count = arm_state->videocore_use_count;
+	active_services = state->unused_service;
+	if (active_services > local_max_services)
+		only_nonzero = 1;
+
+	for (i = 0; (i < active_services) && (j < local_max_services); i++) {
+		VCHIQ_SERVICE_T *service_ptr = state->services[i];
+		if (!service_ptr)
+			continue;
+
+		if (only_nonzero && !service_ptr->service_use_count)
+			continue;
+
+		if (service_ptr->srvstate != VCHIQ_SRVSTATE_FREE) {
+			service_data[j].fourcc = service_ptr->base.fourcc;
+			service_data[j].clientid = service_ptr->client_id;
+			service_data[j++].use_count = service_ptr->
+							service_use_count;
+		}
+	}
+
+	read_unlock_bh(&arm_state->susp_res_lock);
+
+	vchiq_log_warning(vchiq_susp_log_level,
+		"-- Videcore suspend state: %s --",
+		suspend_state_names[vc_suspend_state + VC_SUSPEND_NUM_OFFSET]);
+	vchiq_log_warning(vchiq_susp_log_level,
+		"-- Videcore resume state: %s --",
+		resume_state_names[vc_resume_state + VC_RESUME_NUM_OFFSET]);
+
+	if (only_nonzero)
+		vchiq_log_warning(vchiq_susp_log_level, "Too many active "
+			"services (%d).  Only dumping up to first %d services "
+			"with non-zero use-count", active_services,
+			local_max_services);
+
+	for (i = 0; i < j; i++) {
+		vchiq_log_warning(vchiq_susp_log_level,
+			"----- %c%c%c%c:%d service count %d %s",
+			VCHIQ_FOURCC_AS_4CHARS(service_data[i].fourcc),
+			service_data[i].clientid,
+			service_data[i].use_count,
+			service_data[i].use_count ? nz : "");
+	}
+	vchiq_log_warning(vchiq_susp_log_level,
+		"----- VCHIQ use count count %d", peer_count);
+	vchiq_log_warning(vchiq_susp_log_level,
+		"--- Overall vchiq instance use count %d", vc_use_count);
+
+	vchiq_dump_platform_use_state(state);
+}
+
+VCHIQ_STATUS_T
+vchiq_check_service(VCHIQ_SERVICE_T *service)
+{
+	VCHIQ_ARM_STATE_T *arm_state;
+	VCHIQ_STATUS_T ret = VCHIQ_ERROR;
+
+	if (!service || !service->state)
+		goto out;
+
+	vchiq_log_trace(vchiq_susp_log_level, "%s", __func__);
+
+	arm_state = vchiq_platform_get_arm_state(service->state);
+
+	read_lock_bh(&arm_state->susp_res_lock);
+	if (service->service_use_count)
+		ret = VCHIQ_SUCCESS;
+	read_unlock_bh(&arm_state->susp_res_lock);
+
+	if (ret == VCHIQ_ERROR) {
+		vchiq_log_error(vchiq_susp_log_level,
+			"%s ERROR - %c%c%c%c:%d service count %d, "
+			"state count %d, videocore suspend state %s", __func__,
+			VCHIQ_FOURCC_AS_4CHARS(service->base.fourcc),
+			service->client_id, service->service_use_count,
+			arm_state->videocore_use_count,
+			suspend_state_names[arm_state->vc_suspend_state +
+						VC_SUSPEND_NUM_OFFSET]);
+		vchiq_dump_service_use_state(service->state);
+	}
+out:
+	return ret;
+}
+
+/* stub functions */
+void vchiq_on_remote_use_active(VCHIQ_STATE_T *state)
+{
+	(void)state;
+}
+
+void vchiq_platform_conn_state_changed(VCHIQ_STATE_T *state,
+	VCHIQ_CONNSTATE_T oldstate, VCHIQ_CONNSTATE_T newstate)
+{
+	VCHIQ_ARM_STATE_T *arm_state = vchiq_platform_get_arm_state(state);
+	vchiq_log_info(vchiq_susp_log_level, "%d: %s->%s", state->id,
+		get_conn_state_name(oldstate), get_conn_state_name(newstate));
+	if (state->conn_state == VCHIQ_CONNSTATE_CONNECTED) {
+		write_lock_bh(&arm_state->susp_res_lock);
+		if (!arm_state->first_connect) {
+			char threadname[10];
+			arm_state->first_connect = 1;
+			write_unlock_bh(&arm_state->susp_res_lock);
+			snprintf(threadname, sizeof(threadname), "VCHIQka-%d",
+				state->id);
+			arm_state->ka_thread = kthread_create(
+				&vchiq_keepalive_thread_func,
+				(void *)state,
+				threadname);
+			if (arm_state->ka_thread == NULL) {
+				vchiq_log_error(vchiq_susp_log_level,
+					"vchiq: FATAL: couldn't create thread %s",
+					threadname);
+			} else {
+				wake_up_process(arm_state->ka_thread);
+			}
+		} else
+			write_unlock_bh(&arm_state->susp_res_lock);
+	}
+}
+
+
+/****************************************************************************
+*
+*   vchiq_init - called when the module is loaded.
+*
+***************************************************************************/
+
+static int __init
+vchiq_init(void)
+{
+	int err;
+	void *ptr_err;
+
+	/* create debugfs entries */
+	err = vchiq_debugfs_init();
+	if (err != 0)
+		goto failed_debugfs_init;
+
+	err = alloc_chrdev_region(&vchiq_devid, VCHIQ_MINOR, 1, DEVICE_NAME);
+	if (err != 0) {
+		vchiq_log_error(vchiq_arm_log_level,
+			"Unable to allocate device number");
+		goto failed_alloc_chrdev;
+	}
+	cdev_init(&vchiq_cdev, &vchiq_fops);
+	vchiq_cdev.owner = THIS_MODULE;
+	err = cdev_add(&vchiq_cdev, vchiq_devid, 1);
+	if (err != 0) {
+		vchiq_log_error(vchiq_arm_log_level,
+			"Unable to register device");
+		goto failed_cdev_add;
+	}
+
+	/* create sysfs entries */
+	vchiq_class = class_create(THIS_MODULE, DEVICE_NAME);
+	ptr_err = vchiq_class;
+	if (IS_ERR(ptr_err))
+		goto failed_class_create;
+
+	vchiq_dev = device_create(vchiq_class, NULL,
+		vchiq_devid, NULL, "vchiq");
+	ptr_err = vchiq_dev;
+	if (IS_ERR(ptr_err))
+		goto failed_device_create;
+
+	err = vchiq_platform_init(&g_state);
+	if (err != 0)
+		goto failed_platform_init;
+
+	vchiq_log_info(vchiq_arm_log_level,
+		"vchiq: initialised - version %d (min %d), device %d.%d",
+		VCHIQ_VERSION, VCHIQ_VERSION_MIN,
+		MAJOR(vchiq_devid), MINOR(vchiq_devid));
+
+	return 0;
+
+failed_platform_init:
+	device_destroy(vchiq_class, vchiq_devid);
+failed_device_create:
+	class_destroy(vchiq_class);
+failed_class_create:
+	cdev_del(&vchiq_cdev);
+	err = PTR_ERR(ptr_err);
+failed_cdev_add:
+	unregister_chrdev_region(vchiq_devid, 1);
+failed_alloc_chrdev:
+	vchiq_debugfs_deinit();
+failed_debugfs_init:
+	vchiq_log_warning(vchiq_arm_log_level, "could not load vchiq");
+	return err;
+}
+
+/****************************************************************************
+*
+*   vchiq_exit - called when the module is unloaded.
+*
+***************************************************************************/
+
+static void __exit
+vchiq_exit(void)
+{
+	vchiq_platform_exit(&g_state);
+	device_destroy(vchiq_class, vchiq_devid);
+	class_destroy(vchiq_class);
+	cdev_del(&vchiq_cdev);
+	unregister_chrdev_region(vchiq_devid, 1);
+}
+
+module_init(vchiq_init);
+module_exit(vchiq_exit);
+MODULE_LICENSE("GPL");
+MODULE_AUTHOR("Broadcom Corporation");
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_arm.h
@@ -0,0 +1,223 @@
+/**
+ * Copyright (c) 2014 Raspberry Pi (Trading) Ltd. All rights reserved.
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHIQ_ARM_H
+#define VCHIQ_ARM_H
+
+#include <linux/mutex.h>
+#include <linux/semaphore.h>
+#include <linux/atomic.h>
+#include "vchiq_core.h"
+#include "vchiq_debugfs.h"
+
+
+enum vc_suspend_status {
+	VC_SUSPEND_FORCE_CANCELED = -3, /* Force suspend canceled, too busy */
+	VC_SUSPEND_REJECTED = -2,  /* Videocore rejected suspend request */
+	VC_SUSPEND_FAILED = -1,    /* Videocore suspend failed */
+	VC_SUSPEND_IDLE = 0,       /* VC active, no suspend actions */
+	VC_SUSPEND_REQUESTED,      /* User has requested suspend */
+	VC_SUSPEND_IN_PROGRESS,    /* Slot handler has recvd suspend request */
+	VC_SUSPEND_SUSPENDED       /* Videocore suspend succeeded */
+};
+
+enum vc_resume_status {
+	VC_RESUME_FAILED = -1, /* Videocore resume failed */
+	VC_RESUME_IDLE = 0,    /* VC suspended, no resume actions */
+	VC_RESUME_REQUESTED,   /* User has requested resume */
+	VC_RESUME_IN_PROGRESS, /* Slot handler has received resume request */
+	VC_RESUME_RESUMED      /* Videocore resumed successfully (active) */
+};
+
+
+enum USE_TYPE_E {
+	USE_TYPE_SERVICE,
+	USE_TYPE_SERVICE_NO_RESUME,
+	USE_TYPE_VCHIQ
+};
+
+
+
+typedef struct vchiq_arm_state_struct {
+	/* Keepalive-related data */
+	struct task_struct *ka_thread;
+	struct completion ka_evt;
+	atomic_t ka_use_count;
+	atomic_t ka_use_ack_count;
+	atomic_t ka_release_count;
+
+	struct completion vc_suspend_complete;
+	struct completion vc_resume_complete;
+
+	rwlock_t susp_res_lock;
+	enum vc_suspend_status vc_suspend_state;
+	enum vc_resume_status vc_resume_state;
+
+	unsigned int wake_address;
+
+	struct timer_list suspend_timer;
+	int suspend_timer_timeout;
+	int suspend_timer_running;
+
+	/* Global use count for videocore.
+	** This is equal to the sum of the use counts for all services.  When
+	** this hits zero the videocore suspend procedure will be initiated.
+	*/
+	int videocore_use_count;
+
+	/* Use count to track requests from videocore peer.
+	** This use count is not associated with a service, so needs to be
+	** tracked separately with the state.
+	*/
+	int peer_use_count;
+
+	/* Flag to indicate whether resume is blocked.  This happens when the
+	** ARM is suspending
+	*/
+	struct completion resume_blocker;
+	int resume_blocked;
+	struct completion blocked_blocker;
+	int blocked_count;
+
+	int autosuspend_override;
+
+	/* Flag to indicate that the first vchiq connect has made it through.
+	** This means that both sides should be fully ready, and we should
+	** be able to suspend after this point.
+	*/
+	int first_connect;
+
+	unsigned long long suspend_start_time;
+	unsigned long long sleep_start_time;
+	unsigned long long resume_start_time;
+	unsigned long long last_wake_time;
+
+} VCHIQ_ARM_STATE_T;
+
+extern int vchiq_arm_log_level;
+extern int vchiq_susp_log_level;
+
+extern int __init
+vchiq_platform_init(VCHIQ_STATE_T *state);
+
+extern void __exit
+vchiq_platform_exit(VCHIQ_STATE_T *state);
+
+extern VCHIQ_STATE_T *
+vchiq_get_state(void);
+
+extern VCHIQ_STATUS_T
+vchiq_arm_vcsuspend(VCHIQ_STATE_T *state);
+
+extern VCHIQ_STATUS_T
+vchiq_arm_force_suspend(VCHIQ_STATE_T *state);
+
+extern int
+vchiq_arm_allow_resume(VCHIQ_STATE_T *state);
+
+extern VCHIQ_STATUS_T
+vchiq_arm_vcresume(VCHIQ_STATE_T *state);
+
+extern VCHIQ_STATUS_T
+vchiq_arm_init_state(VCHIQ_STATE_T *state, VCHIQ_ARM_STATE_T *arm_state);
+
+extern int
+vchiq_check_resume(VCHIQ_STATE_T *state);
+
+extern void
+vchiq_check_suspend(VCHIQ_STATE_T *state);
+ VCHIQ_STATUS_T
+vchiq_use_service(VCHIQ_SERVICE_HANDLE_T handle);
+
+extern VCHIQ_STATUS_T
+vchiq_release_service(VCHIQ_SERVICE_HANDLE_T handle);
+
+extern VCHIQ_STATUS_T
+vchiq_check_service(VCHIQ_SERVICE_T *service);
+
+extern VCHIQ_STATUS_T
+vchiq_platform_suspend(VCHIQ_STATE_T *state);
+
+extern int
+vchiq_platform_videocore_wanted(VCHIQ_STATE_T *state);
+
+extern int
+vchiq_platform_use_suspend_timer(void);
+
+extern void
+vchiq_dump_platform_use_state(VCHIQ_STATE_T *state);
+
+extern void
+vchiq_dump_service_use_state(VCHIQ_STATE_T *state);
+
+extern VCHIQ_ARM_STATE_T*
+vchiq_platform_get_arm_state(VCHIQ_STATE_T *state);
+
+extern int
+vchiq_videocore_wanted(VCHIQ_STATE_T *state);
+
+extern VCHIQ_STATUS_T
+vchiq_use_internal(VCHIQ_STATE_T *state, VCHIQ_SERVICE_T *service,
+		enum USE_TYPE_E use_type);
+extern VCHIQ_STATUS_T
+vchiq_release_internal(VCHIQ_STATE_T *state, VCHIQ_SERVICE_T *service);
+
+extern VCHIQ_DEBUGFS_NODE_T *
+vchiq_instance_get_debugfs_node(VCHIQ_INSTANCE_T instance);
+
+extern int
+vchiq_instance_get_use_count(VCHIQ_INSTANCE_T instance);
+
+extern int
+vchiq_instance_get_pid(VCHIQ_INSTANCE_T instance);
+
+extern int
+vchiq_instance_get_trace(VCHIQ_INSTANCE_T instance);
+
+extern void
+vchiq_instance_set_trace(VCHIQ_INSTANCE_T instance, int trace);
+
+extern void
+set_suspend_state(VCHIQ_ARM_STATE_T *arm_state,
+	enum vc_suspend_status new_state);
+
+extern void
+set_resume_state(VCHIQ_ARM_STATE_T *arm_state,
+	enum vc_resume_status new_state);
+
+extern void
+start_suspend_timer(VCHIQ_ARM_STATE_T *arm_state);
+
+
+#endif /* VCHIQ_ARM_H */
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_build_info.h
@@ -0,0 +1,37 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+const char *vchiq_get_build_hostname(void);
+const char *vchiq_get_build_version(void);
+const char *vchiq_get_build_time(void);
+const char *vchiq_get_build_date(void);
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_cfg.h
@@ -0,0 +1,66 @@
+/**
+ * Copyright (c) 2010-2014 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHIQ_CFG_H
+#define VCHIQ_CFG_H
+
+#define VCHIQ_MAGIC              VCHIQ_MAKE_FOURCC('V', 'C', 'H', 'I')
+/* The version of VCHIQ - change with any non-trivial change */
+#define VCHIQ_VERSION            7
+/* The minimum compatible version - update to match VCHIQ_VERSION with any
+** incompatible change */
+#define VCHIQ_VERSION_MIN        3
+
+/* The version that introduced the VCHIQ_IOC_LIB_VERSION ioctl */
+#define VCHIQ_VERSION_LIB_VERSION 7
+
+/* The version that introduced the VCHIQ_IOC_CLOSE_DELIVERED ioctl */
+#define VCHIQ_VERSION_CLOSE_DELIVERED 7
+
+#define VCHIQ_MAX_STATES         1
+#define VCHIQ_MAX_SERVICES       4096
+#define VCHIQ_MAX_SLOTS          128
+#define VCHIQ_MAX_SLOTS_PER_SIDE 64
+
+#define VCHIQ_NUM_CURRENT_BULKS        32
+#define VCHIQ_NUM_SERVICE_BULKS        4
+
+#ifndef VCHIQ_ENABLE_DEBUG
+#define VCHIQ_ENABLE_DEBUG             1
+#endif
+
+#ifndef VCHIQ_ENABLE_STATS
+#define VCHIQ_ENABLE_STATS             1
+#endif
+
+#endif /* VCHIQ_CFG_H */
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_connected.c
@@ -0,0 +1,119 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#include "vchiq_connected.h"
+#include "vchiq_core.h"
+#include <linux/module.h>
+#include <linux/mutex.h>
+
+#define  MAX_CALLBACKS  10
+
+static   int                        g_connected;
+static   int                        g_num_deferred_callbacks;
+static   VCHIQ_CONNECTED_CALLBACK_T g_deferred_callback[MAX_CALLBACKS];
+static   int                        g_once_init;
+static   struct mutex               g_connected_mutex;
+
+/****************************************************************************
+*
+* Function to initialize our lock.
+*
+***************************************************************************/
+
+static void connected_init(void)
+{
+	if (!g_once_init) {
+		mutex_init(&g_connected_mutex);
+		g_once_init = 1;
+	}
+}
+
+/****************************************************************************
+*
+* This function is used to defer initialization until the vchiq stack is
+* initialized. If the stack is already initialized, then the callback will
+* be made immediately, otherwise it will be deferred until
+* vchiq_call_connected_callbacks is called.
+*
+***************************************************************************/
+
+void vchiq_add_connected_callback(VCHIQ_CONNECTED_CALLBACK_T callback)
+{
+	connected_init();
+
+	if (mutex_lock_interruptible(&g_connected_mutex) != 0)
+		return;
+
+	if (g_connected)
+		/* We're already connected. Call the callback immediately. */
+
+		callback();
+	else {
+		if (g_num_deferred_callbacks >= MAX_CALLBACKS)
+			vchiq_log_error(vchiq_core_log_level,
+				"There already %d callback registered - "
+				"please increase MAX_CALLBACKS",
+				g_num_deferred_callbacks);
+		else {
+			g_deferred_callback[g_num_deferred_callbacks] =
+				callback;
+			g_num_deferred_callbacks++;
+		}
+	}
+	mutex_unlock(&g_connected_mutex);
+}
+
+/****************************************************************************
+*
+* This function is called by the vchiq stack once it has been connected to
+* the videocore and clients can start to use the stack.
+*
+***************************************************************************/
+
+void vchiq_call_connected_callbacks(void)
+{
+	int i;
+
+	connected_init();
+
+	if (mutex_lock_interruptible(&g_connected_mutex) != 0)
+		return;
+
+	for (i = 0; i <  g_num_deferred_callbacks; i++)
+		g_deferred_callback[i]();
+
+	g_num_deferred_callbacks = 0;
+	g_connected = 1;
+	mutex_unlock(&g_connected_mutex);
+}
+EXPORT_SYMBOL(vchiq_add_connected_callback);
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_connected.h
@@ -0,0 +1,50 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHIQ_CONNECTED_H
+#define VCHIQ_CONNECTED_H
+
+/* ---- Include Files ----------------------------------------------------- */
+
+/* ---- Constants and Types ---------------------------------------------- */
+
+typedef void (*VCHIQ_CONNECTED_CALLBACK_T)(void);
+
+/* ---- Variable Externs ------------------------------------------------- */
+
+/* ---- Function Prototypes ---------------------------------------------- */
+
+void vchiq_add_connected_callback(VCHIQ_CONNECTED_CALLBACK_T callback);
+void vchiq_call_connected_callbacks(void);
+
+#endif /* VCHIQ_CONNECTED_H */
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_core.c
@@ -0,0 +1,3861 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#include "vchiq_core.h"
+
+#define VCHIQ_SLOT_HANDLER_STACK 8192
+
+#define HANDLE_STATE_SHIFT 12
+
+#define SLOT_INFO_FROM_INDEX(state, index) (state->slot_info + (index))
+#define SLOT_DATA_FROM_INDEX(state, index) (state->slot_data + (index))
+#define SLOT_INDEX_FROM_DATA(state, data) \
+	(((unsigned int)((char *)data - (char *)state->slot_data)) / \
+	VCHIQ_SLOT_SIZE)
+#define SLOT_INDEX_FROM_INFO(state, info) \
+	((unsigned int)(info - state->slot_info))
+#define SLOT_QUEUE_INDEX_FROM_POS(pos) \
+	((int)((unsigned int)(pos) / VCHIQ_SLOT_SIZE))
+
+#define BULK_INDEX(x) (x & (VCHIQ_NUM_SERVICE_BULKS - 1))
+
+#define SRVTRACE_LEVEL(srv) \
+	(((srv) && (srv)->trace) ? VCHIQ_LOG_TRACE : vchiq_core_msg_log_level)
+#define SRVTRACE_ENABLED(srv, lev) \
+	(((srv) && (srv)->trace) || (vchiq_core_msg_log_level >= (lev)))
+
+struct vchiq_open_payload {
+	int fourcc;
+	int client_id;
+	short version;
+	short version_min;
+};
+
+struct vchiq_openack_payload {
+	short version;
+};
+
+/* we require this for consistency between endpoints */
+vchiq_static_assert(sizeof(VCHIQ_HEADER_T) == 8);
+vchiq_static_assert(IS_POW2(sizeof(VCHIQ_HEADER_T)));
+vchiq_static_assert(IS_POW2(VCHIQ_NUM_CURRENT_BULKS));
+vchiq_static_assert(IS_POW2(VCHIQ_NUM_SERVICE_BULKS));
+vchiq_static_assert(IS_POW2(VCHIQ_MAX_SERVICES));
+vchiq_static_assert(VCHIQ_VERSION >= VCHIQ_VERSION_MIN);
+
+/* Run time control of log level, based on KERN_XXX level. */
+int vchiq_core_log_level = VCHIQ_LOG_DEFAULT;
+int vchiq_core_msg_log_level = VCHIQ_LOG_DEFAULT;
+int vchiq_sync_log_level = VCHIQ_LOG_DEFAULT;
+
+static atomic_t pause_bulks_count = ATOMIC_INIT(0);
+
+static DEFINE_SPINLOCK(service_spinlock);
+DEFINE_SPINLOCK(bulk_waiter_spinlock);
+DEFINE_SPINLOCK(quota_spinlock);
+
+VCHIQ_STATE_T *vchiq_states[VCHIQ_MAX_STATES];
+static unsigned int handle_seq;
+
+static const char *const srvstate_names[] = {
+	"FREE",
+	"HIDDEN",
+	"LISTENING",
+	"OPENING",
+	"OPEN",
+	"OPENSYNC",
+	"CLOSESENT",
+	"CLOSERECVD",
+	"CLOSEWAIT",
+	"CLOSED"
+};
+
+static const char *const reason_names[] = {
+	"SERVICE_OPENED",
+	"SERVICE_CLOSED",
+	"MESSAGE_AVAILABLE",
+	"BULK_TRANSMIT_DONE",
+	"BULK_RECEIVE_DONE",
+	"BULK_TRANSMIT_ABORTED",
+	"BULK_RECEIVE_ABORTED"
+};
+
+static const char *const conn_state_names[] = {
+	"DISCONNECTED",
+	"CONNECTING",
+	"CONNECTED",
+	"PAUSING",
+	"PAUSE_SENT",
+	"PAUSED",
+	"RESUMING",
+	"PAUSE_TIMEOUT",
+	"RESUME_TIMEOUT"
+};
+
+
+static void
+release_message_sync(VCHIQ_STATE_T *state, VCHIQ_HEADER_T *header);
+
+static const char *msg_type_str(unsigned int msg_type)
+{
+	switch (msg_type) {
+	case VCHIQ_MSG_PADDING:       return "PADDING";
+	case VCHIQ_MSG_CONNECT:       return "CONNECT";
+	case VCHIQ_MSG_OPEN:          return "OPEN";
+	case VCHIQ_MSG_OPENACK:       return "OPENACK";
+	case VCHIQ_MSG_CLOSE:         return "CLOSE";
+	case VCHIQ_MSG_DATA:          return "DATA";
+	case VCHIQ_MSG_BULK_RX:       return "BULK_RX";
+	case VCHIQ_MSG_BULK_TX:       return "BULK_TX";
+	case VCHIQ_MSG_BULK_RX_DONE:  return "BULK_RX_DONE";
+	case VCHIQ_MSG_BULK_TX_DONE:  return "BULK_TX_DONE";
+	case VCHIQ_MSG_PAUSE:         return "PAUSE";
+	case VCHIQ_MSG_RESUME:        return "RESUME";
+	case VCHIQ_MSG_REMOTE_USE:    return "REMOTE_USE";
+	case VCHIQ_MSG_REMOTE_RELEASE:      return "REMOTE_RELEASE";
+	case VCHIQ_MSG_REMOTE_USE_ACTIVE:   return "REMOTE_USE_ACTIVE";
+	}
+	return "???";
+}
+
+static inline void
+vchiq_set_service_state(VCHIQ_SERVICE_T *service, int newstate)
+{
+	vchiq_log_info(vchiq_core_log_level, "%d: srv:%d %s->%s",
+		service->state->id, service->localport,
+		srvstate_names[service->srvstate],
+		srvstate_names[newstate]);
+	service->srvstate = newstate;
+}
+
+VCHIQ_SERVICE_T *
+find_service_by_handle(VCHIQ_SERVICE_HANDLE_T handle)
+{
+	VCHIQ_SERVICE_T *service;
+
+	spin_lock(&service_spinlock);
+	service = handle_to_service(handle);
+	if (service && (service->srvstate != VCHIQ_SRVSTATE_FREE) &&
+		(service->handle == handle)) {
+		BUG_ON(service->ref_count == 0);
+		service->ref_count++;
+	} else
+		service = NULL;
+	spin_unlock(&service_spinlock);
+
+	if (!service)
+		vchiq_log_info(vchiq_core_log_level,
+			"Invalid service handle 0x%x", handle);
+
+	return service;
+}
+
+VCHIQ_SERVICE_T *
+find_service_by_port(VCHIQ_STATE_T *state, int localport)
+{
+	VCHIQ_SERVICE_T *service = NULL;
+	if ((unsigned int)localport <= VCHIQ_PORT_MAX) {
+		spin_lock(&service_spinlock);
+		service = state->services[localport];
+		if (service && (service->srvstate != VCHIQ_SRVSTATE_FREE)) {
+			BUG_ON(service->ref_count == 0);
+			service->ref_count++;
+		} else
+			service = NULL;
+		spin_unlock(&service_spinlock);
+	}
+
+	if (!service)
+		vchiq_log_info(vchiq_core_log_level,
+			"Invalid port %d", localport);
+
+	return service;
+}
+
+VCHIQ_SERVICE_T *
+find_service_for_instance(VCHIQ_INSTANCE_T instance,
+	VCHIQ_SERVICE_HANDLE_T handle) {
+	VCHIQ_SERVICE_T *service;
+
+	spin_lock(&service_spinlock);
+	service = handle_to_service(handle);
+	if (service && (service->srvstate != VCHIQ_SRVSTATE_FREE) &&
+		(service->handle == handle) &&
+		(service->instance == instance)) {
+		BUG_ON(service->ref_count == 0);
+		service->ref_count++;
+	} else
+		service = NULL;
+	spin_unlock(&service_spinlock);
+
+	if (!service)
+		vchiq_log_info(vchiq_core_log_level,
+			"Invalid service handle 0x%x", handle);
+
+	return service;
+}
+
+VCHIQ_SERVICE_T *
+find_closed_service_for_instance(VCHIQ_INSTANCE_T instance,
+	VCHIQ_SERVICE_HANDLE_T handle) {
+	VCHIQ_SERVICE_T *service;
+
+	spin_lock(&service_spinlock);
+	service = handle_to_service(handle);
+	if (service &&
+		((service->srvstate == VCHIQ_SRVSTATE_FREE) ||
+		 (service->srvstate == VCHIQ_SRVSTATE_CLOSED)) &&
+		(service->handle == handle) &&
+		(service->instance == instance)) {
+		BUG_ON(service->ref_count == 0);
+		service->ref_count++;
+	} else
+		service = NULL;
+	spin_unlock(&service_spinlock);
+
+	if (!service)
+		vchiq_log_info(vchiq_core_log_level,
+			"Invalid service handle 0x%x", handle);
+
+	return service;
+}
+
+VCHIQ_SERVICE_T *
+next_service_by_instance(VCHIQ_STATE_T *state, VCHIQ_INSTANCE_T instance,
+	int *pidx)
+{
+	VCHIQ_SERVICE_T *service = NULL;
+	int idx = *pidx;
+
+	spin_lock(&service_spinlock);
+	while (idx < state->unused_service) {
+		VCHIQ_SERVICE_T *srv = state->services[idx++];
+		if (srv && (srv->srvstate != VCHIQ_SRVSTATE_FREE) &&
+			(srv->instance == instance)) {
+			service = srv;
+			BUG_ON(service->ref_count == 0);
+			service->ref_count++;
+			break;
+		}
+	}
+	spin_unlock(&service_spinlock);
+
+	*pidx = idx;
+
+	return service;
+}
+
+void
+lock_service(VCHIQ_SERVICE_T *service)
+{
+	spin_lock(&service_spinlock);
+	BUG_ON(!service || (service->ref_count == 0));
+	if (service)
+		service->ref_count++;
+	spin_unlock(&service_spinlock);
+}
+
+void
+unlock_service(VCHIQ_SERVICE_T *service)
+{
+	VCHIQ_STATE_T *state = service->state;
+	spin_lock(&service_spinlock);
+	BUG_ON(!service || (service->ref_count == 0));
+	if (service && service->ref_count) {
+		service->ref_count--;
+		if (!service->ref_count) {
+			BUG_ON(service->srvstate != VCHIQ_SRVSTATE_FREE);
+			state->services[service->localport] = NULL;
+		} else
+			service = NULL;
+	}
+	spin_unlock(&service_spinlock);
+
+	if (service && service->userdata_term)
+		service->userdata_term(service->base.userdata);
+
+	kfree(service);
+}
+
+int
+vchiq_get_client_id(VCHIQ_SERVICE_HANDLE_T handle)
+{
+	VCHIQ_SERVICE_T *service = find_service_by_handle(handle);
+	int id;
+
+	id = service ? service->client_id : 0;
+	if (service)
+		unlock_service(service);
+
+	return id;
+}
+
+void *
+vchiq_get_service_userdata(VCHIQ_SERVICE_HANDLE_T handle)
+{
+	VCHIQ_SERVICE_T *service = handle_to_service(handle);
+
+	return service ? service->base.userdata : NULL;
+}
+
+int
+vchiq_get_service_fourcc(VCHIQ_SERVICE_HANDLE_T handle)
+{
+	VCHIQ_SERVICE_T *service = handle_to_service(handle);
+
+	return service ? service->base.fourcc : 0;
+}
+
+static void
+mark_service_closing_internal(VCHIQ_SERVICE_T *service, int sh_thread)
+{
+	VCHIQ_STATE_T *state = service->state;
+	VCHIQ_SERVICE_QUOTA_T *service_quota;
+
+	service->closing = 1;
+
+	/* Synchronise with other threads. */
+	mutex_lock(&state->recycle_mutex);
+	mutex_unlock(&state->recycle_mutex);
+	if (!sh_thread || (state->conn_state != VCHIQ_CONNSTATE_PAUSE_SENT)) {
+		/* If we're pausing then the slot_mutex is held until resume
+		 * by the slot handler.  Therefore don't try to acquire this
+		 * mutex if we're the slot handler and in the pause sent state.
+		 * We don't need to in this case anyway. */
+		mutex_lock(&state->slot_mutex);
+		mutex_unlock(&state->slot_mutex);
+	}
+
+	/* Unblock any sending thread. */
+	service_quota = &state->service_quotas[service->localport];
+	up(&service_quota->quota_event);
+}
+
+static void
+mark_service_closing(VCHIQ_SERVICE_T *service)
+{
+	mark_service_closing_internal(service, 0);
+}
+
+static inline VCHIQ_STATUS_T
+make_service_callback(VCHIQ_SERVICE_T *service, VCHIQ_REASON_T reason,
+	VCHIQ_HEADER_T *header, void *bulk_userdata)
+{
+	VCHIQ_STATUS_T status;
+	vchiq_log_trace(vchiq_core_log_level, "%d: callback:%d (%s, %x, %x)",
+		service->state->id, service->localport, reason_names[reason],
+		(unsigned int)header, (unsigned int)bulk_userdata);
+	status = service->base.callback(reason, header, service->handle,
+		bulk_userdata);
+	if (status == VCHIQ_ERROR) {
+		vchiq_log_warning(vchiq_core_log_level,
+			"%d: ignoring ERROR from callback to service %x",
+			service->state->id, service->handle);
+		status = VCHIQ_SUCCESS;
+	}
+	return status;
+}
+
+inline void
+vchiq_set_conn_state(VCHIQ_STATE_T *state, VCHIQ_CONNSTATE_T newstate)
+{
+	VCHIQ_CONNSTATE_T oldstate = state->conn_state;
+	vchiq_log_info(vchiq_core_log_level, "%d: %s->%s", state->id,
+		conn_state_names[oldstate],
+		conn_state_names[newstate]);
+	state->conn_state = newstate;
+	vchiq_platform_conn_state_changed(state, oldstate, newstate);
+}
+
+static inline void
+remote_event_create(REMOTE_EVENT_T *event)
+{
+	event->armed = 0;
+	/* Don't clear the 'fired' flag because it may already have been set
+	** by the other side. */
+	sema_init(event->event, 0);
+}
+
+static inline void
+remote_event_destroy(REMOTE_EVENT_T *event)
+{
+	(void)event;
+}
+
+static inline int
+remote_event_wait(REMOTE_EVENT_T *event)
+{
+	if (!event->fired) {
+		event->armed = 1;
+		dsb();
+		if (!event->fired) {
+			if (down_interruptible(event->event) != 0) {
+				event->armed = 0;
+				return 0;
+			}
+		}
+		event->armed = 0;
+		wmb();
+	}
+
+	event->fired = 0;
+	return 1;
+}
+
+static inline void
+remote_event_signal_local(REMOTE_EVENT_T *event)
+{
+	event->armed = 0;
+	up(event->event);
+}
+
+static inline void
+remote_event_poll(REMOTE_EVENT_T *event)
+{
+	if (event->fired && event->armed)
+		remote_event_signal_local(event);
+}
+
+void
+remote_event_pollall(VCHIQ_STATE_T *state)
+{
+	remote_event_poll(&state->local->sync_trigger);
+	remote_event_poll(&state->local->sync_release);
+	remote_event_poll(&state->local->trigger);
+	remote_event_poll(&state->local->recycle);
+}
+
+/* Round up message sizes so that any space at the end of a slot is always big
+** enough for a header. This relies on header size being a power of two, which
+** has been verified earlier by a static assertion. */
+
+static inline unsigned int
+calc_stride(unsigned int size)
+{
+	/* Allow room for the header */
+	size += sizeof(VCHIQ_HEADER_T);
+
+	/* Round up */
+	return (size + sizeof(VCHIQ_HEADER_T) - 1) & ~(sizeof(VCHIQ_HEADER_T)
+		- 1);
+}
+
+/* Called by the slot handler thread */
+static VCHIQ_SERVICE_T *
+get_listening_service(VCHIQ_STATE_T *state, int fourcc)
+{
+	int i;
+
+	WARN_ON(fourcc == VCHIQ_FOURCC_INVALID);
+
+	for (i = 0; i < state->unused_service; i++) {
+		VCHIQ_SERVICE_T *service = state->services[i];
+		if (service &&
+			(service->public_fourcc == fourcc) &&
+			((service->srvstate == VCHIQ_SRVSTATE_LISTENING) ||
+			((service->srvstate == VCHIQ_SRVSTATE_OPEN) &&
+			(service->remoteport == VCHIQ_PORT_FREE)))) {
+			lock_service(service);
+			return service;
+		}
+	}
+
+	return NULL;
+}
+
+/* Called by the slot handler thread */
+static VCHIQ_SERVICE_T *
+get_connected_service(VCHIQ_STATE_T *state, unsigned int port)
+{
+	int i;
+	for (i = 0; i < state->unused_service; i++) {
+		VCHIQ_SERVICE_T *service = state->services[i];
+		if (service && (service->srvstate == VCHIQ_SRVSTATE_OPEN)
+			&& (service->remoteport == port)) {
+			lock_service(service);
+			return service;
+		}
+	}
+	return NULL;
+}
+
+inline void
+request_poll(VCHIQ_STATE_T *state, VCHIQ_SERVICE_T *service, int poll_type)
+{
+	uint32_t value;
+
+	if (service) {
+		do {
+			value = atomic_read(&service->poll_flags);
+		} while (atomic_cmpxchg(&service->poll_flags, value,
+			value | (1 << poll_type)) != value);
+
+		do {
+			value = atomic_read(&state->poll_services[
+				service->localport>>5]);
+		} while (atomic_cmpxchg(
+			&state->poll_services[service->localport>>5],
+			value, value | (1 << (service->localport & 0x1f)))
+			!= value);
+	}
+
+	state->poll_needed = 1;
+	wmb();
+
+	/* ... and ensure the slot handler runs. */
+	remote_event_signal_local(&state->local->trigger);
+}
+
+/* Called from queue_message, by the slot handler and application threads,
+** with slot_mutex held */
+static VCHIQ_HEADER_T *
+reserve_space(VCHIQ_STATE_T *state, int space, int is_blocking)
+{
+	VCHIQ_SHARED_STATE_T *local = state->local;
+	int tx_pos = state->local_tx_pos;
+	int slot_space = VCHIQ_SLOT_SIZE - (tx_pos & VCHIQ_SLOT_MASK);
+
+	if (space > slot_space) {
+		VCHIQ_HEADER_T *header;
+		/* Fill the remaining space with padding */
+		WARN_ON(state->tx_data == NULL);
+		header = (VCHIQ_HEADER_T *)
+			(state->tx_data + (tx_pos & VCHIQ_SLOT_MASK));
+		header->msgid = VCHIQ_MSGID_PADDING;
+		header->size = slot_space - sizeof(VCHIQ_HEADER_T);
+
+		tx_pos += slot_space;
+	}
+
+	/* If necessary, get the next slot. */
+	if ((tx_pos & VCHIQ_SLOT_MASK) == 0) {
+		int slot_index;
+
+		/* If there is no free slot... */
+
+		if (down_trylock(&state->slot_available_event) != 0) {
+			/* ...wait for one. */
+
+			VCHIQ_STATS_INC(state, slot_stalls);
+
+			/* But first, flush through the last slot. */
+			state->local_tx_pos = tx_pos;
+			local->tx_pos = tx_pos;
+			remote_event_signal(&state->remote->trigger);
+
+			if (!is_blocking ||
+				(down_interruptible(
+				&state->slot_available_event) != 0))
+				return NULL; /* No space available */
+		}
+
+		BUG_ON(tx_pos ==
+			(state->slot_queue_available * VCHIQ_SLOT_SIZE));
+
+		slot_index = local->slot_queue[
+			SLOT_QUEUE_INDEX_FROM_POS(tx_pos) &
+			VCHIQ_SLOT_QUEUE_MASK];
+		state->tx_data =
+			(char *)SLOT_DATA_FROM_INDEX(state, slot_index);
+	}
+
+	state->local_tx_pos = tx_pos + space;
+
+	return (VCHIQ_HEADER_T *)(state->tx_data + (tx_pos & VCHIQ_SLOT_MASK));
+}
+
+/* Called by the recycle thread. */
+static void
+process_free_queue(VCHIQ_STATE_T *state)
+{
+	VCHIQ_SHARED_STATE_T *local = state->local;
+	BITSET_T service_found[BITSET_SIZE(VCHIQ_MAX_SERVICES)];
+	int slot_queue_available;
+
+	/* Use a read memory barrier to ensure that any state that may have
+	** been modified by another thread is not masked by stale prefetched
+	** values. */
+	rmb();
+
+	/* Find slots which have been freed by the other side, and return them
+	** to the available queue. */
+	slot_queue_available = state->slot_queue_available;
+
+	while (slot_queue_available != local->slot_queue_recycle) {
+		unsigned int pos;
+		int slot_index = local->slot_queue[slot_queue_available++ &
+			VCHIQ_SLOT_QUEUE_MASK];
+		char *data = (char *)SLOT_DATA_FROM_INDEX(state, slot_index);
+		int data_found = 0;
+
+		vchiq_log_trace(vchiq_core_log_level, "%d: pfq %d=%x %x %x",
+			state->id, slot_index, (unsigned int)data,
+			local->slot_queue_recycle, slot_queue_available);
+
+		/* Initialise the bitmask for services which have used this
+		** slot */
+		BITSET_ZERO(service_found);
+
+		pos = 0;
+
+		while (pos < VCHIQ_SLOT_SIZE) {
+			VCHIQ_HEADER_T *header =
+				(VCHIQ_HEADER_T *)(data + pos);
+			int msgid = header->msgid;
+			if (VCHIQ_MSG_TYPE(msgid) == VCHIQ_MSG_DATA) {
+				int port = VCHIQ_MSG_SRCPORT(msgid);
+				VCHIQ_SERVICE_QUOTA_T *service_quota =
+					&state->service_quotas[port];
+				int count;
+				spin_lock(&quota_spinlock);
+				count = service_quota->message_use_count;
+				if (count > 0)
+					service_quota->message_use_count =
+						count - 1;
+				spin_unlock(&quota_spinlock);
+
+				if (count == service_quota->message_quota)
+					/* Signal the service that it
+					** has dropped below its quota
+					*/
+					up(&service_quota->quota_event);
+				else if (count == 0) {
+					vchiq_log_error(vchiq_core_log_level,
+						"service %d "
+						"message_use_count=%d "
+						"(header %x, msgid %x, "
+						"header->msgid %x, "
+						"header->size %x)",
+						port,
+						service_quota->
+							message_use_count,
+						(unsigned int)header, msgid,
+						header->msgid,
+						header->size);
+					WARN(1, "invalid message use count\n");
+				}
+				if (!BITSET_IS_SET(service_found, port)) {
+					/* Set the found bit for this service */
+					BITSET_SET(service_found, port);
+
+					spin_lock(&quota_spinlock);
+					count = service_quota->slot_use_count;
+					if (count > 0)
+						service_quota->slot_use_count =
+							count - 1;
+					spin_unlock(&quota_spinlock);
+
+					if (count > 0) {
+						/* Signal the service in case
+						** it has dropped below its
+						** quota */
+						up(&service_quota->quota_event);
+						vchiq_log_trace(
+							vchiq_core_log_level,
+							"%d: pfq:%d %x@%x - "
+							"slot_use->%d",
+							state->id, port,
+							header->size,
+							(unsigned int)header,
+							count - 1);
+					} else {
+						vchiq_log_error(
+							vchiq_core_log_level,
+								"service %d "
+								"slot_use_count"
+								"=%d (header %x"
+								", msgid %x, "
+								"header->msgid"
+								" %x, header->"
+								"size %x)",
+							port, count,
+							(unsigned int)header,
+							msgid,
+							header->msgid,
+							header->size);
+						WARN(1, "bad slot use count\n");
+					}
+				}
+
+				data_found = 1;
+			}
+
+			pos += calc_stride(header->size);
+			if (pos > VCHIQ_SLOT_SIZE) {
+				vchiq_log_error(vchiq_core_log_level,
+					"pfq - pos %x: header %x, msgid %x, "
+					"header->msgid %x, header->size %x",
+					pos, (unsigned int)header, msgid,
+					header->msgid, header->size);
+				WARN(1, "invalid slot position\n");
+			}
+		}
+
+		if (data_found) {
+			int count;
+			spin_lock(&quota_spinlock);
+			count = state->data_use_count;
+			if (count > 0)
+				state->data_use_count =
+					count - 1;
+			spin_unlock(&quota_spinlock);
+			if (count == state->data_quota)
+				up(&state->data_quota_event);
+		}
+
+		state->slot_queue_available = slot_queue_available;
+		up(&state->slot_available_event);
+	}
+}
+
+/* Called by the slot handler and application threads */
+static VCHIQ_STATUS_T
+queue_message(VCHIQ_STATE_T *state, VCHIQ_SERVICE_T *service,
+	int msgid, const VCHIQ_ELEMENT_T *elements,
+	int count, int size, int is_blocking)
+{
+	VCHIQ_SHARED_STATE_T *local;
+	VCHIQ_SERVICE_QUOTA_T *service_quota = NULL;
+	VCHIQ_HEADER_T *header;
+	int type = VCHIQ_MSG_TYPE(msgid);
+
+	unsigned int stride;
+
+	local = state->local;
+
+	stride = calc_stride(size);
+
+	WARN_ON(!(stride <= VCHIQ_SLOT_SIZE));
+
+	if ((type != VCHIQ_MSG_RESUME) &&
+		(mutex_lock_interruptible(&state->slot_mutex) != 0))
+		return VCHIQ_RETRY;
+
+	if (type == VCHIQ_MSG_DATA) {
+		int tx_end_index;
+
+		BUG_ON(!service);
+
+		if (service->closing) {
+			/* The service has been closed */
+			mutex_unlock(&state->slot_mutex);
+			return VCHIQ_ERROR;
+		}
+
+		service_quota = &state->service_quotas[service->localport];
+
+		spin_lock(&quota_spinlock);
+
+		/* Ensure this service doesn't use more than its quota of
+		** messages or slots */
+		tx_end_index = SLOT_QUEUE_INDEX_FROM_POS(
+			state->local_tx_pos + stride - 1);
+
+		/* Ensure data messages don't use more than their quota of
+		** slots */
+		while ((tx_end_index != state->previous_data_index) &&
+			(state->data_use_count == state->data_quota)) {
+			VCHIQ_STATS_INC(state, data_stalls);
+			spin_unlock(&quota_spinlock);
+			mutex_unlock(&state->slot_mutex);
+
+			if (down_interruptible(&state->data_quota_event)
+				!= 0)
+				return VCHIQ_RETRY;
+
+			mutex_lock(&state->slot_mutex);
+			spin_lock(&quota_spinlock);
+			tx_end_index = SLOT_QUEUE_INDEX_FROM_POS(
+				state->local_tx_pos + stride - 1);
+			if ((tx_end_index == state->previous_data_index) ||
+				(state->data_use_count < state->data_quota)) {
+				/* Pass the signal on to other waiters */
+				up(&state->data_quota_event);
+				break;
+			}
+		}
+
+		while ((service_quota->message_use_count ==
+				service_quota->message_quota) ||
+			((tx_end_index != service_quota->previous_tx_index) &&
+			(service_quota->slot_use_count ==
+				service_quota->slot_quota))) {
+			spin_unlock(&quota_spinlock);
+			vchiq_log_trace(vchiq_core_log_level,
+				"%d: qm:%d %s,%x - quota stall "
+				"(msg %d, slot %d)",
+				state->id, service->localport,
+				msg_type_str(type), size,
+				service_quota->message_use_count,
+				service_quota->slot_use_count);
+			VCHIQ_SERVICE_STATS_INC(service, quota_stalls);
+			mutex_unlock(&state->slot_mutex);
+			if (down_interruptible(&service_quota->quota_event)
+				!= 0)
+				return VCHIQ_RETRY;
+			if (service->closing)
+				return VCHIQ_ERROR;
+			if (mutex_lock_interruptible(&state->slot_mutex) != 0)
+				return VCHIQ_RETRY;
+			if (service->srvstate != VCHIQ_SRVSTATE_OPEN) {
+				/* The service has been closed */
+				mutex_unlock(&state->slot_mutex);
+				return VCHIQ_ERROR;
+			}
+			spin_lock(&quota_spinlock);
+			tx_end_index = SLOT_QUEUE_INDEX_FROM_POS(
+				state->local_tx_pos + stride - 1);
+		}
+
+		spin_unlock(&quota_spinlock);
+	}
+
+	header = reserve_space(state, stride, is_blocking);
+
+	if (!header) {
+		if (service)
+			VCHIQ_SERVICE_STATS_INC(service, slot_stalls);
+		mutex_unlock(&state->slot_mutex);
+		return VCHIQ_RETRY;
+	}
+
+	if (type == VCHIQ_MSG_DATA) {
+		int i, pos;
+		int tx_end_index;
+		int slot_use_count;
+
+		vchiq_log_info(vchiq_core_log_level,
+			"%d: qm %s@%x,%x (%d->%d)",
+			state->id,
+			msg_type_str(VCHIQ_MSG_TYPE(msgid)),
+			(unsigned int)header, size,
+			VCHIQ_MSG_SRCPORT(msgid),
+			VCHIQ_MSG_DSTPORT(msgid));
+
+		BUG_ON(!service);
+
+		for (i = 0, pos = 0; i < (unsigned int)count;
+			pos += elements[i++].size)
+			if (elements[i].size) {
+				if (vchiq_copy_from_user
+					(header->data + pos, elements[i].data,
+					(size_t) elements[i].size) !=
+					VCHIQ_SUCCESS) {
+					mutex_unlock(&state->slot_mutex);
+					VCHIQ_SERVICE_STATS_INC(service,
+						error_count);
+					return VCHIQ_ERROR;
+				}
+				if (i == 0) {
+					if (SRVTRACE_ENABLED(service,
+							VCHIQ_LOG_INFO))
+						vchiq_log_dump_mem("Sent", 0,
+							header->data + pos,
+							min(64u,
+							elements[0].size));
+				}
+			}
+
+		spin_lock(&quota_spinlock);
+		service_quota->message_use_count++;
+
+		tx_end_index =
+			SLOT_QUEUE_INDEX_FROM_POS(state->local_tx_pos - 1);
+
+		/* If this transmission can't fit in the last slot used by any
+		** service, the data_use_count must be increased. */
+		if (tx_end_index != state->previous_data_index) {
+			state->previous_data_index = tx_end_index;
+			state->data_use_count++;
+		}
+
+		/* If this isn't the same slot last used by this service,
+		** the service's slot_use_count must be increased. */
+		if (tx_end_index != service_quota->previous_tx_index) {
+			service_quota->previous_tx_index = tx_end_index;
+			slot_use_count = ++service_quota->slot_use_count;
+		} else {
+			slot_use_count = 0;
+		}
+
+		spin_unlock(&quota_spinlock);
+
+		if (slot_use_count)
+			vchiq_log_trace(vchiq_core_log_level,
+				"%d: qm:%d %s,%x - slot_use->%d (hdr %p)",
+				state->id, service->localport,
+				msg_type_str(VCHIQ_MSG_TYPE(msgid)), size,
+				slot_use_count, header);
+
+		VCHIQ_SERVICE_STATS_INC(service, ctrl_tx_count);
+		VCHIQ_SERVICE_STATS_ADD(service, ctrl_tx_bytes, size);
+	} else {
+		vchiq_log_info(vchiq_core_log_level,
+			"%d: qm %s@%x,%x (%d->%d)", state->id,
+			msg_type_str(VCHIQ_MSG_TYPE(msgid)),
+			(unsigned int)header, size,
+			VCHIQ_MSG_SRCPORT(msgid),
+			VCHIQ_MSG_DSTPORT(msgid));
+		if (size != 0) {
+			WARN_ON(!((count == 1) && (size == elements[0].size)));
+			memcpy(header->data, elements[0].data,
+				elements[0].size);
+		}
+		VCHIQ_STATS_INC(state, ctrl_tx_count);
+	}
+
+	header->msgid = msgid;
+	header->size = size;
+
+	{
+		int svc_fourcc;
+
+		svc_fourcc = service
+			? service->base.fourcc
+			: VCHIQ_MAKE_FOURCC('?', '?', '?', '?');
+
+		vchiq_log_info(SRVTRACE_LEVEL(service),
+			"Sent Msg %s(%u) to %c%c%c%c s:%u d:%d len:%d",
+			msg_type_str(VCHIQ_MSG_TYPE(msgid)),
+			VCHIQ_MSG_TYPE(msgid),
+			VCHIQ_FOURCC_AS_4CHARS(svc_fourcc),
+			VCHIQ_MSG_SRCPORT(msgid),
+			VCHIQ_MSG_DSTPORT(msgid),
+			size);
+	}
+
+	/* Make sure the new header is visible to the peer. */
+	wmb();
+
+	/* Make the new tx_pos visible to the peer. */
+	local->tx_pos = state->local_tx_pos;
+	wmb();
+
+	if (service && (type == VCHIQ_MSG_CLOSE))
+		vchiq_set_service_state(service, VCHIQ_SRVSTATE_CLOSESENT);
+
+	if (VCHIQ_MSG_TYPE(msgid) != VCHIQ_MSG_PAUSE)
+		mutex_unlock(&state->slot_mutex);
+
+	remote_event_signal(&state->remote->trigger);
+
+	return VCHIQ_SUCCESS;
+}
+
+/* Called by the slot handler and application threads */
+static VCHIQ_STATUS_T
+queue_message_sync(VCHIQ_STATE_T *state, VCHIQ_SERVICE_T *service,
+	int msgid, const VCHIQ_ELEMENT_T *elements,
+	int count, int size, int is_blocking)
+{
+	VCHIQ_SHARED_STATE_T *local;
+	VCHIQ_HEADER_T *header;
+
+	local = state->local;
+
+	if ((VCHIQ_MSG_TYPE(msgid) != VCHIQ_MSG_RESUME) &&
+		(mutex_lock_interruptible(&state->sync_mutex) != 0))
+		return VCHIQ_RETRY;
+
+	remote_event_wait(&local->sync_release);
+
+	rmb();
+
+	header = (VCHIQ_HEADER_T *)SLOT_DATA_FROM_INDEX(state,
+		local->slot_sync);
+
+	{
+		int oldmsgid = header->msgid;
+		if (oldmsgid != VCHIQ_MSGID_PADDING)
+			vchiq_log_error(vchiq_core_log_level,
+				"%d: qms - msgid %x, not PADDING",
+				state->id, oldmsgid);
+	}
+
+	if (service) {
+		int i, pos;
+
+		vchiq_log_info(vchiq_sync_log_level,
+			"%d: qms %s@%x,%x (%d->%d)", state->id,
+			msg_type_str(VCHIQ_MSG_TYPE(msgid)),
+			(unsigned int)header, size,
+			VCHIQ_MSG_SRCPORT(msgid),
+			VCHIQ_MSG_DSTPORT(msgid));
+
+		for (i = 0, pos = 0; i < (unsigned int)count;
+			pos += elements[i++].size)
+			if (elements[i].size) {
+				if (vchiq_copy_from_user
+					(header->data + pos, elements[i].data,
+					(size_t) elements[i].size) !=
+					VCHIQ_SUCCESS) {
+					mutex_unlock(&state->sync_mutex);
+					VCHIQ_SERVICE_STATS_INC(service,
+						error_count);
+					return VCHIQ_ERROR;
+				}
+				if (i == 0) {
+					if (vchiq_sync_log_level >=
+						VCHIQ_LOG_TRACE)
+						vchiq_log_dump_mem("Sent Sync",
+							0, header->data + pos,
+							min(64u,
+							elements[0].size));
+				}
+			}
+
+		VCHIQ_SERVICE_STATS_INC(service, ctrl_tx_count);
+		VCHIQ_SERVICE_STATS_ADD(service, ctrl_tx_bytes, size);
+	} else {
+		vchiq_log_info(vchiq_sync_log_level,
+			"%d: qms %s@%x,%x (%d->%d)", state->id,
+			msg_type_str(VCHIQ_MSG_TYPE(msgid)),
+			(unsigned int)header, size,
+			VCHIQ_MSG_SRCPORT(msgid),
+			VCHIQ_MSG_DSTPORT(msgid));
+		if (size != 0) {
+			WARN_ON(!((count == 1) && (size == elements[0].size)));
+			memcpy(header->data, elements[0].data,
+				elements[0].size);
+		}
+		VCHIQ_STATS_INC(state, ctrl_tx_count);
+	}
+
+	header->size = size;
+	header->msgid = msgid;
+
+	if (vchiq_sync_log_level >= VCHIQ_LOG_TRACE) {
+		int svc_fourcc;
+
+		svc_fourcc = service
+			? service->base.fourcc
+			: VCHIQ_MAKE_FOURCC('?', '?', '?', '?');
+
+		vchiq_log_trace(vchiq_sync_log_level,
+			"Sent Sync Msg %s(%u) to %c%c%c%c s:%u d:%d len:%d",
+			msg_type_str(VCHIQ_MSG_TYPE(msgid)),
+			VCHIQ_MSG_TYPE(msgid),
+			VCHIQ_FOURCC_AS_4CHARS(svc_fourcc),
+			VCHIQ_MSG_SRCPORT(msgid),
+			VCHIQ_MSG_DSTPORT(msgid),
+			size);
+	}
+
+	/* Make sure the new header is visible to the peer. */
+	wmb();
+
+	remote_event_signal(&state->remote->sync_trigger);
+
+	if (VCHIQ_MSG_TYPE(msgid) != VCHIQ_MSG_PAUSE)
+		mutex_unlock(&state->sync_mutex);
+
+	return VCHIQ_SUCCESS;
+}
+
+static inline void
+claim_slot(VCHIQ_SLOT_INFO_T *slot)
+{
+	slot->use_count++;
+}
+
+static void
+release_slot(VCHIQ_STATE_T *state, VCHIQ_SLOT_INFO_T *slot_info,
+	VCHIQ_HEADER_T *header, VCHIQ_SERVICE_T *service)
+{
+	int release_count;
+
+	mutex_lock(&state->recycle_mutex);
+
+	if (header) {
+		int msgid = header->msgid;
+		if (((msgid & VCHIQ_MSGID_CLAIMED) == 0) ||
+			(service && service->closing)) {
+			mutex_unlock(&state->recycle_mutex);
+			return;
+		}
+
+		/* Rewrite the message header to prevent a double
+		** release */
+		header->msgid = msgid & ~VCHIQ_MSGID_CLAIMED;
+	}
+
+	release_count = slot_info->release_count;
+	slot_info->release_count = ++release_count;
+
+	if (release_count == slot_info->use_count) {
+		int slot_queue_recycle;
+		/* Add to the freed queue */
+
+		/* A read barrier is necessary here to prevent speculative
+		** fetches of remote->slot_queue_recycle from overtaking the
+		** mutex. */
+		rmb();
+
+		slot_queue_recycle = state->remote->slot_queue_recycle;
+		state->remote->slot_queue[slot_queue_recycle &
+			VCHIQ_SLOT_QUEUE_MASK] =
+			SLOT_INDEX_FROM_INFO(state, slot_info);
+		state->remote->slot_queue_recycle = slot_queue_recycle + 1;
+		vchiq_log_info(vchiq_core_log_level,
+			"%d: release_slot %d - recycle->%x",
+			state->id, SLOT_INDEX_FROM_INFO(state, slot_info),
+			state->remote->slot_queue_recycle);
+
+		/* A write barrier is necessary, but remote_event_signal
+		** contains one. */
+		remote_event_signal(&state->remote->recycle);
+	}
+
+	mutex_unlock(&state->recycle_mutex);
+}
+
+/* Called by the slot handler - don't hold the bulk mutex */
+static VCHIQ_STATUS_T
+notify_bulks(VCHIQ_SERVICE_T *service, VCHIQ_BULK_QUEUE_T *queue,
+	int retry_poll)
+{
+	VCHIQ_STATUS_T status = VCHIQ_SUCCESS;
+
+	vchiq_log_trace(vchiq_core_log_level,
+		"%d: nb:%d %cx - p=%x rn=%x r=%x",
+		service->state->id, service->localport,
+		(queue == &service->bulk_tx) ? 't' : 'r',
+		queue->process, queue->remote_notify, queue->remove);
+
+	if (service->state->is_master) {
+		while (queue->remote_notify != queue->process) {
+			VCHIQ_BULK_T *bulk =
+				&queue->bulks[BULK_INDEX(queue->remote_notify)];
+			int msgtype = (bulk->dir == VCHIQ_BULK_TRANSMIT) ?
+				VCHIQ_MSG_BULK_RX_DONE : VCHIQ_MSG_BULK_TX_DONE;
+			int msgid = VCHIQ_MAKE_MSG(msgtype, service->localport,
+				service->remoteport);
+			VCHIQ_ELEMENT_T element = { &bulk->actual, 4 };
+			/* Only reply to non-dummy bulk requests */
+			if (bulk->remote_data) {
+				status = queue_message(service->state, NULL,
+					msgid, &element, 1, 4, 0);
+				if (status != VCHIQ_SUCCESS)
+					break;
+			}
+			queue->remote_notify++;
+		}
+	} else {
+		queue->remote_notify = queue->process;
+	}
+
+	if (status == VCHIQ_SUCCESS) {
+		while (queue->remove != queue->remote_notify) {
+			VCHIQ_BULK_T *bulk =
+				&queue->bulks[BULK_INDEX(queue->remove)];
+
+			/* Only generate callbacks for non-dummy bulk
+			** requests, and non-terminated services */
+			if (bulk->data && service->instance) {
+				if (bulk->actual != VCHIQ_BULK_ACTUAL_ABORTED) {
+					if (bulk->dir == VCHIQ_BULK_TRANSMIT) {
+						VCHIQ_SERVICE_STATS_INC(service,
+							bulk_tx_count);
+						VCHIQ_SERVICE_STATS_ADD(service,
+							bulk_tx_bytes,
+							bulk->actual);
+					} else {
+						VCHIQ_SERVICE_STATS_INC(service,
+							bulk_rx_count);
+						VCHIQ_SERVICE_STATS_ADD(service,
+							bulk_rx_bytes,
+							bulk->actual);
+					}
+				} else {
+					VCHIQ_SERVICE_STATS_INC(service,
+						bulk_aborted_count);
+				}
+				if (bulk->mode == VCHIQ_BULK_MODE_BLOCKING) {
+					struct bulk_waiter *waiter;
+					spin_lock(&bulk_waiter_spinlock);
+					waiter = bulk->userdata;
+					if (waiter) {
+						waiter->actual = bulk->actual;
+						up(&waiter->event);
+					}
+					spin_unlock(&bulk_waiter_spinlock);
+				} else if (bulk->mode ==
+					VCHIQ_BULK_MODE_CALLBACK) {
+					VCHIQ_REASON_T reason = (bulk->dir ==
+						VCHIQ_BULK_TRANSMIT) ?
+						((bulk->actual ==
+						VCHIQ_BULK_ACTUAL_ABORTED) ?
+						VCHIQ_BULK_TRANSMIT_ABORTED :
+						VCHIQ_BULK_TRANSMIT_DONE) :
+						((bulk->actual ==
+						VCHIQ_BULK_ACTUAL_ABORTED) ?
+						VCHIQ_BULK_RECEIVE_ABORTED :
+						VCHIQ_BULK_RECEIVE_DONE);
+					status = make_service_callback(service,
+						reason,	NULL, bulk->userdata);
+					if (status == VCHIQ_RETRY)
+						break;
+				}
+			}
+
+			queue->remove++;
+			up(&service->bulk_remove_event);
+		}
+		if (!retry_poll)
+			status = VCHIQ_SUCCESS;
+	}
+
+	if (status == VCHIQ_RETRY)
+		request_poll(service->state, service,
+			(queue == &service->bulk_tx) ?
+			VCHIQ_POLL_TXNOTIFY : VCHIQ_POLL_RXNOTIFY);
+
+	return status;
+}
+
+/* Called by the slot handler thread */
+static void
+poll_services(VCHIQ_STATE_T *state)
+{
+	int group, i;
+
+	for (group = 0; group < BITSET_SIZE(state->unused_service); group++) {
+		uint32_t flags;
+		flags = atomic_xchg(&state->poll_services[group], 0);
+		for (i = 0; flags; i++) {
+			if (flags & (1 << i)) {
+				VCHIQ_SERVICE_T *service =
+					find_service_by_port(state,
+						(group<<5) + i);
+				uint32_t service_flags;
+				flags &= ~(1 << i);
+				if (!service)
+					continue;
+				service_flags =
+					atomic_xchg(&service->poll_flags, 0);
+				if (service_flags &
+					(1 << VCHIQ_POLL_REMOVE)) {
+					vchiq_log_info(vchiq_core_log_level,
+						"%d: ps - remove %d<->%d",
+						state->id, service->localport,
+						service->remoteport);
+
+					/* Make it look like a client, because
+					   it must be removed and not left in
+					   the LISTENING state. */
+					service->public_fourcc =
+						VCHIQ_FOURCC_INVALID;
+
+					if (vchiq_close_service_internal(
+						service, 0/*!close_recvd*/) !=
+						VCHIQ_SUCCESS)
+						request_poll(state, service,
+							VCHIQ_POLL_REMOVE);
+				} else if (service_flags &
+					(1 << VCHIQ_POLL_TERMINATE)) {
+					vchiq_log_info(vchiq_core_log_level,
+						"%d: ps - terminate %d<->%d",
+						state->id, service->localport,
+						service->remoteport);
+					if (vchiq_close_service_internal(
+						service, 0/*!close_recvd*/) !=
+						VCHIQ_SUCCESS)
+						request_poll(state, service,
+							VCHIQ_POLL_TERMINATE);
+				}
+				if (service_flags & (1 << VCHIQ_POLL_TXNOTIFY))
+					notify_bulks(service,
+						&service->bulk_tx,
+						1/*retry_poll*/);
+				if (service_flags & (1 << VCHIQ_POLL_RXNOTIFY))
+					notify_bulks(service,
+						&service->bulk_rx,
+						1/*retry_poll*/);
+				unlock_service(service);
+			}
+		}
+	}
+}
+
+/* Called by the slot handler or application threads, holding the bulk mutex. */
+static int
+resolve_bulks(VCHIQ_SERVICE_T *service, VCHIQ_BULK_QUEUE_T *queue)
+{
+	VCHIQ_STATE_T *state = service->state;
+	int resolved = 0;
+	int rc;
+
+	while ((queue->process != queue->local_insert) &&
+		(queue->process != queue->remote_insert)) {
+		VCHIQ_BULK_T *bulk = &queue->bulks[BULK_INDEX(queue->process)];
+
+		vchiq_log_trace(vchiq_core_log_level,
+			"%d: rb:%d %cx - li=%x ri=%x p=%x",
+			state->id, service->localport,
+			(queue == &service->bulk_tx) ? 't' : 'r',
+			queue->local_insert, queue->remote_insert,
+			queue->process);
+
+		WARN_ON(!((int)(queue->local_insert - queue->process) > 0));
+		WARN_ON(!((int)(queue->remote_insert - queue->process) > 0));
+
+		rc = mutex_lock_interruptible(&state->bulk_transfer_mutex);
+		if (rc != 0)
+			break;
+
+		vchiq_transfer_bulk(bulk);
+		mutex_unlock(&state->bulk_transfer_mutex);
+
+		if (SRVTRACE_ENABLED(service, VCHIQ_LOG_INFO)) {
+			const char *header = (queue == &service->bulk_tx) ?
+				"Send Bulk to" : "Recv Bulk from";
+			if (bulk->actual != VCHIQ_BULK_ACTUAL_ABORTED)
+				vchiq_log_info(SRVTRACE_LEVEL(service),
+					"%s %c%c%c%c d:%d len:%d %x<->%x",
+					header,
+					VCHIQ_FOURCC_AS_4CHARS(
+						service->base.fourcc),
+					service->remoteport,
+					bulk->size,
+					(unsigned int)bulk->data,
+					(unsigned int)bulk->remote_data);
+			else
+				vchiq_log_info(SRVTRACE_LEVEL(service),
+					"%s %c%c%c%c d:%d ABORTED - tx len:%d,"
+					" rx len:%d %x<->%x",
+					header,
+					VCHIQ_FOURCC_AS_4CHARS(
+						service->base.fourcc),
+					service->remoteport,
+					bulk->size,
+					bulk->remote_size,
+					(unsigned int)bulk->data,
+					(unsigned int)bulk->remote_data);
+		}
+
+		vchiq_complete_bulk(bulk);
+		queue->process++;
+		resolved++;
+	}
+	return resolved;
+}
+
+/* Called with the bulk_mutex held */
+static void
+abort_outstanding_bulks(VCHIQ_SERVICE_T *service, VCHIQ_BULK_QUEUE_T *queue)
+{
+	int is_tx = (queue == &service->bulk_tx);
+	vchiq_log_trace(vchiq_core_log_level,
+		"%d: aob:%d %cx - li=%x ri=%x p=%x",
+		service->state->id, service->localport, is_tx ? 't' : 'r',
+		queue->local_insert, queue->remote_insert, queue->process);
+
+	WARN_ON(!((int)(queue->local_insert - queue->process) >= 0));
+	WARN_ON(!((int)(queue->remote_insert - queue->process) >= 0));
+
+	while ((queue->process != queue->local_insert) ||
+		(queue->process != queue->remote_insert)) {
+		VCHIQ_BULK_T *bulk = &queue->bulks[BULK_INDEX(queue->process)];
+
+		if (queue->process == queue->remote_insert) {
+			/* fabricate a matching dummy bulk */
+			bulk->remote_data = NULL;
+			bulk->remote_size = 0;
+			queue->remote_insert++;
+		}
+
+		if (queue->process != queue->local_insert) {
+			vchiq_complete_bulk(bulk);
+
+			vchiq_log_info(SRVTRACE_LEVEL(service),
+				"%s %c%c%c%c d:%d ABORTED - tx len:%d, "
+				"rx len:%d",
+				is_tx ? "Send Bulk to" : "Recv Bulk from",
+				VCHIQ_FOURCC_AS_4CHARS(service->base.fourcc),
+				service->remoteport,
+				bulk->size,
+				bulk->remote_size);
+		} else {
+			/* fabricate a matching dummy bulk */
+			bulk->data = NULL;
+			bulk->size = 0;
+			bulk->actual = VCHIQ_BULK_ACTUAL_ABORTED;
+			bulk->dir = is_tx ? VCHIQ_BULK_TRANSMIT :
+				VCHIQ_BULK_RECEIVE;
+			queue->local_insert++;
+		}
+
+		queue->process++;
+	}
+}
+
+/* Called from the slot handler thread */
+static void
+pause_bulks(VCHIQ_STATE_T *state)
+{
+	if (unlikely(atomic_inc_return(&pause_bulks_count) != 1)) {
+		WARN_ON_ONCE(1);
+		atomic_set(&pause_bulks_count, 1);
+		return;
+	}
+
+	/* Block bulk transfers from all services */
+	mutex_lock(&state->bulk_transfer_mutex);
+}
+
+/* Called from the slot handler thread */
+static void
+resume_bulks(VCHIQ_STATE_T *state)
+{
+	int i;
+	if (unlikely(atomic_dec_return(&pause_bulks_count) != 0)) {
+		WARN_ON_ONCE(1);
+		atomic_set(&pause_bulks_count, 0);
+		return;
+	}
+
+	/* Allow bulk transfers from all services */
+	mutex_unlock(&state->bulk_transfer_mutex);
+
+	if (state->deferred_bulks == 0)
+		return;
+
+	/* Deal with any bulks which had to be deferred due to being in
+	 * paused state.  Don't try to match up to number of deferred bulks
+	 * in case we've had something come and close the service in the
+	 * interim - just process all bulk queues for all services */
+	vchiq_log_info(vchiq_core_log_level, "%s: processing %d deferred bulks",
+		__func__, state->deferred_bulks);
+
+	for (i = 0; i < state->unused_service; i++) {
+		VCHIQ_SERVICE_T *service = state->services[i];
+		int resolved_rx = 0;
+		int resolved_tx = 0;
+		if (!service || (service->srvstate != VCHIQ_SRVSTATE_OPEN))
+			continue;
+
+		mutex_lock(&service->bulk_mutex);
+		resolved_rx = resolve_bulks(service, &service->bulk_rx);
+		resolved_tx = resolve_bulks(service, &service->bulk_tx);
+		mutex_unlock(&service->bulk_mutex);
+		if (resolved_rx)
+			notify_bulks(service, &service->bulk_rx, 1);
+		if (resolved_tx)
+			notify_bulks(service, &service->bulk_tx, 1);
+	}
+	state->deferred_bulks = 0;
+}
+
+static int
+parse_open(VCHIQ_STATE_T *state, VCHIQ_HEADER_T *header)
+{
+	VCHIQ_SERVICE_T *service = NULL;
+	int msgid, size;
+	int type;
+	unsigned int localport, remoteport;
+
+	msgid = header->msgid;
+	size = header->size;
+	type = VCHIQ_MSG_TYPE(msgid);
+	localport = VCHIQ_MSG_DSTPORT(msgid);
+	remoteport = VCHIQ_MSG_SRCPORT(msgid);
+	if (size >= sizeof(struct vchiq_open_payload)) {
+		const struct vchiq_open_payload *payload =
+			(struct vchiq_open_payload *)header->data;
+		unsigned int fourcc;
+
+		fourcc = payload->fourcc;
+		vchiq_log_info(vchiq_core_log_level,
+			"%d: prs OPEN@%x (%d->'%c%c%c%c')",
+			state->id, (unsigned int)header,
+			localport,
+			VCHIQ_FOURCC_AS_4CHARS(fourcc));
+
+		service = get_listening_service(state, fourcc);
+
+		if (service) {
+			/* A matching service exists */
+			short version = payload->version;
+			short version_min = payload->version_min;
+			if ((service->version < version_min) ||
+				(version < service->version_min)) {
+				/* Version mismatch */
+				vchiq_loud_error_header();
+				vchiq_loud_error("%d: service %d (%c%c%c%c) "
+					"version mismatch - local (%d, min %d)"
+					" vs. remote (%d, min %d)",
+					state->id, service->localport,
+					VCHIQ_FOURCC_AS_4CHARS(fourcc),
+					service->version, service->version_min,
+					version, version_min);
+				vchiq_loud_error_footer();
+				unlock_service(service);
+				service = NULL;
+				goto fail_open;
+			}
+			service->peer_version = version;
+
+			if (service->srvstate == VCHIQ_SRVSTATE_LISTENING) {
+				struct vchiq_openack_payload ack_payload = {
+					service->version
+				};
+				VCHIQ_ELEMENT_T body = {
+					&ack_payload,
+					sizeof(ack_payload)
+				};
+
+				/* Acknowledge the OPEN */
+				if (service->sync) {
+					if (queue_message_sync(state, NULL,
+						VCHIQ_MAKE_MSG(
+							VCHIQ_MSG_OPENACK,
+							service->localport,
+							remoteport),
+						&body, 1, sizeof(ack_payload),
+						0) == VCHIQ_RETRY)
+						goto bail_not_ready;
+				} else {
+					if (queue_message(state, NULL,
+						VCHIQ_MAKE_MSG(
+							VCHIQ_MSG_OPENACK,
+							service->localport,
+							remoteport),
+						&body, 1, sizeof(ack_payload),
+						0) == VCHIQ_RETRY)
+						goto bail_not_ready;
+				}
+
+				/* The service is now open */
+				vchiq_set_service_state(service,
+					service->sync ? VCHIQ_SRVSTATE_OPENSYNC
+					: VCHIQ_SRVSTATE_OPEN);
+			}
+
+			service->remoteport = remoteport;
+			service->client_id = ((int *)header->data)[1];
+			if (make_service_callback(service, VCHIQ_SERVICE_OPENED,
+				NULL, NULL) == VCHIQ_RETRY) {
+				/* Bail out if not ready */
+				service->remoteport = VCHIQ_PORT_FREE;
+				goto bail_not_ready;
+			}
+
+			/* Success - the message has been dealt with */
+			unlock_service(service);
+			return 1;
+		}
+	}
+
+fail_open:
+	/* No available service, or an invalid request - send a CLOSE */
+	if (queue_message(state, NULL,
+		VCHIQ_MAKE_MSG(VCHIQ_MSG_CLOSE, 0, VCHIQ_MSG_SRCPORT(msgid)),
+		NULL, 0, 0, 0) == VCHIQ_RETRY)
+		goto bail_not_ready;
+
+	return 1;
+
+bail_not_ready:
+	if (service)
+		unlock_service(service);
+
+	return 0;
+}
+
+/* Called by the slot handler thread */
+static void
+parse_rx_slots(VCHIQ_STATE_T *state)
+{
+	VCHIQ_SHARED_STATE_T *remote = state->remote;
+	VCHIQ_SERVICE_T *service = NULL;
+	int tx_pos;
+	DEBUG_INITIALISE(state->local)
+
+	tx_pos = remote->tx_pos;
+
+	while (state->rx_pos != tx_pos) {
+		VCHIQ_HEADER_T *header;
+		int msgid, size;
+		int type;
+		unsigned int localport, remoteport;
+
+		DEBUG_TRACE(PARSE_LINE);
+		if (!state->rx_data) {
+			int rx_index;
+			WARN_ON(!((state->rx_pos & VCHIQ_SLOT_MASK) == 0));
+			rx_index = remote->slot_queue[
+				SLOT_QUEUE_INDEX_FROM_POS(state->rx_pos) &
+				VCHIQ_SLOT_QUEUE_MASK];
+			state->rx_data = (char *)SLOT_DATA_FROM_INDEX(state,
+				rx_index);
+			state->rx_info = SLOT_INFO_FROM_INDEX(state, rx_index);
+
+			/* Initialise use_count to one, and increment
+			** release_count at the end of the slot to avoid
+			** releasing the slot prematurely. */
+			state->rx_info->use_count = 1;
+			state->rx_info->release_count = 0;
+		}
+
+		header = (VCHIQ_HEADER_T *)(state->rx_data +
+			(state->rx_pos & VCHIQ_SLOT_MASK));
+		DEBUG_VALUE(PARSE_HEADER, (int)header);
+		msgid = header->msgid;
+		DEBUG_VALUE(PARSE_MSGID, msgid);
+		size = header->size;
+		type = VCHIQ_MSG_TYPE(msgid);
+		localport = VCHIQ_MSG_DSTPORT(msgid);
+		remoteport = VCHIQ_MSG_SRCPORT(msgid);
+
+		if (type != VCHIQ_MSG_DATA)
+			VCHIQ_STATS_INC(state, ctrl_rx_count);
+
+		switch (type) {
+		case VCHIQ_MSG_OPENACK:
+		case VCHIQ_MSG_CLOSE:
+		case VCHIQ_MSG_DATA:
+		case VCHIQ_MSG_BULK_RX:
+		case VCHIQ_MSG_BULK_TX:
+		case VCHIQ_MSG_BULK_RX_DONE:
+		case VCHIQ_MSG_BULK_TX_DONE:
+			service = find_service_by_port(state, localport);
+			if ((!service ||
+			     ((service->remoteport != remoteport) &&
+			      (service->remoteport != VCHIQ_PORT_FREE))) &&
+			    (localport == 0) &&
+			    (type == VCHIQ_MSG_CLOSE)) {
+				/* This could be a CLOSE from a client which
+				   hadn't yet received the OPENACK - look for
+				   the connected service */
+				if (service)
+					unlock_service(service);
+				service = get_connected_service(state,
+					remoteport);
+				if (service)
+					vchiq_log_warning(vchiq_core_log_level,
+						"%d: prs %s@%x (%d->%d) - "
+						"found connected service %d",
+						state->id, msg_type_str(type),
+						(unsigned int)header,
+						remoteport, localport,
+						service->localport);
+			}
+
+			if (!service) {
+				vchiq_log_error(vchiq_core_log_level,
+					"%d: prs %s@%x (%d->%d) - "
+					"invalid/closed service %d",
+					state->id, msg_type_str(type),
+					(unsigned int)header,
+					remoteport, localport, localport);
+				goto skip_message;
+			}
+			break;
+		default:
+			break;
+		}
+
+		if (SRVTRACE_ENABLED(service, VCHIQ_LOG_INFO)) {
+			int svc_fourcc;
+
+			svc_fourcc = service
+				? service->base.fourcc
+				: VCHIQ_MAKE_FOURCC('?', '?', '?', '?');
+			vchiq_log_info(SRVTRACE_LEVEL(service),
+				"Rcvd Msg %s(%u) from %c%c%c%c s:%d d:%d "
+				"len:%d",
+				msg_type_str(type), type,
+				VCHIQ_FOURCC_AS_4CHARS(svc_fourcc),
+				remoteport, localport, size);
+			if (size > 0)
+				vchiq_log_dump_mem("Rcvd", 0, header->data,
+					min(64, size));
+		}
+
+		if (((unsigned int)header & VCHIQ_SLOT_MASK) + calc_stride(size)
+			> VCHIQ_SLOT_SIZE) {
+			vchiq_log_error(vchiq_core_log_level,
+				"header %x (msgid %x) - size %x too big for "
+				"slot",
+				(unsigned int)header, (unsigned int)msgid,
+				(unsigned int)size);
+			WARN(1, "oversized for slot\n");
+		}
+
+		switch (type) {
+		case VCHIQ_MSG_OPEN:
+			WARN_ON(!(VCHIQ_MSG_DSTPORT(msgid) == 0));
+			if (!parse_open(state, header))
+				goto bail_not_ready;
+			break;
+		case VCHIQ_MSG_OPENACK:
+			if (size >= sizeof(struct vchiq_openack_payload)) {
+				const struct vchiq_openack_payload *payload =
+					(struct vchiq_openack_payload *)
+					header->data;
+				service->peer_version = payload->version;
+			}
+			vchiq_log_info(vchiq_core_log_level,
+				"%d: prs OPENACK@%x,%x (%d->%d) v:%d",
+				state->id, (unsigned int)header, size,
+				remoteport, localport, service->peer_version);
+			if (service->srvstate ==
+				VCHIQ_SRVSTATE_OPENING) {
+				service->remoteport = remoteport;
+				vchiq_set_service_state(service,
+					VCHIQ_SRVSTATE_OPEN);
+				up(&service->remove_event);
+			} else
+				vchiq_log_error(vchiq_core_log_level,
+					"OPENACK received in state %s",
+					srvstate_names[service->srvstate]);
+			break;
+		case VCHIQ_MSG_CLOSE:
+			WARN_ON(size != 0); /* There should be no data */
+
+			vchiq_log_info(vchiq_core_log_level,
+				"%d: prs CLOSE@%x (%d->%d)",
+				state->id, (unsigned int)header,
+				remoteport, localport);
+
+			mark_service_closing_internal(service, 1);
+
+			if (vchiq_close_service_internal(service,
+				1/*close_recvd*/) == VCHIQ_RETRY)
+				goto bail_not_ready;
+
+			vchiq_log_info(vchiq_core_log_level,
+				"Close Service %c%c%c%c s:%u d:%d",
+				VCHIQ_FOURCC_AS_4CHARS(service->base.fourcc),
+				service->localport,
+				service->remoteport);
+			break;
+		case VCHIQ_MSG_DATA:
+			vchiq_log_trace(vchiq_core_log_level,
+				"%d: prs DATA@%x,%x (%d->%d)",
+				state->id, (unsigned int)header, size,
+				remoteport, localport);
+
+			if ((service->remoteport == remoteport)
+				&& (service->srvstate ==
+				VCHIQ_SRVSTATE_OPEN)) {
+				header->msgid = msgid | VCHIQ_MSGID_CLAIMED;
+				claim_slot(state->rx_info);
+				DEBUG_TRACE(PARSE_LINE);
+				if (make_service_callback(service,
+					VCHIQ_MESSAGE_AVAILABLE, header,
+					NULL) == VCHIQ_RETRY) {
+					DEBUG_TRACE(PARSE_LINE);
+					goto bail_not_ready;
+				}
+				VCHIQ_SERVICE_STATS_INC(service, ctrl_rx_count);
+				VCHIQ_SERVICE_STATS_ADD(service, ctrl_rx_bytes,
+					size);
+			} else {
+				VCHIQ_STATS_INC(state, error_count);
+			}
+			break;
+		case VCHIQ_MSG_CONNECT:
+			vchiq_log_info(vchiq_core_log_level,
+				"%d: prs CONNECT@%x",
+				state->id, (unsigned int)header);
+			up(&state->connect);
+			break;
+		case VCHIQ_MSG_BULK_RX:
+		case VCHIQ_MSG_BULK_TX: {
+			VCHIQ_BULK_QUEUE_T *queue;
+			WARN_ON(!state->is_master);
+			queue = (type == VCHIQ_MSG_BULK_RX) ?
+				&service->bulk_tx : &service->bulk_rx;
+			if ((service->remoteport == remoteport)
+				&& (service->srvstate ==
+				VCHIQ_SRVSTATE_OPEN)) {
+				VCHIQ_BULK_T *bulk;
+				int resolved = 0;
+
+				DEBUG_TRACE(PARSE_LINE);
+				if (mutex_lock_interruptible(
+					&service->bulk_mutex) != 0) {
+					DEBUG_TRACE(PARSE_LINE);
+					goto bail_not_ready;
+				}
+
+				WARN_ON(!(queue->remote_insert < queue->remove +
+					VCHIQ_NUM_SERVICE_BULKS));
+				bulk = &queue->bulks[
+					BULK_INDEX(queue->remote_insert)];
+				bulk->remote_data =
+					(void *)((int *)header->data)[0];
+				bulk->remote_size = ((int *)header->data)[1];
+				wmb();
+
+				vchiq_log_info(vchiq_core_log_level,
+					"%d: prs %s@%x (%d->%d) %x@%x",
+					state->id, msg_type_str(type),
+					(unsigned int)header,
+					remoteport, localport,
+					bulk->remote_size,
+					(unsigned int)bulk->remote_data);
+
+				queue->remote_insert++;
+
+				if (atomic_read(&pause_bulks_count)) {
+					state->deferred_bulks++;
+					vchiq_log_info(vchiq_core_log_level,
+						"%s: deferring bulk (%d)",
+						__func__,
+						state->deferred_bulks);
+					if (state->conn_state !=
+						VCHIQ_CONNSTATE_PAUSE_SENT)
+						vchiq_log_error(
+							vchiq_core_log_level,
+							"%s: bulks paused in "
+							"unexpected state %s",
+							__func__,
+							conn_state_names[
+							state->conn_state]);
+				} else if (state->conn_state ==
+					VCHIQ_CONNSTATE_CONNECTED) {
+					DEBUG_TRACE(PARSE_LINE);
+					resolved = resolve_bulks(service,
+						queue);
+				}
+
+				mutex_unlock(&service->bulk_mutex);
+				if (resolved)
+					notify_bulks(service, queue,
+						1/*retry_poll*/);
+			}
+		} break;
+		case VCHIQ_MSG_BULK_RX_DONE:
+		case VCHIQ_MSG_BULK_TX_DONE:
+			WARN_ON(state->is_master);
+			if ((service->remoteport == remoteport)
+				&& (service->srvstate !=
+				VCHIQ_SRVSTATE_FREE)) {
+				VCHIQ_BULK_QUEUE_T *queue;
+				VCHIQ_BULK_T *bulk;
+
+				queue = (type == VCHIQ_MSG_BULK_RX_DONE) ?
+					&service->bulk_rx : &service->bulk_tx;
+
+				DEBUG_TRACE(PARSE_LINE);
+				if (mutex_lock_interruptible(
+					&service->bulk_mutex) != 0) {
+					DEBUG_TRACE(PARSE_LINE);
+					goto bail_not_ready;
+				}
+				if ((int)(queue->remote_insert -
+					queue->local_insert) >= 0) {
+					vchiq_log_error(vchiq_core_log_level,
+						"%d: prs %s@%x (%d->%d) "
+						"unexpected (ri=%d,li=%d)",
+						state->id, msg_type_str(type),
+						(unsigned int)header,
+						remoteport, localport,
+						queue->remote_insert,
+						queue->local_insert);
+					mutex_unlock(&service->bulk_mutex);
+					break;
+				}
+
+				BUG_ON(queue->process == queue->local_insert);
+				BUG_ON(queue->process != queue->remote_insert);
+
+				bulk = &queue->bulks[
+					BULK_INDEX(queue->remote_insert)];
+				bulk->actual = *(int *)header->data;
+				queue->remote_insert++;
+
+				vchiq_log_info(vchiq_core_log_level,
+					"%d: prs %s@%x (%d->%d) %x@%x",
+					state->id, msg_type_str(type),
+					(unsigned int)header,
+					remoteport, localport,
+					bulk->actual, (unsigned int)bulk->data);
+
+				vchiq_log_trace(vchiq_core_log_level,
+					"%d: prs:%d %cx li=%x ri=%x p=%x",
+					state->id, localport,
+					(type == VCHIQ_MSG_BULK_RX_DONE) ?
+						'r' : 't',
+					queue->local_insert,
+					queue->remote_insert, queue->process);
+
+				DEBUG_TRACE(PARSE_LINE);
+				WARN_ON(queue->process == queue->local_insert);
+				vchiq_complete_bulk(bulk);
+				queue->process++;
+				mutex_unlock(&service->bulk_mutex);
+				DEBUG_TRACE(PARSE_LINE);
+				notify_bulks(service, queue, 1/*retry_poll*/);
+				DEBUG_TRACE(PARSE_LINE);
+			}
+			break;
+		case VCHIQ_MSG_PADDING:
+			vchiq_log_trace(vchiq_core_log_level,
+				"%d: prs PADDING@%x,%x",
+				state->id, (unsigned int)header, size);
+			break;
+		case VCHIQ_MSG_PAUSE:
+			/* If initiated, signal the application thread */
+			vchiq_log_trace(vchiq_core_log_level,
+				"%d: prs PAUSE@%x,%x",
+				state->id, (unsigned int)header, size);
+			if (state->conn_state == VCHIQ_CONNSTATE_PAUSED) {
+				vchiq_log_error(vchiq_core_log_level,
+					"%d: PAUSE received in state PAUSED",
+					state->id);
+				break;
+			}
+			if (state->conn_state != VCHIQ_CONNSTATE_PAUSE_SENT) {
+				/* Send a PAUSE in response */
+				if (queue_message(state, NULL,
+					VCHIQ_MAKE_MSG(VCHIQ_MSG_PAUSE, 0, 0),
+					NULL, 0, 0, 0) == VCHIQ_RETRY)
+					goto bail_not_ready;
+				if (state->is_master)
+					pause_bulks(state);
+			}
+			/* At this point slot_mutex is held */
+			vchiq_set_conn_state(state, VCHIQ_CONNSTATE_PAUSED);
+			vchiq_platform_paused(state);
+			break;
+		case VCHIQ_MSG_RESUME:
+			vchiq_log_trace(vchiq_core_log_level,
+				"%d: prs RESUME@%x,%x",
+				state->id, (unsigned int)header, size);
+			/* Release the slot mutex */
+			mutex_unlock(&state->slot_mutex);
+			if (state->is_master)
+				resume_bulks(state);
+			vchiq_set_conn_state(state, VCHIQ_CONNSTATE_CONNECTED);
+			vchiq_platform_resumed(state);
+			break;
+
+		case VCHIQ_MSG_REMOTE_USE:
+			vchiq_on_remote_use(state);
+			break;
+		case VCHIQ_MSG_REMOTE_RELEASE:
+			vchiq_on_remote_release(state);
+			break;
+		case VCHIQ_MSG_REMOTE_USE_ACTIVE:
+			vchiq_on_remote_use_active(state);
+			break;
+
+		default:
+			vchiq_log_error(vchiq_core_log_level,
+				"%d: prs invalid msgid %x@%x,%x",
+				state->id, msgid, (unsigned int)header, size);
+			WARN(1, "invalid message\n");
+			break;
+		}
+
+skip_message:
+		if (service) {
+			unlock_service(service);
+			service = NULL;
+		}
+
+		state->rx_pos += calc_stride(size);
+
+		DEBUG_TRACE(PARSE_LINE);
+		/* Perform some housekeeping when the end of the slot is
+		** reached. */
+		if ((state->rx_pos & VCHIQ_SLOT_MASK) == 0) {
+			/* Remove the extra reference count. */
+			release_slot(state, state->rx_info, NULL, NULL);
+			state->rx_data = NULL;
+		}
+	}
+
+bail_not_ready:
+	if (service)
+		unlock_service(service);
+}
+
+/* Called by the slot handler thread */
+static int
+slot_handler_func(void *v)
+{
+	VCHIQ_STATE_T *state = (VCHIQ_STATE_T *) v;
+	VCHIQ_SHARED_STATE_T *local = state->local;
+	DEBUG_INITIALISE(local)
+
+	while (1) {
+		DEBUG_COUNT(SLOT_HANDLER_COUNT);
+		DEBUG_TRACE(SLOT_HANDLER_LINE);
+		remote_event_wait(&local->trigger);
+
+		rmb();
+
+		DEBUG_TRACE(SLOT_HANDLER_LINE);
+		if (state->poll_needed) {
+			/* Check if we need to suspend - may change our
+			 * conn_state */
+			vchiq_platform_check_suspend(state);
+
+			state->poll_needed = 0;
+
+			/* Handle service polling and other rare conditions here
+			** out of the mainline code */
+			switch (state->conn_state) {
+			case VCHIQ_CONNSTATE_CONNECTED:
+				/* Poll the services as requested */
+				poll_services(state);
+				break;
+
+			case VCHIQ_CONNSTATE_PAUSING:
+				if (state->is_master)
+					pause_bulks(state);
+				if (queue_message(state, NULL,
+					VCHIQ_MAKE_MSG(VCHIQ_MSG_PAUSE, 0, 0),
+					NULL, 0, 0, 0) != VCHIQ_RETRY) {
+					vchiq_set_conn_state(state,
+						VCHIQ_CONNSTATE_PAUSE_SENT);
+				} else {
+					if (state->is_master)
+						resume_bulks(state);
+					/* Retry later */
+					state->poll_needed = 1;
+				}
+				break;
+
+			case VCHIQ_CONNSTATE_PAUSED:
+				vchiq_platform_resume(state);
+				break;
+
+			case VCHIQ_CONNSTATE_RESUMING:
+				if (queue_message(state, NULL,
+					VCHIQ_MAKE_MSG(VCHIQ_MSG_RESUME, 0, 0),
+					NULL, 0, 0, 0) != VCHIQ_RETRY) {
+					if (state->is_master)
+						resume_bulks(state);
+					vchiq_set_conn_state(state,
+						VCHIQ_CONNSTATE_CONNECTED);
+					vchiq_platform_resumed(state);
+				} else {
+					/* This should really be impossible,
+					** since the PAUSE should have flushed
+					** through outstanding messages. */
+					vchiq_log_error(vchiq_core_log_level,
+						"Failed to send RESUME "
+						"message");
+					BUG();
+				}
+				break;
+
+			case VCHIQ_CONNSTATE_PAUSE_TIMEOUT:
+			case VCHIQ_CONNSTATE_RESUME_TIMEOUT:
+				vchiq_platform_handle_timeout(state);
+				break;
+			default:
+				break;
+			}
+
+
+		}
+
+		DEBUG_TRACE(SLOT_HANDLER_LINE);
+		parse_rx_slots(state);
+	}
+	return 0;
+}
+
+
+/* Called by the recycle thread */
+static int
+recycle_func(void *v)
+{
+	VCHIQ_STATE_T *state = (VCHIQ_STATE_T *) v;
+	VCHIQ_SHARED_STATE_T *local = state->local;
+
+	while (1) {
+		remote_event_wait(&local->recycle);
+
+		process_free_queue(state);
+	}
+	return 0;
+}
+
+
+/* Called by the sync thread */
+static int
+sync_func(void *v)
+{
+	VCHIQ_STATE_T *state = (VCHIQ_STATE_T *) v;
+	VCHIQ_SHARED_STATE_T *local = state->local;
+	VCHIQ_HEADER_T *header = (VCHIQ_HEADER_T *)SLOT_DATA_FROM_INDEX(state,
+		state->remote->slot_sync);
+
+	while (1) {
+		VCHIQ_SERVICE_T *service;
+		int msgid, size;
+		int type;
+		unsigned int localport, remoteport;
+
+		remote_event_wait(&local->sync_trigger);
+
+		rmb();
+
+		msgid = header->msgid;
+		size = header->size;
+		type = VCHIQ_MSG_TYPE(msgid);
+		localport = VCHIQ_MSG_DSTPORT(msgid);
+		remoteport = VCHIQ_MSG_SRCPORT(msgid);
+
+		service = find_service_by_port(state, localport);
+
+		if (!service) {
+			vchiq_log_error(vchiq_sync_log_level,
+				"%d: sf %s@%x (%d->%d) - "
+				"invalid/closed service %d",
+				state->id, msg_type_str(type),
+				(unsigned int)header,
+				remoteport, localport, localport);
+			release_message_sync(state, header);
+			continue;
+		}
+
+		if (vchiq_sync_log_level >= VCHIQ_LOG_TRACE) {
+			int svc_fourcc;
+
+			svc_fourcc = service
+				? service->base.fourcc
+				: VCHIQ_MAKE_FOURCC('?', '?', '?', '?');
+			vchiq_log_trace(vchiq_sync_log_level,
+				"Rcvd Msg %s from %c%c%c%c s:%d d:%d len:%d",
+				msg_type_str(type),
+				VCHIQ_FOURCC_AS_4CHARS(svc_fourcc),
+				remoteport, localport, size);
+			if (size > 0)
+				vchiq_log_dump_mem("Rcvd", 0, header->data,
+					min(64, size));
+		}
+
+		switch (type) {
+		case VCHIQ_MSG_OPENACK:
+			if (size >= sizeof(struct vchiq_openack_payload)) {
+				const struct vchiq_openack_payload *payload =
+					(struct vchiq_openack_payload *)
+					header->data;
+				service->peer_version = payload->version;
+			}
+			vchiq_log_info(vchiq_sync_log_level,
+				"%d: sf OPENACK@%x,%x (%d->%d) v:%d",
+				state->id, (unsigned int)header, size,
+				remoteport, localport, service->peer_version);
+			if (service->srvstate == VCHIQ_SRVSTATE_OPENING) {
+				service->remoteport = remoteport;
+				vchiq_set_service_state(service,
+					VCHIQ_SRVSTATE_OPENSYNC);
+				up(&service->remove_event);
+			}
+			release_message_sync(state, header);
+			break;
+
+		case VCHIQ_MSG_DATA:
+			vchiq_log_trace(vchiq_sync_log_level,
+				"%d: sf DATA@%x,%x (%d->%d)",
+				state->id, (unsigned int)header, size,
+				remoteport, localport);
+
+			if ((service->remoteport == remoteport) &&
+				(service->srvstate ==
+				VCHIQ_SRVSTATE_OPENSYNC)) {
+				if (make_service_callback(service,
+					VCHIQ_MESSAGE_AVAILABLE, header,
+					NULL) == VCHIQ_RETRY)
+					vchiq_log_error(vchiq_sync_log_level,
+						"synchronous callback to "
+						"service %d returns "
+						"VCHIQ_RETRY",
+						localport);
+			}
+			break;
+
+		default:
+			vchiq_log_error(vchiq_sync_log_level,
+				"%d: sf unexpected msgid %x@%x,%x",
+				state->id, msgid, (unsigned int)header, size);
+			release_message_sync(state, header);
+			break;
+		}
+
+		unlock_service(service);
+	}
+
+	return 0;
+}
+
+
+static void
+init_bulk_queue(VCHIQ_BULK_QUEUE_T *queue)
+{
+	queue->local_insert = 0;
+	queue->remote_insert = 0;
+	queue->process = 0;
+	queue->remote_notify = 0;
+	queue->remove = 0;
+}
+
+
+inline const char *
+get_conn_state_name(VCHIQ_CONNSTATE_T conn_state)
+{
+	return conn_state_names[conn_state];
+}
+
+
+VCHIQ_SLOT_ZERO_T *
+vchiq_init_slots(void *mem_base, int mem_size)
+{
+	int mem_align = (VCHIQ_SLOT_SIZE - (int)mem_base) & VCHIQ_SLOT_MASK;
+	VCHIQ_SLOT_ZERO_T *slot_zero =
+		(VCHIQ_SLOT_ZERO_T *)((char *)mem_base + mem_align);
+	int num_slots = (mem_size - mem_align)/VCHIQ_SLOT_SIZE;
+	int first_data_slot = VCHIQ_SLOT_ZERO_SLOTS;
+
+	/* Ensure there is enough memory to run an absolutely minimum system */
+	num_slots -= first_data_slot;
+
+	if (num_slots < 4) {
+		vchiq_log_error(vchiq_core_log_level,
+			"vchiq_init_slots - insufficient memory %x bytes",
+			mem_size);
+		return NULL;
+	}
+
+	memset(slot_zero, 0, sizeof(VCHIQ_SLOT_ZERO_T));
+
+	slot_zero->magic = VCHIQ_MAGIC;
+	slot_zero->version = VCHIQ_VERSION;
+	slot_zero->version_min = VCHIQ_VERSION_MIN;
+	slot_zero->slot_zero_size = sizeof(VCHIQ_SLOT_ZERO_T);
+	slot_zero->slot_size = VCHIQ_SLOT_SIZE;
+	slot_zero->max_slots = VCHIQ_MAX_SLOTS;
+	slot_zero->max_slots_per_side = VCHIQ_MAX_SLOTS_PER_SIDE;
+
+	slot_zero->master.slot_sync = first_data_slot;
+	slot_zero->master.slot_first = first_data_slot + 1;
+	slot_zero->master.slot_last = first_data_slot + (num_slots/2) - 1;
+	slot_zero->slave.slot_sync = first_data_slot + (num_slots/2);
+	slot_zero->slave.slot_first = first_data_slot + (num_slots/2) + 1;
+	slot_zero->slave.slot_last = first_data_slot + num_slots - 1;
+
+	return slot_zero;
+}
+
+VCHIQ_STATUS_T
+vchiq_init_state(VCHIQ_STATE_T *state, VCHIQ_SLOT_ZERO_T *slot_zero,
+		 int is_master)
+{
+	VCHIQ_SHARED_STATE_T *local;
+	VCHIQ_SHARED_STATE_T *remote;
+	VCHIQ_STATUS_T status;
+	char threadname[10];
+	static int id;
+	int i;
+
+	vchiq_log_warning(vchiq_core_log_level,
+		"%s: slot_zero = 0x%08lx, is_master = %d",
+		__func__, (unsigned long)slot_zero, is_master);
+
+	/* Check the input configuration */
+
+	if (slot_zero->magic != VCHIQ_MAGIC) {
+		vchiq_loud_error_header();
+		vchiq_loud_error("Invalid VCHIQ magic value found.");
+		vchiq_loud_error("slot_zero=%x: magic=%x (expected %x)",
+			(unsigned int)slot_zero, slot_zero->magic, VCHIQ_MAGIC);
+		vchiq_loud_error_footer();
+		return VCHIQ_ERROR;
+	}
+
+	if (slot_zero->version < VCHIQ_VERSION_MIN) {
+		vchiq_loud_error_header();
+		vchiq_loud_error("Incompatible VCHIQ versions found.");
+		vchiq_loud_error("slot_zero=%x: VideoCore version=%d "
+			"(minimum %d)",
+			(unsigned int)slot_zero, slot_zero->version,
+			VCHIQ_VERSION_MIN);
+		vchiq_loud_error("Restart with a newer VideoCore image.");
+		vchiq_loud_error_footer();
+		return VCHIQ_ERROR;
+	}
+
+	if (VCHIQ_VERSION < slot_zero->version_min) {
+		vchiq_loud_error_header();
+		vchiq_loud_error("Incompatible VCHIQ versions found.");
+		vchiq_loud_error("slot_zero=%x: version=%d (VideoCore "
+			"minimum %d)",
+			(unsigned int)slot_zero, VCHIQ_VERSION,
+			slot_zero->version_min);
+		vchiq_loud_error("Restart with a newer kernel.");
+		vchiq_loud_error_footer();
+		return VCHIQ_ERROR;
+	}
+
+	if ((slot_zero->slot_zero_size != sizeof(VCHIQ_SLOT_ZERO_T)) ||
+		 (slot_zero->slot_size != VCHIQ_SLOT_SIZE) ||
+		 (slot_zero->max_slots != VCHIQ_MAX_SLOTS) ||
+		 (slot_zero->max_slots_per_side != VCHIQ_MAX_SLOTS_PER_SIDE)) {
+		vchiq_loud_error_header();
+		if (slot_zero->slot_zero_size != sizeof(VCHIQ_SLOT_ZERO_T))
+			vchiq_loud_error("slot_zero=%x: slot_zero_size=%x "
+				"(expected %x)",
+				(unsigned int)slot_zero,
+				slot_zero->slot_zero_size,
+				sizeof(VCHIQ_SLOT_ZERO_T));
+		if (slot_zero->slot_size != VCHIQ_SLOT_SIZE)
+			vchiq_loud_error("slot_zero=%x: slot_size=%d "
+				"(expected %d",
+				(unsigned int)slot_zero, slot_zero->slot_size,
+				VCHIQ_SLOT_SIZE);
+		if (slot_zero->max_slots != VCHIQ_MAX_SLOTS)
+			vchiq_loud_error("slot_zero=%x: max_slots=%d "
+				"(expected %d)",
+				(unsigned int)slot_zero, slot_zero->max_slots,
+				VCHIQ_MAX_SLOTS);
+		if (slot_zero->max_slots_per_side != VCHIQ_MAX_SLOTS_PER_SIDE)
+			vchiq_loud_error("slot_zero=%x: max_slots_per_side=%d "
+				"(expected %d)",
+				(unsigned int)slot_zero,
+				slot_zero->max_slots_per_side,
+				VCHIQ_MAX_SLOTS_PER_SIDE);
+		vchiq_loud_error_footer();
+		return VCHIQ_ERROR;
+	}
+
+	if (is_master) {
+		local = &slot_zero->master;
+		remote = &slot_zero->slave;
+	} else {
+		local = &slot_zero->slave;
+		remote = &slot_zero->master;
+	}
+
+	if (local->initialised) {
+		vchiq_loud_error_header();
+		if (remote->initialised)
+			vchiq_loud_error("local state has already been "
+				"initialised");
+		else
+			vchiq_loud_error("master/slave mismatch - two %ss",
+				is_master ? "master" : "slave");
+		vchiq_loud_error_footer();
+		return VCHIQ_ERROR;
+	}
+
+	memset(state, 0, sizeof(VCHIQ_STATE_T));
+
+	state->id = id++;
+	state->is_master = is_master;
+
+	/*
+		initialize shared state pointers
+	 */
+
+	state->local = local;
+	state->remote = remote;
+	state->slot_data = (VCHIQ_SLOT_T *)slot_zero;
+
+	/*
+		initialize events and mutexes
+	 */
+
+	sema_init(&state->connect, 0);
+	mutex_init(&state->mutex);
+	sema_init(&state->trigger_event, 0);
+	sema_init(&state->recycle_event, 0);
+	sema_init(&state->sync_trigger_event, 0);
+	sema_init(&state->sync_release_event, 0);
+
+	mutex_init(&state->slot_mutex);
+	mutex_init(&state->recycle_mutex);
+	mutex_init(&state->sync_mutex);
+	mutex_init(&state->bulk_transfer_mutex);
+
+	sema_init(&state->slot_available_event, 0);
+	sema_init(&state->slot_remove_event, 0);
+	sema_init(&state->data_quota_event, 0);
+
+	state->slot_queue_available = 0;
+
+	for (i = 0; i < VCHIQ_MAX_SERVICES; i++) {
+		VCHIQ_SERVICE_QUOTA_T *service_quota =
+			&state->service_quotas[i];
+		sema_init(&service_quota->quota_event, 0);
+	}
+
+	for (i = local->slot_first; i <= local->slot_last; i++) {
+		local->slot_queue[state->slot_queue_available++] = i;
+		up(&state->slot_available_event);
+	}
+
+	state->default_slot_quota = state->slot_queue_available/2;
+	state->default_message_quota =
+		min((unsigned short)(state->default_slot_quota * 256),
+		(unsigned short)~0);
+
+	state->previous_data_index = -1;
+	state->data_use_count = 0;
+	state->data_quota = state->slot_queue_available - 1;
+
+	local->trigger.event = &state->trigger_event;
+	remote_event_create(&local->trigger);
+	local->tx_pos = 0;
+
+	local->recycle.event = &state->recycle_event;
+	remote_event_create(&local->recycle);
+	local->slot_queue_recycle = state->slot_queue_available;
+
+	local->sync_trigger.event = &state->sync_trigger_event;
+	remote_event_create(&local->sync_trigger);
+
+	local->sync_release.event = &state->sync_release_event;
+	remote_event_create(&local->sync_release);
+
+	/* At start-of-day, the slot is empty and available */
+	((VCHIQ_HEADER_T *)SLOT_DATA_FROM_INDEX(state, local->slot_sync))->msgid
+		= VCHIQ_MSGID_PADDING;
+	remote_event_signal_local(&local->sync_release);
+
+	local->debug[DEBUG_ENTRIES] = DEBUG_MAX;
+
+	status = vchiq_platform_init_state(state);
+
+	/*
+		bring up slot handler thread
+	 */
+	snprintf(threadname, sizeof(threadname), "VCHIQ-%d", state->id);
+	state->slot_handler_thread = kthread_create(&slot_handler_func,
+		(void *)state,
+		threadname);
+
+	if (state->slot_handler_thread == NULL) {
+		vchiq_loud_error_header();
+		vchiq_loud_error("couldn't create thread %s", threadname);
+		vchiq_loud_error_footer();
+		return VCHIQ_ERROR;
+	}
+	set_user_nice(state->slot_handler_thread, -19);
+	wake_up_process(state->slot_handler_thread);
+
+	snprintf(threadname, sizeof(threadname), "VCHIQr-%d", state->id);
+	state->recycle_thread = kthread_create(&recycle_func,
+		(void *)state,
+		threadname);
+	if (state->recycle_thread == NULL) {
+		vchiq_loud_error_header();
+		vchiq_loud_error("couldn't create thread %s", threadname);
+		vchiq_loud_error_footer();
+		return VCHIQ_ERROR;
+	}
+	set_user_nice(state->recycle_thread, -19);
+	wake_up_process(state->recycle_thread);
+
+	snprintf(threadname, sizeof(threadname), "VCHIQs-%d", state->id);
+	state->sync_thread = kthread_create(&sync_func,
+		(void *)state,
+		threadname);
+	if (state->sync_thread == NULL) {
+		vchiq_loud_error_header();
+		vchiq_loud_error("couldn't create thread %s", threadname);
+		vchiq_loud_error_footer();
+		return VCHIQ_ERROR;
+	}
+	set_user_nice(state->sync_thread, -20);
+	wake_up_process(state->sync_thread);
+
+	BUG_ON(state->id >= VCHIQ_MAX_STATES);
+	vchiq_states[state->id] = state;
+
+	/* Indicate readiness to the other side */
+	local->initialised = 1;
+
+	return status;
+}
+
+/* Called from application thread when a client or server service is created. */
+VCHIQ_SERVICE_T *
+vchiq_add_service_internal(VCHIQ_STATE_T *state,
+	const VCHIQ_SERVICE_PARAMS_T *params, int srvstate,
+	VCHIQ_INSTANCE_T instance, VCHIQ_USERDATA_TERM_T userdata_term)
+{
+	VCHIQ_SERVICE_T *service;
+
+	service = kmalloc(sizeof(VCHIQ_SERVICE_T), GFP_KERNEL);
+	if (service) {
+		service->base.fourcc   = params->fourcc;
+		service->base.callback = params->callback;
+		service->base.userdata = params->userdata;
+		service->handle        = VCHIQ_SERVICE_HANDLE_INVALID;
+		service->ref_count     = 1;
+		service->srvstate      = VCHIQ_SRVSTATE_FREE;
+		service->userdata_term = userdata_term;
+		service->localport     = VCHIQ_PORT_FREE;
+		service->remoteport    = VCHIQ_PORT_FREE;
+
+		service->public_fourcc = (srvstate == VCHIQ_SRVSTATE_OPENING) ?
+			VCHIQ_FOURCC_INVALID : params->fourcc;
+		service->client_id     = 0;
+		service->auto_close    = 1;
+		service->sync          = 0;
+		service->closing       = 0;
+		service->trace         = 0;
+		atomic_set(&service->poll_flags, 0);
+		service->version       = params->version;
+		service->version_min   = params->version_min;
+		service->state         = state;
+		service->instance      = instance;
+		service->service_use_count = 0;
+		init_bulk_queue(&service->bulk_tx);
+		init_bulk_queue(&service->bulk_rx);
+		sema_init(&service->remove_event, 0);
+		sema_init(&service->bulk_remove_event, 0);
+		mutex_init(&service->bulk_mutex);
+		memset(&service->stats, 0, sizeof(service->stats));
+	} else {
+		vchiq_log_error(vchiq_core_log_level,
+			"Out of memory");
+	}
+
+	if (service) {
+		VCHIQ_SERVICE_T **pservice = NULL;
+		int i;
+
+		/* Although it is perfectly possible to use service_spinlock
+		** to protect the creation of services, it is overkill as it
+		** disables interrupts while the array is searched.
+		** The only danger is of another thread trying to create a
+		** service - service deletion is safe.
+		** Therefore it is preferable to use state->mutex which,
+		** although slower to claim, doesn't block interrupts while
+		** it is held.
+		*/
+
+		mutex_lock(&state->mutex);
+
+		/* Prepare to use a previously unused service */
+		if (state->unused_service < VCHIQ_MAX_SERVICES)
+			pservice = &state->services[state->unused_service];
+
+		if (srvstate == VCHIQ_SRVSTATE_OPENING) {
+			for (i = 0; i < state->unused_service; i++) {
+				VCHIQ_SERVICE_T *srv = state->services[i];
+				if (!srv) {
+					pservice = &state->services[i];
+					break;
+				}
+			}
+		} else {
+			for (i = (state->unused_service - 1); i >= 0; i--) {
+				VCHIQ_SERVICE_T *srv = state->services[i];
+				if (!srv)
+					pservice = &state->services[i];
+				else if ((srv->public_fourcc == params->fourcc)
+					&& ((srv->instance != instance) ||
+					(srv->base.callback !=
+					params->callback))) {
+					/* There is another server using this
+					** fourcc which doesn't match. */
+					pservice = NULL;
+					break;
+				}
+			}
+		}
+
+		if (pservice) {
+			service->localport = (pservice - state->services);
+			if (!handle_seq)
+				handle_seq = VCHIQ_MAX_STATES *
+					 VCHIQ_MAX_SERVICES;
+			service->handle = handle_seq |
+				(state->id * VCHIQ_MAX_SERVICES) |
+				service->localport;
+			handle_seq += VCHIQ_MAX_STATES * VCHIQ_MAX_SERVICES;
+			*pservice = service;
+			if (pservice == &state->services[state->unused_service])
+				state->unused_service++;
+		}
+
+		mutex_unlock(&state->mutex);
+
+		if (!pservice) {
+			kfree(service);
+			service = NULL;
+		}
+	}
+
+	if (service) {
+		VCHIQ_SERVICE_QUOTA_T *service_quota =
+			&state->service_quotas[service->localport];
+		service_quota->slot_quota = state->default_slot_quota;
+		service_quota->message_quota = state->default_message_quota;
+		if (service_quota->slot_use_count == 0)
+			service_quota->previous_tx_index =
+				SLOT_QUEUE_INDEX_FROM_POS(state->local_tx_pos)
+				- 1;
+
+		/* Bring this service online */
+		vchiq_set_service_state(service, srvstate);
+
+		vchiq_log_info(vchiq_core_msg_log_level,
+			"%s Service %c%c%c%c SrcPort:%d",
+			(srvstate == VCHIQ_SRVSTATE_OPENING)
+			? "Open" : "Add",
+			VCHIQ_FOURCC_AS_4CHARS(params->fourcc),
+			service->localport);
+	}
+
+	/* Don't unlock the service - leave it with a ref_count of 1. */
+
+	return service;
+}
+
+VCHIQ_STATUS_T
+vchiq_open_service_internal(VCHIQ_SERVICE_T *service, int client_id)
+{
+	struct vchiq_open_payload payload = {
+		service->base.fourcc,
+		client_id,
+		service->version,
+		service->version_min
+	};
+	VCHIQ_ELEMENT_T body = { &payload, sizeof(payload) };
+	VCHIQ_STATUS_T status = VCHIQ_SUCCESS;
+
+	service->client_id = client_id;
+	vchiq_use_service_internal(service);
+	status = queue_message(service->state, NULL,
+		VCHIQ_MAKE_MSG(VCHIQ_MSG_OPEN, service->localport, 0),
+		&body, 1, sizeof(payload), 1);
+	if (status == VCHIQ_SUCCESS) {
+		/* Wait for the ACK/NAK */
+		if (down_interruptible(&service->remove_event) != 0) {
+			status = VCHIQ_RETRY;
+			vchiq_release_service_internal(service);
+		} else if ((service->srvstate != VCHIQ_SRVSTATE_OPEN) &&
+			(service->srvstate != VCHIQ_SRVSTATE_OPENSYNC)) {
+			if (service->srvstate != VCHIQ_SRVSTATE_CLOSEWAIT)
+				vchiq_log_error(vchiq_core_log_level,
+					"%d: osi - srvstate = %s (ref %d)",
+					service->state->id,
+					srvstate_names[service->srvstate],
+					service->ref_count);
+			status = VCHIQ_ERROR;
+			VCHIQ_SERVICE_STATS_INC(service, error_count);
+			vchiq_release_service_internal(service);
+		}
+	}
+	return status;
+}
+
+static void
+release_service_messages(VCHIQ_SERVICE_T *service)
+{
+	VCHIQ_STATE_T *state = service->state;
+	int slot_last = state->remote->slot_last;
+	int i;
+
+	/* Release any claimed messages */
+	for (i = state->remote->slot_first; i <= slot_last; i++) {
+		VCHIQ_SLOT_INFO_T *slot_info =
+			SLOT_INFO_FROM_INDEX(state, i);
+		if (slot_info->release_count != slot_info->use_count) {
+			char *data =
+				(char *)SLOT_DATA_FROM_INDEX(state, i);
+			unsigned int pos, end;
+
+			end = VCHIQ_SLOT_SIZE;
+			if (data == state->rx_data)
+				/* This buffer is still being read from - stop
+				** at the current read position */
+				end = state->rx_pos & VCHIQ_SLOT_MASK;
+
+			pos = 0;
+
+			while (pos < end) {
+				VCHIQ_HEADER_T *header =
+					(VCHIQ_HEADER_T *)(data + pos);
+				int msgid = header->msgid;
+				int port = VCHIQ_MSG_DSTPORT(msgid);
+				if ((port == service->localport) &&
+					(msgid & VCHIQ_MSGID_CLAIMED)) {
+					vchiq_log_info(vchiq_core_log_level,
+						"  fsi - hdr %x",
+						(unsigned int)header);
+					release_slot(state, slot_info, header,
+						NULL);
+				}
+				pos += calc_stride(header->size);
+				if (pos > VCHIQ_SLOT_SIZE) {
+					vchiq_log_error(vchiq_core_log_level,
+						"fsi - pos %x: header %x, "
+						"msgid %x, header->msgid %x, "
+						"header->size %x",
+						pos, (unsigned int)header,
+						msgid, header->msgid,
+						header->size);
+					WARN(1, "invalid slot position\n");
+				}
+			}
+		}
+	}
+}
+
+static int
+do_abort_bulks(VCHIQ_SERVICE_T *service)
+{
+	VCHIQ_STATUS_T status;
+
+	/* Abort any outstanding bulk transfers */
+	if (mutex_lock_interruptible(&service->bulk_mutex) != 0)
+		return 0;
+	abort_outstanding_bulks(service, &service->bulk_tx);
+	abort_outstanding_bulks(service, &service->bulk_rx);
+	mutex_unlock(&service->bulk_mutex);
+
+	status = notify_bulks(service, &service->bulk_tx, 0/*!retry_poll*/);
+	if (status == VCHIQ_SUCCESS)
+		status = notify_bulks(service, &service->bulk_rx,
+			0/*!retry_poll*/);
+	return (status == VCHIQ_SUCCESS);
+}
+
+static VCHIQ_STATUS_T
+close_service_complete(VCHIQ_SERVICE_T *service, int failstate)
+{
+	VCHIQ_STATUS_T status;
+	int is_server = (service->public_fourcc != VCHIQ_FOURCC_INVALID);
+	int newstate;
+
+	switch (service->srvstate) {
+	case VCHIQ_SRVSTATE_OPEN:
+	case VCHIQ_SRVSTATE_CLOSESENT:
+	case VCHIQ_SRVSTATE_CLOSERECVD:
+		if (is_server) {
+			if (service->auto_close) {
+				service->client_id = 0;
+				service->remoteport = VCHIQ_PORT_FREE;
+				newstate = VCHIQ_SRVSTATE_LISTENING;
+			} else
+				newstate = VCHIQ_SRVSTATE_CLOSEWAIT;
+		} else
+			newstate = VCHIQ_SRVSTATE_CLOSED;
+		vchiq_set_service_state(service, newstate);
+		break;
+	case VCHIQ_SRVSTATE_LISTENING:
+		break;
+	default:
+		vchiq_log_error(vchiq_core_log_level,
+			"close_service_complete(%x) called in state %s",
+			service->handle, srvstate_names[service->srvstate]);
+		WARN(1, "close_service_complete in unexpected state\n");
+		return VCHIQ_ERROR;
+	}
+
+	status = make_service_callback(service,
+		VCHIQ_SERVICE_CLOSED, NULL, NULL);
+
+	if (status != VCHIQ_RETRY) {
+		int uc = service->service_use_count;
+		int i;
+		/* Complete the close process */
+		for (i = 0; i < uc; i++)
+			/* cater for cases where close is forced and the
+			** client may not close all it's handles */
+			vchiq_release_service_internal(service);
+
+		service->client_id = 0;
+		service->remoteport = VCHIQ_PORT_FREE;
+
+		if (service->srvstate == VCHIQ_SRVSTATE_CLOSED)
+			vchiq_free_service_internal(service);
+		else if (service->srvstate != VCHIQ_SRVSTATE_CLOSEWAIT) {
+			if (is_server)
+				service->closing = 0;
+
+			up(&service->remove_event);
+		}
+	} else
+		vchiq_set_service_state(service, failstate);
+
+	return status;
+}
+
+/* Called by the slot handler */
+VCHIQ_STATUS_T
+vchiq_close_service_internal(VCHIQ_SERVICE_T *service, int close_recvd)
+{
+	VCHIQ_STATE_T *state = service->state;
+	VCHIQ_STATUS_T status = VCHIQ_SUCCESS;
+	int is_server = (service->public_fourcc != VCHIQ_FOURCC_INVALID);
+
+	vchiq_log_info(vchiq_core_log_level, "%d: csi:%d,%d (%s)",
+		service->state->id, service->localport, close_recvd,
+		srvstate_names[service->srvstate]);
+
+	switch (service->srvstate) {
+	case VCHIQ_SRVSTATE_CLOSED:
+	case VCHIQ_SRVSTATE_HIDDEN:
+	case VCHIQ_SRVSTATE_LISTENING:
+	case VCHIQ_SRVSTATE_CLOSEWAIT:
+		if (close_recvd)
+			vchiq_log_error(vchiq_core_log_level,
+				"vchiq_close_service_internal(1) called "
+				"in state %s",
+				srvstate_names[service->srvstate]);
+		else if (is_server) {
+			if (service->srvstate == VCHIQ_SRVSTATE_LISTENING) {
+				status = VCHIQ_ERROR;
+			} else {
+				service->client_id = 0;
+				service->remoteport = VCHIQ_PORT_FREE;
+				if (service->srvstate ==
+					VCHIQ_SRVSTATE_CLOSEWAIT)
+					vchiq_set_service_state(service,
+						VCHIQ_SRVSTATE_LISTENING);
+			}
+			up(&service->remove_event);
+		} else
+			vchiq_free_service_internal(service);
+		break;
+	case VCHIQ_SRVSTATE_OPENING:
+		if (close_recvd) {
+			/* The open was rejected - tell the user */
+			vchiq_set_service_state(service,
+				VCHIQ_SRVSTATE_CLOSEWAIT);
+			up(&service->remove_event);
+		} else {
+			/* Shutdown mid-open - let the other side know */
+			status = queue_message(state, service,
+				VCHIQ_MAKE_MSG
+				(VCHIQ_MSG_CLOSE,
+				service->localport,
+				VCHIQ_MSG_DSTPORT(service->remoteport)),
+				NULL, 0, 0, 0);
+		}
+		break;
+
+	case VCHIQ_SRVSTATE_OPENSYNC:
+		mutex_lock(&state->sync_mutex);
+		/* Drop through */
+
+	case VCHIQ_SRVSTATE_OPEN:
+		if (state->is_master || close_recvd) {
+			if (!do_abort_bulks(service))
+				status = VCHIQ_RETRY;
+		}
+
+		release_service_messages(service);
+
+		if (status == VCHIQ_SUCCESS)
+			status = queue_message(state, service,
+				VCHIQ_MAKE_MSG
+				(VCHIQ_MSG_CLOSE,
+				service->localport,
+				VCHIQ_MSG_DSTPORT(service->remoteport)),
+				NULL, 0, 0, 0);
+
+		if (status == VCHIQ_SUCCESS) {
+			if (!close_recvd)
+				break;
+		} else if (service->srvstate == VCHIQ_SRVSTATE_OPENSYNC) {
+			mutex_unlock(&state->sync_mutex);
+			break;
+		} else
+			break;
+
+		status = close_service_complete(service,
+				VCHIQ_SRVSTATE_CLOSERECVD);
+		break;
+
+	case VCHIQ_SRVSTATE_CLOSESENT:
+		if (!close_recvd)
+			/* This happens when a process is killed mid-close */
+			break;
+
+		if (!state->is_master) {
+			if (!do_abort_bulks(service)) {
+				status = VCHIQ_RETRY;
+				break;
+			}
+		}
+
+		if (status == VCHIQ_SUCCESS)
+			status = close_service_complete(service,
+				VCHIQ_SRVSTATE_CLOSERECVD);
+		break;
+
+	case VCHIQ_SRVSTATE_CLOSERECVD:
+		if (!close_recvd && is_server)
+			/* Force into LISTENING mode */
+			vchiq_set_service_state(service,
+				VCHIQ_SRVSTATE_LISTENING);
+		status = close_service_complete(service,
+			VCHIQ_SRVSTATE_CLOSERECVD);
+		break;
+
+	default:
+		vchiq_log_error(vchiq_core_log_level,
+			"vchiq_close_service_internal(%d) called in state %s",
+			close_recvd, srvstate_names[service->srvstate]);
+		break;
+	}
+
+	return status;
+}
+
+/* Called from the application process upon process death */
+void
+vchiq_terminate_service_internal(VCHIQ_SERVICE_T *service)
+{
+	VCHIQ_STATE_T *state = service->state;
+
+	vchiq_log_info(vchiq_core_log_level, "%d: tsi - (%d<->%d)",
+		state->id, service->localport, service->remoteport);
+
+	mark_service_closing(service);
+
+	/* Mark the service for removal by the slot handler */
+	request_poll(state, service, VCHIQ_POLL_REMOVE);
+}
+
+/* Called from the slot handler */
+void
+vchiq_free_service_internal(VCHIQ_SERVICE_T *service)
+{
+	VCHIQ_STATE_T *state = service->state;
+
+	vchiq_log_info(vchiq_core_log_level, "%d: fsi - (%d)",
+		state->id, service->localport);
+
+	switch (service->srvstate) {
+	case VCHIQ_SRVSTATE_OPENING:
+	case VCHIQ_SRVSTATE_CLOSED:
+	case VCHIQ_SRVSTATE_HIDDEN:
+	case VCHIQ_SRVSTATE_LISTENING:
+	case VCHIQ_SRVSTATE_CLOSEWAIT:
+		break;
+	default:
+		vchiq_log_error(vchiq_core_log_level,
+			"%d: fsi - (%d) in state %s",
+			state->id, service->localport,
+			srvstate_names[service->srvstate]);
+		return;
+	}
+
+	vchiq_set_service_state(service, VCHIQ_SRVSTATE_FREE);
+
+	up(&service->remove_event);
+
+	/* Release the initial lock */
+	unlock_service(service);
+}
+
+VCHIQ_STATUS_T
+vchiq_connect_internal(VCHIQ_STATE_T *state, VCHIQ_INSTANCE_T instance)
+{
+	VCHIQ_SERVICE_T *service;
+	int i;
+
+	/* Find all services registered to this client and enable them. */
+	i = 0;
+	while ((service = next_service_by_instance(state, instance,
+		&i)) !=	NULL) {
+		if (service->srvstate == VCHIQ_SRVSTATE_HIDDEN)
+			vchiq_set_service_state(service,
+				VCHIQ_SRVSTATE_LISTENING);
+		unlock_service(service);
+	}
+
+	if (state->conn_state == VCHIQ_CONNSTATE_DISCONNECTED) {
+		if (queue_message(state, NULL,
+			VCHIQ_MAKE_MSG(VCHIQ_MSG_CONNECT, 0, 0), NULL, 0,
+			0, 1) == VCHIQ_RETRY)
+			return VCHIQ_RETRY;
+
+		vchiq_set_conn_state(state, VCHIQ_CONNSTATE_CONNECTING);
+	}
+
+	if (state->conn_state == VCHIQ_CONNSTATE_CONNECTING) {
+		if (down_interruptible(&state->connect) != 0)
+			return VCHIQ_RETRY;
+
+		vchiq_set_conn_state(state, VCHIQ_CONNSTATE_CONNECTED);
+		up(&state->connect);
+	}
+
+	return VCHIQ_SUCCESS;
+}
+
+VCHIQ_STATUS_T
+vchiq_shutdown_internal(VCHIQ_STATE_T *state, VCHIQ_INSTANCE_T instance)
+{
+	VCHIQ_SERVICE_T *service;
+	int i;
+
+	/* Find all services registered to this client and enable them. */
+	i = 0;
+	while ((service = next_service_by_instance(state, instance,
+		&i)) !=	NULL) {
+		(void)vchiq_remove_service(service->handle);
+		unlock_service(service);
+	}
+
+	return VCHIQ_SUCCESS;
+}
+
+VCHIQ_STATUS_T
+vchiq_pause_internal(VCHIQ_STATE_T *state)
+{
+	VCHIQ_STATUS_T status = VCHIQ_SUCCESS;
+
+	switch (state->conn_state) {
+	case VCHIQ_CONNSTATE_CONNECTED:
+		/* Request a pause */
+		vchiq_set_conn_state(state, VCHIQ_CONNSTATE_PAUSING);
+		request_poll(state, NULL, 0);
+		break;
+	default:
+		vchiq_log_error(vchiq_core_log_level,
+			"vchiq_pause_internal in state %s\n",
+			conn_state_names[state->conn_state]);
+		status = VCHIQ_ERROR;
+		VCHIQ_STATS_INC(state, error_count);
+		break;
+	}
+
+	return status;
+}
+
+VCHIQ_STATUS_T
+vchiq_resume_internal(VCHIQ_STATE_T *state)
+{
+	VCHIQ_STATUS_T status = VCHIQ_SUCCESS;
+
+	if (state->conn_state == VCHIQ_CONNSTATE_PAUSED) {
+		vchiq_set_conn_state(state, VCHIQ_CONNSTATE_RESUMING);
+		request_poll(state, NULL, 0);
+	} else {
+		status = VCHIQ_ERROR;
+		VCHIQ_STATS_INC(state, error_count);
+	}
+
+	return status;
+}
+
+VCHIQ_STATUS_T
+vchiq_close_service(VCHIQ_SERVICE_HANDLE_T handle)
+{
+	/* Unregister the service */
+	VCHIQ_SERVICE_T *service = find_service_by_handle(handle);
+	VCHIQ_STATUS_T status = VCHIQ_SUCCESS;
+
+	if (!service)
+		return VCHIQ_ERROR;
+
+	vchiq_log_info(vchiq_core_log_level,
+		"%d: close_service:%d",
+		service->state->id, service->localport);
+
+	if ((service->srvstate == VCHIQ_SRVSTATE_FREE) ||
+		(service->srvstate == VCHIQ_SRVSTATE_LISTENING) ||
+		(service->srvstate == VCHIQ_SRVSTATE_HIDDEN)) {
+		unlock_service(service);
+		return VCHIQ_ERROR;
+	}
+
+	mark_service_closing(service);
+
+	if (current == service->state->slot_handler_thread) {
+		status = vchiq_close_service_internal(service,
+			0/*!close_recvd*/);
+		BUG_ON(status == VCHIQ_RETRY);
+	} else {
+	/* Mark the service for termination by the slot handler */
+		request_poll(service->state, service, VCHIQ_POLL_TERMINATE);
+	}
+
+	while (1) {
+		if (down_interruptible(&service->remove_event) != 0) {
+			status = VCHIQ_RETRY;
+			break;
+		}
+
+		if ((service->srvstate == VCHIQ_SRVSTATE_FREE) ||
+			(service->srvstate == VCHIQ_SRVSTATE_LISTENING) ||
+			(service->srvstate == VCHIQ_SRVSTATE_OPEN))
+			break;
+
+		vchiq_log_warning(vchiq_core_log_level,
+			"%d: close_service:%d - waiting in state %s",
+			service->state->id, service->localport,
+			srvstate_names[service->srvstate]);
+	}
+
+	if ((status == VCHIQ_SUCCESS) &&
+		(service->srvstate != VCHIQ_SRVSTATE_FREE) &&
+		(service->srvstate != VCHIQ_SRVSTATE_LISTENING))
+		status = VCHIQ_ERROR;
+
+	unlock_service(service);
+
+	return status;
+}
+
+VCHIQ_STATUS_T
+vchiq_remove_service(VCHIQ_SERVICE_HANDLE_T handle)
+{
+	/* Unregister the service */
+	VCHIQ_SERVICE_T *service = find_service_by_handle(handle);
+	VCHIQ_STATUS_T status = VCHIQ_SUCCESS;
+
+	if (!service)
+		return VCHIQ_ERROR;
+
+	vchiq_log_info(vchiq_core_log_level,
+		"%d: remove_service:%d",
+		service->state->id, service->localport);
+
+	if (service->srvstate == VCHIQ_SRVSTATE_FREE) {
+		unlock_service(service);
+		return VCHIQ_ERROR;
+	}
+
+	mark_service_closing(service);
+
+	if ((service->srvstate == VCHIQ_SRVSTATE_HIDDEN) ||
+		(current == service->state->slot_handler_thread)) {
+		/* Make it look like a client, because it must be removed and
+		   not left in the LISTENING state. */
+		service->public_fourcc = VCHIQ_FOURCC_INVALID;
+
+		status = vchiq_close_service_internal(service,
+			0/*!close_recvd*/);
+		BUG_ON(status == VCHIQ_RETRY);
+	} else {
+		/* Mark the service for removal by the slot handler */
+		request_poll(service->state, service, VCHIQ_POLL_REMOVE);
+	}
+	while (1) {
+		if (down_interruptible(&service->remove_event) != 0) {
+			status = VCHIQ_RETRY;
+			break;
+		}
+
+		if ((service->srvstate == VCHIQ_SRVSTATE_FREE) ||
+			(service->srvstate == VCHIQ_SRVSTATE_OPEN))
+			break;
+
+		vchiq_log_warning(vchiq_core_log_level,
+			"%d: remove_service:%d - waiting in state %s",
+			service->state->id, service->localport,
+			srvstate_names[service->srvstate]);
+	}
+
+	if ((status == VCHIQ_SUCCESS) &&
+		(service->srvstate != VCHIQ_SRVSTATE_FREE))
+		status = VCHIQ_ERROR;
+
+	unlock_service(service);
+
+	return status;
+}
+
+
+/* This function may be called by kernel threads or user threads.
+ * User threads may receive VCHIQ_RETRY to indicate that a signal has been
+ * received and the call should be retried after being returned to user
+ * context.
+ * When called in blocking mode, the userdata field points to a bulk_waiter
+ * structure.
+ */
+VCHIQ_STATUS_T
+vchiq_bulk_transfer(VCHIQ_SERVICE_HANDLE_T handle,
+	VCHI_MEM_HANDLE_T memhandle, void *offset, int size, void *userdata,
+	VCHIQ_BULK_MODE_T mode, VCHIQ_BULK_DIR_T dir)
+{
+	VCHIQ_SERVICE_T *service = find_service_by_handle(handle);
+	VCHIQ_BULK_QUEUE_T *queue;
+	VCHIQ_BULK_T *bulk;
+	VCHIQ_STATE_T *state;
+	struct bulk_waiter *bulk_waiter = NULL;
+	const char dir_char = (dir == VCHIQ_BULK_TRANSMIT) ? 't' : 'r';
+	const int dir_msgtype = (dir == VCHIQ_BULK_TRANSMIT) ?
+		VCHIQ_MSG_BULK_TX : VCHIQ_MSG_BULK_RX;
+	VCHIQ_STATUS_T status = VCHIQ_ERROR;
+
+	if (!service ||
+		 (service->srvstate != VCHIQ_SRVSTATE_OPEN) ||
+		 ((memhandle == VCHI_MEM_HANDLE_INVALID) && (offset == NULL)) ||
+		 (vchiq_check_service(service) != VCHIQ_SUCCESS))
+		goto error_exit;
+
+	switch (mode) {
+	case VCHIQ_BULK_MODE_NOCALLBACK:
+	case VCHIQ_BULK_MODE_CALLBACK:
+		break;
+	case VCHIQ_BULK_MODE_BLOCKING:
+		bulk_waiter = (struct bulk_waiter *)userdata;
+		sema_init(&bulk_waiter->event, 0);
+		bulk_waiter->actual = 0;
+		bulk_waiter->bulk = NULL;
+		break;
+	case VCHIQ_BULK_MODE_WAITING:
+		bulk_waiter = (struct bulk_waiter *)userdata;
+		bulk = bulk_waiter->bulk;
+		goto waiting;
+	default:
+		goto error_exit;
+	}
+
+	state = service->state;
+
+	queue = (dir == VCHIQ_BULK_TRANSMIT) ?
+		&service->bulk_tx : &service->bulk_rx;
+
+	if (mutex_lock_interruptible(&service->bulk_mutex) != 0) {
+		status = VCHIQ_RETRY;
+		goto error_exit;
+	}
+
+	if (queue->local_insert == queue->remove + VCHIQ_NUM_SERVICE_BULKS) {
+		VCHIQ_SERVICE_STATS_INC(service, bulk_stalls);
+		do {
+			mutex_unlock(&service->bulk_mutex);
+			if (down_interruptible(&service->bulk_remove_event)
+				!= 0) {
+				status = VCHIQ_RETRY;
+				goto error_exit;
+			}
+			if (mutex_lock_interruptible(&service->bulk_mutex)
+				!= 0) {
+				status = VCHIQ_RETRY;
+				goto error_exit;
+			}
+		} while (queue->local_insert == queue->remove +
+				VCHIQ_NUM_SERVICE_BULKS);
+	}
+
+	bulk = &queue->bulks[BULK_INDEX(queue->local_insert)];
+
+	bulk->mode = mode;
+	bulk->dir = dir;
+	bulk->userdata = userdata;
+	bulk->size = size;
+	bulk->actual = VCHIQ_BULK_ACTUAL_ABORTED;
+
+	if (vchiq_prepare_bulk_data(bulk, memhandle, offset, size, dir) !=
+		VCHIQ_SUCCESS)
+		goto unlock_error_exit;
+
+	wmb();
+
+	vchiq_log_info(vchiq_core_log_level,
+		"%d: bt (%d->%d) %cx %x@%x %x",
+		state->id,
+		service->localport, service->remoteport, dir_char,
+		size, (unsigned int)bulk->data, (unsigned int)userdata);
+
+	if (state->is_master) {
+		queue->local_insert++;
+		if (resolve_bulks(service, queue))
+			request_poll(state, service,
+				(dir == VCHIQ_BULK_TRANSMIT) ?
+				VCHIQ_POLL_TXNOTIFY : VCHIQ_POLL_RXNOTIFY);
+	} else {
+		int payload[2] = { (int)bulk->data, bulk->size };
+		VCHIQ_ELEMENT_T element = { payload, sizeof(payload) };
+
+		status = queue_message(state, NULL,
+			VCHIQ_MAKE_MSG(dir_msgtype,
+				service->localport, service->remoteport),
+			&element, 1, sizeof(payload), 1);
+		if (status != VCHIQ_SUCCESS) {
+			vchiq_complete_bulk(bulk);
+			goto unlock_error_exit;
+		}
+		queue->local_insert++;
+	}
+
+	mutex_unlock(&service->bulk_mutex);
+
+	vchiq_log_trace(vchiq_core_log_level,
+		"%d: bt:%d %cx li=%x ri=%x p=%x",
+		state->id,
+		service->localport, dir_char,
+		queue->local_insert, queue->remote_insert, queue->process);
+
+waiting:
+	unlock_service(service);
+
+	status = VCHIQ_SUCCESS;
+
+	if (bulk_waiter) {
+		bulk_waiter->bulk = bulk;
+		if (down_interruptible(&bulk_waiter->event) != 0)
+			status = VCHIQ_RETRY;
+		else if (bulk_waiter->actual == VCHIQ_BULK_ACTUAL_ABORTED)
+			status = VCHIQ_ERROR;
+	}
+
+	return status;
+
+unlock_error_exit:
+	mutex_unlock(&service->bulk_mutex);
+
+error_exit:
+	if (service)
+		unlock_service(service);
+	return status;
+}
+
+VCHIQ_STATUS_T
+vchiq_queue_message(VCHIQ_SERVICE_HANDLE_T handle,
+	const VCHIQ_ELEMENT_T *elements, unsigned int count)
+{
+	VCHIQ_SERVICE_T *service = find_service_by_handle(handle);
+	VCHIQ_STATUS_T status = VCHIQ_ERROR;
+
+	unsigned int size = 0;
+	unsigned int i;
+
+	if (!service ||
+		(vchiq_check_service(service) != VCHIQ_SUCCESS))
+		goto error_exit;
+
+	for (i = 0; i < (unsigned int)count; i++) {
+		if (elements[i].size) {
+			if (elements[i].data == NULL) {
+				VCHIQ_SERVICE_STATS_INC(service, error_count);
+				goto error_exit;
+			}
+			size += elements[i].size;
+		}
+	}
+
+	if (size > VCHIQ_MAX_MSG_SIZE) {
+		VCHIQ_SERVICE_STATS_INC(service, error_count);
+		goto error_exit;
+	}
+
+	switch (service->srvstate) {
+	case VCHIQ_SRVSTATE_OPEN:
+		status = queue_message(service->state, service,
+				VCHIQ_MAKE_MSG(VCHIQ_MSG_DATA,
+					service->localport,
+					service->remoteport),
+				elements, count, size, 1);
+		break;
+	case VCHIQ_SRVSTATE_OPENSYNC:
+		status = queue_message_sync(service->state, service,
+				VCHIQ_MAKE_MSG(VCHIQ_MSG_DATA,
+					service->localport,
+					service->remoteport),
+				elements, count, size, 1);
+		break;
+	default:
+		status = VCHIQ_ERROR;
+		break;
+	}
+
+error_exit:
+	if (service)
+		unlock_service(service);
+
+	return status;
+}
+
+void
+vchiq_release_message(VCHIQ_SERVICE_HANDLE_T handle, VCHIQ_HEADER_T *header)
+{
+	VCHIQ_SERVICE_T *service = find_service_by_handle(handle);
+	VCHIQ_SHARED_STATE_T *remote;
+	VCHIQ_STATE_T *state;
+	int slot_index;
+
+	if (!service)
+		return;
+
+	state = service->state;
+	remote = state->remote;
+
+	slot_index = SLOT_INDEX_FROM_DATA(state, (void *)header);
+
+	if ((slot_index >= remote->slot_first) &&
+		(slot_index <= remote->slot_last)) {
+		int msgid = header->msgid;
+		if (msgid & VCHIQ_MSGID_CLAIMED) {
+			VCHIQ_SLOT_INFO_T *slot_info =
+				SLOT_INFO_FROM_INDEX(state, slot_index);
+
+			release_slot(state, slot_info, header, service);
+		}
+	} else if (slot_index == remote->slot_sync)
+		release_message_sync(state, header);
+
+	unlock_service(service);
+}
+
+static void
+release_message_sync(VCHIQ_STATE_T *state, VCHIQ_HEADER_T *header)
+{
+	header->msgid = VCHIQ_MSGID_PADDING;
+	wmb();
+	remote_event_signal(&state->remote->sync_release);
+}
+
+VCHIQ_STATUS_T
+vchiq_get_peer_version(VCHIQ_SERVICE_HANDLE_T handle, short *peer_version)
+{
+   VCHIQ_STATUS_T status = VCHIQ_ERROR;
+   VCHIQ_SERVICE_T *service = find_service_by_handle(handle);
+
+   if (!service ||
+      (vchiq_check_service(service) != VCHIQ_SUCCESS) ||
+      !peer_version)
+      goto exit;
+   *peer_version = service->peer_version;
+   status = VCHIQ_SUCCESS;
+
+exit:
+   if (service)
+      unlock_service(service);
+   return status;
+}
+
+VCHIQ_STATUS_T
+vchiq_get_config(VCHIQ_INSTANCE_T instance,
+	int config_size, VCHIQ_CONFIG_T *pconfig)
+{
+	VCHIQ_CONFIG_T config;
+
+	(void)instance;
+
+	config.max_msg_size           = VCHIQ_MAX_MSG_SIZE;
+	config.bulk_threshold         = VCHIQ_MAX_MSG_SIZE;
+	config.max_outstanding_bulks  = VCHIQ_NUM_SERVICE_BULKS;
+	config.max_services           = VCHIQ_MAX_SERVICES;
+	config.version                = VCHIQ_VERSION;
+	config.version_min            = VCHIQ_VERSION_MIN;
+
+	if (config_size > sizeof(VCHIQ_CONFIG_T))
+		return VCHIQ_ERROR;
+
+	memcpy(pconfig, &config,
+		min(config_size, (int)(sizeof(VCHIQ_CONFIG_T))));
+
+	return VCHIQ_SUCCESS;
+}
+
+VCHIQ_STATUS_T
+vchiq_set_service_option(VCHIQ_SERVICE_HANDLE_T handle,
+	VCHIQ_SERVICE_OPTION_T option, int value)
+{
+	VCHIQ_SERVICE_T *service = find_service_by_handle(handle);
+	VCHIQ_STATUS_T status = VCHIQ_ERROR;
+
+	if (service) {
+		switch (option) {
+		case VCHIQ_SERVICE_OPTION_AUTOCLOSE:
+			service->auto_close = value;
+			status = VCHIQ_SUCCESS;
+			break;
+
+		case VCHIQ_SERVICE_OPTION_SLOT_QUOTA: {
+			VCHIQ_SERVICE_QUOTA_T *service_quota =
+				&service->state->service_quotas[
+					service->localport];
+			if (value == 0)
+				value = service->state->default_slot_quota;
+			if ((value >= service_quota->slot_use_count) &&
+				 (value < (unsigned short)~0)) {
+				service_quota->slot_quota = value;
+				if ((value >= service_quota->slot_use_count) &&
+					(service_quota->message_quota >=
+					 service_quota->message_use_count)) {
+					/* Signal the service that it may have
+					** dropped below its quota */
+					up(&service_quota->quota_event);
+				}
+				status = VCHIQ_SUCCESS;
+			}
+		} break;
+
+		case VCHIQ_SERVICE_OPTION_MESSAGE_QUOTA: {
+			VCHIQ_SERVICE_QUOTA_T *service_quota =
+				&service->state->service_quotas[
+					service->localport];
+			if (value == 0)
+				value = service->state->default_message_quota;
+			if ((value >= service_quota->message_use_count) &&
+				 (value < (unsigned short)~0)) {
+				service_quota->message_quota = value;
+				if ((value >=
+					service_quota->message_use_count) &&
+					(service_quota->slot_quota >=
+					service_quota->slot_use_count))
+					/* Signal the service that it may have
+					** dropped below its quota */
+					up(&service_quota->quota_event);
+				status = VCHIQ_SUCCESS;
+			}
+		} break;
+
+		case VCHIQ_SERVICE_OPTION_SYNCHRONOUS:
+			if ((service->srvstate == VCHIQ_SRVSTATE_HIDDEN) ||
+				(service->srvstate ==
+				VCHIQ_SRVSTATE_LISTENING)) {
+				service->sync = value;
+				status = VCHIQ_SUCCESS;
+			}
+			break;
+
+		case VCHIQ_SERVICE_OPTION_TRACE:
+			service->trace = value;
+			status = VCHIQ_SUCCESS;
+			break;
+
+		default:
+			break;
+		}
+		unlock_service(service);
+	}
+
+	return status;
+}
+
+void
+vchiq_dump_shared_state(void *dump_context, VCHIQ_STATE_T *state,
+	VCHIQ_SHARED_STATE_T *shared, const char *label)
+{
+	static const char *const debug_names[] = {
+		"<entries>",
+		"SLOT_HANDLER_COUNT",
+		"SLOT_HANDLER_LINE",
+		"PARSE_LINE",
+		"PARSE_HEADER",
+		"PARSE_MSGID",
+		"AWAIT_COMPLETION_LINE",
+		"DEQUEUE_MESSAGE_LINE",
+		"SERVICE_CALLBACK_LINE",
+		"MSG_QUEUE_FULL_COUNT",
+		"COMPLETION_QUEUE_FULL_COUNT"
+	};
+	int i;
+
+	char buf[80];
+	int len;
+	len = snprintf(buf, sizeof(buf),
+		"  %s: slots %d-%d tx_pos=%x recycle=%x",
+		label, shared->slot_first, shared->slot_last,
+		shared->tx_pos, shared->slot_queue_recycle);
+	vchiq_dump(dump_context, buf, len + 1);
+
+	len = snprintf(buf, sizeof(buf),
+		"    Slots claimed:");
+	vchiq_dump(dump_context, buf, len + 1);
+
+	for (i = shared->slot_first; i <= shared->slot_last; i++) {
+		VCHIQ_SLOT_INFO_T slot_info = *SLOT_INFO_FROM_INDEX(state, i);
+		if (slot_info.use_count != slot_info.release_count) {
+			len = snprintf(buf, sizeof(buf),
+				"      %d: %d/%d", i, slot_info.use_count,
+				slot_info.release_count);
+			vchiq_dump(dump_context, buf, len + 1);
+		}
+	}
+
+	for (i = 1; i < shared->debug[DEBUG_ENTRIES]; i++) {
+		len = snprintf(buf, sizeof(buf), "    DEBUG: %s = %d(%x)",
+			debug_names[i], shared->debug[i], shared->debug[i]);
+		vchiq_dump(dump_context, buf, len + 1);
+	}
+}
+
+void
+vchiq_dump_state(void *dump_context, VCHIQ_STATE_T *state)
+{
+	char buf[80];
+	int len;
+	int i;
+
+	len = snprintf(buf, sizeof(buf), "State %d: %s", state->id,
+		conn_state_names[state->conn_state]);
+	vchiq_dump(dump_context, buf, len + 1);
+
+	len = snprintf(buf, sizeof(buf),
+		"  tx_pos=%x(@%x), rx_pos=%x(@%x)",
+		state->local->tx_pos,
+		(uint32_t)state->tx_data +
+			(state->local_tx_pos & VCHIQ_SLOT_MASK),
+		state->rx_pos,
+		(uint32_t)state->rx_data +
+			(state->rx_pos & VCHIQ_SLOT_MASK));
+	vchiq_dump(dump_context, buf, len + 1);
+
+	len = snprintf(buf, sizeof(buf),
+		"  Version: %d (min %d)",
+		VCHIQ_VERSION, VCHIQ_VERSION_MIN);
+	vchiq_dump(dump_context, buf, len + 1);
+
+	if (VCHIQ_ENABLE_STATS) {
+		len = snprintf(buf, sizeof(buf),
+			"  Stats: ctrl_tx_count=%d, ctrl_rx_count=%d, "
+			"error_count=%d",
+			state->stats.ctrl_tx_count, state->stats.ctrl_rx_count,
+			state->stats.error_count);
+		vchiq_dump(dump_context, buf, len + 1);
+	}
+
+	len = snprintf(buf, sizeof(buf),
+		"  Slots: %d available (%d data), %d recyclable, %d stalls "
+		"(%d data)",
+		((state->slot_queue_available * VCHIQ_SLOT_SIZE) -
+			state->local_tx_pos) / VCHIQ_SLOT_SIZE,
+		state->data_quota - state->data_use_count,
+		state->local->slot_queue_recycle - state->slot_queue_available,
+		state->stats.slot_stalls, state->stats.data_stalls);
+	vchiq_dump(dump_context, buf, len + 1);
+
+	vchiq_dump_platform_state(dump_context);
+
+	vchiq_dump_shared_state(dump_context, state, state->local, "Local");
+	vchiq_dump_shared_state(dump_context, state, state->remote, "Remote");
+
+	vchiq_dump_platform_instances(dump_context);
+
+	for (i = 0; i < state->unused_service; i++) {
+		VCHIQ_SERVICE_T *service = find_service_by_port(state, i);
+
+		if (service) {
+			vchiq_dump_service_state(dump_context, service);
+			unlock_service(service);
+		}
+	}
+}
+
+void
+vchiq_dump_service_state(void *dump_context, VCHIQ_SERVICE_T *service)
+{
+	char buf[80];
+	int len;
+
+	len = snprintf(buf, sizeof(buf), "Service %d: %s (ref %u)",
+		service->localport, srvstate_names[service->srvstate],
+		service->ref_count - 1); /*Don't include the lock just taken*/
+
+	if (service->srvstate != VCHIQ_SRVSTATE_FREE) {
+		char remoteport[30];
+		VCHIQ_SERVICE_QUOTA_T *service_quota =
+			&service->state->service_quotas[service->localport];
+		int fourcc = service->base.fourcc;
+		int tx_pending, rx_pending;
+		if (service->remoteport != VCHIQ_PORT_FREE) {
+			int len2 = snprintf(remoteport, sizeof(remoteport),
+				"%d", service->remoteport);
+			if (service->public_fourcc != VCHIQ_FOURCC_INVALID)
+				snprintf(remoteport + len2,
+					sizeof(remoteport) - len2,
+					" (client %x)", service->client_id);
+		} else
+			strcpy(remoteport, "n/a");
+
+		len += snprintf(buf + len, sizeof(buf) - len,
+			" '%c%c%c%c' remote %s (msg use %d/%d, slot use %d/%d)",
+			VCHIQ_FOURCC_AS_4CHARS(fourcc),
+			remoteport,
+			service_quota->message_use_count,
+			service_quota->message_quota,
+			service_quota->slot_use_count,
+			service_quota->slot_quota);
+
+		vchiq_dump(dump_context, buf, len + 1);
+
+		tx_pending = service->bulk_tx.local_insert -
+			service->bulk_tx.remote_insert;
+
+		rx_pending = service->bulk_rx.local_insert -
+			service->bulk_rx.remote_insert;
+
+		len = snprintf(buf, sizeof(buf),
+			"  Bulk: tx_pending=%d (size %d),"
+			" rx_pending=%d (size %d)",
+			tx_pending,
+			tx_pending ? service->bulk_tx.bulks[
+			BULK_INDEX(service->bulk_tx.remove)].size : 0,
+			rx_pending,
+			rx_pending ? service->bulk_rx.bulks[
+			BULK_INDEX(service->bulk_rx.remove)].size : 0);
+
+		if (VCHIQ_ENABLE_STATS) {
+			vchiq_dump(dump_context, buf, len + 1);
+
+			len = snprintf(buf, sizeof(buf),
+				"  Ctrl: tx_count=%d, tx_bytes=%llu, "
+				"rx_count=%d, rx_bytes=%llu",
+				service->stats.ctrl_tx_count,
+				service->stats.ctrl_tx_bytes,
+				service->stats.ctrl_rx_count,
+				service->stats.ctrl_rx_bytes);
+			vchiq_dump(dump_context, buf, len + 1);
+
+			len = snprintf(buf, sizeof(buf),
+				"  Bulk: tx_count=%d, tx_bytes=%llu, "
+				"rx_count=%d, rx_bytes=%llu",
+				service->stats.bulk_tx_count,
+				service->stats.bulk_tx_bytes,
+				service->stats.bulk_rx_count,
+				service->stats.bulk_rx_bytes);
+			vchiq_dump(dump_context, buf, len + 1);
+
+			len = snprintf(buf, sizeof(buf),
+				"  %d quota stalls, %d slot stalls, "
+				"%d bulk stalls, %d aborted, %d errors",
+				service->stats.quota_stalls,
+				service->stats.slot_stalls,
+				service->stats.bulk_stalls,
+				service->stats.bulk_aborted_count,
+				service->stats.error_count);
+		 }
+	}
+
+	vchiq_dump(dump_context, buf, len + 1);
+
+	if (service->srvstate != VCHIQ_SRVSTATE_FREE)
+		vchiq_dump_platform_service_state(dump_context, service);
+}
+
+
+void
+vchiq_loud_error_header(void)
+{
+	vchiq_log_error(vchiq_core_log_level,
+		"============================================================"
+		"================");
+	vchiq_log_error(vchiq_core_log_level,
+		"============================================================"
+		"================");
+	vchiq_log_error(vchiq_core_log_level, "=====");
+}
+
+void
+vchiq_loud_error_footer(void)
+{
+	vchiq_log_error(vchiq_core_log_level, "=====");
+	vchiq_log_error(vchiq_core_log_level,
+		"============================================================"
+		"================");
+	vchiq_log_error(vchiq_core_log_level,
+		"============================================================"
+		"================");
+}
+
+
+VCHIQ_STATUS_T vchiq_send_remote_use(VCHIQ_STATE_T *state)
+{
+	VCHIQ_STATUS_T status = VCHIQ_RETRY;
+	if (state->conn_state != VCHIQ_CONNSTATE_DISCONNECTED)
+		status = queue_message(state, NULL,
+			VCHIQ_MAKE_MSG(VCHIQ_MSG_REMOTE_USE, 0, 0),
+			NULL, 0, 0, 0);
+	return status;
+}
+
+VCHIQ_STATUS_T vchiq_send_remote_release(VCHIQ_STATE_T *state)
+{
+	VCHIQ_STATUS_T status = VCHIQ_RETRY;
+	if (state->conn_state != VCHIQ_CONNSTATE_DISCONNECTED)
+		status = queue_message(state, NULL,
+			VCHIQ_MAKE_MSG(VCHIQ_MSG_REMOTE_RELEASE, 0, 0),
+			NULL, 0, 0, 0);
+	return status;
+}
+
+VCHIQ_STATUS_T vchiq_send_remote_use_active(VCHIQ_STATE_T *state)
+{
+	VCHIQ_STATUS_T status = VCHIQ_RETRY;
+	if (state->conn_state != VCHIQ_CONNSTATE_DISCONNECTED)
+		status = queue_message(state, NULL,
+			VCHIQ_MAKE_MSG(VCHIQ_MSG_REMOTE_USE_ACTIVE, 0, 0),
+			NULL, 0, 0, 0);
+	return status;
+}
+
+void vchiq_log_dump_mem(const char *label, uint32_t addr, const void *voidMem,
+	size_t numBytes)
+{
+	const uint8_t  *mem = (const uint8_t *)voidMem;
+	size_t          offset;
+	char            lineBuf[100];
+	char           *s;
+
+	while (numBytes > 0) {
+		s = lineBuf;
+
+		for (offset = 0; offset < 16; offset++) {
+			if (offset < numBytes)
+				s += snprintf(s, 4, "%02x ", mem[offset]);
+			else
+				s += snprintf(s, 4, "   ");
+		}
+
+		for (offset = 0; offset < 16; offset++) {
+			if (offset < numBytes) {
+				uint8_t ch = mem[offset];
+
+				if ((ch < ' ') || (ch > '~'))
+					ch = '.';
+				*s++ = (char)ch;
+			}
+		}
+		*s++ = '\0';
+
+		if ((label != NULL) && (*label != '\0'))
+			vchiq_log_trace(VCHIQ_LOG_TRACE,
+				"%s: %08x: %s", label, addr, lineBuf);
+		else
+			vchiq_log_trace(VCHIQ_LOG_TRACE,
+				"%08x: %s", addr, lineBuf);
+
+		addr += 16;
+		mem += 16;
+		if (numBytes > 16)
+			numBytes -= 16;
+		else
+			numBytes = 0;
+	}
+}
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_core.h
@@ -0,0 +1,711 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHIQ_CORE_H
+#define VCHIQ_CORE_H
+
+#include <linux/mutex.h>
+#include <linux/semaphore.h>
+#include <linux/kthread.h>
+
+#include "vchiq_cfg.h"
+
+#include "vchiq.h"
+
+/* Run time control of log level, based on KERN_XXX level. */
+#define VCHIQ_LOG_DEFAULT  4
+#define VCHIQ_LOG_ERROR    3
+#define VCHIQ_LOG_WARNING  4
+#define VCHIQ_LOG_INFO     6
+#define VCHIQ_LOG_TRACE    7
+
+#define VCHIQ_LOG_PREFIX   KERN_INFO "vchiq: "
+
+#ifndef vchiq_log_error
+#define vchiq_log_error(cat, fmt, ...) \
+	do { if (cat >= VCHIQ_LOG_ERROR) \
+		printk(VCHIQ_LOG_PREFIX fmt "\n", ##__VA_ARGS__); } while (0)
+#endif
+#ifndef vchiq_log_warning
+#define vchiq_log_warning(cat, fmt, ...) \
+	do { if (cat >= VCHIQ_LOG_WARNING) \
+		 printk(VCHIQ_LOG_PREFIX fmt "\n", ##__VA_ARGS__); } while (0)
+#endif
+#ifndef vchiq_log_info
+#define vchiq_log_info(cat, fmt, ...) \
+	do { if (cat >= VCHIQ_LOG_INFO) \
+		printk(VCHIQ_LOG_PREFIX fmt "\n", ##__VA_ARGS__); } while (0)
+#endif
+#ifndef vchiq_log_trace
+#define vchiq_log_trace(cat, fmt, ...) \
+	do { if (cat >= VCHIQ_LOG_TRACE) \
+		printk(VCHIQ_LOG_PREFIX fmt "\n", ##__VA_ARGS__); } while (0)
+#endif
+
+#define vchiq_loud_error(...) \
+	vchiq_log_error(vchiq_core_log_level, "===== " __VA_ARGS__)
+
+#ifndef vchiq_static_assert
+#define vchiq_static_assert(cond) __attribute__((unused)) \
+	extern int vchiq_static_assert[(cond) ? 1 : -1]
+#endif
+
+#define IS_POW2(x) (x && ((x & (x - 1)) == 0))
+
+/* Ensure that the slot size and maximum number of slots are powers of 2 */
+vchiq_static_assert(IS_POW2(VCHIQ_SLOT_SIZE));
+vchiq_static_assert(IS_POW2(VCHIQ_MAX_SLOTS));
+vchiq_static_assert(IS_POW2(VCHIQ_MAX_SLOTS_PER_SIDE));
+
+#define VCHIQ_SLOT_MASK        (VCHIQ_SLOT_SIZE - 1)
+#define VCHIQ_SLOT_QUEUE_MASK  (VCHIQ_MAX_SLOTS_PER_SIDE - 1)
+#define VCHIQ_SLOT_ZERO_SLOTS  ((sizeof(VCHIQ_SLOT_ZERO_T) + \
+	VCHIQ_SLOT_SIZE - 1) / VCHIQ_SLOT_SIZE)
+
+#define VCHIQ_MSG_PADDING            0  /* -                                 */
+#define VCHIQ_MSG_CONNECT            1  /* -                                 */
+#define VCHIQ_MSG_OPEN               2  /* + (srcport, -), fourcc, client_id */
+#define VCHIQ_MSG_OPENACK            3  /* + (srcport, dstport)              */
+#define VCHIQ_MSG_CLOSE              4  /* + (srcport, dstport)              */
+#define VCHIQ_MSG_DATA               5  /* + (srcport, dstport)              */
+#define VCHIQ_MSG_BULK_RX            6  /* + (srcport, dstport), data, size  */
+#define VCHIQ_MSG_BULK_TX            7  /* + (srcport, dstport), data, size  */
+#define VCHIQ_MSG_BULK_RX_DONE       8  /* + (srcport, dstport), actual      */
+#define VCHIQ_MSG_BULK_TX_DONE       9  /* + (srcport, dstport), actual      */
+#define VCHIQ_MSG_PAUSE             10  /* -                                 */
+#define VCHIQ_MSG_RESUME            11  /* -                                 */
+#define VCHIQ_MSG_REMOTE_USE        12  /* -                                 */
+#define VCHIQ_MSG_REMOTE_RELEASE    13  /* -                                 */
+#define VCHIQ_MSG_REMOTE_USE_ACTIVE 14  /* -                                 */
+
+#define VCHIQ_PORT_MAX                 (VCHIQ_MAX_SERVICES - 1)
+#define VCHIQ_PORT_FREE                0x1000
+#define VCHIQ_PORT_IS_VALID(port)      (port < VCHIQ_PORT_FREE)
+#define VCHIQ_MAKE_MSG(type, srcport, dstport) \
+	((type<<24) | (srcport<<12) | (dstport<<0))
+#define VCHIQ_MSG_TYPE(msgid)          ((unsigned int)msgid >> 24)
+#define VCHIQ_MSG_SRCPORT(msgid) \
+	(unsigned short)(((unsigned int)msgid >> 12) & 0xfff)
+#define VCHIQ_MSG_DSTPORT(msgid) \
+	((unsigned short)msgid & 0xfff)
+
+#define VCHIQ_FOURCC_AS_4CHARS(fourcc)	\
+	((fourcc) >> 24) & 0xff, \
+	((fourcc) >> 16) & 0xff, \
+	((fourcc) >>  8) & 0xff, \
+	(fourcc) & 0xff
+
+/* Ensure the fields are wide enough */
+vchiq_static_assert(VCHIQ_MSG_SRCPORT(VCHIQ_MAKE_MSG(0, 0, VCHIQ_PORT_MAX))
+	== 0);
+vchiq_static_assert(VCHIQ_MSG_TYPE(VCHIQ_MAKE_MSG(0, VCHIQ_PORT_MAX, 0)) == 0);
+vchiq_static_assert((unsigned int)VCHIQ_PORT_MAX <
+	(unsigned int)VCHIQ_PORT_FREE);
+
+#define VCHIQ_MSGID_PADDING            VCHIQ_MAKE_MSG(VCHIQ_MSG_PADDING, 0, 0)
+#define VCHIQ_MSGID_CLAIMED            0x40000000
+
+#define VCHIQ_FOURCC_INVALID           0x00000000
+#define VCHIQ_FOURCC_IS_LEGAL(fourcc)  (fourcc != VCHIQ_FOURCC_INVALID)
+
+#define VCHIQ_BULK_ACTUAL_ABORTED -1
+
+typedef uint32_t BITSET_T;
+
+vchiq_static_assert((sizeof(BITSET_T) * 8) == 32);
+
+#define BITSET_SIZE(b)        ((b + 31) >> 5)
+#define BITSET_WORD(b)        (b >> 5)
+#define BITSET_BIT(b)         (1 << (b & 31))
+#define BITSET_ZERO(bs)       memset(bs, 0, sizeof(bs))
+#define BITSET_IS_SET(bs, b)  (bs[BITSET_WORD(b)] & BITSET_BIT(b))
+#define BITSET_SET(bs, b)     (bs[BITSET_WORD(b)] |= BITSET_BIT(b))
+#define BITSET_CLR(bs, b)     (bs[BITSET_WORD(b)] &= ~BITSET_BIT(b))
+
+#if VCHIQ_ENABLE_STATS
+#define VCHIQ_STATS_INC(state, stat) (state->stats. stat++)
+#define VCHIQ_SERVICE_STATS_INC(service, stat) (service->stats. stat++)
+#define VCHIQ_SERVICE_STATS_ADD(service, stat, addend) \
+	(service->stats. stat += addend)
+#else
+#define VCHIQ_STATS_INC(state, stat) ((void)0)
+#define VCHIQ_SERVICE_STATS_INC(service, stat) ((void)0)
+#define VCHIQ_SERVICE_STATS_ADD(service, stat, addend) ((void)0)
+#endif
+
+enum {
+	DEBUG_ENTRIES,
+#if VCHIQ_ENABLE_DEBUG
+	DEBUG_SLOT_HANDLER_COUNT,
+	DEBUG_SLOT_HANDLER_LINE,
+	DEBUG_PARSE_LINE,
+	DEBUG_PARSE_HEADER,
+	DEBUG_PARSE_MSGID,
+	DEBUG_AWAIT_COMPLETION_LINE,
+	DEBUG_DEQUEUE_MESSAGE_LINE,
+	DEBUG_SERVICE_CALLBACK_LINE,
+	DEBUG_MSG_QUEUE_FULL_COUNT,
+	DEBUG_COMPLETION_QUEUE_FULL_COUNT,
+#endif
+	DEBUG_MAX
+};
+
+#if VCHIQ_ENABLE_DEBUG
+
+#define DEBUG_INITIALISE(local) int *debug_ptr = (local)->debug;
+#define DEBUG_TRACE(d) \
+	do { debug_ptr[DEBUG_ ## d] = __LINE__; dsb(); } while (0)
+#define DEBUG_VALUE(d, v) \
+	do { debug_ptr[DEBUG_ ## d] = (v); dsb(); } while (0)
+#define DEBUG_COUNT(d) \
+	do { debug_ptr[DEBUG_ ## d]++; dsb(); } while (0)
+
+#else /* VCHIQ_ENABLE_DEBUG */
+
+#define DEBUG_INITIALISE(local)
+#define DEBUG_TRACE(d)
+#define DEBUG_VALUE(d, v)
+#define DEBUG_COUNT(d)
+
+#endif /* VCHIQ_ENABLE_DEBUG */
+
+typedef enum {
+	VCHIQ_CONNSTATE_DISCONNECTED,
+	VCHIQ_CONNSTATE_CONNECTING,
+	VCHIQ_CONNSTATE_CONNECTED,
+	VCHIQ_CONNSTATE_PAUSING,
+	VCHIQ_CONNSTATE_PAUSE_SENT,
+	VCHIQ_CONNSTATE_PAUSED,
+	VCHIQ_CONNSTATE_RESUMING,
+	VCHIQ_CONNSTATE_PAUSE_TIMEOUT,
+	VCHIQ_CONNSTATE_RESUME_TIMEOUT
+} VCHIQ_CONNSTATE_T;
+
+enum {
+	VCHIQ_SRVSTATE_FREE,
+	VCHIQ_SRVSTATE_HIDDEN,
+	VCHIQ_SRVSTATE_LISTENING,
+	VCHIQ_SRVSTATE_OPENING,
+	VCHIQ_SRVSTATE_OPEN,
+	VCHIQ_SRVSTATE_OPENSYNC,
+	VCHIQ_SRVSTATE_CLOSESENT,
+	VCHIQ_SRVSTATE_CLOSERECVD,
+	VCHIQ_SRVSTATE_CLOSEWAIT,
+	VCHIQ_SRVSTATE_CLOSED
+};
+
+enum {
+	VCHIQ_POLL_TERMINATE,
+	VCHIQ_POLL_REMOVE,
+	VCHIQ_POLL_TXNOTIFY,
+	VCHIQ_POLL_RXNOTIFY,
+	VCHIQ_POLL_COUNT
+};
+
+typedef enum {
+	VCHIQ_BULK_TRANSMIT,
+	VCHIQ_BULK_RECEIVE
+} VCHIQ_BULK_DIR_T;
+
+typedef void (*VCHIQ_USERDATA_TERM_T)(void *userdata);
+
+typedef struct vchiq_bulk_struct {
+	short mode;
+	short dir;
+	void *userdata;
+	VCHI_MEM_HANDLE_T handle;
+	void *data;
+	int size;
+	void *remote_data;
+	int remote_size;
+	int actual;
+} VCHIQ_BULK_T;
+
+typedef struct vchiq_bulk_queue_struct {
+	int local_insert;  /* Where to insert the next local bulk */
+	int remote_insert; /* Where to insert the next remote bulk (master) */
+	int process;       /* Bulk to transfer next */
+	int remote_notify; /* Bulk to notify the remote client of next (mstr) */
+	int remove;        /* Bulk to notify the local client of, and remove,
+			   ** next */
+	VCHIQ_BULK_T bulks[VCHIQ_NUM_SERVICE_BULKS];
+} VCHIQ_BULK_QUEUE_T;
+
+typedef struct remote_event_struct {
+	int armed;
+	int fired;
+	struct semaphore *event;
+} REMOTE_EVENT_T;
+
+typedef struct opaque_platform_state_t *VCHIQ_PLATFORM_STATE_T;
+
+typedef struct vchiq_state_struct VCHIQ_STATE_T;
+
+typedef struct vchiq_slot_struct {
+	char data[VCHIQ_SLOT_SIZE];
+} VCHIQ_SLOT_T;
+
+typedef struct vchiq_slot_info_struct {
+	/* Use two counters rather than one to avoid the need for a mutex. */
+	short use_count;
+	short release_count;
+} VCHIQ_SLOT_INFO_T;
+
+typedef struct vchiq_service_struct {
+	VCHIQ_SERVICE_BASE_T base;
+	VCHIQ_SERVICE_HANDLE_T handle;
+	unsigned int ref_count;
+	int srvstate;
+	VCHIQ_USERDATA_TERM_T userdata_term;
+	unsigned int localport;
+	unsigned int remoteport;
+	int public_fourcc;
+	int client_id;
+	char auto_close;
+	char sync;
+	char closing;
+	char trace;
+	atomic_t poll_flags;
+	short version;
+	short version_min;
+	short peer_version;
+
+	VCHIQ_STATE_T *state;
+	VCHIQ_INSTANCE_T instance;
+
+	int service_use_count;
+
+	VCHIQ_BULK_QUEUE_T bulk_tx;
+	VCHIQ_BULK_QUEUE_T bulk_rx;
+
+	struct semaphore remove_event;
+	struct semaphore bulk_remove_event;
+	struct mutex bulk_mutex;
+
+	struct service_stats_struct {
+		int quota_stalls;
+		int slot_stalls;
+		int bulk_stalls;
+		int error_count;
+		int ctrl_tx_count;
+		int ctrl_rx_count;
+		int bulk_tx_count;
+		int bulk_rx_count;
+		int bulk_aborted_count;
+		uint64_t ctrl_tx_bytes;
+		uint64_t ctrl_rx_bytes;
+		uint64_t bulk_tx_bytes;
+		uint64_t bulk_rx_bytes;
+	} stats;
+} VCHIQ_SERVICE_T;
+
+/* The quota information is outside VCHIQ_SERVICE_T so that it can be
+	statically allocated, since for accounting reasons a service's slot
+	usage is carried over between users of the same port number.
+ */
+typedef struct vchiq_service_quota_struct {
+	unsigned short slot_quota;
+	unsigned short slot_use_count;
+	unsigned short message_quota;
+	unsigned short message_use_count;
+	struct semaphore quota_event;
+	int previous_tx_index;
+} VCHIQ_SERVICE_QUOTA_T;
+
+typedef struct vchiq_shared_state_struct {
+
+	/* A non-zero value here indicates that the content is valid. */
+	int initialised;
+
+	/* The first and last (inclusive) slots allocated to the owner. */
+	int slot_first;
+	int slot_last;
+
+	/* The slot allocated to synchronous messages from the owner. */
+	int slot_sync;
+
+	/* Signalling this event indicates that owner's slot handler thread
+	** should run. */
+	REMOTE_EVENT_T trigger;
+
+	/* Indicates the byte position within the stream where the next message
+	** will be written. The least significant bits are an index into the
+	** slot. The next bits are the index of the slot in slot_queue. */
+	int tx_pos;
+
+	/* This event should be signalled when a slot is recycled. */
+	REMOTE_EVENT_T recycle;
+
+	/* The slot_queue index where the next recycled slot will be written. */
+	int slot_queue_recycle;
+
+	/* This event should be signalled when a synchronous message is sent. */
+	REMOTE_EVENT_T sync_trigger;
+
+	/* This event should be signalled when a synchronous message has been
+	** released. */
+	REMOTE_EVENT_T sync_release;
+
+	/* A circular buffer of slot indexes. */
+	int slot_queue[VCHIQ_MAX_SLOTS_PER_SIDE];
+
+	/* Debugging state */
+	int debug[DEBUG_MAX];
+} VCHIQ_SHARED_STATE_T;
+
+typedef struct vchiq_slot_zero_struct {
+	int magic;
+	short version;
+	short version_min;
+	int slot_zero_size;
+	int slot_size;
+	int max_slots;
+	int max_slots_per_side;
+	int platform_data[2];
+	VCHIQ_SHARED_STATE_T master;
+	VCHIQ_SHARED_STATE_T slave;
+	VCHIQ_SLOT_INFO_T slots[VCHIQ_MAX_SLOTS];
+} VCHIQ_SLOT_ZERO_T;
+
+struct vchiq_state_struct {
+	int id;
+	int initialised;
+	VCHIQ_CONNSTATE_T conn_state;
+	int is_master;
+
+	VCHIQ_SHARED_STATE_T *local;
+	VCHIQ_SHARED_STATE_T *remote;
+	VCHIQ_SLOT_T *slot_data;
+
+	unsigned short default_slot_quota;
+	unsigned short default_message_quota;
+
+	/* Event indicating connect message received */
+	struct semaphore connect;
+
+	/* Mutex protecting services */
+	struct mutex mutex;
+	VCHIQ_INSTANCE_T *instance;
+
+	/* Processes incoming messages */
+	struct task_struct *slot_handler_thread;
+
+	/* Processes recycled slots */
+	struct task_struct *recycle_thread;
+
+	/* Processes synchronous messages */
+	struct task_struct *sync_thread;
+
+	/* Local implementation of the trigger remote event */
+	struct semaphore trigger_event;
+
+	/* Local implementation of the recycle remote event */
+	struct semaphore recycle_event;
+
+	/* Local implementation of the sync trigger remote event */
+	struct semaphore sync_trigger_event;
+
+	/* Local implementation of the sync release remote event */
+	struct semaphore sync_release_event;
+
+	char *tx_data;
+	char *rx_data;
+	VCHIQ_SLOT_INFO_T *rx_info;
+
+	struct mutex slot_mutex;
+
+	struct mutex recycle_mutex;
+
+	struct mutex sync_mutex;
+
+	struct mutex bulk_transfer_mutex;
+
+	/* Indicates the byte position within the stream from where the next
+	** message will be read. The least significant bits are an index into
+	** the slot.The next bits are the index of the slot in
+	** remote->slot_queue. */
+	int rx_pos;
+
+	/* A cached copy of local->tx_pos. Only write to local->tx_pos, and read
+		from remote->tx_pos. */
+	int local_tx_pos;
+
+	/* The slot_queue index of the slot to become available next. */
+	int slot_queue_available;
+
+	/* A flag to indicate if any poll has been requested */
+	int poll_needed;
+
+	/* Ths index of the previous slot used for data messages. */
+	int previous_data_index;
+
+	/* The number of slots occupied by data messages. */
+	unsigned short data_use_count;
+
+	/* The maximum number of slots to be occupied by data messages. */
+	unsigned short data_quota;
+
+	/* An array of bit sets indicating which services must be polled. */
+	atomic_t poll_services[BITSET_SIZE(VCHIQ_MAX_SERVICES)];
+
+	/* The number of the first unused service */
+	int unused_service;
+
+	/* Signalled when a free slot becomes available. */
+	struct semaphore slot_available_event;
+
+	struct semaphore slot_remove_event;
+
+	/* Signalled when a free data slot becomes available. */
+	struct semaphore data_quota_event;
+
+	/* Incremented when there are bulk transfers which cannot be processed
+	 * whilst paused and must be processed on resume */
+	int deferred_bulks;
+
+	struct state_stats_struct {
+		int slot_stalls;
+		int data_stalls;
+		int ctrl_tx_count;
+		int ctrl_rx_count;
+		int error_count;
+	} stats;
+
+	VCHIQ_SERVICE_T * services[VCHIQ_MAX_SERVICES];
+	VCHIQ_SERVICE_QUOTA_T service_quotas[VCHIQ_MAX_SERVICES];
+	VCHIQ_SLOT_INFO_T slot_info[VCHIQ_MAX_SLOTS];
+
+	VCHIQ_PLATFORM_STATE_T platform_state;
+};
+
+struct bulk_waiter {
+	VCHIQ_BULK_T *bulk;
+	struct semaphore event;
+	int actual;
+};
+
+extern spinlock_t bulk_waiter_spinlock;
+
+extern int vchiq_core_log_level;
+extern int vchiq_core_msg_log_level;
+extern int vchiq_sync_log_level;
+
+extern VCHIQ_STATE_T *vchiq_states[VCHIQ_MAX_STATES];
+
+extern const char *
+get_conn_state_name(VCHIQ_CONNSTATE_T conn_state);
+
+extern VCHIQ_SLOT_ZERO_T *
+vchiq_init_slots(void *mem_base, int mem_size);
+
+extern VCHIQ_STATUS_T
+vchiq_init_state(VCHIQ_STATE_T *state, VCHIQ_SLOT_ZERO_T *slot_zero,
+	int is_master);
+
+extern VCHIQ_STATUS_T
+vchiq_connect_internal(VCHIQ_STATE_T *state, VCHIQ_INSTANCE_T instance);
+
+extern VCHIQ_SERVICE_T *
+vchiq_add_service_internal(VCHIQ_STATE_T *state,
+	const VCHIQ_SERVICE_PARAMS_T *params, int srvstate,
+	VCHIQ_INSTANCE_T instance, VCHIQ_USERDATA_TERM_T userdata_term);
+
+extern VCHIQ_STATUS_T
+vchiq_open_service_internal(VCHIQ_SERVICE_T *service, int client_id);
+
+extern VCHIQ_STATUS_T
+vchiq_close_service_internal(VCHIQ_SERVICE_T *service, int close_recvd);
+
+extern void
+vchiq_terminate_service_internal(VCHIQ_SERVICE_T *service);
+
+extern void
+vchiq_free_service_internal(VCHIQ_SERVICE_T *service);
+
+extern VCHIQ_STATUS_T
+vchiq_shutdown_internal(VCHIQ_STATE_T *state, VCHIQ_INSTANCE_T instance);
+
+extern VCHIQ_STATUS_T
+vchiq_pause_internal(VCHIQ_STATE_T *state);
+
+extern VCHIQ_STATUS_T
+vchiq_resume_internal(VCHIQ_STATE_T *state);
+
+extern void
+remote_event_pollall(VCHIQ_STATE_T *state);
+
+extern VCHIQ_STATUS_T
+vchiq_bulk_transfer(VCHIQ_SERVICE_HANDLE_T handle,
+	VCHI_MEM_HANDLE_T memhandle, void *offset, int size, void *userdata,
+	VCHIQ_BULK_MODE_T mode, VCHIQ_BULK_DIR_T dir);
+
+extern void
+vchiq_dump_state(void *dump_context, VCHIQ_STATE_T *state);
+
+extern void
+vchiq_dump_service_state(void *dump_context, VCHIQ_SERVICE_T *service);
+
+extern void
+vchiq_loud_error_header(void);
+
+extern void
+vchiq_loud_error_footer(void);
+
+extern void
+request_poll(VCHIQ_STATE_T *state, VCHIQ_SERVICE_T *service, int poll_type);
+
+static inline VCHIQ_SERVICE_T *
+handle_to_service(VCHIQ_SERVICE_HANDLE_T handle)
+{
+	VCHIQ_STATE_T *state = vchiq_states[(handle / VCHIQ_MAX_SERVICES) &
+		(VCHIQ_MAX_STATES - 1)];
+	if (!state)
+		return NULL;
+
+	return state->services[handle & (VCHIQ_MAX_SERVICES - 1)];
+}
+
+extern VCHIQ_SERVICE_T *
+find_service_by_handle(VCHIQ_SERVICE_HANDLE_T handle);
+
+extern VCHIQ_SERVICE_T *
+find_service_by_port(VCHIQ_STATE_T *state, int localport);
+
+extern VCHIQ_SERVICE_T *
+find_service_for_instance(VCHIQ_INSTANCE_T instance,
+	VCHIQ_SERVICE_HANDLE_T handle);
+
+extern VCHIQ_SERVICE_T *
+find_closed_service_for_instance(VCHIQ_INSTANCE_T instance,
+	VCHIQ_SERVICE_HANDLE_T handle);
+
+extern VCHIQ_SERVICE_T *
+next_service_by_instance(VCHIQ_STATE_T *state, VCHIQ_INSTANCE_T instance,
+	int *pidx);
+
+extern void
+lock_service(VCHIQ_SERVICE_T *service);
+
+extern void
+unlock_service(VCHIQ_SERVICE_T *service);
+
+/* The following functions are called from vchiq_core, and external
+** implementations must be provided. */
+
+extern VCHIQ_STATUS_T
+vchiq_prepare_bulk_data(VCHIQ_BULK_T *bulk,
+	VCHI_MEM_HANDLE_T memhandle, void *offset, int size, int dir);
+
+extern void
+vchiq_transfer_bulk(VCHIQ_BULK_T *bulk);
+
+extern void
+vchiq_complete_bulk(VCHIQ_BULK_T *bulk);
+
+extern VCHIQ_STATUS_T
+vchiq_copy_from_user(void *dst, const void *src, int size);
+
+extern void
+remote_event_signal(REMOTE_EVENT_T *event);
+
+void
+vchiq_platform_check_suspend(VCHIQ_STATE_T *state);
+
+extern void
+vchiq_platform_paused(VCHIQ_STATE_T *state);
+
+extern VCHIQ_STATUS_T
+vchiq_platform_resume(VCHIQ_STATE_T *state);
+
+extern void
+vchiq_platform_resumed(VCHIQ_STATE_T *state);
+
+extern void
+vchiq_dump(void *dump_context, const char *str, int len);
+
+extern void
+vchiq_dump_platform_state(void *dump_context);
+
+extern void
+vchiq_dump_platform_instances(void *dump_context);
+
+extern void
+vchiq_dump_platform_service_state(void *dump_context,
+	VCHIQ_SERVICE_T *service);
+
+extern VCHIQ_STATUS_T
+vchiq_use_service_internal(VCHIQ_SERVICE_T *service);
+
+extern VCHIQ_STATUS_T
+vchiq_release_service_internal(VCHIQ_SERVICE_T *service);
+
+extern void
+vchiq_on_remote_use(VCHIQ_STATE_T *state);
+
+extern void
+vchiq_on_remote_release(VCHIQ_STATE_T *state);
+
+extern VCHIQ_STATUS_T
+vchiq_platform_init_state(VCHIQ_STATE_T *state);
+
+extern VCHIQ_STATUS_T
+vchiq_check_service(VCHIQ_SERVICE_T *service);
+
+extern void
+vchiq_on_remote_use_active(VCHIQ_STATE_T *state);
+
+extern VCHIQ_STATUS_T
+vchiq_send_remote_use(VCHIQ_STATE_T *state);
+
+extern VCHIQ_STATUS_T
+vchiq_send_remote_release(VCHIQ_STATE_T *state);
+
+extern VCHIQ_STATUS_T
+vchiq_send_remote_use_active(VCHIQ_STATE_T *state);
+
+extern void
+vchiq_platform_conn_state_changed(VCHIQ_STATE_T *state,
+	VCHIQ_CONNSTATE_T oldstate, VCHIQ_CONNSTATE_T newstate);
+
+extern void
+vchiq_platform_handle_timeout(VCHIQ_STATE_T *state);
+
+extern void
+vchiq_set_conn_state(VCHIQ_STATE_T *state, VCHIQ_CONNSTATE_T newstate);
+
+
+extern void
+vchiq_log_dump_mem(const char *label, uint32_t addr, const void *voidMem,
+	size_t numBytes);
+
+#endif
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_debugfs.c
@@ -0,0 +1,383 @@
+/**
+ * Copyright (c) 2014 Raspberry Pi (Trading) Ltd. All rights reserved.
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+
+#include <linux/debugfs.h>
+#include "vchiq_core.h"
+#include "vchiq_arm.h"
+#include "vchiq_debugfs.h"
+
+#ifdef CONFIG_DEBUG_FS
+
+/****************************************************************************
+*
+*   log category entries
+*
+***************************************************************************/
+#define DEBUGFS_WRITE_BUF_SIZE 256
+
+#define VCHIQ_LOG_ERROR_STR   "error"
+#define VCHIQ_LOG_WARNING_STR "warning"
+#define VCHIQ_LOG_INFO_STR    "info"
+#define VCHIQ_LOG_TRACE_STR   "trace"
+
+
+/* Top-level debug info */
+struct vchiq_debugfs_info {
+	/* Global 'vchiq' debugfs entry used by all instances */
+	struct dentry *vchiq_cfg_dir;
+
+	/* one entry per client process */
+	struct dentry *clients;
+
+	/* log categories */
+	struct dentry *log_categories;
+};
+
+static struct vchiq_debugfs_info debugfs_info;
+
+/* Log category debugfs entries */
+struct vchiq_debugfs_log_entry {
+	const char *name;
+	int *plevel;
+	struct dentry *dir;
+};
+
+static struct vchiq_debugfs_log_entry vchiq_debugfs_log_entries[] = {
+	{ "core", &vchiq_core_log_level },
+	{ "msg",  &vchiq_core_msg_log_level },
+	{ "sync", &vchiq_sync_log_level },
+	{ "susp", &vchiq_susp_log_level },
+	{ "arm",  &vchiq_arm_log_level },
+};
+static int n_log_entries =
+	sizeof(vchiq_debugfs_log_entries)/sizeof(vchiq_debugfs_log_entries[0]);
+
+
+static struct dentry *vchiq_clients_top(void);
+static struct dentry *vchiq_debugfs_top(void);
+
+static int debugfs_log_show(struct seq_file *f, void *offset)
+{
+	int *levp = f->private;
+	char *log_value = NULL;
+
+	switch (*levp) {
+	case VCHIQ_LOG_ERROR:
+		log_value = VCHIQ_LOG_ERROR_STR;
+		break;
+	case VCHIQ_LOG_WARNING:
+		log_value = VCHIQ_LOG_WARNING_STR;
+		break;
+	case VCHIQ_LOG_INFO:
+		log_value = VCHIQ_LOG_INFO_STR;
+		break;
+	case VCHIQ_LOG_TRACE:
+		log_value = VCHIQ_LOG_TRACE_STR;
+		break;
+	default:
+		break;
+	}
+
+	seq_printf(f, "%s\n", log_value ? log_value : "(null)");
+
+	return 0;
+}
+
+static int debugfs_log_open(struct inode *inode, struct file *file)
+{
+	return single_open(file, debugfs_log_show, inode->i_private);
+}
+
+static int debugfs_log_write(struct file *file,
+	const char __user *buffer,
+	size_t count, loff_t *ppos)
+{
+	struct seq_file *f = (struct seq_file *)file->private_data;
+	int *levp = f->private;
+	char kbuf[DEBUGFS_WRITE_BUF_SIZE + 1];
+
+	memset(kbuf, 0, DEBUGFS_WRITE_BUF_SIZE + 1);
+	if (count >= DEBUGFS_WRITE_BUF_SIZE)
+		count = DEBUGFS_WRITE_BUF_SIZE;
+
+	if (copy_from_user(kbuf, buffer, count) != 0)
+		return -EFAULT;
+	kbuf[count - 1] = 0;
+
+	if (strncmp("error", kbuf, strlen("error")) == 0)
+		*levp = VCHIQ_LOG_ERROR;
+	else if (strncmp("warning", kbuf, strlen("warning")) == 0)
+		*levp = VCHIQ_LOG_WARNING;
+	else if (strncmp("info", kbuf, strlen("info")) == 0)
+		*levp = VCHIQ_LOG_INFO;
+	else if (strncmp("trace", kbuf, strlen("trace")) == 0)
+		*levp = VCHIQ_LOG_TRACE;
+	else
+		*levp = VCHIQ_LOG_DEFAULT;
+
+	*ppos += count;
+
+	return count;
+}
+
+static const struct file_operations debugfs_log_fops = {
+	.owner		= THIS_MODULE,
+	.open		= debugfs_log_open,
+	.write		= debugfs_log_write,
+	.read		= seq_read,
+	.llseek		= seq_lseek,
+	.release	= single_release,
+};
+
+/* create an entry under <debugfs>/vchiq/log for each log category */
+static int vchiq_debugfs_create_log_entries(struct dentry *top)
+{
+	struct dentry *dir;
+	size_t i;
+	int ret = 0;
+	dir = debugfs_create_dir("log", vchiq_debugfs_top());
+	if (!dir)
+		return -ENOMEM;
+	debugfs_info.log_categories = dir;
+
+	for (i = 0; i < n_log_entries; i++) {
+		void *levp = (void *)vchiq_debugfs_log_entries[i].plevel;
+		dir = debugfs_create_file(vchiq_debugfs_log_entries[i].name,
+					  0644,
+					  debugfs_info.log_categories,
+					  levp,
+					  &debugfs_log_fops);
+		if (!dir) {
+			ret = -ENOMEM;
+			break;
+		}
+
+		vchiq_debugfs_log_entries[i].dir = dir;
+	}
+	return ret;
+}
+
+static int debugfs_usecount_show(struct seq_file *f, void *offset)
+{
+	VCHIQ_INSTANCE_T instance = f->private;
+	int use_count;
+
+	use_count = vchiq_instance_get_use_count(instance);
+	seq_printf(f, "%d\n", use_count);
+
+	return 0;
+}
+
+static int debugfs_usecount_open(struct inode *inode, struct file *file)
+{
+	return single_open(file, debugfs_usecount_show, inode->i_private);
+}
+
+static const struct file_operations debugfs_usecount_fops = {
+	.owner		= THIS_MODULE,
+	.open		= debugfs_usecount_open,
+	.read		= seq_read,
+	.llseek		= seq_lseek,
+	.release	= single_release,
+};
+
+static int debugfs_trace_show(struct seq_file *f, void *offset)
+{
+	VCHIQ_INSTANCE_T instance = f->private;
+	int trace;
+
+	trace = vchiq_instance_get_trace(instance);
+	seq_printf(f, "%s\n", trace ? "Y" : "N");
+
+	return 0;
+}
+
+static int debugfs_trace_open(struct inode *inode, struct file *file)
+{
+	return single_open(file, debugfs_trace_show, inode->i_private);
+}
+
+static int debugfs_trace_write(struct file *file,
+	const char __user *buffer,
+	size_t count, loff_t *ppos)
+{
+	struct seq_file *f = (struct seq_file *)file->private_data;
+	VCHIQ_INSTANCE_T instance = f->private;
+	char firstchar;
+
+	if (copy_from_user(&firstchar, buffer, 1) != 0)
+		return -EFAULT;
+
+	switch (firstchar) {
+	case 'Y':
+	case 'y':
+	case '1':
+		vchiq_instance_set_trace(instance, 1);
+		break;
+	case 'N':
+	case 'n':
+	case '0':
+		vchiq_instance_set_trace(instance, 0);
+		break;
+	default:
+		break;
+	}
+
+	*ppos += count;
+
+	return count;
+}
+
+static const struct file_operations debugfs_trace_fops = {
+	.owner		= THIS_MODULE,
+	.open		= debugfs_trace_open,
+	.write		= debugfs_trace_write,
+	.read		= seq_read,
+	.llseek		= seq_lseek,
+	.release	= single_release,
+};
+
+/* add an instance (process) to the debugfs entries */
+int vchiq_debugfs_add_instance(VCHIQ_INSTANCE_T instance)
+{
+	char pidstr[16];
+	struct dentry *top, *use_count, *trace;
+	struct dentry *clients = vchiq_clients_top();
+
+	snprintf(pidstr, sizeof(pidstr), "%d",
+		 vchiq_instance_get_pid(instance));
+
+	top = debugfs_create_dir(pidstr, clients);
+	if (!top)
+		goto fail_top;
+
+	use_count = debugfs_create_file("use_count",
+					0444, top,
+					instance,
+					&debugfs_usecount_fops);
+	if (!use_count)
+		goto fail_use_count;
+
+	trace = debugfs_create_file("trace",
+				    0644, top,
+				    instance,
+				    &debugfs_trace_fops);
+	if (!trace)
+		goto fail_trace;
+
+	vchiq_instance_get_debugfs_node(instance)->dentry = top;
+
+	return 0;
+
+fail_trace:
+	debugfs_remove(use_count);
+fail_use_count:
+	debugfs_remove(top);
+fail_top:
+	return -ENOMEM;
+}
+
+void vchiq_debugfs_remove_instance(VCHIQ_INSTANCE_T instance)
+{
+	VCHIQ_DEBUGFS_NODE_T *node = vchiq_instance_get_debugfs_node(instance);
+	debugfs_remove_recursive(node->dentry);
+}
+
+
+int vchiq_debugfs_init(void)
+{
+	BUG_ON(debugfs_info.vchiq_cfg_dir != NULL);
+
+	debugfs_info.vchiq_cfg_dir = debugfs_create_dir("vchiq", NULL);
+	if (debugfs_info.vchiq_cfg_dir == NULL)
+		goto fail;
+
+	debugfs_info.clients = debugfs_create_dir("clients",
+				vchiq_debugfs_top());
+	if (!debugfs_info.clients)
+		goto fail;
+
+	if (vchiq_debugfs_create_log_entries(vchiq_debugfs_top()) != 0)
+		goto fail;
+
+	return 0;
+
+fail:
+	vchiq_debugfs_deinit();
+	vchiq_log_error(vchiq_arm_log_level,
+		"%s: failed to create debugfs directory",
+		__func__);
+
+	return -ENOMEM;
+}
+
+/* remove all the debugfs entries */
+void vchiq_debugfs_deinit(void)
+{
+	debugfs_remove_recursive(vchiq_debugfs_top());
+}
+
+static struct dentry *vchiq_clients_top(void)
+{
+	return debugfs_info.clients;
+}
+
+static struct dentry *vchiq_debugfs_top(void)
+{
+	BUG_ON(debugfs_info.vchiq_cfg_dir == NULL);
+	return debugfs_info.vchiq_cfg_dir;
+}
+
+#else /* CONFIG_DEBUG_FS */
+
+int vchiq_debugfs_init(void)
+{
+	return 0;
+}
+
+void vchiq_debugfs_deinit(void)
+{
+}
+
+int vchiq_debugfs_add_instance(VCHIQ_INSTANCE_T instance)
+{
+	return 0;
+}
+
+void vchiq_debugfs_remove_instance(VCHIQ_INSTANCE_T instance)
+{
+}
+
+#endif /* CONFIG_DEBUG_FS */
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_debugfs.h
@@ -0,0 +1,52 @@
+/**
+ * Copyright (c) 2014 Raspberry Pi (Trading) Ltd. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHIQ_DEBUGFS_H
+#define VCHIQ_DEBUGFS_H
+
+#include "vchiq_core.h"
+
+typedef struct vchiq_debugfs_node_struct
+{
+    struct dentry *dentry;
+} VCHIQ_DEBUGFS_NODE_T;
+
+int vchiq_debugfs_init(void);
+
+void vchiq_debugfs_deinit(void);
+
+int vchiq_debugfs_add_instance(VCHIQ_INSTANCE_T instance);
+
+void vchiq_debugfs_remove_instance(VCHIQ_INSTANCE_T instance);
+
+#endif /* VCHIQ_DEBUGFS_H */
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_genversion
@@ -0,0 +1,87 @@
+#!/usr/bin/perl -w
+
+use strict;
+
+#
+# Generate a version from available information
+#
+
+my $prefix = shift @ARGV;
+my $root = shift @ARGV;
+
+
+if ( not defined $root ) {
+	die "usage: $0 prefix root-dir\n";
+}
+
+if ( ! -d $root ) {
+	die "root directory $root not found\n";
+}
+
+my $version = "unknown";
+my $tainted = "";
+
+if ( -d "$root/.git" ) {
+	# attempt to work out git version. only do so
+	# on a linux build host, as cygwin builds are
+	# already slow enough
+
+	if ( -f "/usr/bin/git" || -f "/usr/local/bin/git" ) {
+		if (not open(F, "git --git-dir $root/.git rev-parse --verify HEAD|")) {
+			$version = "no git version";
+		}
+		else {
+			$version = <F>;
+			$version =~ s/[ \r\n]*$//;     # chomp may not be enough (cygwin).
+			$version =~ s/^[ \r\n]*//;     # chomp may not be enough (cygwin).
+		}
+
+		if (open(G, "git --git-dir $root/.git status --porcelain|")) {
+			$tainted = <G>;
+			$tainted =~ s/[ \r\n]*$//;     # chomp may not be enough (cygwin).
+			$tainted =~ s/^[ \r\n]*//;     # chomp may not be enough (cygwin).
+			if (length $tainted) {
+			$version = join ' ', $version, "(tainted)";
+		}
+		else {
+			$version = join ' ', $version, "(clean)";
+         }
+		}
+	}
+}
+
+my $hostname = `hostname`;
+$hostname =~ s/[ \r\n]*$//;     # chomp may not be enough (cygwin).
+$hostname =~ s/^[ \r\n]*//;     # chomp may not be enough (cygwin).
+
+
+print STDERR "Version $version\n";
+print <<EOF;
+#include "${prefix}_build_info.h"
+#include <linux/broadcom/vc_debug_sym.h>
+
+VC_DEBUG_DECLARE_STRING_VAR( ${prefix}_build_hostname, "$hostname" );
+VC_DEBUG_DECLARE_STRING_VAR( ${prefix}_build_version, "$version" );
+VC_DEBUG_DECLARE_STRING_VAR( ${prefix}_build_time,    __TIME__ );
+VC_DEBUG_DECLARE_STRING_VAR( ${prefix}_build_date,    __DATE__ );
+
+const char *vchiq_get_build_hostname( void )
+{
+   return vchiq_build_hostname;
+}
+
+const char *vchiq_get_build_version( void )
+{
+   return vchiq_build_version;
+}
+
+const char *vchiq_get_build_date( void )
+{
+   return vchiq_build_date;
+}
+
+const char *vchiq_get_build_time( void )
+{
+   return vchiq_build_time;
+}
+EOF
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_if.h
@@ -0,0 +1,189 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHIQ_IF_H
+#define VCHIQ_IF_H
+
+#include "interface/vchi/vchi_mh.h"
+
+#define VCHIQ_SERVICE_HANDLE_INVALID 0
+
+#define VCHIQ_SLOT_SIZE     4096
+#define VCHIQ_MAX_MSG_SIZE  (VCHIQ_SLOT_SIZE - sizeof(VCHIQ_HEADER_T))
+#define VCHIQ_CHANNEL_SIZE  VCHIQ_MAX_MSG_SIZE /* For backwards compatibility */
+
+#define VCHIQ_MAKE_FOURCC(x0, x1, x2, x3) \
+			(((x0) << 24) | ((x1) << 16) | ((x2) << 8) | (x3))
+#define VCHIQ_GET_SERVICE_USERDATA(service) vchiq_get_service_userdata(service)
+#define VCHIQ_GET_SERVICE_FOURCC(service)   vchiq_get_service_fourcc(service)
+
+typedef enum {
+	VCHIQ_SERVICE_OPENED,         /* service, -, -             */
+	VCHIQ_SERVICE_CLOSED,         /* service, -, -             */
+	VCHIQ_MESSAGE_AVAILABLE,      /* service, header, -        */
+	VCHIQ_BULK_TRANSMIT_DONE,     /* service, -, bulk_userdata */
+	VCHIQ_BULK_RECEIVE_DONE,      /* service, -, bulk_userdata */
+	VCHIQ_BULK_TRANSMIT_ABORTED,  /* service, -, bulk_userdata */
+	VCHIQ_BULK_RECEIVE_ABORTED    /* service, -, bulk_userdata */
+} VCHIQ_REASON_T;
+
+typedef enum {
+	VCHIQ_ERROR   = -1,
+	VCHIQ_SUCCESS = 0,
+	VCHIQ_RETRY   = 1
+} VCHIQ_STATUS_T;
+
+typedef enum {
+	VCHIQ_BULK_MODE_CALLBACK,
+	VCHIQ_BULK_MODE_BLOCKING,
+	VCHIQ_BULK_MODE_NOCALLBACK,
+	VCHIQ_BULK_MODE_WAITING		/* Reserved for internal use */
+} VCHIQ_BULK_MODE_T;
+
+typedef enum {
+	VCHIQ_SERVICE_OPTION_AUTOCLOSE,
+	VCHIQ_SERVICE_OPTION_SLOT_QUOTA,
+	VCHIQ_SERVICE_OPTION_MESSAGE_QUOTA,
+	VCHIQ_SERVICE_OPTION_SYNCHRONOUS,
+	VCHIQ_SERVICE_OPTION_TRACE
+} VCHIQ_SERVICE_OPTION_T;
+
+typedef struct vchiq_header_struct {
+	/* The message identifier - opaque to applications. */
+	int msgid;
+
+	/* Size of message data. */
+	unsigned int size;
+
+	char data[0];           /* message */
+} VCHIQ_HEADER_T;
+
+typedef struct {
+	const void *data;
+	unsigned int size;
+} VCHIQ_ELEMENT_T;
+
+typedef unsigned int VCHIQ_SERVICE_HANDLE_T;
+
+typedef VCHIQ_STATUS_T (*VCHIQ_CALLBACK_T)(VCHIQ_REASON_T, VCHIQ_HEADER_T *,
+	VCHIQ_SERVICE_HANDLE_T, void *);
+
+typedef struct vchiq_service_base_struct {
+	int fourcc;
+	VCHIQ_CALLBACK_T callback;
+	void *userdata;
+} VCHIQ_SERVICE_BASE_T;
+
+typedef struct vchiq_service_params_struct {
+	int fourcc;
+	VCHIQ_CALLBACK_T callback;
+	void *userdata;
+	short version;       /* Increment for non-trivial changes */
+	short version_min;   /* Update for incompatible changes */
+} VCHIQ_SERVICE_PARAMS_T;
+
+typedef struct vchiq_config_struct {
+	unsigned int max_msg_size;
+	unsigned int bulk_threshold; /* The message size above which it
+					is better to use a bulk transfer
+					(<= max_msg_size) */
+	unsigned int max_outstanding_bulks;
+	unsigned int max_services;
+	short version;      /* The version of VCHIQ */
+	short version_min;  /* The minimum compatible version of VCHIQ */
+} VCHIQ_CONFIG_T;
+
+typedef struct vchiq_instance_struct *VCHIQ_INSTANCE_T;
+typedef void (*VCHIQ_REMOTE_USE_CALLBACK_T)(void *cb_arg);
+
+extern VCHIQ_STATUS_T vchiq_initialise(VCHIQ_INSTANCE_T *pinstance);
+extern VCHIQ_STATUS_T vchiq_shutdown(VCHIQ_INSTANCE_T instance);
+extern VCHIQ_STATUS_T vchiq_connect(VCHIQ_INSTANCE_T instance);
+extern VCHIQ_STATUS_T vchiq_add_service(VCHIQ_INSTANCE_T instance,
+	const VCHIQ_SERVICE_PARAMS_T *params,
+	VCHIQ_SERVICE_HANDLE_T *pservice);
+extern VCHIQ_STATUS_T vchiq_open_service(VCHIQ_INSTANCE_T instance,
+	const VCHIQ_SERVICE_PARAMS_T *params,
+	VCHIQ_SERVICE_HANDLE_T *pservice);
+extern VCHIQ_STATUS_T vchiq_close_service(VCHIQ_SERVICE_HANDLE_T service);
+extern VCHIQ_STATUS_T vchiq_remove_service(VCHIQ_SERVICE_HANDLE_T service);
+extern VCHIQ_STATUS_T vchiq_use_service(VCHIQ_SERVICE_HANDLE_T service);
+extern VCHIQ_STATUS_T vchiq_use_service_no_resume(
+	VCHIQ_SERVICE_HANDLE_T service);
+extern VCHIQ_STATUS_T vchiq_release_service(VCHIQ_SERVICE_HANDLE_T service);
+
+extern VCHIQ_STATUS_T vchiq_queue_message(VCHIQ_SERVICE_HANDLE_T service,
+	const VCHIQ_ELEMENT_T *elements, unsigned int count);
+extern void           vchiq_release_message(VCHIQ_SERVICE_HANDLE_T service,
+	VCHIQ_HEADER_T *header);
+extern VCHIQ_STATUS_T vchiq_queue_bulk_transmit(VCHIQ_SERVICE_HANDLE_T service,
+	const void *data, unsigned int size, void *userdata);
+extern VCHIQ_STATUS_T vchiq_queue_bulk_receive(VCHIQ_SERVICE_HANDLE_T service,
+	void *data, unsigned int size, void *userdata);
+extern VCHIQ_STATUS_T vchiq_queue_bulk_transmit_handle(
+	VCHIQ_SERVICE_HANDLE_T service, VCHI_MEM_HANDLE_T handle,
+	const void *offset, unsigned int size, void *userdata);
+extern VCHIQ_STATUS_T vchiq_queue_bulk_receive_handle(
+	VCHIQ_SERVICE_HANDLE_T service, VCHI_MEM_HANDLE_T handle,
+	void *offset, unsigned int size, void *userdata);
+extern VCHIQ_STATUS_T vchiq_bulk_transmit(VCHIQ_SERVICE_HANDLE_T service,
+	const void *data, unsigned int size, void *userdata,
+	VCHIQ_BULK_MODE_T mode);
+extern VCHIQ_STATUS_T vchiq_bulk_receive(VCHIQ_SERVICE_HANDLE_T service,
+	void *data, unsigned int size, void *userdata,
+	VCHIQ_BULK_MODE_T mode);
+extern VCHIQ_STATUS_T vchiq_bulk_transmit_handle(VCHIQ_SERVICE_HANDLE_T service,
+	VCHI_MEM_HANDLE_T handle, const void *offset, unsigned int size,
+	void *userdata,	VCHIQ_BULK_MODE_T mode);
+extern VCHIQ_STATUS_T vchiq_bulk_receive_handle(VCHIQ_SERVICE_HANDLE_T service,
+	VCHI_MEM_HANDLE_T handle, void *offset, unsigned int size,
+	void *userdata, VCHIQ_BULK_MODE_T mode);
+extern int   vchiq_get_client_id(VCHIQ_SERVICE_HANDLE_T service);
+extern void *vchiq_get_service_userdata(VCHIQ_SERVICE_HANDLE_T service);
+extern int   vchiq_get_service_fourcc(VCHIQ_SERVICE_HANDLE_T service);
+extern VCHIQ_STATUS_T vchiq_get_config(VCHIQ_INSTANCE_T instance,
+	int config_size, VCHIQ_CONFIG_T *pconfig);
+extern VCHIQ_STATUS_T vchiq_set_service_option(VCHIQ_SERVICE_HANDLE_T service,
+	VCHIQ_SERVICE_OPTION_T option, int value);
+
+extern VCHIQ_STATUS_T vchiq_remote_use(VCHIQ_INSTANCE_T instance,
+	VCHIQ_REMOTE_USE_CALLBACK_T callback, void *cb_arg);
+extern VCHIQ_STATUS_T vchiq_remote_release(VCHIQ_INSTANCE_T instance);
+
+extern VCHIQ_STATUS_T vchiq_dump_phys_mem(VCHIQ_SERVICE_HANDLE_T service,
+	void *ptr, size_t num_bytes);
+
+extern VCHIQ_STATUS_T vchiq_get_peer_version(VCHIQ_SERVICE_HANDLE_T handle,
+      short *peer_version);
+
+#endif /* VCHIQ_IF_H */
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_ioctl.h
@@ -0,0 +1,131 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHIQ_IOCTLS_H
+#define VCHIQ_IOCTLS_H
+
+#include <linux/ioctl.h>
+#include "vchiq_if.h"
+
+#define VCHIQ_IOC_MAGIC 0xc4
+#define VCHIQ_INVALID_HANDLE (~0)
+
+typedef struct {
+	VCHIQ_SERVICE_PARAMS_T params;
+	int is_open;
+	int is_vchi;
+	unsigned int handle;       /* OUT */
+} VCHIQ_CREATE_SERVICE_T;
+
+typedef struct {
+	unsigned int handle;
+	unsigned int count;
+	const VCHIQ_ELEMENT_T *elements;
+} VCHIQ_QUEUE_MESSAGE_T;
+
+typedef struct {
+	unsigned int handle;
+	void *data;
+	unsigned int size;
+	void *userdata;
+	VCHIQ_BULK_MODE_T mode;
+} VCHIQ_QUEUE_BULK_TRANSFER_T;
+
+typedef struct {
+	VCHIQ_REASON_T reason;
+	VCHIQ_HEADER_T *header;
+	void *service_userdata;
+	void *bulk_userdata;
+} VCHIQ_COMPLETION_DATA_T;
+
+typedef struct {
+	unsigned int count;
+	VCHIQ_COMPLETION_DATA_T *buf;
+	unsigned int msgbufsize;
+	unsigned int msgbufcount; /* IN/OUT */
+	void **msgbufs;
+} VCHIQ_AWAIT_COMPLETION_T;
+
+typedef struct {
+	unsigned int handle;
+	int blocking;
+	unsigned int bufsize;
+	void *buf;
+} VCHIQ_DEQUEUE_MESSAGE_T;
+
+typedef struct {
+	unsigned int config_size;
+	VCHIQ_CONFIG_T *pconfig;
+} VCHIQ_GET_CONFIG_T;
+
+typedef struct {
+	unsigned int handle;
+	VCHIQ_SERVICE_OPTION_T option;
+	int value;
+} VCHIQ_SET_SERVICE_OPTION_T;
+
+typedef struct {
+	void     *virt_addr;
+	size_t    num_bytes;
+} VCHIQ_DUMP_MEM_T;
+
+#define VCHIQ_IOC_CONNECT              _IO(VCHIQ_IOC_MAGIC,   0)
+#define VCHIQ_IOC_SHUTDOWN             _IO(VCHIQ_IOC_MAGIC,   1)
+#define VCHIQ_IOC_CREATE_SERVICE \
+	_IOWR(VCHIQ_IOC_MAGIC, 2, VCHIQ_CREATE_SERVICE_T)
+#define VCHIQ_IOC_REMOVE_SERVICE       _IO(VCHIQ_IOC_MAGIC,   3)
+#define VCHIQ_IOC_QUEUE_MESSAGE \
+	_IOW(VCHIQ_IOC_MAGIC,  4, VCHIQ_QUEUE_MESSAGE_T)
+#define VCHIQ_IOC_QUEUE_BULK_TRANSMIT \
+	_IOWR(VCHIQ_IOC_MAGIC, 5, VCHIQ_QUEUE_BULK_TRANSFER_T)
+#define VCHIQ_IOC_QUEUE_BULK_RECEIVE \
+	_IOWR(VCHIQ_IOC_MAGIC, 6, VCHIQ_QUEUE_BULK_TRANSFER_T)
+#define VCHIQ_IOC_AWAIT_COMPLETION \
+	_IOWR(VCHIQ_IOC_MAGIC, 7, VCHIQ_AWAIT_COMPLETION_T)
+#define VCHIQ_IOC_DEQUEUE_MESSAGE \
+	_IOWR(VCHIQ_IOC_MAGIC, 8, VCHIQ_DEQUEUE_MESSAGE_T)
+#define VCHIQ_IOC_GET_CLIENT_ID        _IO(VCHIQ_IOC_MAGIC,   9)
+#define VCHIQ_IOC_GET_CONFIG \
+	_IOWR(VCHIQ_IOC_MAGIC, 10, VCHIQ_GET_CONFIG_T)
+#define VCHIQ_IOC_CLOSE_SERVICE        _IO(VCHIQ_IOC_MAGIC,   11)
+#define VCHIQ_IOC_USE_SERVICE          _IO(VCHIQ_IOC_MAGIC,   12)
+#define VCHIQ_IOC_RELEASE_SERVICE      _IO(VCHIQ_IOC_MAGIC,   13)
+#define VCHIQ_IOC_SET_SERVICE_OPTION \
+	_IOW(VCHIQ_IOC_MAGIC,  14, VCHIQ_SET_SERVICE_OPTION_T)
+#define VCHIQ_IOC_DUMP_PHYS_MEM \
+	_IOW(VCHIQ_IOC_MAGIC,  15, VCHIQ_DUMP_MEM_T)
+#define VCHIQ_IOC_LIB_VERSION          _IO(VCHIQ_IOC_MAGIC,   16)
+#define VCHIQ_IOC_CLOSE_DELIVERED      _IO(VCHIQ_IOC_MAGIC,   17)
+#define VCHIQ_IOC_MAX                  17
+
+#endif
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_kern_lib.c
@@ -0,0 +1,456 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+/* ---- Include Files ---------------------------------------------------- */
+
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/mutex.h>
+
+#include "vchiq_core.h"
+#include "vchiq_arm.h"
+
+/* ---- Public Variables ------------------------------------------------- */
+
+/* ---- Private Constants and Types -------------------------------------- */
+
+struct bulk_waiter_node {
+	struct bulk_waiter bulk_waiter;
+	int pid;
+	struct list_head list;
+};
+
+struct vchiq_instance_struct {
+	VCHIQ_STATE_T *state;
+
+	int connected;
+
+	struct list_head bulk_waiter_list;
+	struct mutex bulk_waiter_list_mutex;
+};
+
+static VCHIQ_STATUS_T
+vchiq_blocking_bulk_transfer(VCHIQ_SERVICE_HANDLE_T handle, void *data,
+	unsigned int size, VCHIQ_BULK_DIR_T dir);
+
+/****************************************************************************
+*
+*   vchiq_initialise
+*
+***************************************************************************/
+#define VCHIQ_INIT_RETRIES 10
+VCHIQ_STATUS_T vchiq_initialise(VCHIQ_INSTANCE_T *instanceOut)
+{
+	VCHIQ_STATUS_T status = VCHIQ_ERROR;
+	VCHIQ_STATE_T *state;
+	VCHIQ_INSTANCE_T instance = NULL;
+        int i;
+
+	vchiq_log_trace(vchiq_core_log_level, "%s called", __func__);
+
+        /* VideoCore may not be ready due to boot up timing.
+           It may never be ready if kernel and firmware are mismatched, so don't block forever. */
+        for (i=0; i<VCHIQ_INIT_RETRIES; i++) {
+		state = vchiq_get_state();
+		if (state)
+			break;
+		udelay(500);
+	}
+	if (i==VCHIQ_INIT_RETRIES) {
+		vchiq_log_error(vchiq_core_log_level,
+			"%s: videocore not initialized\n", __func__);
+		goto failed;
+	} else if (i>0) {
+		vchiq_log_warning(vchiq_core_log_level,
+			"%s: videocore initialized after %d retries\n", __func__, i);
+	}
+
+	instance = kzalloc(sizeof(*instance), GFP_KERNEL);
+	if (!instance) {
+		vchiq_log_error(vchiq_core_log_level,
+			"%s: error allocating vchiq instance\n", __func__);
+		goto failed;
+	}
+
+	instance->connected = 0;
+	instance->state = state;
+	mutex_init(&instance->bulk_waiter_list_mutex);
+	INIT_LIST_HEAD(&instance->bulk_waiter_list);
+
+	*instanceOut = instance;
+
+	status = VCHIQ_SUCCESS;
+
+failed:
+	vchiq_log_trace(vchiq_core_log_level,
+		"%s(%p): returning %d", __func__, instance, status);
+
+	return status;
+}
+EXPORT_SYMBOL(vchiq_initialise);
+
+/****************************************************************************
+*
+*   vchiq_shutdown
+*
+***************************************************************************/
+
+VCHIQ_STATUS_T vchiq_shutdown(VCHIQ_INSTANCE_T instance)
+{
+	VCHIQ_STATUS_T status;
+	VCHIQ_STATE_T *state = instance->state;
+
+	vchiq_log_trace(vchiq_core_log_level,
+		"%s(%p) called", __func__, instance);
+
+	if (mutex_lock_interruptible(&state->mutex) != 0)
+		return VCHIQ_RETRY;
+
+	/* Remove all services */
+	status = vchiq_shutdown_internal(state, instance);
+
+	mutex_unlock(&state->mutex);
+
+	vchiq_log_trace(vchiq_core_log_level,
+		"%s(%p): returning %d", __func__, instance, status);
+
+	if (status == VCHIQ_SUCCESS) {
+		struct list_head *pos, *next;
+		list_for_each_safe(pos, next,
+				&instance->bulk_waiter_list) {
+			struct bulk_waiter_node *waiter;
+			waiter = list_entry(pos,
+					struct bulk_waiter_node,
+					list);
+			list_del(pos);
+			vchiq_log_info(vchiq_arm_log_level,
+					"bulk_waiter - cleaned up %x "
+					"for pid %d",
+					(unsigned int)waiter, waiter->pid);
+			kfree(waiter);
+		}
+		kfree(instance);
+	}
+
+	return status;
+}
+EXPORT_SYMBOL(vchiq_shutdown);
+
+/****************************************************************************
+*
+*   vchiq_is_connected
+*
+***************************************************************************/
+
+int vchiq_is_connected(VCHIQ_INSTANCE_T instance)
+{
+	return instance->connected;
+}
+
+/****************************************************************************
+*
+*   vchiq_connect
+*
+***************************************************************************/
+
+VCHIQ_STATUS_T vchiq_connect(VCHIQ_INSTANCE_T instance)
+{
+	VCHIQ_STATUS_T status;
+	VCHIQ_STATE_T *state = instance->state;
+
+	vchiq_log_trace(vchiq_core_log_level,
+		"%s(%p) called", __func__, instance);
+
+	if (mutex_lock_interruptible(&state->mutex) != 0) {
+		vchiq_log_trace(vchiq_core_log_level,
+			"%s: call to mutex_lock failed", __func__);
+		status = VCHIQ_RETRY;
+		goto failed;
+	}
+	status = vchiq_connect_internal(state, instance);
+
+	if (status == VCHIQ_SUCCESS)
+		instance->connected = 1;
+
+	mutex_unlock(&state->mutex);
+
+failed:
+	vchiq_log_trace(vchiq_core_log_level,
+		"%s(%p): returning %d", __func__, instance, status);
+
+	return status;
+}
+EXPORT_SYMBOL(vchiq_connect);
+
+/****************************************************************************
+*
+*   vchiq_add_service
+*
+***************************************************************************/
+
+VCHIQ_STATUS_T vchiq_add_service(
+	VCHIQ_INSTANCE_T              instance,
+	const VCHIQ_SERVICE_PARAMS_T *params,
+	VCHIQ_SERVICE_HANDLE_T       *phandle)
+{
+	VCHIQ_STATUS_T status;
+	VCHIQ_STATE_T *state = instance->state;
+	VCHIQ_SERVICE_T *service = NULL;
+	int srvstate;
+
+	vchiq_log_trace(vchiq_core_log_level,
+		"%s(%p) called", __func__, instance);
+
+	*phandle = VCHIQ_SERVICE_HANDLE_INVALID;
+
+	srvstate = vchiq_is_connected(instance)
+		? VCHIQ_SRVSTATE_LISTENING
+		: VCHIQ_SRVSTATE_HIDDEN;
+
+	service = vchiq_add_service_internal(
+		state,
+		params,
+		srvstate,
+		instance,
+		NULL);
+
+	if (service) {
+		*phandle = service->handle;
+		status = VCHIQ_SUCCESS;
+	} else
+		status = VCHIQ_ERROR;
+
+	vchiq_log_trace(vchiq_core_log_level,
+		"%s(%p): returning %d", __func__, instance, status);
+
+	return status;
+}
+EXPORT_SYMBOL(vchiq_add_service);
+
+/****************************************************************************
+*
+*   vchiq_open_service
+*
+***************************************************************************/
+
+VCHIQ_STATUS_T vchiq_open_service(
+	VCHIQ_INSTANCE_T              instance,
+	const VCHIQ_SERVICE_PARAMS_T *params,
+	VCHIQ_SERVICE_HANDLE_T       *phandle)
+{
+	VCHIQ_STATUS_T   status = VCHIQ_ERROR;
+	VCHIQ_STATE_T   *state = instance->state;
+	VCHIQ_SERVICE_T *service = NULL;
+
+	vchiq_log_trace(vchiq_core_log_level,
+		"%s(%p) called", __func__, instance);
+
+	*phandle = VCHIQ_SERVICE_HANDLE_INVALID;
+
+	if (!vchiq_is_connected(instance))
+		goto failed;
+
+	service = vchiq_add_service_internal(state,
+		params,
+		VCHIQ_SRVSTATE_OPENING,
+		instance,
+		NULL);
+
+	if (service) {
+		status = vchiq_open_service_internal(service, current->pid);
+		if (status == VCHIQ_SUCCESS)
+			*phandle = service->handle;
+		else
+			vchiq_remove_service(service->handle);
+	}
+
+failed:
+	vchiq_log_trace(vchiq_core_log_level,
+		"%s(%p): returning %d", __func__, instance, status);
+
+	return status;
+}
+EXPORT_SYMBOL(vchiq_open_service);
+
+VCHIQ_STATUS_T
+vchiq_queue_bulk_transmit(VCHIQ_SERVICE_HANDLE_T handle,
+	const void *data, unsigned int size, void *userdata)
+{
+	return vchiq_bulk_transfer(handle,
+		VCHI_MEM_HANDLE_INVALID, (void *)data, size, userdata,
+		VCHIQ_BULK_MODE_CALLBACK, VCHIQ_BULK_TRANSMIT);
+}
+EXPORT_SYMBOL(vchiq_queue_bulk_transmit);
+
+VCHIQ_STATUS_T
+vchiq_queue_bulk_receive(VCHIQ_SERVICE_HANDLE_T handle, void *data,
+	unsigned int size, void *userdata)
+{
+	return vchiq_bulk_transfer(handle,
+		VCHI_MEM_HANDLE_INVALID, data, size, userdata,
+		VCHIQ_BULK_MODE_CALLBACK, VCHIQ_BULK_RECEIVE);
+}
+EXPORT_SYMBOL(vchiq_queue_bulk_receive);
+
+VCHIQ_STATUS_T
+vchiq_bulk_transmit(VCHIQ_SERVICE_HANDLE_T handle, const void *data,
+	unsigned int size, void *userdata, VCHIQ_BULK_MODE_T mode)
+{
+	VCHIQ_STATUS_T status;
+
+	switch (mode) {
+	case VCHIQ_BULK_MODE_NOCALLBACK:
+	case VCHIQ_BULK_MODE_CALLBACK:
+		status = vchiq_bulk_transfer(handle,
+			VCHI_MEM_HANDLE_INVALID, (void *)data, size, userdata,
+			mode, VCHIQ_BULK_TRANSMIT);
+		break;
+	case VCHIQ_BULK_MODE_BLOCKING:
+		status = vchiq_blocking_bulk_transfer(handle,
+			(void *)data, size, VCHIQ_BULK_TRANSMIT);
+		break;
+	default:
+		return VCHIQ_ERROR;
+	}
+
+	return status;
+}
+EXPORT_SYMBOL(vchiq_bulk_transmit);
+
+VCHIQ_STATUS_T
+vchiq_bulk_receive(VCHIQ_SERVICE_HANDLE_T handle, void *data,
+	unsigned int size, void *userdata, VCHIQ_BULK_MODE_T mode)
+{
+	VCHIQ_STATUS_T status;
+
+	switch (mode) {
+	case VCHIQ_BULK_MODE_NOCALLBACK:
+	case VCHIQ_BULK_MODE_CALLBACK:
+		status = vchiq_bulk_transfer(handle,
+			VCHI_MEM_HANDLE_INVALID, data, size, userdata,
+			mode, VCHIQ_BULK_RECEIVE);
+		break;
+	case VCHIQ_BULK_MODE_BLOCKING:
+		status = vchiq_blocking_bulk_transfer(handle,
+			(void *)data, size, VCHIQ_BULK_RECEIVE);
+		break;
+	default:
+		return VCHIQ_ERROR;
+	}
+
+	return status;
+}
+EXPORT_SYMBOL(vchiq_bulk_receive);
+
+static VCHIQ_STATUS_T
+vchiq_blocking_bulk_transfer(VCHIQ_SERVICE_HANDLE_T handle, void *data,
+	unsigned int size, VCHIQ_BULK_DIR_T dir)
+{
+	VCHIQ_INSTANCE_T instance;
+	VCHIQ_SERVICE_T *service;
+	VCHIQ_STATUS_T status;
+	struct bulk_waiter_node *waiter = NULL;
+	struct list_head *pos;
+
+	service = find_service_by_handle(handle);
+	if (!service)
+		return VCHIQ_ERROR;
+
+	instance = service->instance;
+
+	unlock_service(service);
+
+	mutex_lock(&instance->bulk_waiter_list_mutex);
+	list_for_each(pos, &instance->bulk_waiter_list) {
+		if (list_entry(pos, struct bulk_waiter_node,
+				list)->pid == current->pid) {
+			waiter = list_entry(pos,
+				struct bulk_waiter_node,
+				list);
+			list_del(pos);
+			break;
+		}
+	}
+	mutex_unlock(&instance->bulk_waiter_list_mutex);
+
+	if (waiter) {
+		VCHIQ_BULK_T *bulk = waiter->bulk_waiter.bulk;
+		if (bulk) {
+			/* This thread has an outstanding bulk transfer. */
+			if ((bulk->data != data) ||
+				(bulk->size != size)) {
+				/* This is not a retry of the previous one.
+				** Cancel the signal when the transfer
+				** completes. */
+				spin_lock(&bulk_waiter_spinlock);
+				bulk->userdata = NULL;
+				spin_unlock(&bulk_waiter_spinlock);
+			}
+		}
+	}
+
+	if (!waiter) {
+		waiter = kzalloc(sizeof(struct bulk_waiter_node), GFP_KERNEL);
+		if (!waiter) {
+			vchiq_log_error(vchiq_core_log_level,
+				"%s - out of memory", __func__);
+			return VCHIQ_ERROR;
+		}
+	}
+
+	status = vchiq_bulk_transfer(handle, VCHI_MEM_HANDLE_INVALID,
+		data, size, &waiter->bulk_waiter, VCHIQ_BULK_MODE_BLOCKING,
+		dir);
+	if ((status != VCHIQ_RETRY) || fatal_signal_pending(current) ||
+		!waiter->bulk_waiter.bulk) {
+		VCHIQ_BULK_T *bulk = waiter->bulk_waiter.bulk;
+		if (bulk) {
+			/* Cancel the signal when the transfer
+			 ** completes. */
+			spin_lock(&bulk_waiter_spinlock);
+			bulk->userdata = NULL;
+			spin_unlock(&bulk_waiter_spinlock);
+		}
+		kfree(waiter);
+	} else {
+		waiter->pid = current->pid;
+		mutex_lock(&instance->bulk_waiter_list_mutex);
+		list_add(&waiter->list, &instance->bulk_waiter_list);
+		mutex_unlock(&instance->bulk_waiter_list_mutex);
+		vchiq_log_info(vchiq_arm_log_level,
+				"saved bulk_waiter %x for pid %d",
+				(unsigned int)waiter, current->pid);
+	}
+
+	return status;
+}
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_memdrv.h
@@ -0,0 +1,71 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHIQ_MEMDRV_H
+#define VCHIQ_MEMDRV_H
+
+/* ---- Include Files ----------------------------------------------------- */
+
+#include <linux/kernel.h>
+#include "vchiq_if.h"
+
+/* ---- Constants and Types ---------------------------------------------- */
+
+typedef struct {
+	 void                   *armSharedMemVirt;
+	 dma_addr_t              armSharedMemPhys;
+	 size_t                  armSharedMemSize;
+
+	 void                   *vcSharedMemVirt;
+	 dma_addr_t              vcSharedMemPhys;
+	 size_t                  vcSharedMemSize;
+} VCHIQ_SHARED_MEM_INFO_T;
+
+/* ---- Variable Externs ------------------------------------------------- */
+
+/* ---- Function Prototypes ---------------------------------------------- */
+
+void vchiq_get_shared_mem_info(VCHIQ_SHARED_MEM_INFO_T *info);
+
+VCHIQ_STATUS_T vchiq_memdrv_initialise(void);
+
+VCHIQ_STATUS_T vchiq_userdrv_create_instance(
+	const VCHIQ_PLATFORM_DATA_T * platform_data);
+
+VCHIQ_STATUS_T vchiq_userdrv_suspend(
+	const VCHIQ_PLATFORM_DATA_T * platform_data);
+
+VCHIQ_STATUS_T vchiq_userdrv_resume(
+	const VCHIQ_PLATFORM_DATA_T * platform_data);
+
+#endif
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_pagelist.h
@@ -0,0 +1,58 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHIQ_PAGELIST_H
+#define VCHIQ_PAGELIST_H
+
+#ifndef PAGE_SIZE
+#define PAGE_SIZE 4096
+#endif
+#define CACHE_LINE_SIZE 32
+#define PAGELIST_WRITE 0
+#define PAGELIST_READ 1
+#define PAGELIST_READ_WITH_FRAGMENTS 2
+
+typedef struct pagelist_struct {
+	unsigned long length;
+	unsigned short type;
+	unsigned short offset;
+	unsigned long addrs[1];	/* N.B. 12 LSBs hold the number of following
+				   pages at consecutive addresses. */
+} PAGELIST_T;
+
+typedef struct fragments_struct {
+	char headbuf[CACHE_LINE_SIZE];
+	char tailbuf[CACHE_LINE_SIZE];
+} FRAGMENTS_T;
+
+#endif /* VCHIQ_PAGELIST_H */
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_shim.c
@@ -0,0 +1,853 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+#include <linux/module.h>
+#include <linux/types.h>
+
+#include "interface/vchi/vchi.h"
+#include "vchiq.h"
+#include "vchiq_core.h"
+
+#include "vchiq_util.h"
+
+#include <stddef.h>
+
+#define vchiq_status_to_vchi(status) ((int32_t)status)
+
+typedef struct {
+	VCHIQ_SERVICE_HANDLE_T handle;
+
+	VCHIU_QUEUE_T queue;
+
+	VCHI_CALLBACK_T callback;
+	void *callback_param;
+} SHIM_SERVICE_T;
+
+/* ----------------------------------------------------------------------
+ * return pointer to the mphi message driver function table
+ * -------------------------------------------------------------------- */
+const VCHI_MESSAGE_DRIVER_T *
+vchi_mphi_message_driver_func_table(void)
+{
+	return NULL;
+}
+
+/* ----------------------------------------------------------------------
+ * return a pointer to the 'single' connection driver fops
+ * -------------------------------------------------------------------- */
+const VCHI_CONNECTION_API_T *
+single_get_func_table(void)
+{
+	return NULL;
+}
+
+VCHI_CONNECTION_T *vchi_create_connection(
+	const VCHI_CONNECTION_API_T *function_table,
+	const VCHI_MESSAGE_DRIVER_T *low_level)
+{
+	(void)function_table;
+	(void)low_level;
+	return NULL;
+}
+
+/***********************************************************
+ * Name: vchi_msg_peek
+ *
+ * Arguments:  const VCHI_SERVICE_HANDLE_T handle,
+ *             void **data,
+ *             uint32_t *msg_size,
+
+
+ *             VCHI_FLAGS_T flags
+ *
+ * Description: Routine to return a pointer to the current message (to allow in
+ *              place processing). The message can be removed using
+ *              vchi_msg_remove when you're finished
+ *
+ * Returns: int32_t - success == 0
+ *
+ ***********************************************************/
+int32_t vchi_msg_peek(VCHI_SERVICE_HANDLE_T handle,
+	void **data,
+	uint32_t *msg_size,
+	VCHI_FLAGS_T flags)
+{
+	SHIM_SERVICE_T *service = (SHIM_SERVICE_T *)handle;
+	VCHIQ_HEADER_T *header;
+
+	WARN_ON((flags != VCHI_FLAGS_NONE) &&
+		(flags != VCHI_FLAGS_BLOCK_UNTIL_OP_COMPLETE));
+
+	if (flags == VCHI_FLAGS_NONE)
+		if (vchiu_queue_is_empty(&service->queue))
+			return -1;
+
+	header = vchiu_queue_peek(&service->queue);
+
+	*data = header->data;
+	*msg_size = header->size;
+
+	return 0;
+}
+EXPORT_SYMBOL(vchi_msg_peek);
+
+/***********************************************************
+ * Name: vchi_msg_remove
+ *
+ * Arguments:  const VCHI_SERVICE_HANDLE_T handle,
+ *
+ * Description: Routine to remove a message (after it has been read with
+ *              vchi_msg_peek)
+ *
+ * Returns: int32_t - success == 0
+ *
+ ***********************************************************/
+int32_t vchi_msg_remove(VCHI_SERVICE_HANDLE_T handle)
+{
+	SHIM_SERVICE_T *service = (SHIM_SERVICE_T *)handle;
+	VCHIQ_HEADER_T *header;
+
+	header = vchiu_queue_pop(&service->queue);
+
+	vchiq_release_message(service->handle, header);
+
+	return 0;
+}
+EXPORT_SYMBOL(vchi_msg_remove);
+
+/***********************************************************
+ * Name: vchi_msg_queue
+ *
+ * Arguments:  VCHI_SERVICE_HANDLE_T handle,
+ *             const void *data,
+ *             uint32_t data_size,
+ *             VCHI_FLAGS_T flags,
+ *             void *msg_handle,
+ *
+ * Description: Thin wrapper to queue a message onto a connection
+ *
+ * Returns: int32_t - success == 0
+ *
+ ***********************************************************/
+int32_t vchi_msg_queue(VCHI_SERVICE_HANDLE_T handle,
+	const void *data,
+	uint32_t data_size,
+	VCHI_FLAGS_T flags,
+	void *msg_handle)
+{
+	SHIM_SERVICE_T *service = (SHIM_SERVICE_T *)handle;
+	VCHIQ_ELEMENT_T element = {data, data_size};
+	VCHIQ_STATUS_T status;
+
+	(void)msg_handle;
+
+	WARN_ON(flags != VCHI_FLAGS_BLOCK_UNTIL_QUEUED);
+
+	status = vchiq_queue_message(service->handle, &element, 1);
+
+	/* vchiq_queue_message() may return VCHIQ_RETRY, so we need to
+	** implement a retry mechanism since this function is supposed
+	** to block until queued
+	*/
+	while (status == VCHIQ_RETRY) {
+		msleep(1);
+		status = vchiq_queue_message(service->handle, &element, 1);
+	}
+
+	return vchiq_status_to_vchi(status);
+}
+EXPORT_SYMBOL(vchi_msg_queue);
+
+/***********************************************************
+ * Name: vchi_bulk_queue_receive
+ *
+ * Arguments:  VCHI_BULK_HANDLE_T handle,
+ *             void *data_dst,
+ *             const uint32_t data_size,
+ *             VCHI_FLAGS_T flags
+ *             void *bulk_handle
+ *
+ * Description: Routine to setup a rcv buffer
+ *
+ * Returns: int32_t - success == 0
+ *
+ ***********************************************************/
+int32_t vchi_bulk_queue_receive(VCHI_SERVICE_HANDLE_T handle,
+	void *data_dst,
+	uint32_t data_size,
+	VCHI_FLAGS_T flags,
+	void *bulk_handle)
+{
+	SHIM_SERVICE_T *service = (SHIM_SERVICE_T *)handle;
+	VCHIQ_BULK_MODE_T mode;
+	VCHIQ_STATUS_T status;
+
+	switch ((int)flags) {
+	case VCHI_FLAGS_CALLBACK_WHEN_OP_COMPLETE
+		| VCHI_FLAGS_BLOCK_UNTIL_QUEUED:
+		WARN_ON(!service->callback);
+		mode = VCHIQ_BULK_MODE_CALLBACK;
+		break;
+	case VCHI_FLAGS_BLOCK_UNTIL_OP_COMPLETE:
+		mode = VCHIQ_BULK_MODE_BLOCKING;
+		break;
+	case VCHI_FLAGS_BLOCK_UNTIL_QUEUED:
+	case VCHI_FLAGS_NONE:
+		mode = VCHIQ_BULK_MODE_NOCALLBACK;
+		break;
+	default:
+		WARN(1, "unsupported message\n");
+		return vchiq_status_to_vchi(VCHIQ_ERROR);
+	}
+
+	status = vchiq_bulk_receive(service->handle, data_dst, data_size,
+		bulk_handle, mode);
+
+	/* vchiq_bulk_receive() may return VCHIQ_RETRY, so we need to
+	** implement a retry mechanism since this function is supposed
+	** to block until queued
+	*/
+	while (status == VCHIQ_RETRY) {
+		msleep(1);
+		status = vchiq_bulk_receive(service->handle, data_dst,
+			data_size, bulk_handle, mode);
+	}
+
+	return vchiq_status_to_vchi(status);
+}
+EXPORT_SYMBOL(vchi_bulk_queue_receive);
+
+/***********************************************************
+ * Name: vchi_bulk_queue_transmit
+ *
+ * Arguments:  VCHI_BULK_HANDLE_T handle,
+ *             const void *data_src,
+ *             uint32_t data_size,
+ *             VCHI_FLAGS_T flags,
+ *             void *bulk_handle
+ *
+ * Description: Routine to transmit some data
+ *
+ * Returns: int32_t - success == 0
+ *
+ ***********************************************************/
+int32_t vchi_bulk_queue_transmit(VCHI_SERVICE_HANDLE_T handle,
+	const void *data_src,
+	uint32_t data_size,
+	VCHI_FLAGS_T flags,
+	void *bulk_handle)
+{
+	SHIM_SERVICE_T *service = (SHIM_SERVICE_T *)handle;
+	VCHIQ_BULK_MODE_T mode;
+	VCHIQ_STATUS_T status;
+
+	switch ((int)flags) {
+	case VCHI_FLAGS_CALLBACK_WHEN_OP_COMPLETE
+		| VCHI_FLAGS_BLOCK_UNTIL_QUEUED:
+		WARN_ON(!service->callback);
+		mode = VCHIQ_BULK_MODE_CALLBACK;
+		break;
+	case VCHI_FLAGS_BLOCK_UNTIL_DATA_READ:
+	case VCHI_FLAGS_BLOCK_UNTIL_OP_COMPLETE:
+		mode = VCHIQ_BULK_MODE_BLOCKING;
+		break;
+	case VCHI_FLAGS_BLOCK_UNTIL_QUEUED:
+	case VCHI_FLAGS_NONE:
+		mode = VCHIQ_BULK_MODE_NOCALLBACK;
+		break;
+	default:
+		WARN(1, "unsupported message\n");
+		return vchiq_status_to_vchi(VCHIQ_ERROR);
+	}
+
+	status = vchiq_bulk_transmit(service->handle, data_src, data_size,
+		bulk_handle, mode);
+
+	/* vchiq_bulk_transmit() may return VCHIQ_RETRY, so we need to
+	** implement a retry mechanism since this function is supposed
+	** to block until queued
+	*/
+	while (status == VCHIQ_RETRY) {
+		msleep(1);
+		status = vchiq_bulk_transmit(service->handle, data_src,
+			data_size, bulk_handle, mode);
+	}
+
+	return vchiq_status_to_vchi(status);
+}
+EXPORT_SYMBOL(vchi_bulk_queue_transmit);
+
+/***********************************************************
+ * Name: vchi_msg_dequeue
+ *
+ * Arguments:  VCHI_SERVICE_HANDLE_T handle,
+ *             void *data,
+ *             uint32_t max_data_size_to_read,
+ *             uint32_t *actual_msg_size
+ *             VCHI_FLAGS_T flags
+ *
+ * Description: Routine to dequeue a message into the supplied buffer
+ *
+ * Returns: int32_t - success == 0
+ *
+ ***********************************************************/
+int32_t vchi_msg_dequeue(VCHI_SERVICE_HANDLE_T handle,
+	void *data,
+	uint32_t max_data_size_to_read,
+	uint32_t *actual_msg_size,
+	VCHI_FLAGS_T flags)
+{
+	SHIM_SERVICE_T *service = (SHIM_SERVICE_T *)handle;
+	VCHIQ_HEADER_T *header;
+
+	WARN_ON((flags != VCHI_FLAGS_NONE) &&
+		(flags != VCHI_FLAGS_BLOCK_UNTIL_OP_COMPLETE));
+
+	if (flags == VCHI_FLAGS_NONE)
+		if (vchiu_queue_is_empty(&service->queue))
+			return -1;
+
+	header = vchiu_queue_pop(&service->queue);
+
+	memcpy(data, header->data, header->size < max_data_size_to_read ?
+		header->size : max_data_size_to_read);
+
+	*actual_msg_size = header->size;
+
+	vchiq_release_message(service->handle, header);
+
+	return 0;
+}
+EXPORT_SYMBOL(vchi_msg_dequeue);
+
+/***********************************************************
+ * Name: vchi_msg_queuev
+ *
+ * Arguments:  VCHI_SERVICE_HANDLE_T handle,
+ *             VCHI_MSG_VECTOR_T *vector,
+ *             uint32_t count,
+ *             VCHI_FLAGS_T flags,
+ *             void *msg_handle
+ *
+ * Description: Thin wrapper to queue a message onto a connection
+ *
+ * Returns: int32_t - success == 0
+ *
+ ***********************************************************/
+
+vchiq_static_assert(sizeof(VCHI_MSG_VECTOR_T) == sizeof(VCHIQ_ELEMENT_T));
+vchiq_static_assert(offsetof(VCHI_MSG_VECTOR_T, vec_base) ==
+	offsetof(VCHIQ_ELEMENT_T, data));
+vchiq_static_assert(offsetof(VCHI_MSG_VECTOR_T, vec_len) ==
+	offsetof(VCHIQ_ELEMENT_T, size));
+
+int32_t vchi_msg_queuev(VCHI_SERVICE_HANDLE_T handle,
+	VCHI_MSG_VECTOR_T *vector,
+	uint32_t count,
+	VCHI_FLAGS_T flags,
+	void *msg_handle)
+{
+	SHIM_SERVICE_T *service = (SHIM_SERVICE_T *)handle;
+
+	(void)msg_handle;
+
+	WARN_ON(flags != VCHI_FLAGS_BLOCK_UNTIL_QUEUED);
+
+	return vchiq_status_to_vchi(vchiq_queue_message(service->handle,
+		(const VCHIQ_ELEMENT_T *)vector, count));
+}
+EXPORT_SYMBOL(vchi_msg_queuev);
+
+/***********************************************************
+ * Name: vchi_held_msg_release
+ *
+ * Arguments:  VCHI_HELD_MSG_T *message
+ *
+ * Description: Routine to release a held message (after it has been read with
+ *              vchi_msg_hold)
+ *
+ * Returns: int32_t - success == 0
+ *
+ ***********************************************************/
+int32_t vchi_held_msg_release(VCHI_HELD_MSG_T *message)
+{
+	vchiq_release_message((VCHIQ_SERVICE_HANDLE_T)message->service,
+		(VCHIQ_HEADER_T *)message->message);
+
+	return 0;
+}
+EXPORT_SYMBOL(vchi_held_msg_release);
+
+/***********************************************************
+ * Name: vchi_msg_hold
+ *
+ * Arguments:  VCHI_SERVICE_HANDLE_T handle,
+ *             void **data,
+ *             uint32_t *msg_size,
+ *             VCHI_FLAGS_T flags,
+ *             VCHI_HELD_MSG_T *message_handle
+ *
+ * Description: Routine to return a pointer to the current message (to allow
+ *              in place processing). The message is dequeued - don't forget
+ *              to release the message using vchi_held_msg_release when you're
+ *              finished.
+ *
+ * Returns: int32_t - success == 0
+ *
+ ***********************************************************/
+int32_t vchi_msg_hold(VCHI_SERVICE_HANDLE_T handle,
+	void **data,
+	uint32_t *msg_size,
+	VCHI_FLAGS_T flags,
+	VCHI_HELD_MSG_T *message_handle)
+{
+	SHIM_SERVICE_T *service = (SHIM_SERVICE_T *)handle;
+	VCHIQ_HEADER_T *header;
+
+	WARN_ON((flags != VCHI_FLAGS_NONE) &&
+		(flags != VCHI_FLAGS_BLOCK_UNTIL_OP_COMPLETE));
+
+	if (flags == VCHI_FLAGS_NONE)
+		if (vchiu_queue_is_empty(&service->queue))
+			return -1;
+
+	header = vchiu_queue_pop(&service->queue);
+
+	*data = header->data;
+	*msg_size = header->size;
+
+	message_handle->service =
+		(struct opaque_vchi_service_t *)service->handle;
+	message_handle->message = header;
+
+	return 0;
+}
+EXPORT_SYMBOL(vchi_msg_hold);
+
+/***********************************************************
+ * Name: vchi_initialise
+ *
+ * Arguments: VCHI_INSTANCE_T *instance_handle
+ *
+ * Description: Initialises the hardware but does not transmit anything
+ *              When run as a Host App this will be called twice hence the need
+ *              to malloc the state information
+ *
+ * Returns: 0 if successful, failure otherwise
+ *
+ ***********************************************************/
+
+int32_t vchi_initialise(VCHI_INSTANCE_T *instance_handle)
+{
+	VCHIQ_INSTANCE_T instance;
+	VCHIQ_STATUS_T status;
+
+	status = vchiq_initialise(&instance);
+
+	*instance_handle = (VCHI_INSTANCE_T)instance;
+
+	return vchiq_status_to_vchi(status);
+}
+EXPORT_SYMBOL(vchi_initialise);
+
+/***********************************************************
+ * Name: vchi_connect
+ *
+ * Arguments: VCHI_CONNECTION_T **connections
+ *            const uint32_t num_connections
+ *            VCHI_INSTANCE_T instance_handle)
+ *
+ * Description: Starts the command service on each connection,
+ *              causing INIT messages to be pinged back and forth
+ *
+ * Returns: 0 if successful, failure otherwise
+ *
+ ***********************************************************/
+int32_t vchi_connect(VCHI_CONNECTION_T **connections,
+	const uint32_t num_connections,
+	VCHI_INSTANCE_T instance_handle)
+{
+	VCHIQ_INSTANCE_T instance = (VCHIQ_INSTANCE_T)instance_handle;
+
+	(void)connections;
+	(void)num_connections;
+
+	return vchiq_connect(instance);
+}
+EXPORT_SYMBOL(vchi_connect);
+
+
+/***********************************************************
+ * Name: vchi_disconnect
+ *
+ * Arguments: VCHI_INSTANCE_T instance_handle
+ *
+ * Description: Stops the command service on each connection,
+ *              causing DE-INIT messages to be pinged back and forth
+ *
+ * Returns: 0 if successful, failure otherwise
+ *
+ ***********************************************************/
+int32_t vchi_disconnect(VCHI_INSTANCE_T instance_handle)
+{
+	VCHIQ_INSTANCE_T instance = (VCHIQ_INSTANCE_T)instance_handle;
+	return vchiq_status_to_vchi(vchiq_shutdown(instance));
+}
+EXPORT_SYMBOL(vchi_disconnect);
+
+
+/***********************************************************
+ * Name: vchi_service_open
+ * Name: vchi_service_create
+ *
+ * Arguments: VCHI_INSTANCE_T *instance_handle
+ *            SERVICE_CREATION_T *setup,
+ *            VCHI_SERVICE_HANDLE_T *handle
+ *
+ * Description: Routine to open a service
+ *
+ * Returns: int32_t - success == 0
+ *
+ ***********************************************************/
+
+static VCHIQ_STATUS_T shim_callback(VCHIQ_REASON_T reason,
+	VCHIQ_HEADER_T *header, VCHIQ_SERVICE_HANDLE_T handle, void *bulk_user)
+{
+	SHIM_SERVICE_T *service =
+		(SHIM_SERVICE_T *)VCHIQ_GET_SERVICE_USERDATA(handle);
+
+        if (!service->callback)
+		goto release;
+
+	switch (reason) {
+	case VCHIQ_MESSAGE_AVAILABLE:
+		vchiu_queue_push(&service->queue, header);
+
+		service->callback(service->callback_param,
+				  VCHI_CALLBACK_MSG_AVAILABLE, NULL);
+
+		goto done;
+		break;
+
+	case VCHIQ_BULK_TRANSMIT_DONE:
+		service->callback(service->callback_param,
+				  VCHI_CALLBACK_BULK_SENT, bulk_user);
+		break;
+
+	case VCHIQ_BULK_RECEIVE_DONE:
+		service->callback(service->callback_param,
+				  VCHI_CALLBACK_BULK_RECEIVED, bulk_user);
+		break;
+
+	case VCHIQ_SERVICE_CLOSED:
+		service->callback(service->callback_param,
+				  VCHI_CALLBACK_SERVICE_CLOSED, NULL);
+		break;
+
+	case VCHIQ_SERVICE_OPENED:
+		/* No equivalent VCHI reason */
+		break;
+
+	case VCHIQ_BULK_TRANSMIT_ABORTED:
+		service->callback(service->callback_param,
+				  VCHI_CALLBACK_BULK_TRANSMIT_ABORTED,
+				  bulk_user);
+		break;
+
+	case VCHIQ_BULK_RECEIVE_ABORTED:
+		service->callback(service->callback_param,
+				  VCHI_CALLBACK_BULK_RECEIVE_ABORTED,
+				  bulk_user);
+		break;
+
+	default:
+		WARN(1, "not supported\n");
+		break;
+	}
+
+release:
+        vchiq_release_message(service->handle, header);
+done:
+	return VCHIQ_SUCCESS;
+}
+
+static SHIM_SERVICE_T *service_alloc(VCHIQ_INSTANCE_T instance,
+	SERVICE_CREATION_T *setup)
+{
+	SHIM_SERVICE_T *service = kzalloc(sizeof(SHIM_SERVICE_T), GFP_KERNEL);
+
+	(void)instance;
+
+	if (service) {
+		if (vchiu_queue_init(&service->queue, 64)) {
+			service->callback = setup->callback;
+			service->callback_param = setup->callback_param;
+		} else {
+			kfree(service);
+			service = NULL;
+		}
+	}
+
+	return service;
+}
+
+static void service_free(SHIM_SERVICE_T *service)
+{
+	if (service) {
+		vchiu_queue_delete(&service->queue);
+		kfree(service);
+	}
+}
+
+int32_t vchi_service_open(VCHI_INSTANCE_T instance_handle,
+	SERVICE_CREATION_T *setup,
+	VCHI_SERVICE_HANDLE_T *handle)
+{
+	VCHIQ_INSTANCE_T instance = (VCHIQ_INSTANCE_T)instance_handle;
+	SHIM_SERVICE_T *service = service_alloc(instance, setup);
+	if (service) {
+		VCHIQ_SERVICE_PARAMS_T params;
+		VCHIQ_STATUS_T status;
+
+		memset(&params, 0, sizeof(params));
+		params.fourcc = setup->service_id;
+		params.callback = shim_callback;
+		params.userdata = service;
+		params.version = setup->version.version;
+		params.version_min = setup->version.version_min;
+
+		status = vchiq_open_service(instance, &params,
+			&service->handle);
+		if (status != VCHIQ_SUCCESS) {
+			service_free(service);
+			service = NULL;
+		}
+	}
+
+	*handle = (VCHI_SERVICE_HANDLE_T)service;
+
+	return (service != NULL) ? 0 : -1;
+}
+EXPORT_SYMBOL(vchi_service_open);
+
+int32_t vchi_service_create(VCHI_INSTANCE_T instance_handle,
+	SERVICE_CREATION_T *setup,
+	VCHI_SERVICE_HANDLE_T *handle)
+{
+	VCHIQ_INSTANCE_T instance = (VCHIQ_INSTANCE_T)instance_handle;
+	SHIM_SERVICE_T *service = service_alloc(instance, setup);
+	if (service) {
+		VCHIQ_SERVICE_PARAMS_T params;
+		VCHIQ_STATUS_T status;
+
+		memset(&params, 0, sizeof(params));
+		params.fourcc = setup->service_id;
+		params.callback = shim_callback;
+		params.userdata = service;
+		params.version = setup->version.version;
+		params.version_min = setup->version.version_min;
+		status = vchiq_add_service(instance, &params, &service->handle);
+
+		if (status != VCHIQ_SUCCESS) {
+			service_free(service);
+			service = NULL;
+		}
+	}
+
+	*handle = (VCHI_SERVICE_HANDLE_T)service;
+
+	return (service != NULL) ? 0 : -1;
+}
+EXPORT_SYMBOL(vchi_service_create);
+
+int32_t vchi_service_close(const VCHI_SERVICE_HANDLE_T handle)
+{
+	int32_t ret = -1;
+	SHIM_SERVICE_T *service = (SHIM_SERVICE_T *)handle;
+	if (service) {
+		VCHIQ_STATUS_T status = vchiq_close_service(service->handle);
+		if (status == VCHIQ_SUCCESS) {
+			service_free(service);
+			service = NULL;
+		}
+
+		ret = vchiq_status_to_vchi(status);
+	}
+	return ret;
+}
+EXPORT_SYMBOL(vchi_service_close);
+
+int32_t vchi_service_destroy(const VCHI_SERVICE_HANDLE_T handle)
+{
+	int32_t ret = -1;
+	SHIM_SERVICE_T *service = (SHIM_SERVICE_T *)handle;
+	if (service) {
+		VCHIQ_STATUS_T status = vchiq_remove_service(service->handle);
+		if (status == VCHIQ_SUCCESS) {
+			service_free(service);
+			service = NULL;
+		}
+
+		ret = vchiq_status_to_vchi(status);
+	}
+	return ret;
+}
+EXPORT_SYMBOL(vchi_service_destroy);
+
+int32_t vchi_service_set_option(const VCHI_SERVICE_HANDLE_T handle,
+				VCHI_SERVICE_OPTION_T option,
+				int value)
+{
+	int32_t ret = -1;
+	SHIM_SERVICE_T *service = (SHIM_SERVICE_T *)handle;
+	VCHIQ_SERVICE_OPTION_T vchiq_option;
+	switch (option) {
+	case VCHI_SERVICE_OPTION_TRACE:
+		vchiq_option = VCHIQ_SERVICE_OPTION_TRACE;
+		break;
+	default:
+		service = NULL;
+		break;
+	}
+	if (service) {
+		VCHIQ_STATUS_T status =
+			vchiq_set_service_option(service->handle,
+						vchiq_option,
+						value);
+
+		ret = vchiq_status_to_vchi(status);
+	}
+	return ret;
+}
+EXPORT_SYMBOL(vchi_service_set_option);
+
+int32_t vchi_get_peer_version( const VCHI_SERVICE_HANDLE_T handle, short *peer_version )
+{
+   int32_t ret = -1;
+   SHIM_SERVICE_T *service = (SHIM_SERVICE_T *)handle;
+   if(service)
+   {
+      VCHIQ_STATUS_T status = vchiq_get_peer_version(service->handle, peer_version);
+      ret = vchiq_status_to_vchi( status );
+   }
+   return ret;
+}
+EXPORT_SYMBOL(vchi_get_peer_version);
+
+/* ----------------------------------------------------------------------
+ * read a uint32_t from buffer.
+ * network format is defined to be little endian
+ * -------------------------------------------------------------------- */
+uint32_t
+vchi_readbuf_uint32(const void *_ptr)
+{
+	const unsigned char *ptr = _ptr;
+	return ptr[0] | (ptr[1] << 8) | (ptr[2] << 16) | (ptr[3] << 24);
+}
+
+/* ----------------------------------------------------------------------
+ * write a uint32_t to buffer.
+ * network format is defined to be little endian
+ * -------------------------------------------------------------------- */
+void
+vchi_writebuf_uint32(void *_ptr, uint32_t value)
+{
+	unsigned char *ptr = _ptr;
+	ptr[0] = (unsigned char)((value >> 0)  & 0xFF);
+	ptr[1] = (unsigned char)((value >> 8)  & 0xFF);
+	ptr[2] = (unsigned char)((value >> 16) & 0xFF);
+	ptr[3] = (unsigned char)((value >> 24) & 0xFF);
+}
+
+/* ----------------------------------------------------------------------
+ * read a uint16_t from buffer.
+ * network format is defined to be little endian
+ * -------------------------------------------------------------------- */
+uint16_t
+vchi_readbuf_uint16(const void *_ptr)
+{
+	const unsigned char *ptr = _ptr;
+	return ptr[0] | (ptr[1] << 8);
+}
+
+/* ----------------------------------------------------------------------
+ * write a uint16_t into the buffer.
+ * network format is defined to be little endian
+ * -------------------------------------------------------------------- */
+void
+vchi_writebuf_uint16(void *_ptr, uint16_t value)
+{
+	unsigned char *ptr = _ptr;
+	ptr[0] = (value >> 0)  & 0xFF;
+	ptr[1] = (value >> 8)  & 0xFF;
+}
+
+/***********************************************************
+ * Name: vchi_service_use
+ *
+ * Arguments: const VCHI_SERVICE_HANDLE_T handle
+ *
+ * Description: Routine to increment refcount on a service
+ *
+ * Returns: void
+ *
+ ***********************************************************/
+int32_t vchi_service_use(const VCHI_SERVICE_HANDLE_T handle)
+{
+	int32_t ret = -1;
+	SHIM_SERVICE_T *service = (SHIM_SERVICE_T *)handle;
+	if (service)
+		ret = vchiq_status_to_vchi(vchiq_use_service(service->handle));
+	return ret;
+}
+EXPORT_SYMBOL(vchi_service_use);
+
+/***********************************************************
+ * Name: vchi_service_release
+ *
+ * Arguments: const VCHI_SERVICE_HANDLE_T handle
+ *
+ * Description: Routine to decrement refcount on a service
+ *
+ * Returns: void
+ *
+ ***********************************************************/
+int32_t vchi_service_release(const VCHI_SERVICE_HANDLE_T handle)
+{
+	int32_t ret = -1;
+	SHIM_SERVICE_T *service = (SHIM_SERVICE_T *)handle;
+	if (service)
+		ret = vchiq_status_to_vchi(
+			vchiq_release_service(service->handle));
+	return ret;
+}
+EXPORT_SYMBOL(vchi_service_release);
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_util.c
@@ -0,0 +1,151 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#include "vchiq_util.h"
+
+static inline int is_pow2(int i)
+{
+	return i && !(i & (i - 1));
+}
+
+int vchiu_queue_init(VCHIU_QUEUE_T *queue, int size)
+{
+	WARN_ON(!is_pow2(size));
+
+	queue->size = size;
+	queue->read = 0;
+	queue->write = 0;
+
+	sema_init(&queue->pop, 0);
+	sema_init(&queue->push, 0);
+
+	queue->storage = kzalloc(size * sizeof(VCHIQ_HEADER_T *), GFP_KERNEL);
+	if (queue->storage == NULL) {
+		vchiu_queue_delete(queue);
+		return 0;
+	}
+	return 1;
+}
+
+void vchiu_queue_delete(VCHIU_QUEUE_T *queue)
+{
+	if (queue->storage != NULL)
+		kfree(queue->storage);
+}
+
+int vchiu_queue_is_empty(VCHIU_QUEUE_T *queue)
+{
+	return queue->read == queue->write;
+}
+
+int vchiu_queue_is_full(VCHIU_QUEUE_T *queue)
+{
+	return queue->write == queue->read + queue->size;
+}
+
+void vchiu_queue_push(VCHIU_QUEUE_T *queue, VCHIQ_HEADER_T *header)
+{
+	while (queue->write == queue->read + queue->size) {
+		if (down_interruptible(&queue->pop) != 0) {
+			flush_signals(current);
+		}
+	}
+
+	/*
+	 * Write to queue->storage must be visible after read from
+	 * queue->read
+	 */
+	smp_mb();
+
+	queue->storage[queue->write & (queue->size - 1)] = header;
+
+	/*
+	 * Write to queue->storage must be visible before write to
+	 * queue->write
+	 */
+	smp_wmb();
+
+	queue->write++;
+
+	up(&queue->push);
+}
+
+VCHIQ_HEADER_T *vchiu_queue_peek(VCHIU_QUEUE_T *queue)
+{
+	while (queue->write == queue->read) {
+		if (down_interruptible(&queue->push) != 0) {
+			flush_signals(current);
+		}
+	}
+
+	up(&queue->push); // We haven't removed anything from the queue.
+
+	/*
+	 * Read from queue->storage must be visible after read from
+	 * queue->write
+	 */
+	smp_rmb();
+
+	return queue->storage[queue->read & (queue->size - 1)];
+}
+
+VCHIQ_HEADER_T *vchiu_queue_pop(VCHIU_QUEUE_T *queue)
+{
+	VCHIQ_HEADER_T *header;
+
+	while (queue->write == queue->read) {
+		if (down_interruptible(&queue->push) != 0) {
+			flush_signals(current);
+		}
+	}
+
+	/*
+	 * Read from queue->storage must be visible after read from
+	 * queue->write
+	 */
+	smp_rmb();
+
+	header = queue->storage[queue->read & (queue->size - 1)];
+
+	/*
+	 * Read from queue->storage must be visible before write to
+	 * queue->read
+	 */
+	smp_mb();
+
+	queue->read++;
+
+	up(&queue->pop);
+
+	return header;
+}
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_util.h
@@ -0,0 +1,81 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+#ifndef VCHIQ_UTIL_H
+#define VCHIQ_UTIL_H
+
+#include <linux/types.h>
+#include <linux/semaphore.h>
+#include <linux/mutex.h>
+#include <linux/bitops.h>
+#include <linux/kthread.h>
+#include <linux/wait.h>
+#include <linux/vmalloc.h>
+#include <linux/jiffies.h>
+#include <linux/delay.h>
+#include <linux/string.h>
+#include <linux/types.h>
+#include <linux/interrupt.h>
+#include <linux/random.h>
+#include <linux/sched.h>
+#include <linux/ctype.h>
+#include <linux/uaccess.h>
+#include <linux/time.h>  /* for time_t */
+#include <linux/slab.h>
+#include <linux/vmalloc.h>
+
+#include "vchiq_if.h"
+
+typedef struct {
+	int size;
+	int read;
+	int write;
+
+	struct semaphore pop;
+	struct semaphore push;
+
+	VCHIQ_HEADER_T **storage;
+} VCHIU_QUEUE_T;
+
+extern int  vchiu_queue_init(VCHIU_QUEUE_T *queue, int size);
+extern void vchiu_queue_delete(VCHIU_QUEUE_T *queue);
+
+extern int vchiu_queue_is_empty(VCHIU_QUEUE_T *queue);
+extern int vchiu_queue_is_full(VCHIU_QUEUE_T *queue);
+
+extern void vchiu_queue_push(VCHIU_QUEUE_T *queue, VCHIQ_HEADER_T *header);
+
+extern VCHIQ_HEADER_T *vchiu_queue_peek(VCHIU_QUEUE_T *queue);
+extern VCHIQ_HEADER_T *vchiu_queue_pop(VCHIU_QUEUE_T *queue);
+
+#endif
--- /dev/null
+++ b/drivers/misc/vc04_services/interface/vchiq_arm/vchiq_version.c
@@ -0,0 +1,59 @@
+/**
+ * Copyright (c) 2010-2012 Broadcom. All rights reserved.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions
+ * are met:
+ * 1. Redistributions of source code must retain the above copyright
+ *    notice, this list of conditions, and the following disclaimer,
+ *    without modification.
+ * 2. Redistributions in binary form must reproduce the above copyright
+ *    notice, this list of conditions and the following disclaimer in the
+ *    documentation and/or other materials provided with the distribution.
+ * 3. The names of the above-listed copyright holders may not be used
+ *    to endorse or promote products derived from this software without
+ *    specific prior written permission.
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") version 2, as published by the Free
+ * Software Foundation.
+ *
+ * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS
+ * IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
+ * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
+ * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
+ * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
+ * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
+ * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
+ * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
+ * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
+ * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+#include "vchiq_build_info.h"
+#include <linux/broadcom/vc_debug_sym.h>
+
+VC_DEBUG_DECLARE_STRING_VAR( vchiq_build_hostname, "dc4-arm-01" );
+VC_DEBUG_DECLARE_STRING_VAR( vchiq_build_version, "9245b4c35b99b3870e1f7dc598c5692b3c66a6f0 (tainted)" );
+VC_DEBUG_DECLARE_STRING_VAR( vchiq_build_time,    __TIME__ );
+VC_DEBUG_DECLARE_STRING_VAR( vchiq_build_date,    __DATE__ );
+
+const char *vchiq_get_build_hostname( void )
+{
+   return vchiq_build_hostname;
+}
+
+const char *vchiq_get_build_version( void )
+{
+   return vchiq_build_version;
+}
+
+const char *vchiq_get_build_date( void )
+{
+   return vchiq_build_date;
+}
+
+const char *vchiq_get_build_time( void )
+{
+   return vchiq_build_time;
+}
