From e7b1065712e769eb4de7b9d4aa222a4531c2b8fd Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Sat, 20 Sep 2014 18:21:19 +0200
Subject: [PATCH V2] ARM: BCM5301X: select GPIOLIB as optional
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

All routers (or 99% of them) based on BCM5301X use GPIOs to control LEDs
and buttons.

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
V2: Don't select GPIOLIB. We may still think about making it default at
    some point, but we dont' really require it to boot successfully.
---
 arch/arm/mach-bcm/Kconfig | 1 +
 1 file changed, 1 insertion(+)

--- a/arch/arm/mach-bcm/Kconfig
+++ b/arch/arm/mach-bcm/Kconfig
@@ -35,6 +35,7 @@ config ARCH_BCM_MOBILE
 config ARCH_BCM_5301X
 	bool "Broadcom BCM470X / BCM5301X ARM SoC" if ARCH_MULTI_V7
 	depends on MMU
+	select ARCH_WANT_OPTIONAL_GPIOLIB
 	select ARM_GIC
 	select CACHE_L2X0
 	select HAVE_ARM_SCU if SMP
