#!/bin/sh
#
# Copyright (C) 2013-2014 OpenWrt.org
#

. /lib/functions/uci-defaults.sh
. /lib/brcm63xx.sh

case "$(brcm63xx_board_name)" in
a4001n1)
	ucidef_set_led_netdev "lan" "LAN" "A4001N1:green:eth" "eth0"
	ucidef_set_led_usbdev "usb" "USB" "A4001N1:green:3g" "1-1"
	;;
a4001n)
	ucidef_set_led_usbdev "usb" "USB" "A4001N:green:usb" "1-1"
	;;
dgnd3700v1_dgnd3800b)
	ucidef_set_led_netdev "lan" "LAN" "DGND3700v1_3800B:green:lan" "eth0.1"
	ucidef_set_led_netdev "wan" "WAN" "DGND3700v1_3800B:green:inet" "eth0.2"
	ucidef_set_led_netdev "wlan0" "WIFI2G" "DGND3700v1_3800B:green:wifi2g" "wlan0"
	ucidef_set_led_netdev "wlan1" "WIFI5G" "DGND3700v1_3800B:blue:wifi5g" "wlan1"
	ucidef_set_led_usbdev "usb1" "USB1" "DGND3700v1_3800B:green:usb-back" "1-1"
	ucidef_set_led_usbdev "usb2" "USB2" "DGND3700v1_3800B:green:usb-front" "1-2"
	;;
fast2704v2)
	ucidef_set_led_usbdev "usb" "USB" "F@ST2704V2:green:usb" "1-1"
	;;
hg553)
	ucidef_set_led_netdev "lan" "LAN" "HW553:blue:lan" "eth0"
	ucidef_set_led_usbdev "usb1" "USB1" "HW553:red:hspa" "1-1"
	ucidef_set_led_usbdev "usb2" "USB2" "HW553:blue:hspa" "1-2"
	;;
hg556a_*)
	ucidef_set_led_netdev "lan" "LAN" "HW556:red:dsl" "eth0"
	ucidef_set_led_usbdev "usb" "USB" "HW556:red:hspa" "1-2"
	;;
esac

ucidef_commit_leds

exit 0
