From 1759b172f78263de7077a2743e11f3b718682849 Mon Sep 17 00:00:00 2001
From: Tim Harvey <tharvey@gateworks.com>
Date: Tue, 22 Oct 2013 21:51:27 -0700
Subject: [PATCH 1/3] ARM: dts: disable flexcan by default

Typically nodes are disabled by default and enabled when needed.

Signed-off-by: Tim Harvey <tharvey@gateworks.com>
Signed-off-by: Shawn Guo <shawn.guo@linaro.org>
---
 arch/arm/boot/dts/imx6qdl.dtsi | 2 ++
 1 file changed, 2 insertions(+)

--- a/arch/arm/boot/dts/imx6qdl.dtsi
+++ b/arch/arm/boot/dts/imx6qdl.dtsi
@@ -331,6 +331,7 @@
 				interrupts = <0 110 0x04>;
 				clocks = <&clks 108>, <&clks 109>;
 				clock-names = "ipg", "per";
+				status = "disabled";
 			};
 
 			can2: flexcan@02094000 {
@@ -339,6 +340,7 @@
 				interrupts = <0 111 0x04>;
 				clocks = <&clks 110>, <&clks 111>;
 				clock-names = "ipg", "per";
+				status = "disabled";
 			};
 
 			gpt: gpt@02098000 {
