From 1a0086ae912b81a1e6c7213e97059c50a7bfe636 Mon Sep 17 00:00:00 2001
From: Maarten ter Huurne <maarten@treewalker.org>
Date: Sun, 6 May 2012 01:51:09 +0200
Subject: [PATCH 12/16] MIPS: JZ4740: Correct clock gate bit for DMA
 controller

Signed-off-by: Lars-Peter Clausen <lars@metafoo.de>
---
 arch/mips/jz4740/clock.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/mips/jz4740/clock.c
+++ b/arch/mips/jz4740/clock.c
@@ -687,7 +687,7 @@ static struct clk jz4740_clock_simple_cl
 	[3] = {
 		.name = "dma",
 		.parent = &jz_clk_high_speed_peripheral.clk,
-		.gate_bit = JZ_CLOCK_GATE_UART0,
+		.gate_bit = JZ_CLOCK_GATE_DMAC,
 		.ops = &jz_clk_simple_ops,
 	},
 	[4] = {
