--- a/arch/powerpc/Makefile
+++ b/arch/powerpc/Makefile
@@ -240,7 +240,9 @@ all: zImage
 
 # With make 3.82 we cannot mix normal and wildcard targets
 BOOT_TARGETS1 := zImage zImage.initrd uImage
-BOOT_TARGETS2 := zImage% dtbImage% treeImage.% cuImage.% simpleImage.% uImage.%
+BOOT_TARGETS2 := uImage.fit.% zImage% dtbImage% treeImage.% cuImage.% \
+		 simpleImage.% uImage.%
+
 
 PHONY += $(BOOT_TARGETS1) $(BOOT_TARGETS2)
 
@@ -273,6 +275,7 @@ define archhelp
   @echo '* zImage          - Build default images selected by kernel config'
   @echo '  zImage.*        - Compressed kernel image (arch/$(ARCH)/boot/zImage.*)'
   @echo '  uImage          - U-Boot native image format'
+  @echo '  uImage.fit.<dt> - U-Boot Flattened Image Tree image format'
   @echo '  cuImage.<dt>    - Backwards compatible U-Boot image for older'
   @echo '                    versions which do not support device trees'
   @echo '  dtbImage.<dt>   - zImage with an embedded device tree blob'
--- a/arch/powerpc/boot/.gitignore
+++ b/arch/powerpc/boot/.gitignore
@@ -14,6 +14,7 @@ kernel-vmlinux.strip.c
 kernel-vmlinux.strip.gz
 mktree
 uImage
+uImage.fit.*
 cuImage.*
 dtbImage.*
 *.dtb
--- a/arch/powerpc/boot/Makefile
+++ b/arch/powerpc/boot/Makefile
@@ -357,6 +357,9 @@ $(obj)/uImage.initrd.%: vmlinux $(obj)/%
 $(obj)/uImage.%: vmlinux $(obj)/%.dtb $(wrapperbits)
 	$(call if_changed,wrap,uboot-$*,,$(obj)/$*.dtb)
 
+$(obj)/uImage.fit.%: vmlinux $(obj)/%.dtb $(wrapperbits)
+	$(call if_changed,wrap,uboot.fit,,$(obj)/$*.dtb)
+
 $(obj)/cuImage.initrd.%: vmlinux $(obj)/%.dtb $(wrapperbits)
 	$(call if_changed,wrap,cuboot-$*,,$(obj)/$*.dtb,$(obj)/ramdisk.image.gz)
 
@@ -399,6 +402,7 @@ zInstall: $(CONFIGURE) $(addprefix $(obj
 
 # anything not in $(targets)
 clean-files += $(image-) $(initrd-) cuImage.* dtbImage.* treeImage.* \
+	uImage.* \
 	zImage zImage.initrd zImage.chrp zImage.coff zImage.holly \
 	zImage.miboot zImage.pmac zImage.pseries \
 	zImage.maple simpleImage.* otheros.bld *.dtb
--- a/arch/powerpc/boot/wrapper
+++ b/arch/powerpc/boot/wrapper
@@ -48,6 +48,9 @@ CROSS=
 # mkimage wrapper script
 MKIMAGE=$srctree/scripts/mkuboot.sh
 
+# script to generate an .its file for uImage.fit.* images
+MKITS=$srctree/scripts/mkits.sh
+
 # directory for object and other files used by this script
 object=arch/powerpc/boot
 objbin=$object
@@ -365,6 +368,21 @@ uboot-obs600)
     if [ -z "$cacheit" ]; then
 	rm -f "$vmz"
     fi
+    exit 0
+    ;;
+uboot.fit)
+    rm -f "$ofile"
+    ${MKITS} -A ppc -C gzip -a $membase -e $membase -v $version \
+	-d "$srctree/$dtb" -k "$srctree/$vmz" -o "$object/uImage.its"
+
+    # mkimage calls dtc for FIT images so use kernel dtc if necessary
+    export PATH=$PATH:$srctree/scripts/dtc
+
+    ${MKIMAGE} -f "$object/uImage.its" "$ofile"
+    rm "$object/uImage.its"
+    if [ -z "$cacheit" ]; then
+	rm -f "$vmz"
+    fi
     exit 0
     ;;
 esac
