From c949c0bc55571209fe6742f645b1e2eb20099591 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Tue, 17 Jun 2014 16:36:50 +0200
Subject: [PATCH 149/150] MIPS: BCM47XX: Move shared symbols to the config
 BCM47XX
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
Cc: linux-mips@linux-mips.org
Cc: Hauke Mehrtens <hauke@hauke-m.de>
Patchwork: https://patchwork.linux-mips.org/patch/7100/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/Kconfig         | 2 ++
 arch/mips/bcm47xx/Kconfig | 4 ----
 2 files changed, 2 insertions(+), 4 deletions(-)

--- a/arch/mips/Kconfig
+++ b/arch/mips/Kconfig
@@ -124,6 +124,8 @@ config BCM47XX
 	select SYS_SUPPORTS_LITTLE_ENDIAN
 	select SYS_HAS_EARLY_PRINTK
 	select EARLY_PRINTK_8250 if EARLY_PRINTK
+	select GPIOLIB
+	select LEDS_GPIO_REGISTER
 	help
 	 Support for BCM47XX based boards
 
--- a/arch/mips/bcm47xx/Kconfig
+++ b/arch/mips/bcm47xx/Kconfig
@@ -11,8 +11,6 @@ config BCM47XX_SSB
 	select SSB_DRIVER_PCICORE if PCI
 	select SSB_PCICORE_HOSTMODE if PCI
 	select SSB_DRIVER_GPIO
-	select GPIOLIB
-	select LEDS_GPIO_REGISTER
 	default y
 	help
 	 Add support for old Broadcom BCM47xx boards with Sonics Silicon Backplane support.
@@ -29,8 +27,6 @@ config BCM47XX_BCMA
 	select BCMA_HOST_PCI if PCI
 	select BCMA_DRIVER_PCI_HOSTMODE if PCI
 	select BCMA_DRIVER_GPIO
-	select GPIOLIB
-	select LEDS_GPIO_REGISTER
 	default y
 	help
 	 Add support for new Broadcom BCM47xx boards with Broadcom specific Advanced Microcontroller Bus.
