From: Sergey Ryazanov <ryazanov.s.a@gmail.com>
Date: Wed, 4 Mar 2015 05:12:10 +0300
Subject: [PATCH] ath5k: channel change fix

ath5k updates the channel pointer and after that it stops the Rx logic
and apply channel to HW. In case of channel switch, such sequence
creates a small window when a frame, which is received on the old
channel is considered as a frame received on the new one.

The most notable consequence of this situation occurs during the switch
from 2 GHz band (CCK+OFDM) to the 5GHz band (OFDM-only). Frame received
with CCK rate, e.g. beacon received at the 1mbps, causes the following
warning:

  WARNING: at ath5k/base.c:589 ath5k_tasklet_rx+0x318/0x6ec [ath5k]()
  invalid hw_rix: 1a
  [..]
  Call Trace:
  [<802656a8>] show_stack+0x48/0x70
  [<802dd92c>] warn_slowpath_common+0x88/0xbc
  [<802dd98c>] warn_slowpath_fmt+0x2c/0x38
  [<81b51be8>] ath5k_tasklet_rx+0x318/0x6ec [ath5k]
  [<8028ac64>] tasklet_action+0x8c/0xf0
  [<80075804>] __do_softirq+0x180/0x32c
  [<80196ce8>] irq_exit+0x54/0x70
  [<80041848>] ret_from_irq+0x0/0x4
  [<80182fdc>] ioread32+0x4/0xc
  [<81b4c42c>] ath5k_hw_set_sleep_clock+0x2ec/0x474 [ath5k]
  [<81b4cf28>] ath5k_hw_reset+0x50/0xeb8 [ath5k]
  [<81b50900>] ath5k_reset+0xd4/0x310 [ath5k]
  [<81b557e8>] ath5k_config+0x4c/0x104 [ath5k]
  [<80d01770>] ieee80211_hw_config+0x2f4/0x35c [mac80211]
  [<80d09aa8>] ieee80211_scan_work+0x2e4/0x414 [mac80211]
  [<8022c3f4>] process_one_work+0x28c/0x400
  [<802df8f8>] worker_thread+0x258/0x3c0
  [<801b5710>] kthread+0xe0/0xec
  [<800418a8>] ret_from_kernel_thread+0x14/0x1c

The easiest way to reproduce this warning is to run scan with dualband
NIC in noisy environments, when the channel 11 runs multiple APs. In my
tests if the APs num >= 12, the warning appears in the first few
seconds of scanning.

In order to fix this, the Rx disable code moved to a higher level and
placed before the channel pointer update. This is also makes the code a
bit more symmetrical, since we disable and enable the Rx in the same
function.

In fact, at the pointer update time new frames should not appear,
because interrupt generation at this point should already be disabled.
The next patch should address this issue.

CC: Jiri Slaby <jirislaby@gmail.com>
CC: Nick Kossifidis <mickflemm@gmail.com>
CC: Luis R. Rodriguez <mcgrof@do-not-panic.com>
Reported-by: Christophe Prevotaux <cprevotaux@nltinc.com>
Tested-by: Christophe Prevotaux <cprevotaux@nltinc.com>
Tested-by: Eric Bree <ebree@nltinc.com>
Signed-off-by: Sergey Ryazanov <ryazanov.s.a@gmail.com>
---

--- a/drivers/net/wireless/ath/ath5k/base.c
+++ b/drivers/net/wireless/ath/ath5k/base.c
@@ -2858,7 +2858,7 @@ ath5k_reset(struct ath5k_hw *ah, struct 
 {
 	struct ath_common *common = ath5k_hw_common(ah);
 	int ret, ani_mode;
-	bool fast;
+	bool fast = chan && modparam_fastchanswitch ? 1 : 0;
 
 	ATH5K_DBG(ah, ATH5K_DEBUG_RESET, "resetting\n");
 
@@ -2876,11 +2876,29 @@ ath5k_reset(struct ath5k_hw *ah, struct 
 	 * so we should also free any remaining
 	 * tx buffers */
 	ath5k_drain_tx_buffs(ah);
+
+	/* Stop PCU */
+	ath5k_hw_stop_rx_pcu(ah);
+
+	/* Stop DMA
+	 *
+	 * Note: If DMA didn't stop continue
+	 * since only a reset will fix it.
+	 */
+	ret = ath5k_hw_dma_stop(ah);
+
+	/* RF Bus grant won't work if we have pending
+	 * frames
+	 */
+	if (ret && fast) {
+		ATH5K_DBG(ah, ATH5K_DEBUG_RESET,
+			  "DMA didn't stop, falling back to normal reset\n");
+		fast = false;
+	}
+
 	if (chan)
 		ah->curchan = chan;
 
-	fast = ((chan != NULL) && modparam_fastchanswitch) ? 1 : 0;
-
 	ret = ath5k_hw_reset(ah, ah->opmode, ah->curchan, fast, skip_pcu);
 	if (ret) {
 		ATH5K_ERR(ah, "can't reset hardware (%d)\n", ret);
--- a/drivers/net/wireless/ath/ath5k/reset.c
+++ b/drivers/net/wireless/ath/ath5k/reset.c
@@ -1169,30 +1169,6 @@ ath5k_hw_reset(struct ath5k_hw *ah, enum
 	if (ah->ah_version == AR5K_AR5212)
 		ath5k_hw_set_sleep_clock(ah, false);
 
-	/*
-	 * Stop PCU
-	 */
-	ath5k_hw_stop_rx_pcu(ah);
-
-	/*
-	 * Stop DMA
-	 *
-	 * Note: If DMA didn't stop continue
-	 * since only a reset will fix it.
-	 */
-	ret = ath5k_hw_dma_stop(ah);
-
-	/* RF Bus grant won't work if we have pending
-	 * frames */
-	if (ret && fast) {
-		ATH5K_DBG(ah, ATH5K_DEBUG_RESET,
-			"DMA didn't stop, falling back to normal reset\n");
-		fast = false;
-		/* Non fatal, just continue with
-		 * normal reset */
-		ret = 0;
-	}
-
 	mode = channel->hw_value;
 	switch (mode) {
 	case AR5K_MODE_11A:
