From 0bd576e93a188fd3aab769b622fb3d35fa9bc7a7 Mon Sep 17 00:00:00 2001
From: Hauke Mehrtens <hauke@hauke-m.de>
Date: Sat, 3 May 2014 19:55:38 +0200
Subject: [PATCH 15/15] bgmac: some fixes to get bgmac work

Signed-off-by: Hauke Mehrtens <hauke@hauke-m.de>
---
 drivers/net/ethernet/broadcom/Kconfig | 2 +-
 drivers/net/phy/phy_device.c          | 2 +-
 2 files changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/net/ethernet/broadcom/Kconfig
+++ b/drivers/net/ethernet/broadcom/Kconfig
@@ -131,7 +131,7 @@ config BNX2X_SRIOV
 
 config BGMAC
 	tristate "BCMA bus GBit core support"
-	depends on BCMA_HOST_SOC && HAS_DMA && BCM47XX
+	depends on BCMA_HOST_SOC && HAS_DMA
 	select PHYLIB
 	---help---
 	  This driver supports GBit MAC and BCM4706 GBit MAC cores on BCMA bus.
--- a/drivers/net/phy/phy_device.c
+++ b/drivers/net/phy/phy_device.c
@@ -898,7 +898,7 @@ int genphy_update_link(struct phy_device
 		return status;
 
 	if ((status & BMSR_LSTATUS) == 0)
-		phydev->link = 0;
+		phydev->link = 1;
 	else
 		phydev->link = 1;
 
