From be64eb65a1b24ea9528b0fcdd652ee2068da6106 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Thu, 20 Nov 2014 20:56:27 +0100
Subject: [PATCH] MIPS: BCM47XX: Devices database update for 3.x
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 arch/mips/bcm47xx/board.c                          | 1 +
 arch/mips/include/asm/mach-bcm47xx/bcm47xx_board.h | 1 +
 2 files changed, 2 insertions(+)

--- a/arch/mips/bcm47xx/board.c
+++ b/arch/mips/bcm47xx/board.c
@@ -165,9 +165,11 @@ static const
 struct bcm47xx_board_type_list1 bcm47xx_board_list_board_id[] __initconst = {
 	{{BCM47XX_BOARD_NETGEAR_WGR614V8, "Netgear WGR614 V8"}, "U12H072T00_NETGEAR"},
 	{{BCM47XX_BOARD_NETGEAR_WGR614V9, "Netgear WGR614 V9"}, "U12H094T00_NETGEAR"},
+	{{BCM47XX_BOARD_NETGEAR_WGR614_V10, "Netgear WGR614 V10"}, "U12H139T01_NETGEAR"},
 	{{BCM47XX_BOARD_NETGEAR_WNDR3300, "Netgear WNDR3300"}, "U12H093T00_NETGEAR"},
 	{{BCM47XX_BOARD_NETGEAR_WNDR3400V1, "Netgear WNDR3400 V1"}, "U12H155T00_NETGEAR"},
 	{{BCM47XX_BOARD_NETGEAR_WNDR3400V2, "Netgear WNDR3400 V2"}, "U12H187T00_NETGEAR"},
+	{{BCM47XX_BOARD_NETGEAR_WNDR3400_V3, "Netgear WNDR3400 V3"}, "U12H208T00_NETGEAR"},
 	{{BCM47XX_BOARD_NETGEAR_WNDR3400VCNA, "Netgear WNDR3400 Vcna"}, "U12H155T01_NETGEAR"},
 	{{BCM47XX_BOARD_NETGEAR_WNDR3700V3, "Netgear WNDR3700 V3"}, "U12H194T00_NETGEAR"},
 	{{BCM47XX_BOARD_NETGEAR_WNDR4000, "Netgear WNDR4000"}, "U12H181T00_NETGEAR"},
--- a/arch/mips/include/asm/mach-bcm47xx/bcm47xx_board.h
+++ b/arch/mips/include/asm/mach-bcm47xx/bcm47xx_board.h
@@ -86,9 +86,11 @@ enum bcm47xx_board {
 
 	BCM47XX_BOARD_NETGEAR_WGR614V8,
 	BCM47XX_BOARD_NETGEAR_WGR614V9,
+	BCM47XX_BOARD_NETGEAR_WGR614_V10,
 	BCM47XX_BOARD_NETGEAR_WNDR3300,
 	BCM47XX_BOARD_NETGEAR_WNDR3400V1,
 	BCM47XX_BOARD_NETGEAR_WNDR3400V2,
+	BCM47XX_BOARD_NETGEAR_WNDR3400_V3,
 	BCM47XX_BOARD_NETGEAR_WNDR3400VCNA,
 	BCM47XX_BOARD_NETGEAR_WNDR3700V3,
 	BCM47XX_BOARD_NETGEAR_WNDR4000,
--- a/arch/mips/bcm47xx/buttons.c
+++ b/arch/mips/bcm47xx/buttons.c
@@ -327,6 +327,12 @@ bcm47xx_buttons_netgear_wndr3400v1[] __i
 };
 
 static const struct gpio_keys_button
+bcm47xx_buttons_netgear_wndr3400_v3[] __initconst = {
+	BCM47XX_GPIO_KEY(12, KEY_RESTART),
+	BCM47XX_GPIO_KEY(23, KEY_WPS_BUTTON),
+};
+
+static const struct gpio_keys_button
 bcm47xx_buttons_netgear_wndr3700v3[] __initconst = {
 	BCM47XX_GPIO_KEY(2, KEY_RFKILL),
 	BCM47XX_GPIO_KEY(3, KEY_RESTART),
@@ -557,6 +563,9 @@ int __init bcm47xx_buttons_register(void
 	case BCM47XX_BOARD_NETGEAR_WNDR3400V1:
 		err = bcm47xx_copy_bdata(bcm47xx_buttons_netgear_wndr3400v1);
 		break;
+	case BCM47XX_BOARD_NETGEAR_WNDR3400_V3:
+		err = bcm47xx_copy_bdata(bcm47xx_buttons_netgear_wndr3400_v3);
+		break;
 	case BCM47XX_BOARD_NETGEAR_WNDR3700V3:
 		err = bcm47xx_copy_bdata(bcm47xx_buttons_netgear_wndr3700v3);
 		break;
