From c38fe0f410a59e194ef5e58429658506d853f1b4 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Sat, 22 Feb 2014 22:35:58 +0100
Subject: [PATCH] ARM: dt: sun7i: Add SPI muxing options

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/sun7i-a20.dtsi | 14 ++++++++++++++
 1 file changed, 14 insertions(+)

--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -571,6 +571,20 @@
 				allwinner,drive = <3>;
 				allwinner,pull = <0>;
 			};
+
+			spi1_pins_a: spi1@0 {
+				allwinner,pins = "PI16", "PI17", "PI18", "PI19";
+				allwinner,function = "spi1";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
+
+			spi2_pins_a: spi2@0 {
+				allwinner,pins = "PC19", "PC20", "PC21", "PC22";
+				allwinner,function = "spi2";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
 		};
 
 		timer@01c20c00 {
