From 527608f06505b2a014982dd8ac7c85d97af51510 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Sat, 31 Jan 2015 17:40:58 +0100
Subject: [PATCH] bcma: disable OF code
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 drivers/bcma/main.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

diff --git a/drivers/bcma/main.c b/drivers/bcma/main.c
index c44b8d6..e64900f 100644
--- a/drivers/bcma/main.c
+++ b/drivers/bcma/main.c
@@ -124,7 +124,8 @@ static bool bcma_is_core_needed_early(u16 core_id)
 	return false;
 }
 
-#if defined(CONFIG_OF) && defined(CONFIG_OF_ADDRESS)
+/* Backported code requires OF API from kernel 3.13 at least. */
+#if 0
 static struct device_node *bcma_of_find_child_device(struct platform_device *parent,
 						     struct bcma_device *core)
 {
-- 
1.8.4.5

