#!/bin/sh
#
# Copyright (C) 2011 OpenWrt.org
#

[ -e /etc/config/network ] && exit 0

touch /etc/config/network

. /lib/functions/uci-defaults.sh

ucidef_set_interface_loopback

ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
ucidef_add_switch "switch0" "1" "1"

vlan1ports="$(nvram get vlan1ports)"
vlan2ports="$(nvram get vlan2ports)"
if echo "$vlan1ports" | egrep -q "^1 2 3 4 5" && \
   echo "$vlan2ports" | egrep -q "^0 5"; then
	ucidef_add_switch_vlan "switch0" "1" "1 2 3 4 5t"
	ucidef_add_switch_vlan "switch0" "2" "0 5t"
else
	ucidef_add_switch_vlan "switch0" "1" "0 1 2 3 5t"
	ucidef_add_switch_vlan "switch0" "2" "4 5t"
fi

uci commit network

exit 0
