--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -529,6 +529,14 @@
 			status = "disabled";
 		};
 
+		crypto: crypto-engine@01c15000 {
+			compatible = "allwinner,sun7i-a20-crypto";
+			reg = <0x01c15000 0x1000>;
+			interrupts = <0 86 4>;
+			clocks = <&ahb_gates 5>, <&ss_clk>;
+			clock-names = "ahb", "mod";
+		};
+
 		spi2: spi@01c17000 {
 			compatible = "allwinner,sun4i-a10-spi";
 			reg = <0x01c17000 0x1000>;
