From f387fb99b8478a4b50ce140dda3f1f64425c02f6 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Fri, 6 Feb 2015 09:06:55 +0000
Subject: [PATCH 108/114] BCM270x_DT: Rename the activity LED back to the
 prosaic "led0"

---
 arch/arm/boot/dts/bcm2708.dtsi | 2 +-
 arch/arm/boot/dts/bcm2709.dtsi | 2 +-
 2 files changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm/boot/dts/bcm2708.dtsi
+++ b/arch/arm/boot/dts/bcm2708.dtsi
@@ -81,7 +81,7 @@
 			compatible = "gpio-leds";
 
 			act_led: act {
-				label = "ACT";
+				label = "led0";
 				linux,default-trigger = "mmc0";
 			};
 		};
--- a/arch/arm/boot/dts/bcm2709.dtsi
+++ b/arch/arm/boot/dts/bcm2709.dtsi
@@ -81,7 +81,7 @@
 			compatible = "gpio-leds";
 
 			act_led: act {
-				label = "ACT";
+				label = "led0";
 				linux,default-trigger = "mmc0";
 			};
 		};
