From 7eb1f09ec8e25aa2fc3f6fc5fc9405d9f917d503 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Thu, 11 Dec 2014 14:14:58 +0100
Subject: [PATCH 1/2] ARM: mvebu: A385-AP: Enable the NAND controller

The A385 AP has a 1GB NAND chip. Enable it.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/armada-385-db-ap.dts | 13 +++++++++++++
 1 file changed, 13 insertions(+)

diff --git a/arch/arm/boot/dts/armada-385-db-ap.dts b/arch/arm/boot/dts/armada-385-db-ap.dts
index 3a51531eb37b..02db04867d8f 100644
--- a/arch/arm/boot/dts/armada-385-db-ap.dts
+++ b/arch/arm/boot/dts/armada-385-db-ap.dts
@@ -122,6 +122,19 @@
 				phy = <&phy0>;
 				phy-mode = "rgmii-id";
 			};
+
+			nfc: flash@d0000 {
+				status = "okay";
+				#address-cells = <1>;
+				#size-cells = <1>;
+
+				num-cs = <1>;
+				nand-ecc-strength = <4>;
+				nand-ecc-step-size = <512>;
+				marvell,nand-keep-config;
+				marvell,nand-enable-arbiter;
+				nand-on-flash-bbt;
+			};
 		};
 
 		pcie-controller {
-- 
2.2.1

