From 1bd4d8a6de5cda605e8b99fbf081be2ea2959380 Mon Sep 17 00:00:00 2001
From: Thomas Petazzoni <thomas.petazzoni@free-electrons.com>
Date: Fri, 16 Jan 2015 17:11:29 +0100
Subject: ARM: mvebu: use arm_coherent_dma_ops and re-enable hardware I/O
 coherency

Now that we have enabled automatic I/O synchronization barriers, we no
longer need any explicit barriers. We can therefore simplify
arch/arm/mach-mvebu/coherency.c by using the existing
arm_coherent_dma_ops instead of our custom mvebu_hwcc_dma_ops, and
re-enable hardware I/O coherency support.

Signed-off-by: Thomas Petazzoni <thomas.petazzoni@free-electrons.com>
[Andrew Lunn <andrew@lunn.ch>: Remove forgotten comment]
Signed-off-by: Andrew Lunn <andrew@lunn.ch>

--- a/arch/arm/mach-mvebu/coherency.c
+++ b/arch/arm/mach-mvebu/coherency.c
@@ -33,6 +33,7 @@
 #include <asm/smp_plat.h>
 #include <asm/cacheflush.h>
 #include <asm/mach/map.h>
+#include <asm/dma-mapping.h>
 #include "armada-370-xp.h"
 #include "coherency.h"
 #include "mvebu-soc-id.h"
@@ -223,59 +224,6 @@ static void __init armada_375_coherency_
 	coherency_wa_enabled = true;
 }
 
-static inline void mvebu_hwcc_sync_io_barrier(void)
-{
-	if (coherency_wa_enabled) {
-		mvebu_hwcc_armada375_sync_io_barrier_wa();
-		return;
-	}
-
-	writel(0x1, coherency_cpu_base + IO_SYNC_BARRIER_CTL_OFFSET);
-	while (readl(coherency_cpu_base + IO_SYNC_BARRIER_CTL_OFFSET) & 0x1);
-}
-
-static dma_addr_t mvebu_hwcc_dma_map_page(struct device *dev, struct page *page,
-				  unsigned long offset, size_t size,
-				  enum dma_data_direction dir,
-				  struct dma_attrs *attrs)
-{
-	if (dir != DMA_TO_DEVICE)
-		mvebu_hwcc_sync_io_barrier();
-	return pfn_to_dma(dev, page_to_pfn(page)) + offset;
-}
-
-
-static void mvebu_hwcc_dma_unmap_page(struct device *dev, dma_addr_t dma_handle,
-			      size_t size, enum dma_data_direction dir,
-			      struct dma_attrs *attrs)
-{
-	if (dir != DMA_TO_DEVICE)
-		mvebu_hwcc_sync_io_barrier();
-}
-
-static void mvebu_hwcc_dma_sync(struct device *dev, dma_addr_t dma_handle,
-			size_t size, enum dma_data_direction dir)
-{
-	if (dir != DMA_TO_DEVICE)
-		mvebu_hwcc_sync_io_barrier();
-}
-
-static struct dma_map_ops mvebu_hwcc_dma_ops = {
-	.alloc			= arm_dma_alloc,
-	.free			= arm_dma_free,
-	.mmap			= arm_dma_mmap,
-	.map_page		= mvebu_hwcc_dma_map_page,
-	.unmap_page		= mvebu_hwcc_dma_unmap_page,
-	.get_sgtable		= arm_dma_get_sgtable,
-	.map_sg			= arm_dma_map_sg,
-	.unmap_sg		= arm_dma_unmap_sg,
-	.sync_single_for_cpu	= mvebu_hwcc_dma_sync,
-	.sync_single_for_device	= mvebu_hwcc_dma_sync,
-	.sync_sg_for_cpu	= arm_dma_sync_sg_for_cpu,
-	.sync_sg_for_device	= arm_dma_sync_sg_for_device,
-	.set_dma_mask		= arm_dma_set_mask,
-};
-
 static int mvebu_hwcc_notifier(struct notifier_block *nb,
 			       unsigned long event, void *__dev)
 {
@@ -283,7 +231,7 @@ static int mvebu_hwcc_notifier(struct no
 
 	if (event != BUS_NOTIFY_ADD_DEVICE)
 		return NOTIFY_DONE;
-	set_dma_ops(dev, &mvebu_hwcc_dma_ops);
+	set_dma_ops(dev, &arm_coherent_dma_ops);
 
 	return NOTIFY_OK;
 }
@@ -405,14 +353,9 @@ static int coherency_type(void)
 	return type;
 }
 
-/*
- * As a precaution, we currently completely disable hardware I/O
- * coherency, until enough testing is done with automatic I/O
- * synchronization barriers to validate that it is a proper solution.
- */
 int coherency_available(void)
 {
-	return false;
+	return coherency_type() != COHERENCY_FABRIC_TYPE_NONE;
 }
 
 int __init coherency_init(void)
