From d14c5523653ca6ce9f1487922c8ab4e571d17b62 Mon Sep 17 00:00:00 2001
From: Hans de Goede <hdegoede@redhat.com>
Date: Tue, 11 Mar 2014 16:51:44 +0100
Subject: [PATCH] ARM: sun4i: dt: Add AXP209 support to various boards

Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun4i-a10-a1000.dts          |  9 +++++++++
 arch/arm/boot/dts/sun4i-a10-cubieboard.dts     |  9 +++++++++
 arch/arm/boot/dts/sun4i-a10-hackberry.dts      | 15 +++++++++++++++
 arch/arm/boot/dts/sun4i-a10-inet97fv2.dts      |  9 +++++++++
 arch/arm/boot/dts/sun4i-a10-mini-xplus.dts     | 15 +++++++++++++++
 arch/arm/boot/dts/sun4i-a10-olinuxino-lime.dts | 15 +++++++++++++++
 arch/arm/boot/dts/sun4i-a10-pcduino.dts        |  9 +++++++++
 7 files changed, 81 insertions(+)

--- a/arch/arm/boot/dts/sun4i-a10-a1000.dts
+++ b/arch/arm/boot/dts/sun4i-a10-a1000.dts
@@ -65,6 +65,15 @@
 			pinctrl-names = "default";
 			pinctrl-0 = <&i2c0_pins_a>;
 			status = "okay";
+
+			axp: axp20x@34 {
+				reg = <0x34>;
+				interrupts = <0>;
+
+				axp,system-power-controller;
+
+				/include/ "x-powers-axp209.dtsi"
+			};
 		};
 	};
 
--- a/arch/arm/boot/dts/sun4i-a10-cubieboard.dts
+++ b/arch/arm/boot/dts/sun4i-a10-cubieboard.dts
@@ -88,6 +88,15 @@
 			pinctrl-names = "default";
 			pinctrl-0 = <&i2c0_pins_a>;
 			status = "okay";
+
+			axp: axp20x@34 {
+				reg = <0x34>;
+				interrupts = <0>;
+
+				axp,system-power-controller;
+
+				/include/ "x-powers-axp209.dtsi"
+			};
 		};
 
 		i2c1: i2c@01c2b000 {
--- a/arch/arm/boot/dts/sun4i-a10-hackberry.dts
+++ b/arch/arm/boot/dts/sun4i-a10-hackberry.dts
@@ -82,6 +82,21 @@
 			pinctrl-0 = <&uart0_pins_a>;
 			status = "okay";
 		};
+
+		i2c0: i2c@01c2ac00 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c0_pins_a>;
+			status = "okay";
+
+			axp: axp20x@34 {
+				reg = <0x34>;
+				interrupts = <0>;
+
+				axp,system-power-controller;
+
+				/include/ "x-powers-axp209.dtsi"
+			};
+		};
 	};
 
 	regulators {
--- a/arch/arm/boot/dts/sun4i-a10-mini-xplus.dts
+++ b/arch/arm/boot/dts/sun4i-a10-mini-xplus.dts
@@ -55,6 +55,21 @@
 			pinctrl-0 = <&uart0_pins_a>;
 			status = "okay";
 		};
+
+		i2c0: i2c@01c2ac00 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c0_pins_a>;
+			status = "okay";
+
+			axp: axp20x@34 {
+				reg = <0x34>;
+				interrupts = <0>;
+
+				axp,system-power-controller;
+
+				/include/ "x-powers-axp209.dtsi"
+			};
+		};
 	};
 
 	reg_usb1_vbus: usb1-vbus {
--- a/arch/arm/boot/dts/sun4i-a10-olinuxino-lime.dts
+++ b/arch/arm/boot/dts/sun4i-a10-olinuxino-lime.dts
@@ -90,6 +90,21 @@
 			pinctrl-0 = <&uart0_pins_a>;
 			status = "okay";
 		};
+
+		i2c0: i2c@01c2ac00 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c0_pins_a>;
+			status = "okay";
+
+			axp: axp20x@34 {
+				reg = <0x34>;
+				interrupts = <0>;
+
+				axp,system-power-controller;
+
+				/include/ "x-powers-axp209.dtsi"
+			};
+		};
 	};
 
 	leds {
--- a/arch/arm/boot/dts/sun4i-a10-pcduino.dts
+++ b/arch/arm/boot/dts/sun4i-a10-pcduino.dts
@@ -74,6 +74,15 @@
 			pinctrl-names = "default";
 			pinctrl-0 = <&i2c0_pins_a>;
 			status = "okay";
+
+			axp: axp20x@34 {
+				reg = <0x34>;
+				interrupts = <0>;
+
+				axp,system-power-controller;
+
+				/include/ "x-powers-axp209.dtsi"
+			};
 		};
 	};
 
