From eb1075cc48d3c315c7403822c33da9588ab76492 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Wed, 14 Jan 2015 08:33:25 +0100
Subject: [PATCH] ARM: BCM5310X: Enable earlyprintk on tested devices
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dts  | 2 +-
 arch/arm/boot/dts/bcm4708-netgear-r6250.dts        | 2 +-
 arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts        | 2 +-
 arch/arm/boot/dts/bcm47081-buffalo-wzr-600dhp2.dts | 2 +-
 4 files changed, 4 insertions(+), 4 deletions(-)

diff --git a/arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dts b/arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dts
index 5fc0fae..fcb17c6 100644
--- a/arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dts
+++ b/arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dts
@@ -16,7 +16,7 @@
 	model = "Buffalo WZR-1750DHP (BCM4708)";
 
 	chosen {
-		bootargs = "console=ttyS0,115200";
+		bootargs = "console=ttyS0,115200 earlyprintk";
 	};
 
 	memory {
diff --git a/arch/arm/boot/dts/bcm4708-netgear-r6250.dts b/arch/arm/boot/dts/bcm4708-netgear-r6250.dts
index 4ed7de1..05e80b1 100644
--- a/arch/arm/boot/dts/bcm4708-netgear-r6250.dts
+++ b/arch/arm/boot/dts/bcm4708-netgear-r6250.dts
@@ -16,7 +16,7 @@
 	model = "Netgear R6250 V1 (BCM4708)";
 
 	chosen {
-		bootargs = "console=ttyS0,115200";
+		bootargs = "console=ttyS0,115200 earlyprintk";
 	};
 
 	memory {
diff --git a/arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts b/arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts
index fb76378..5dc50e1 100644
--- a/arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts
+++ b/arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts
@@ -16,7 +16,7 @@
 	model = "Asus RT-N18U (BCM47081)";
 
 	chosen {
-		bootargs = "console=ttyS0,115200";
+		bootargs = "console=ttyS0,115200 earlyprintk";
 	};
 
 	memory {
diff --git a/arch/arm/boot/dts/bcm47081-buffalo-wzr-600dhp2.dts b/arch/arm/boot/dts/bcm47081-buffalo-wzr-600dhp2.dts
index bbb414f..20903a5 100644
--- a/arch/arm/boot/dts/bcm47081-buffalo-wzr-600dhp2.dts
+++ b/arch/arm/boot/dts/bcm47081-buffalo-wzr-600dhp2.dts
@@ -16,7 +16,7 @@
 	model = "Buffalo WZR-600DHP2 (BCM47081)";
 
 	chosen {
-		bootargs = "console=ttyS0,115200";
+		bootargs = "console=ttyS0,115200 earlyprintk";
 	};
 
 	memory {
--- a/arch/arm/boot/dts/bcm47081-buffalo-wzr-900dhp.dts
+++ b/arch/arm/boot/dts/bcm47081-buffalo-wzr-900dhp.dts
@@ -16,7 +16,7 @@
 	model = "Buffalo WZR-900DHP (BCM47081)";
 
 	chosen {
-		bootargs = "console=ttyS0,115200";
+		bootargs = "console=ttyS0,115200 earlyprintk";
 	};
 
 	memory {
-- 
1.8.4.5

