--- a/drivers/gpio/Kconfig
+++ b/drivers/gpio/Kconfig
@@ -905,4 +905,12 @@ config GPIO_VIPERBOARD
           River Tech's viperboard.h for detailed meaning
           of the module parameters.
 
+comment "Other GPIO expanders"
+
+config GPIO_NXP_74HC153
+	tristate "NXP 74HC153 Dual 4-input multiplexer"
+	help
+	  Platform driver for NXP 74HC153 Dual 4-input Multiplexer. This
+	  provides a GPIO interface supporting input mode only.
+
 endif
--- a/drivers/gpio/Makefile
+++ b/drivers/gpio/Makefile
@@ -60,6 +60,7 @@ obj-$(CONFIG_GPIO_MSM_V2)	+= gpio-msm-v2
 obj-$(CONFIG_GPIO_MVEBU)        += gpio-mvebu.o
 obj-$(CONFIG_GPIO_MXC)		+= gpio-mxc.o
 obj-$(CONFIG_GPIO_MXS)		+= gpio-mxs.o
+obj-$(CONFIG_GPIO_NXP_74HC153)	+= gpio-nxp-74hc153.o
 obj-$(CONFIG_GPIO_OCTEON)	+= gpio-octeon.o
 obj-$(CONFIG_GPIO_OMAP)		+= gpio-omap.o
 obj-$(CONFIG_GPIO_PCA953X)	+= gpio-pca953x.o
