From b08c144e3a1089cdb725e393fa4f68f83a73e31b Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Sat, 7 Feb 2015 18:04:10 +0100
Subject: [PATCH] watchdog: bcm47xx_wdt.c: allow enabling on BCM5301X arch
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

BCM5301X (ARCH_BCM_5301X) is a new Broadcom architecture using the same
SoC bus driver (bcma) as BCM47XX but based on ARM instead of MIPS.

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
Reviewed-by: Guenter Roeck <linux@roeck-us.net>
Signed-off-by: Wim Van Sebroeck <wim@iguana.be>
---
 drivers/watchdog/Kconfig | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/watchdog/Kconfig b/drivers/watchdog/Kconfig
index 2aaef7b..ca6c949 100644
--- a/drivers/watchdog/Kconfig
+++ b/drivers/watchdog/Kconfig
@@ -1113,7 +1113,7 @@ config ATH79_WDT
 
 config BCM47XX_WDT
 	tristate "Broadcom BCM47xx Watchdog Timer"
-	depends on BCM47XX
+	depends on BCM47XX || ARCH_BCM_5301X
 	select WATCHDOG_CORE
 	help
 	  Hardware driver for the Broadcom BCM47xx Watchdog Timer.
-- 
1.8.4.5

