From 15f4d895578f02cbaed10b0f5f6853b873aba10b Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Wed, 20 Jan 2016 13:12:19 +0100
Subject: [PATCH 031/102] dt-bindings: ARM: Mediatek: add MT2701/7623 string
 to the PMIC wrapper doc

Signed-off-by: John Crispin <blogic@openwrt.org>
Acked-by: Rob Herring <robh@kernel.org>
Cc: devicetree@vger.kernel.org
---
 Documentation/devicetree/bindings/soc/mediatek/pwrap.txt |    1 +
 1 file changed, 1 insertion(+)

--- a/Documentation/devicetree/bindings/soc/mediatek/pwrap.txt
+++ b/Documentation/devicetree/bindings/soc/mediatek/pwrap.txt
@@ -18,6 +18,7 @@ IP Pairing
 
 Required properties in pwrap device node.
 - compatible:
+	"mediatek,mt2701-pwrap" for MT2701/7623 SoCs
 	"mediatek,mt8135-pwrap" for MT8135 SoCs
 	"mediatek,mt8173-pwrap" for MT8173 SoCs
 - interrupts: IRQ for pwrap in SOC
