From 046f7b291b867d22eb2ba03b83201363acc89551 Mon Sep 17 00:00:00 2001
From: jochenberger <fooberger@gmail.com>
Date: Thu, 7 Apr 2016 21:38:46 +0200
Subject: [PATCH 236/381] Enable hid-betopff module

Add force feedback support for Betop based devices
https://github.com/raspberrypi/linux/blob/rpi-4.1.y/drivers/hid/hid-betopff.c
---
 arch/arm/configs/bcm2709_defconfig | 1 +
 arch/arm/configs/bcmrpi_defconfig  | 1 +
 2 files changed, 2 insertions(+)

--- a/arch/arm/configs/bcm2709_defconfig
+++ b/arch/arm/configs/bcm2709_defconfig
@@ -867,6 +867,7 @@ CONFIG_HID_A4TECH=m
 CONFIG_HID_ACRUX=m
 CONFIG_HID_APPLE=m
 CONFIG_HID_BELKIN=m
+CONFIG_HID_BETOP_FF=m
 CONFIG_HID_CHERRY=m
 CONFIG_HID_CHICONY=m
 CONFIG_HID_CYPRESS=m
--- a/arch/arm/configs/bcmrpi_defconfig
+++ b/arch/arm/configs/bcmrpi_defconfig
@@ -859,6 +859,7 @@ CONFIG_HID_A4TECH=m
 CONFIG_HID_ACRUX=m
 CONFIG_HID_APPLE=m
 CONFIG_HID_BELKIN=m
+CONFIG_HID_BETOP_FF=m
 CONFIG_HID_CHERRY=m
 CONFIG_HID_CHICONY=m
 CONFIG_HID_CYPRESS=m
