From 4c5747a390acc9d1da3b332507c8bae7a8ddfc48 Mon Sep 17 00:00:00 2001
From: Kamal Dasu <kdasu.kdev@gmail.com>
Date: Fri, 20 Jan 2017 14:25:51 -0500
Subject: [PATCH] mtd: spi-nor: Add support for gd25q16

Add GigaDevice GD25Q16 (16M-bit) to supported list.

Signed-off-by: Kamal Dasu <kdasu.kdev@gmail.com>
Acked-by: Marek Vasut <marek.vasut@gmail.com>
Signed-off-by: Cyrille Pitchen <cyrille.pitchen@atmel.com>
---
 drivers/mtd/spi-nor/spi-nor.c | 5 +++++
 1 file changed, 5 insertions(+)

--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -971,6 +971,11 @@ static const struct flash_info spi_nor_i
 
 	/* GigaDevice */
 	{
+		"gd25q16", INFO(0xc84015, 0, 64 * 1024,  32,
+			SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ |
+			SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB)
+	},
+	{
 		"gd25q32", INFO(0xc84016, 0, 64 * 1024,  64,
 			SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ |
 			SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB)
