From 40e3b847bff70edc28c5290d209e531da6f9e534 Mon Sep 17 00:00:00 2001
From: Christian Lamparter <chunkeey@googlemail.com>
Date: Fri, 25 Aug 2017 15:47:23 +0200
Subject: [PATCH 10/25] crypto: crypto4xx - replace crypto4xx_dev's
 scatter_buffer_size with constant

scatter_buffer_size is always set to PPC4XX_SD_BUFFER_SIZE.
I don't think there's any point in keeping the variable
around.

Signed-off-by: Christian Lamparter <chunkeey@googlemail.com>
Signed-off-by: Herbert Xu <herbert@gondor.apana.org.au>
---
 drivers/crypto/amcc/crypto4xx_core.c | 7 +++----
 drivers/crypto/amcc/crypto4xx_core.h | 1 -
 2 files changed, 3 insertions(+), 5 deletions(-)

--- a/drivers/crypto/amcc/crypto4xx_core.c
+++ b/drivers/crypto/amcc/crypto4xx_core.c
@@ -396,10 +396,9 @@ static u32 crypto4xx_build_sdr(struct cr
 	if (!dev->sdr)
 		return -ENOMEM;
 
-	dev->scatter_buffer_size = PPC4XX_SD_BUFFER_SIZE;
 	dev->scatter_buffer_va =
 		dma_alloc_coherent(dev->core_dev->device,
-			dev->scatter_buffer_size * PPC4XX_NUM_SD,
+			PPC4XX_SD_BUFFER_SIZE * PPC4XX_NUM_SD,
 			&dev->scatter_buffer_pa, GFP_ATOMIC);
 	if (!dev->scatter_buffer_va) {
 		dma_free_coherent(dev->core_dev->device,
@@ -412,7 +411,7 @@ static u32 crypto4xx_build_sdr(struct cr
 
 	for (i = 0; i < PPC4XX_NUM_SD; i++) {
 		sd_array[i].ptr = dev->scatter_buffer_pa +
-				  dev->scatter_buffer_size * i;
+				  PPC4XX_SD_BUFFER_SIZE * i;
 	}
 
 	return 0;
@@ -427,7 +426,7 @@ static void crypto4xx_destroy_sdr(struct
 
 	if (dev->scatter_buffer_va)
 		dma_free_coherent(dev->core_dev->device,
-				  dev->scatter_buffer_size * PPC4XX_NUM_SD,
+				  PPC4XX_SD_BUFFER_SIZE * PPC4XX_NUM_SD,
 				  dev->scatter_buffer_va,
 				  dev->scatter_buffer_pa);
 }
--- a/drivers/crypto/amcc/crypto4xx_core.h
+++ b/drivers/crypto/amcc/crypto4xx_core.h
@@ -87,7 +87,6 @@ struct crypto4xx_device {
 					program ce sdr_base_register */
 	void *scatter_buffer_va;
 	dma_addr_t scatter_buffer_pa;
-	u32 scatter_buffer_size;
 
 	void *shadow_sa_pool;		/* pool of memory for sa in pd_uinfo */
 	dma_addr_t shadow_sa_pool_pa;
