From 9e638878dd33652b34e51746d369afba6103d77e Mon Sep 17 00:00:00 2001
From: Scott Ellis <scott@jumpnowtek.com>
Date: Thu, 23 Feb 2017 11:56:20 -0500
Subject: [PATCH] Add ads1015 driver to config

---
 arch/arm/configs/bcm2709_defconfig | 3 ++-
 arch/arm/configs/bcmrpi_defconfig  | 3 ++-
 2 files changed, 4 insertions(+), 2 deletions(-)

--- a/arch/arm/configs/bcm2709_defconfig
+++ b/arch/arm/configs/bcm2709_defconfig
@@ -653,6 +653,7 @@ CONFIG_HWMON=m
 CONFIG_SENSORS_LM75=m
 CONFIG_SENSORS_SHT21=m
 CONFIG_SENSORS_SHTC1=m
+CONFIG_SENSORS_ADS1015=m
 CONFIG_SENSORS_INA2XX=m
 CONFIG_THERMAL=y
 CONFIG_THERMAL_BCM2835=y
@@ -833,9 +834,9 @@ CONFIG_VIDEO_OV7640=m
 CONFIG_VIDEO_MT9V011=m
 CONFIG_DRM=m
 CONFIG_DRM_LOAD_EDID_FIRMWARE=y
+CONFIG_DRM_UDL=m
 CONFIG_DRM_PANEL_SIMPLE=m
 CONFIG_DRM_PANEL_RASPBERRYPI_TOUCHSCREEN=m
-CONFIG_DRM_UDL=m
 CONFIG_DRM_VC4=m
 CONFIG_FB=y
 CONFIG_FB_BCM2708=y
--- a/arch/arm/configs/bcmrpi_defconfig
+++ b/arch/arm/configs/bcmrpi_defconfig
@@ -647,6 +647,7 @@ CONFIG_HWMON=m
 CONFIG_SENSORS_LM75=m
 CONFIG_SENSORS_SHT21=m
 CONFIG_SENSORS_SHTC1=m
+CONFIG_SENSORS_ADS1015=m
 CONFIG_SENSORS_INA2XX=m
 CONFIG_THERMAL=y
 CONFIG_THERMAL_BCM2835=y
@@ -827,9 +828,9 @@ CONFIG_VIDEO_OV7640=m
 CONFIG_VIDEO_MT9V011=m
 CONFIG_DRM=m
 CONFIG_DRM_LOAD_EDID_FIRMWARE=y
+CONFIG_DRM_UDL=m
 CONFIG_DRM_PANEL_SIMPLE=m
 CONFIG_DRM_PANEL_RASPBERRYPI_TOUCHSCREEN=m
-CONFIG_DRM_UDL=m
 CONFIG_DRM_VC4=m
 CONFIG_FB=y
 CONFIG_FB_BCM2708=y
