From 3e2cb84235e904f0c127d34705852ba7893ec9ae Mon Sep 17 00:00:00 2001
From: Matthias Reichl <hias@horus.com>
Date: Sun, 22 Jan 2017 12:49:36 +0100
Subject: [PATCH] BCM270x DT: expose 3.3V and 5V system rails

Signed-off-by: Matthias Reichl <hias@horus.com>
---
 arch/arm/boot/dts/bcm270x.dtsi | 16 ++++++++++++++++
 1 file changed, 16 insertions(+)

--- a/arch/arm/boot/dts/bcm270x.dtsi
+++ b/arch/arm/boot/dts/bcm270x.dtsi
@@ -138,4 +138,20 @@
 			status = "disabled";
 		};
 	};
+
+	vdd_5v0_reg: fixedregulator_5v0 {
+		compatible = "regulator-fixed";
+		regulator-name = "5v0";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		regulator-always-on;
+	};
+
+	vdd_3v3_reg: fixedregulator_3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-always-on;
+	};
 };
