From f4eb27ab7c9893a65fd414451459899cdd6334a7 Mon Sep 17 00:00:00 2001
From: arokux <arokux@gmail.com>
Date: Tue, 24 Sep 2013 20:02:39 +0200
Subject: [PATCH] ARM: sun5i: dt: Add bindings for USB Host clocks

---
 arch/arm/boot/dts/sun5i-a13.dtsi | 8 ++++++++
 1 file changed, 8 insertions(+)

diff --git a/arch/arm/boot/dts/sun5i-a13.dtsi b/arch/arm/boot/dts/sun5i-a13.dtsi
index 9ac706a..aad270c 100644
--- a/arch/arm/boot/dts/sun5i-a13.dtsi
+++ b/arch/arm/boot/dts/sun5i-a13.dtsi
@@ -90,6 +90,14 @@
 			clock-output-names = "pll6_sata", "pll6_other", "pll6";
 		};
 
+		usb:usb@0x01c200cc {
+			#clock-cells = <1>;
+			compatible = "allwinner,sun5i-usb-gates-clk";
+			reg = <0x01c200cc 0x4>;
+			clocks = <&pll6 1>;
+			clock-output-names = "usb_ohci0", "usb_phy";
+		};
+
 		/* dummy is 200M */
 		cpu: cpu@01c20054 {
 			#clock-cells = <0>;
-- 
1.8.4

