From 6afd5cb1f92a1965ffa3c0f304f95ab19b49fa84 Mon Sep 17 00:00:00 2001
From: Jyri Sarha <jsarha@ti.com>
Date: Thu, 12 Sep 2013 14:37:08 +0300
Subject: [PATCH 218/752] ASoC: tlv320aic3x: Add codec pins to DT bindings
 document

Add list of codec pins to tlv320aic3x DT bindings document.

Signed-off-by: Jyri Sarha <jsarha@ti.com>
---
 .../devicetree/bindings/sound/tlv320aic3x.txt       |   19 +++++++++++++++++++
 1 file changed, 19 insertions(+)

--- a/Documentation/devicetree/bindings/sound/tlv320aic3x.txt
+++ b/Documentation/devicetree/bindings/sound/tlv320aic3x.txt
@@ -27,6 +27,25 @@ Optional properties:
 - AVDD-supply, IOVDD-supply, DRVDD-supply, DVDD-supply : power supplies for the
   device as covered in Documentation/devicetree/bindings/regulator/regulator.txt
 
+CODEC output pins:
+  * LLOUT
+  * RLOUT
+  * MONO_LOUT
+  * HPLOUT
+  * HPROUT
+  * HPLCOM
+  * HPRCOM
+
+CODEC input pins:
+  * MIC3L
+  * MIC3R
+  * LINE1L
+  * LINE2L
+  * LINE1R
+  * LINE2R
+
+The pins can be used in referring sound node's audio-routing property.
+
 Example:
 
 tlv320aic3x: tlv320aic3x@1b {
