From eb92a178eceae4e5d18bbb442b8e44cb88457d60 Mon Sep 17 00:00:00 2001
From: Joseph Kortje <jpktech@rogers.com>
Date: Wed, 28 Oct 2009 21:25:57 -0400
Subject: [PATCH] [ARM] Gumstix Verdex LCD config options

add options to Kconfig for Verdex LCD support

Signed-off-by: Bobby Powers <bobbypowers@gmail.com>
---
 drivers/video/Kconfig |   31 +++++++++++++++++++++++++++++++
 1 files changed, 31 insertions(+), 0 deletions(-)

--- a/drivers/video/Kconfig
+++ b/drivers/video/Kconfig
@@ -1905,6 +1905,37 @@ config FB_PXA
 	  say M here and read <file:Documentation/kbuild/modules.txt>.
 
 	  If unsure, say N.
+choice
+	depends on FB_PXA
+	prompt "LCD Panel"
+	default FB_PXA_SAMSUNG_LTE430WQ_F0C
+
+config FB_PXA_ALPS_CDOLLAR
+	boolean "Chris Dollar's ALPS screen"
+	---help---
+	  Enable definitions (over-ridable on the kernel command line if
+	  "PXA LCD command line parameters" is also selected) for an ALPS
+	  screen which Chris Dollar uses
+
+config FB_PXA_SHARP_LQ043_PSP
+	boolean "SHARP LQ043... series"
+	---help---
+	  Enable definitions (over-ridable on the kernel command line if
+	  "PXA LCD command line parameters" is also selected) for a SHARP
+	  LQ043... screen, such as the one used by the PSP.  These screens are
+	  the ones normally sold by gumstix with its boards.
+
+config FB_PXA_SAMSUNG_LTE430WQ_F0C
+	boolean "Samsung LTE430WQ-F0C (standard gumstix LCD)"
+	---help---
+	  Enable definitions for a Samsung LTE430WQ-F0C LCD panel, such as the ones resold
+	  by gumstix for use with their "LCD-Ready" boards.
+
+config FB_PXA_NONEOFTHEABOVE
+	boolean "None of the above"
+
+endchoice
+
 
 config FB_PXA_OVERLAY
 	bool "Support PXA27x/PXA3xx Overlay(s) as framebuffer"
