From 6804142b47f2634b0657e4dfcec7a34e982b6ddb Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Wed, 10 Sep 2014 22:29:21 +0200
Subject: [PATCH 10/36] MIPS: lantiq: export soc type
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
---
 arch/mips/include/asm/mach-lantiq/lantiq.h |    2 ++
 arch/mips/lantiq/prom.c                    |    5 +++++
 2 files changed, 7 insertions(+)

--- a/arch/mips/include/asm/mach-lantiq/lantiq.h
+++ b/arch/mips/include/asm/mach-lantiq/lantiq.h
@@ -48,6 +48,8 @@ extern struct clk *clk_get_ppe(void);
 extern unsigned char ltq_boot_select(void);
 /* find out what caused the last cpu reset */
 extern int ltq_reset_cause(void);
+/* find out the soc type */
+extern int ltq_soc_type(void);
 
 #define IOPORT_RESOURCE_START	0x10000000
 #define IOPORT_RESOURCE_END	0xffffffff
--- a/arch/mips/lantiq/prom.c
+++ b/arch/mips/lantiq/prom.c
@@ -36,6 +36,11 @@ const char *get_system_type(void)
 	return soc_info.sys_type;
 }
 
+int ltq_soc_type(void)
+{
+	return soc_info.type;
+}
+
 void prom_free_prom_memory(void)
 {
 }
